(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer false)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerb/")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad11)")
  (net 12 "Net-(J1-Pad13)")
  (net 13 "Net-(J1-Pad14)")
  (net 14 "Net-(J1-Pad15)")
  (net 15 "Net-(J1-Pad16)")
  (net 16 "Net-(J1-Pad17)")
  (net 17 "+5V")
  (net 18 "GND")
  (net 19 "/D8")
  (net 20 "/D7")
  (net 21 "/D6")
  (net 22 "/D5")
  (net 23 "/D4")
  (net 24 "/D3")
  (net 25 "/D2")
  (net 26 "/D1")
  (net 27 "/SRQ")
  (net 28 "/ATN")
  (net 29 "/EOI")
  (net 30 "/DAV")
  (net 31 "/NRFD")
  (net 32 "/NDAC")
  (net 33 "/IFC")
  (net 34 "/REN")
  (net 35 "/RESET")
  (net 36 "unconnected-(U1-Pad6)")
  (net 37 "unconnected-(U3-Pad19)")
  (net 38 "unconnected-(U3-Pad22)")
  (net 39 "/ISP_MISO")
  (net 40 "/ISP_SCK")
  (net 41 "/ISP_MOSI")
  (net 42 "Net-(R5-Pad2)")
  (net 43 "Net-(R7-Pad2)")
  (net 44 "Net-(C5-Pad1)")
  (net 45 "Net-(J4-Pad3)")
  (net 46 "/ETH_MOSI")
  (net 47 "/ETH_SCLK")
  (net 48 "/ETH_MISO")
  (net 49 "+3V3")
  (net 50 "/RXD_GPIB")
  (net 51 "/TXD_GPIB")
  (net 52 "/TXD_USB")
  (net 53 "/RXD_USB")
  (net 54 "unconnected-(U6-Pad9)")
  (net 55 "unconnected-(U6-Pad10)")
  (net 56 "unconnected-(U6-Pad11)")
  (net 57 "unconnected-(U6-Pad12)")
  (net 58 "unconnected-(U6-Pad13)")
  (net 59 "unconnected-(U6-Pad14)")
  (net 60 "unconnected-(U6-Pad15)")
  (net 61 "Net-(R9-Pad2)")
  (net 62 "Net-(U3-Pad30)")
  (net 63 "unconnected-(U4-Pad11)")
  (net 64 "/ETH_RST")
  (net 65 "/ETH_CS")
  (net 66 "Net-(C4-Pad1)")
  (net 67 "Net-(C8-Pad1)")
  (net 68 "Net-(C9-Pad1)")
  (net 69 "Net-(J4-Pad2)")
  (net 70 "/GPIB_TRIG")
  (net 71 "/TE")
  (net 72 "Net-(C10-Pad1)")
  (net 73 "Net-(C11-Pad1)")
  (net 74 "Net-(J5-Pad2)")
  (net 75 "Net-(C12-Pad1)")
  (net 76 "Net-(J3-Pad1)")
  (net 77 "Net-(J5-Pad1)")
  (net 78 "/EXT_TRIG")
  (net 79 "Net-(R15-Pad2)")
  (net 80 "Net-(R12-Pad1)")
  (net 81 "Net-(R12-Pad2)")
  (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B)
    (at 30 -4)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-02A example for new part number: 22-27-2021, 2 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "PN" "NS25-W2P")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J3" (at 1.27 -4.12) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 1.27 4.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -2.22) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.1436781609)
      (net 76 "Net-(J3-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 129 -3)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "link" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 3 -25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "link" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 4) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "j_lib:logo_rpg7x9" (layer "F.Cu")
    (tedit 61CE1C18)
    (at 42.8 -5.2)
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "link" "DNP")
    (attr board_only exclude_from_pos_files)
    (fp_text reference "LOGO1" (at 0.956014 12.7) (layer "F.SilkS") hide)
    (fp_text value "PCB logo" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "j_lib:CENTR_24P_F" (layer "F.Cu")
    (tedit 61E21BFB)
    (at 98 -11 180)
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "link" "https://www.aliexpress.com/item/32795413098.html")
    (attr through_hole)
    (fp_text reference "J1" (at 14.2 6.4 unlocked) (layer "F.SilkS"))
    (fp_text value "Centronics 24, socket" (at 0 13.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -11.88 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at -9.72 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle (at -7.56 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at -5.4 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle (at -3.24 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle (at -1.08 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 6 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle (at 1.08 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "Net-(J1-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle (at 3.24 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 8 "Net-(J1-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle (at 5.4 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle (at 7.56 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle (at 9.72 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle (at 11.88 2.15 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle (at -11.88 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle (at -9.72 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle (at -7.56 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle (at -5.4 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad16)") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole circle (at -3.24 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad17)") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole circle (at -1.08 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" thru_hole circle (at 1.08 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" thru_hole circle (at 3.24 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" thru_hole circle (at 5.4 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" thru_hole circle (at 7.56 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" thru_hole circle (at 9.72 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" thru_hole circle (at 11.88 -2.14 180) (size 1.4 1.4) (drill 0.9) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" thru_hole circle (at 23.4 0 180) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
    (pad "26" thru_hole circle (at -23.4 0 180) (size 6 6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 3 -3)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "link" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 129 -25)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "link" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 4) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 12.36 -22.7475 90)
    (descr "Through hole IDC box header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x08 2.54mm double row")
    (property "PN" "T821-1-16-S1")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J5" (at -4.3475 -4.16 180) (layer "F.SilkS"))
    (fp_text value "IDC_16" (at 1.27 23.88 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 8.89) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 77 "Net-(J5-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 "Net-(J5-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 52 "/TXD_USB") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "/RXD_USB") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 51 "/TXD_GPIB") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/RXD_GPIB") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 64 "/ETH_RST") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "+5V") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/ETH_CS") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle locked (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "+3V3") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/ETH_MISO") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle locked (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "+3V3") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/ETH_MOSI") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle locked (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/ETH_SCLK") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle locked (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 62 -10.54)
    (descr "Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x03 2.54mm double row")
    (property "PN" "75869-331LF")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J2" (at 1.27 -6.1) (layer "F.SilkS"))
    (fp_text value "IDC_6pin" (at 1.27 11.18) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 39 "/ISP_MISO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "+5V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "/ISP_SCK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/ISP_MOSI") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "/RESET") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_USB:USB_B_Lumberg_2411_02_Horizontal" (layer "F.Cu")
    (tedit 5E6EAC30)
    (at 20 -9 -90)
    (descr "USB 2.0 receptacle type B, horizontal version, through-hole, https://downloads.lumberg.com/datenblaetter/en/2411_02.pdf")
    (tags "USB B receptacle horizontal through-hole")
    (property "PN" "TUEB4F2D0B")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J4" (at 1.6 -6 180) (layer "F.SilkS"))
    (fp_text value "USB_B" (at 7.05 10.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 1.25 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 67 "Net-(C8-Pad1)") (pinfunction "VBUS") (pintype "power_out"))
    (pad "2" thru_hole circle locked (at 0 2.5) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 69 "Net-(J4-Pad2)") (pinfunction "D-") (pintype "bidirectional"))
    (pad "3" thru_hole circle locked (at 2 2.5) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 45 "Net-(J4-Pad3)") (pinfunction "D+") (pintype "bidirectional"))
    (pad "4" thru_hole circle locked (at 2 0) (size 1.6 1.6) (drill 0.95) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "5" thru_hole circle locked (at 4.86 -4.75) (size 4 4) (drill 2.3) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 4.86 7.25) (size 4 4) (drill 2.3) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_USB.3dshapes/USB_B_Lumberg_2411_02_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 9 -11.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A220JXACW1BC")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C11" (at 0.1 -2.4 180) (layer "B.SilkS"))
    (fp_text value "22p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 73 "Net-(C11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 121 -19.8 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1203")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R5" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "12k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 42 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-7132-28_AVX-C_Pad2.72x3.50mm_HandSolder" (layer "B.Cu")
    (tedit 5EBA9318)
    (at 52.6 -9.2 -90)
    (descr "Tantalum Capacitor SMD AVX-C (7132-28 Metric), IPC_7351 nominal, (Body size from: http://datasheets.avx.com/F72-F75.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C107K010AT")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C1" (at -0.4 3.4 180) (layer "B.SilkS"))
    (fp_text value "100u" (at 0 -2.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.8625 0 270) (size 2.725 3.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.09174311927)
      (net 49 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.8625 0 270) (size 2.725 3.5) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.09174311927)
      (net 18 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7132-28_AVX-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMB" (layer "B.Cu")
    (tedit 58645DF3)
    (at 52 -16.2)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (property "PN" "SM6T6V8A")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D2" (at -0.6 -3) (layer "B.SilkS"))
    (fp_text value "SM6T6V8A" (at 0 -3.1) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.15 0) (size 2.5 2.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.15 0) (size 2.5 2.3) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "GND") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 84.25 -26)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1203")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R9" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "12k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 61 "Net-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_HC49-SD" (layer "B.Cu")
    (tedit 5A1AD52C)
    (at 80.2 -4.4 180)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (property "PN" "7.372M-SMDHC49S ")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Y1" (at 0 3.55) (layer "B.SilkS"))
    (fp_text value "7.3728MHz" (at 0 -3.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.25 0 180) (size 4.5 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "Net-(C4-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.25 0 180) (size 4.5 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "Net-(C5-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 110.75 -21 90)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "SN75ALS160DW")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U2" (at -6.6 2.65 180) (layer "B.SilkS"))
    (fp_text value "75ALS160" (at 0 -7.35 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -4.65 5.715 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 71 "/TE") (pinfunction "TE") (pintype "input"))
    (pad "2" smd roundrect locked (at -4.65 4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(J1-Pad1)") (pinfunction "B1") (pintype "input"))
    (pad "3" smd roundrect locked (at -4.65 3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "Net-(J1-Pad2)") (pinfunction "B2") (pintype "input"))
    (pad "4" smd roundrect locked (at -4.65 1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(J1-Pad3)") (pinfunction "B3") (pintype "input"))
    (pad "5" smd roundrect locked (at -4.65 0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(J1-Pad4)") (pinfunction "B4") (pintype "input"))
    (pad "6" smd roundrect locked (at -4.65 -0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(J1-Pad13)") (pinfunction "B5") (pintype "input"))
    (pad "7" smd roundrect locked (at -4.65 -1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(J1-Pad14)") (pinfunction "B6") (pintype "input"))
    (pad "8" smd roundrect locked (at -4.65 -3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(J1-Pad15)") (pinfunction "B7") (pintype "input"))
    (pad "9" smd roundrect locked (at -4.65 -4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(J1-Pad16)") (pinfunction "B8") (pintype "input"))
    (pad "10" smd roundrect locked (at -4.65 -5.715 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "GND") (pinfunction "GND") (pintype "input"))
    (pad "11" smd roundrect locked (at 4.65 -5.715 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(R5-Pad2)") (pinfunction "PE") (pintype "input"))
    (pad "12" smd roundrect locked (at 4.65 -4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "/D8") (pinfunction "D8") (pintype "input"))
    (pad "13" smd roundrect locked (at 4.65 -3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "/D7") (pinfunction "D7") (pintype "input"))
    (pad "14" smd roundrect locked (at 4.65 -1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/D6") (pinfunction "D6") (pintype "input"))
    (pad "15" smd roundrect locked (at 4.65 -0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/D5") (pinfunction "D5") (pintype "input"))
    (pad "16" smd roundrect locked (at 4.65 0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "/D4") (pinfunction "D4") (pintype "input"))
    (pad "17" smd roundrect locked (at 4.65 1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "/D3") (pinfunction "D3") (pintype "input"))
    (pad "18" smd roundrect locked (at 4.65 3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "/D2") (pinfunction "D2") (pintype "input"))
    (pad "19" smd roundrect locked (at 4.65 4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "/D1") (pinfunction "D1") (pintype "input"))
    (pad "20" smd roundrect locked (at 4.65 5.715 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "+5V") (pinfunction "VCC") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 62.75 -24.75 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3902")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R8" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "3k9" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "/TXD_GPIB") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 38 -3)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3902")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R11" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "3k9" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "Net-(J3-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "Net-(C10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 119 -24.6 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C2" (at 0 2 180) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 17 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "j_lib:W5500_bo" (layer "B.Cu")
    (tedit 617C735E)
    (at 47 -24.905)
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "link" "W5500 breakout")
    (attr through_hole)
    (fp_text reference "U1" (at 0.8 3.505) (layer "B.SilkS"))
    (fp_text value "W5500_breakout" (at 0 10.5) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at -10.16 18.5) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "GND") (pintype "input"))
    (pad "2" thru_hole circle locked (at -10.16 15.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "GND") (pintype "input"))
    (pad "3" thru_hole circle locked (at -10.16 13.42) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/ETH_MOSI") (pinfunction "MOSI") (pintype "input"))
    (pad "4" thru_hole circle locked (at -10.16 10.88) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/ETH_SCLK") (pinfunction "SCLK") (pintype "input"))
    (pad "5" thru_hole circle locked (at -10.16 8.34) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 65 "/ETH_CS") (pinfunction "CS") (pintype "input"))
    (pad "6" thru_hole circle locked (at -10.16 5.8) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 36 "unconnected-(U1-Pad6)") (pinfunction "INT") (pintype "input+no_connect"))
    (pad "7" thru_hole circle locked (at 10.16 5.8) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/ETH_MISO") (pinfunction "MISO") (pintype "input"))
    (pad "8" thru_hole circle locked (at 10.16 8.34) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 64 "/ETH_RST") (pinfunction "RST") (pintype "input"))
    (pad "9" thru_hole circle locked (at 10.16 10.88) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask))
    (pad "10" thru_hole circle locked (at 10.16 13.42) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 49 "+3V3") (pinfunction "3V") (pintype "input"))
    (pad "11" thru_hole circle locked (at 10.16 15.96) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 49 "+3V3") (pinfunction "3V") (pintype "input"))
    (pad "12" thru_hole circle locked (at 10.16 18.5) (size 1.6 1.6) (drill 1) (layers *.Cu *.Mask)
      (net 18 "GND") (pinfunction "GND") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 27 -17)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C8" (at -0.8 -1.6) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 67 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 42.8 -17.0625 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BAV99")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D1" (at -0.3375 2.6 180) (layer "B.SilkS"))
    (fp_text value "BAV99" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "+5V") (pinfunction "A") (pintype "passive"))
    (pad "3" smd roundrect locked (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(C10-Pad1)") (pinfunction "K") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 67.8 -8.4 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1200")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R2" (at 3.2 0 180) (layer "B.SilkS"))
    (fp_text value "120R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "/ISP_MOSI") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "/SRQ") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 89.8 -4.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A220JXACW1BC")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C4" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "22p" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 66 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 9 -24 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3902")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R14" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "3k9" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "Net-(J5-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 68 -22)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2402")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R16" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "2k4" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "Net-(J5-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "/GPIB_TRIG") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 63.5 -13.75)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1200")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R3" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "120R" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/ISP_MISO") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "/IFC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 68 -17.75 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C7" (at 0 2 180) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 17 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 20 -14.8 90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "CH340G")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "LCSC")
    (attr smd)
    (fp_text reference "U6" (at 4.6 1 180) (layer "B.SilkS"))
    (fp_text value "CH340G" (at 0 -5.9 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.475 4.445 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -2.475 3.175 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(R15-Pad2)") (pinfunction "TXD") (pintype "output"))
    (pad "3" smd roundrect locked (at -2.475 1.905 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(R12-Pad2)") (pinfunction "RXD") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 0.635 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(C9-Pad1)") (pinfunction "V3") (pintype "passive"))
    (pad "5" smd roundrect locked (at -2.475 -0.635 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "Net-(J4-Pad3)") (pinfunction "UD+") (pintype "bidirectional"))
    (pad "6" smd roundrect locked (at -2.475 -1.905 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 69 "Net-(J4-Pad2)") (pinfunction "UD-") (pintype "bidirectional"))
    (pad "7" smd roundrect locked (at -2.475 -3.175 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(C12-Pad1)") (pinfunction "XI") (pintype "input"))
    (pad "8" smd roundrect locked (at -2.475 -4.445 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(C11-Pad1)") (pinfunction "XO") (pintype "output"))
    (pad "9" smd roundrect locked (at 2.475 -4.445 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "unconnected-(U6-Pad9)") (pinfunction "~{CTS}") (pintype "input+no_connect"))
    (pad "10" smd roundrect locked (at 2.475 -3.175 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "unconnected-(U6-Pad10)") (pinfunction "~{DSR}") (pintype "input+no_connect"))
    (pad "11" smd roundrect locked (at 2.475 -1.905 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "unconnected-(U6-Pad11)") (pinfunction "~{RI}") (pintype "input+no_connect"))
    (pad "12" smd roundrect locked (at 2.475 -0.635 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "unconnected-(U6-Pad12)") (pinfunction "~{DCD}") (pintype "input+no_connect"))
    (pad "13" smd roundrect locked (at 2.475 0.635 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "unconnected-(U6-Pad13)") (pinfunction "~{DTR}") (pintype "output+no_connect"))
    (pad "14" smd roundrect locked (at 2.475 1.905 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "unconnected-(U6-Pad14)") (pinfunction "~{RTS}") (pintype "output+no_connect"))
    (pad "15" smd roundrect locked (at 2.475 3.175 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "unconnected-(U6-Pad15)") (pinfunction "R232") (pintype "input+no_connect"))
    (pad "16" smd roundrect locked (at 2.475 4.445 90) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(C8-Pad1)") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 36.6 -24 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1203")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R12" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "12k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "Net-(R12-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 81 "Net-(R12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 63.5 -16.75)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1200")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R4" (at -0.3 -1.65) (layer "B.SilkS"))
    (fp_text value "120R" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/ISP_SCK") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/REN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 29.8 -11.4 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2402")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R15" (at -3.4 0 180) (layer "B.SilkS"))
    (fp_text value "2k4" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "/TXD_USB") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "Net-(R15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 68 -24.75 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3902")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R18" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "3k9" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "Net-(J5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 46.8 -16 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3903")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R10" (at -3.2 -1 180) (layer "B.SilkS"))
    (fp_text value "39k" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 54.75 -23 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C6" (at 0.95 1.6) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 17 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_HC49-SD" (layer "B.Cu")
    (tedit 5A1AD52C)
    (at 12 -14 -90)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (property "PN" "12.00M-SMDHC49S")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Y2" (at -6.4 -3.8 180) (layer "B.SilkS"))
    (fp_text value "12MHz" (at 0 -3.55 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.25 0 270) (size 4.5 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "Net-(C12-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.25 0 270) (size 4.5 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "Net-(C11-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 43 -3)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y471KXACW1BC")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C10" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "470p" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 72 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 9 -17.75 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A220JXACW1BC")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C12" (at -0.05 2.4 180) (layer "B.SilkS"))
    (fp_text value "22p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 75 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 70.8 -4.4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A220JXACW1BC")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C5" (at 0.2 -1.8) (layer "B.SilkS"))
    (fp_text value "22p" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 44 "Net-(C5-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 26.8 -13 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C9" (at 2.6 0.2 180) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 68 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 121 -16.35 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1203")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R6" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "12k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "/TE") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 32.4 -11.4 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3902")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R17" (at -3.4 0.8 180) (layer "B.SilkS"))
    (fp_text value "3k9" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 52 "/TXD_USB") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm" (layer "B.Cu")
    (tedit 5A02F146)
    (at 76.75 -20.8 180)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (property "PN" "AT90S4433")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "possible to use Atmega8")
    (property "link" "")
    (property "supplier" "NA")
    (attr smd)
    (fp_text reference "U3" (at 2.35 6) (layer "B.SilkS"))
    (fp_text value "AT90S4433" (at 0 -6.05) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.25 2.8 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/D6") (pinfunction "PD3") (pintype "bidirectional"))
    (pad "2" smd rect locked (at -4.25 2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/D7") (pinfunction "PD4") (pintype "bidirectional"))
    (pad "3" smd rect locked (at -4.25 1.2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect locked (at -4.25 0.4 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd rect locked (at -4.25 -0.4 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "6" smd rect locked (at -4.25 -1.2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pinfunction "VCC") (pintype "passive"))
    (pad "7" smd rect locked (at -4.25 -2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "Net-(C4-Pad1)") (pinfunction "PB6/XTAL1") (pintype "bidirectional"))
    (pad "8" smd rect locked (at -4.25 -2.8 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 44 "Net-(C5-Pad1)") (pinfunction "PB7/XTAL2") (pintype "bidirectional"))
    (pad "9" smd rect locked (at -2.8 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 19 "/D8") (pinfunction "PD5") (pintype "bidirectional"))
    (pad "10" smd rect locked (at -2 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "/EOI") (pinfunction "PD6") (pintype "bidirectional"))
    (pad "11" smd rect locked (at -1.2 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/ATN") (pinfunction "PD7") (pintype "bidirectional"))
    (pad "12" smd rect locked (at -0.4 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "/NDAC") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "13" smd rect locked (at 0.4 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "/NRFD") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd rect locked (at 1.2 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "/DAV") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "15" smd rect locked (at 2 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 41 "/ISP_MOSI") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "16" smd rect locked (at 2.8 -4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/ISP_MISO") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "17" smd rect locked (at 4.25 -2.8 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/ISP_SCK") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "18" smd rect locked (at 4.25 -2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pinfunction "AVCC") (pintype "power_in"))
    (pad "19" smd rect locked (at 4.25 -1.2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "unconnected-(U3-Pad19)") (pinfunction "ADC6") (pintype "input+no_connect"))
    (pad "20" smd rect locked (at 4.25 -0.4 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pinfunction "AREF") (pintype "passive"))
    (pad "21" smd rect locked (at 4.25 0.4 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "GND") (pinfunction "AGND") (pintype "power_in"))
    (pad "22" smd rect locked (at 4.25 1.2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "unconnected-(U3-Pad22)") (pinfunction "ADC7") (pintype "input+no_connect"))
    (pad "23" smd rect locked (at 4.25 2 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 70 "/GPIB_TRIG") (pinfunction "PC0") (pintype "bidirectional"))
    (pad "24" smd rect locked (at 4.25 2.8 180) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/D1") (pinfunction "PC1") (pintype "bidirectional"))
    (pad "25" smd rect locked (at 2.8 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/D2") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "26" smd rect locked (at 2 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 24 "/D3") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "27" smd rect locked (at 1.2 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 23 "/D4") (pinfunction "PC4") (pintype "bidirectional"))
    (pad "28" smd rect locked (at 0.4 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 71 "/TE") (pinfunction "PC5") (pintype "bidirectional"))
    (pad "29" smd rect locked (at -0.4 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/RESET") (pinfunction "PC6/~{RESET}") (pintype "bidirectional"))
    (pad "30" smd rect locked (at -1.2 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 62 "Net-(U3-Pad30)") (pinfunction "PD0") (pintype "bidirectional"))
    (pad "31" smd rect locked (at -2 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "Net-(R7-Pad2)") (pinfunction "PD1") (pintype "bidirectional"))
    (pad "32" smd rect locked (at -2.8 4.25 90) (size 1.6 0.55) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/D5") (pinfunction "PD2") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 42 -26)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2402")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R13" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "2k4" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "Net-(J5-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "/EXT_TRIG") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 102.25 -25.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C3" (at -2.9 0.15 180) (layer "B.SilkS"))
    (fp_text value "1u" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 17 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 94 -21 90)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "SN75ALS161DW ")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U5" (at -1.8 -7.6 180) (layer "B.SilkS"))
    (fp_text value "75ALS161" (at 0 -7.35 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -4.65 5.715 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 71 "/TE") (pinfunction "TE") (pintype "bidirectional"))
    (pad "2" smd roundrect locked (at -4.65 4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(J1-Pad17)") (pinfunction "REN_G") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -4.65 3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(J1-Pad9)") (pinfunction "IFC_G") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -4.65 1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(J1-Pad8)") (pinfunction "NDAC_G") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at -4.65 0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "Net-(J1-Pad7)") (pinfunction "NRFD_G") (pintype "bidirectional"))
    (pad "6" smd roundrect locked (at -4.65 -0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "Net-(J1-Pad6)") (pinfunction "DAV_G") (pintype "bidirectional"))
    (pad "7" smd roundrect locked (at -4.65 -1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(J1-Pad5)") (pinfunction "EOI_G") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at -4.65 -3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J1-Pad11)") (pinfunction "ATN_G") (pintype "bidirectional"))
    (pad "9" smd roundrect locked (at -4.65 -4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J1-Pad10)") (pinfunction "SRQ_G") (pintype "bidirectional"))
    (pad "10" smd roundrect locked (at -4.65 -5.715 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "GND") (pinfunction "GND") (pintype "bidirectional"))
    (pad "11" smd roundrect locked (at 4.65 -5.715 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "Net-(R9-Pad2)") (pinfunction "DC") (pintype "bidirectional"))
    (pad "12" smd roundrect locked (at 4.65 -4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "/SRQ") (pinfunction "SRQ_D") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at 4.65 -3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/ATN") (pinfunction "ATN_D") (pintype "bidirectional"))
    (pad "14" smd roundrect locked (at 4.65 -1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "/EOI") (pinfunction "EOI_D") (pintype "bidirectional"))
    (pad "15" smd roundrect locked (at 4.65 -0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "/DAV") (pinfunction "DAV_D") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at 4.65 0.635 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "/NRFD") (pinfunction "NRFD_D") (pintype "bidirectional"))
    (pad "17" smd roundrect locked (at 4.65 1.905 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "/NDAC") (pinfunction "NDAC_D") (pintype "bidirectional"))
    (pad "18" smd roundrect locked (at 4.65 3.175 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "/IFC") (pinfunction "IFC_D") (pintype "bidirectional"))
    (pad "19" smd roundrect locked (at 4.65 4.445 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "/REN") (pinfunction "REN_D") (pintype "bidirectional"))
    (pad "20" smd roundrect locked (at 4.65 5.715 90) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "+5V") (pinfunction "VCC") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 63 -2.6)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1203")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R1" (at 3.4 0) (layer "B.SilkS"))
    (fp_text value "12k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/RESET") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 62.75 -22)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2402")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R7" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "2k4" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "/TXD_GPIB") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 43 "Net-(R7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (layer "B.Cu")
    (tedit 5E476F32)
    (at 48.5 -24.905)
    (descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "PN" "74HCT08PW.112")
    (property "Sheetfile" "rnvm_lisa.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U4" (at 4.7 -1.895) (layer "B.SilkS"))
    (fp_text value "74HCT08" (at 0 -3.45) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.8625 1.95) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "/RXD_USB") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.8625 1.3) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "/RXD_USB") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.8625 0.65) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(R12-Pad1)") (pintype "output"))
    (pad "4" smd roundrect locked (at -2.8625 0) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(C10-Pad1)") (pintype "input"))
    (pad "5" smd roundrect locked (at -2.8625 -0.65) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(C10-Pad1)") (pintype "input"))
    (pad "6" smd roundrect locked (at -2.8625 -1.3) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 78 "/EXT_TRIG") (pintype "output"))
    (pad "7" smd roundrect locked (at -2.8625 -1.95) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.8625 -1.95) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 62 "Net-(U3-Pad30)") (pintype "output"))
    (pad "9" smd roundrect locked (at 2.8625 -1.3) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "/RXD_GPIB") (pintype "input"))
    (pad "10" smd roundrect locked (at 2.8625 -0.65) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "/RXD_GPIB") (pintype "input"))
    (pad "11" smd roundrect locked (at 2.8625 0) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 63 "unconnected-(U4-Pad11)") (pintype "output+no_connect"))
    (pad "12" smd roundrect locked (at 2.8625 0.65) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "GND") (pintype "input"))
    (pad "13" smd roundrect locked (at 2.8625 1.3) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "GND") (pintype "input"))
    (pad "14" smd roundrect locked (at 2.8625 1.95) (size 1.475 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 0 0) (end 132 -28) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "NVM\nLISA PCB REV 1" (at 118.6 -26) (layer "F.SilkS"))
  (zone (net 18) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.22) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 132 0)
        (xy 0 0)
        (xy 0 -28)
        (xy 132 -28)
      )
    )
  )
)
