(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:CP" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "Device_CP" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 4) (at 0 0 0))
      (symbol "CP_0_1"
        (rectangle (start -2.286 0.508) (end 2.286 1.016)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.794)
            (xy -1.27 1.778)
          )
          (fill (type none))
        )
        (rectangle (start 2.286 -0.508) (end -2.286 -1.016)
          (fill (type outline))
        )
      )
      (symbol "CP_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:L_Core_Ferrite" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at -1.27 0 90))
      (property "Value" "Device_L_Core_Ferrite" (id 1) (at 2.794 0 90))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 4) (at 0 0 0))
      (symbol "L_Core_Ferrite_0_1"
        (arc (start 0 -2.54) (mid 0.635 -1.905) (end 0 -1.27)
          (fill (type none))
        )
        (arc (start 0 -1.27) (mid 0.635 -0.635) (end 0 0)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -2.794)
            (xy 1.016 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -1.778)
            (xy 1.016 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -0.762)
            (xy 1.016 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0.254)
            (xy 1.016 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.27)
            (xy 1.016 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 2.286)
            (xy 1.016 2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -2.286)
            (xy 1.524 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -1.27)
            (xy 1.524 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -0.254)
            (xy 1.524 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 0.762)
            (xy 1.524 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 1.778)
            (xy 1.524 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 2.794)
            (xy 1.524 2.286)
          )
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.635 0.635) (end 0 1.27)
          (fill (type none))
        )
        (arc (start 0 1.27) (mid 0.635 1.905) (end 0 2.54)
          (fill (type none))
        )
      )
      (symbol "L_Core_Ferrite_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:1N4007" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "1N4007" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal" (id 2) (at 0 -4.445 0))
      (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "1000V 1A General Purpose Rectifier Diode, DO-41" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "D*DO?41*" (id 6) (at 0 0 0))
      (symbol "1N4007_0_1"
        (polyline
          (pts
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "1N4007_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Regulator_Linear:LM317_TO-220" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 3.175 0))
      (property "Value" "LM317_TO-220" (id 1) (at 0 3.175 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 0 6.35 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "Adjustable Voltage Regulator 1A Positive" (id 4) (at 0 0 0))
      (property "ki_description" "1.5A 35V Adjustable Linear Regulator, TO-220" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?220*" (id 6) (at 0 0 0))
      (symbol "LM317_TO-220_0_1"
        (rectangle (start -5.08 1.905) (end 5.08 -5.08)
          (fill (type background))
        )
      )
      (symbol "LM317_TO-220_1_1"
        (pin input line (at 0 -7.62 90) (length 2.54)
          (name "ADJ")
          (number "1")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "2")
        )
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "3")
        )
      )
    )
    (symbol "Regulator_Linear:LM337_TO220" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 -3.175 0))
      (property "Value" "LM337_TO220" (id 1) (at 0 -3.175 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 0 -5.08 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337-n.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "Adjustable Voltage Regulator 1.5A Negative" (id 4) (at 0 0 0))
      (property "ki_description" "Negative 1.5A 35V Adjustable Linear Regulator, TO-220" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?220*" (id 6) (at 0 0 0))
      (symbol "LM337_TO220_0_1"
        (rectangle (start -5.08 5.08) (end 5.08 -1.905)
          (fill (type background))
        )
      )
      (symbol "LM337_TO220_1_1"
        (pin input line (at 0 7.62 270) (length 2.54)
          (name "ADJ")
          (number "1")
        )
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "2")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "3")
        )
      )
    )
    (symbol "Regulator_Linear:LM7805_TO220" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 3.175 0))
      (property "Value" "LM7805_TO220" (id 1) (at 0 3.175 0))
      (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 0 5.715 0))
      (property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF" (id 3) (at 0 -1.27 0))
      (property "ki_keywords" "Voltage Regulator 1A Positive" (id 4) (at 0 0 0))
      (property "ki_description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?220*" (id 6) (at 0 0 0))
      (symbol "LM7805_TO220_0_1"
        (rectangle (start -5.08 1.905) (end 5.08 -5.08)
          (fill (type background))
        )
      )
      (symbol "LM7805_TO220_1_1"
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "3")
        )
      )
    )
  )
  (junction (at 135.255 95.25) (diameter 0) (color 0 0 0 0))
  (junction (at 127 76.835) (diameter 0) (color 0 0 0 0))
  (junction (at 132.715 135.255) (diameter 0) (color 0 0 0 0))
  (junction (at 139.065 59.69) (diameter 0) (color 0 0 0 0))
  (junction (at 161.29 135.255) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 102.235) (diameter 0) (color 0 0 0 0))
  (junction (at 154.305 94.615) (diameter 0) (color 0 0 0 0))
  (junction (at 150.495 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 113.03 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 127 95.25) (diameter 0) (color 0 0 0 0))
  (junction (at 161.925 102.235) (diameter 0) (color 0 0 0 0))
  (junction (at 194.31 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 194.31 94.615) (diameter 0) (color 0 0 0 0))
  (junction (at 161.29 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 154.305 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 194.31 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 139.065 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 141.605 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 141.605 135.255) (diameter 0) (color 0 0 0 0))
  (junction (at 132.715 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 113.03 104.14) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 50.165) (diameter 0) (color 0 0 0 0))
  (junction (at 194.31 102.235) (diameter 0) (color 0 0 0 0))
  (junction (at 127 135.255) (diameter 0) (color 0 0 0 0))
  (junction (at 135.255 76.835) (diameter 0) (color 0 0 0 0))
  (junction (at 131.445 76.835) (diameter 0) (color 0 0 0 0))
  (junction (at 127 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 102.235) (diameter 0) (color 0 0 0 0))
  (junction (at 142.24 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 111.125 76.835) (diameter 0) (color 0 0 0 0))
  (junction (at 113.03 95.25) (diameter 0) (color 0 0 0 0))
  (junction (at 186.69 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 111.125 128.905) (diameter 0) (color 0 0 0 0))
  (junction (at 135.255 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 186.69 78.74) (diameter 0) (color 0 0 0 0))
  (junction (at 154.305 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 106.045 76.835) (diameter 0) (color 0 0 0 0))
  (junction (at 186.69 94.615) (diameter 0) (color 0 0 0 0))
  (junction (at 106.045 104.14) (diameter 0) (color 0 0 0 0))
  (junction (at 106.045 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 161.925 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 194.31 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 106.045 128.905) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 86.36) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 132.715 147.32) (xy 141.605 147.32)))
  (wire (pts (xy 127 147.32) (xy 127 141.605)))
  (wire (pts (xy 127 128.905) (xy 123.19 128.905)))
  (wire (pts (xy 127 141.605) (xy 123.19 141.605)))
  (wire (pts (xy 141.605 135.255) (xy 132.715 135.255)))
  (wire (pts (xy 186.69 94.615) (xy 194.31 94.615)))
  (wire (pts (xy 132.715 135.255) (xy 132.715 139.7)))
  (wire (pts (xy 104.775 104.14) (xy 106.045 104.14)))
  (wire (pts (xy 135.255 102.235) (xy 135.255 95.25)))
  (wire (pts (xy 113.03 83.185) (xy 113.03 95.25)))
  (wire (pts (xy 177.8 110.49) (xy 208.28 110.49)))
  (wire (pts (xy 127 135.255) (xy 132.715 135.255)))
  (wire (pts (xy 106.045 147.32) (xy 113.03 147.32)))
  (wire (pts (xy 141.605 147.32) (xy 150.495 147.32)))
  (wire (pts (xy 177.8 86.36) (xy 186.69 86.36)))
  (wire (pts (xy 132.715 147.32) (xy 127 147.32)))
  (wire (pts (xy 131.445 104.14) (xy 131.445 86.36)))
  (wire (pts (xy 127 83.185) (xy 127 76.835)))
  (wire (pts (xy 104.14 76.835) (xy 106.045 76.835)))
  (wire (pts (xy 127 76.835) (xy 123.19 76.835)))
  (wire (pts (xy 154.305 86.995) (xy 154.305 86.36)))
  (wire (pts (xy 177.8 71.12) (xy 179.07 71.12)))
  (wire (pts (xy 161.925 102.235) (xy 177.8 102.235)))
  (wire (pts (xy 161.925 71.12) (xy 177.8 71.12)))
  (wire (pts (xy 194.31 71.12) (xy 208.28 71.12)))
  (wire (pts (xy 177.8 102.235) (xy 179.07 102.235)))
  (wire (pts (xy 142.24 102.235) (xy 135.255 102.235)))
  (wire (pts (xy 150.495 147.32) (xy 150.495 142.875)))
  (wire (pts (xy 123.19 135.255) (xy 127 135.255)))
  (wire (pts (xy 113.03 135.255) (xy 113.03 147.32)))
  (wire (pts (xy 113.03 95.25) (xy 115.57 95.25)))
  (wire (pts (xy 154.305 94.615) (xy 161.925 94.615)))
  (wire (pts (xy 141.605 139.7) (xy 141.605 135.255)))
  (wire (pts (xy 106.045 128.905) (xy 111.125 128.905)))
  (wire (pts (xy 139.065 59.69) (xy 139.065 86.36)))
  (wire (pts (xy 127 89.535) (xy 123.19 89.535)))
  (wire (pts (xy 161.29 135.255) (xy 168.91 135.255)))
  (wire (pts (xy 115.57 135.255) (xy 113.03 135.255)))
  (wire (pts (xy 194.31 86.995) (xy 194.31 86.36)))
  (wire (pts (xy 131.445 86.36) (xy 135.255 86.36)))
  (wire (pts (xy 127 95.25) (xy 127 89.535)))
  (wire (pts (xy 135.255 86.36) (xy 135.255 84.455)))
  (wire (pts (xy 135.255 87.63) (xy 135.255 86.36)))
  (wire (pts (xy 105.41 147.32) (xy 106.045 147.32)))
  (wire (pts (xy 177.8 62.23) (xy 208.28 62.23)))
  (wire (pts (xy 135.255 71.12) (xy 135.255 76.835)))
  (wire (pts (xy 123.19 83.185) (xy 127 83.185)))
  (wire (pts (xy 154.305 86.36) (xy 142.24 86.36)))
  (wire (pts (xy 111.125 76.835) (xy 115.57 76.835)))
  (wire (pts (xy 186.69 86.36) (xy 194.31 86.36)))
  (wire (pts (xy 113.03 104.14) (xy 131.445 104.14)))
  (wire (pts (xy 158.115 135.255) (xy 161.29 135.255)))
  (wire (pts (xy 142.24 71.12) (xy 135.255 71.12)))
  (wire (pts (xy 154.305 86.36) (xy 177.8 86.36)))
  (wire (pts (xy 127 135.255) (xy 127 128.905)))
  (wire (pts (xy 106.045 76.835) (xy 111.125 76.835)))
  (wire (pts (xy 150.495 147.32) (xy 161.29 147.32)))
  (wire (pts (xy 177.8 71.12) (xy 177.8 78.74)))
  (wire (pts (xy 106.045 134.62) (xy 106.045 128.905)))
  (wire (pts (xy 111.125 141.605) (xy 111.125 128.905)))
  (wire (pts (xy 115.57 141.605) (xy 111.125 141.605)))
  (wire (pts (xy 161.29 142.875) (xy 161.29 147.32)))
  (wire (pts (xy 142.24 78.74) (xy 142.24 86.36)))
  (wire (pts (xy 113.03 96.52) (xy 113.03 95.25)))
  (wire (pts (xy 194.31 102.235) (xy 208.28 102.235)))
  (wire (pts (xy 106.045 96.52) (xy 106.045 76.835)))
  (wire (pts (xy 135.255 76.835) (xy 131.445 76.835)))
  (wire (pts (xy 142.24 94.615) (xy 142.24 86.36)))
  (wire (pts (xy 131.445 50.165) (xy 131.445 76.835)))
  (wire (pts (xy 177.8 93.98) (xy 177.8 102.235)))
  (wire (pts (xy 111.125 89.535) (xy 111.125 76.835)))
  (wire (pts (xy 123.19 95.25) (xy 127 95.25)))
  (wire (pts (xy 104.14 128.905) (xy 106.045 128.905)))
  (wire (pts (xy 149.86 57.785) (xy 149.86 59.69)))
  (wire (pts (xy 177.8 102.235) (xy 177.8 110.49)))
  (wire (pts (xy 194.31 86.36) (xy 207.645 86.36)))
  (wire (pts (xy 149.86 50.165) (xy 208.28 50.165)))
  (wire (pts (xy 111.125 128.905) (xy 115.57 128.905)))
  (wire (pts (xy 146.685 102.235) (xy 142.24 102.235)))
  (wire (pts (xy 139.065 57.785) (xy 139.065 59.69)))
  (wire (pts (xy 146.685 50.165) (xy 149.86 50.165)))
  (wire (pts (xy 149.86 59.69) (xy 139.065 59.69)))
  (wire (pts (xy 186.69 78.74) (xy 194.31 78.74)))
  (wire (pts (xy 142.875 135.255) (xy 141.605 135.255)))
  (wire (pts (xy 177.8 71.12) (xy 177.8 62.23)))
  (wire (pts (xy 139.065 86.36) (xy 135.255 86.36)))
  (wire (pts (xy 146.685 71.12) (xy 142.24 71.12)))
  (wire (pts (xy 135.255 95.25) (xy 127 95.25)))
  (wire (pts (xy 115.57 83.185) (xy 113.03 83.185)))
  (wire (pts (xy 139.065 86.36) (xy 142.24 86.36)))
  (wire (pts (xy 104.775 95.25) (xy 113.03 95.25)))
  (wire (pts (xy 186.69 86.995) (xy 186.69 86.36)))
  (wire (pts (xy 161.29 147.32) (xy 168.91 147.32)))
  (wire (pts (xy 131.445 76.835) (xy 127 76.835)))
  (wire (pts (xy 106.045 104.14) (xy 113.03 104.14)))
  (wire (pts (xy 115.57 89.535) (xy 111.125 89.535)))
  (wire (pts (xy 154.305 78.74) (xy 161.925 78.74)))
  (wire (pts (xy 113.03 147.32) (xy 115.57 147.32)))
  (wire (pts (xy 106.045 142.24) (xy 106.045 147.32)))
  (wire (pts (xy 123.19 147.32) (xy 127 147.32)))
  (text "+-15V is 16V actually" (at 184.785 59.69 0))
  (hierarchical_label "F5V_D" (shape input) (at 168.91 135.255 0))
  (hierarchical_label "REC_S_HI" (shape input) (at 96.52 76.835 180))
  (hierarchical_label "REC_S_LO" (shape input) (at 97.155 95.25 180))
  (hierarchical_label "F5V_A" (shape input) (at 208.28 50.165 0))
  (hierarchical_label "REC_N_HI" (shape input) (at 96.52 128.905 180))
  (hierarchical_label "REC_N_LO" (shape input) (at 97.79 147.32 180))
  (hierarchical_label "F+8V" (shape input) (at 208.28 71.12 0))
  (hierarchical_label "F+15V" (shape input) (at 208.28 62.23 0))
  (hierarchical_label "F-15V" (shape input) (at 208.28 110.49 0))
  (hierarchical_label "FGND_D" (shape input) (at 168.91 147.32 0))
  (hierarchical_label "F-8V" (shape input) (at 208.28 102.235 0))
  (hierarchical_label "FGND_A" (shape input) (at 207.645 86.36 0))
  (hierarchical_label "REC_S_MID" (shape input) (at 97.155 104.14 180))
  (symbol (lib_id "Device:R") (at 161.925 98.425 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R65" (id 0) (at 165.735 97.79 0))
    (property "Value" "220R" (id 1) (at 166.37 99.695 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 160.147 98.425 90))
    (property "Datasheet" "~" (id 3) (at 161.925 98.425 0))
    (property "comment" "" (id 4) (at 161.925 98.425 0))
    (property "PN" "MMA02040C2200" (id 5) (at 161.925 98.425 0))
    (property "supplier" "TME" (id 6) (at 161.925 98.425 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4007") (at 119.38 135.255 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D17" (id 0) (at 115.57 132.715 0))
    (property "Value" "1N5819" (id 1) (at 122.555 132.715 0))
    (property "Footprint" "Diode_SMD:D_MELF" (id 2) (at 119.38 130.81 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 119.38 135.255 0))
    (property "comment" "" (id 4) (at 119.38 135.255 0))
    (property "PN" "SM5819" (id 5) (at 119.38 135.255 0))
    (property "supplier" "TME" (id 6) (at 119.38 135.255 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4007") (at 119.38 147.32 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D19" (id 0) (at 115.57 144.78 0))
    (property "Value" "1N5819" (id 1) (at 121.92 144.78 0))
    (property "Footprint" "Diode_SMD:D_MELF" (id 2) (at 119.38 142.875 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 119.38 147.32 0))
    (property "comment" "" (id 4) (at 119.38 147.32 0))
    (property "PN" "SM5819" (id 5) (at 119.38 147.32 0))
    (property "supplier" "TME" (id 6) (at 119.38 147.32 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 135.255 91.44 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C62" (id 0) (at 135.89 93.98 0))
    (property "Value" "1m2" (id 1) (at 135.89 96.52 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (id 2) (at 136.2202 95.25 0))
    (property "Datasheet" "~" (id 3) (at 135.255 91.44 0))
    (property "link" "" (id 4) (at 135.255 91.44 0))
    (property "supplier" "TME" (id 5) (at 135.255 91.44 0))
    (property "PN" "EEUFR1V122B" (id 6) (at 135.255 91.44 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Regulator_Linear:LM337_TO220") (at 154.305 102.235 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U16" (id 0) (at 154.305 106.0196 0))
    (property "Value" "LM337_TO220" (id 1) (at 154.305 108.331 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 154.305 107.315 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337-n.pdf" (id 3) (at 154.305 102.235 0))
    (property "comment" "" (id 4) (at 154.305 102.235 0))
    (property "PN" "LM337TG" (id 5) (at 154.305 102.235 0))
    (property "supplier" "TME" (id 6) (at 154.305 102.235 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Diode:1N4007") (at 119.38 83.185 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D12" (id 0) (at 115.57 80.645 0))
    (property "Value" "1N5819" (id 1) (at 122.555 80.645 0))
    (property "Footprint" "Diode_SMD:D_MELF" (id 2) (at 119.38 78.74 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 119.38 83.185 0))
    (property "comment" "" (id 4) (at 119.38 83.185 0))
    (property "PN" "SM5819" (id 5) (at 119.38 83.185 0))
    (property "supplier" "TME" (id 6) (at 119.38 83.185 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 154.305 82.55 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R60" (id 0) (at 158.115 81.915 0))
    (property "Value" "2k61" (id 1) (at 158.75 83.82 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 152.527 82.55 90))
    (property "Datasheet" "~" (id 3) (at 154.305 82.55 0))
    (property "link" "" (id 4) (at 154.305 82.55 0))
    (property "supplier" "MOUSER" (id 5) (at 154.305 82.55 0))
    (property "PN" "MMA02040C2611FB3" (id 6) (at 154.305 82.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Regulator_Linear:LM7805_TO220") (at 150.495 135.255 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U18" (id 0) (at 150.495 129.1082 0))
    (property "Value" "LM7805_TO220" (id 1) (at 150.495 131.4196 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 150.495 129.54 0))
    (property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF" (id 3) (at 150.495 136.525 0))
    (property "comment" "" (id 4) (at 150.495 135.255 0))
    (property "PN" "L7805ABV" (id 5) (at 150.495 135.255 0))
    (property "supplier" "TME" (id 6) (at 150.495 135.255 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:C") (at 106.045 100.33 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C63" (id 0) (at 108.585 106.045 0))
    (property "Value" "220n" (id 1) (at 110.49 107.95 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 105.0798 96.52 0))
    (property "Datasheet" "~" (id 3) (at 106.045 100.33 0))
    (property "comment" "" (id 4) (at 106.045 100.33 0))
    (property "PN" "VJ0805Y224KXATW1BC" (id 5) (at 106.045 100.33 0))
    (property "supplier" "TME" (id 6) (at 106.045 100.33 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4007") (at 119.38 128.905 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D16" (id 0) (at 115.57 126.365 0))
    (property "Value" "1N5819" (id 1) (at 122.555 126.365 0))
    (property "Footprint" "Diode_SMD:D_MELF" (id 2) (at 119.38 124.46 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 119.38 128.905 0))
    (property "comment" "" (id 4) (at 119.38 128.905 0))
    (property "PN" "SM5819" (id 5) (at 119.38 128.905 0))
    (property "supplier" "TME" (id 6) (at 119.38 128.905 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Core_Ferrite") (at 100.965 104.14 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L9" (id 0) (at 100.965 98.425 90))
    (property "Value" "68u" (id 1) (at 100.965 100.7364 90))
    (property "Footprint" "Inductor_SMD:L_Bourns_SRN6045TA" (id 2) (at 100.965 104.14 0))
    (property "Datasheet" "~" (id 3) (at 100.965 104.14 0))
    (property "comment" "" (id 4) (at 100.965 104.14 0))
    (property "PN" "SRN6045TA-680M" (id 5) (at 100.965 104.14 0))
    (property "supplier" "TME" (id 6) (at 100.965 104.14 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 177.8 90.17 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C60" (id 0) (at 180.7972 89.0016 0))
    (property "Value" "22u" (id 1) (at 180.7972 91.313 0))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (id 2) (at 178.7652 93.98 0))
    (property "Datasheet" "~" (id 3) (at 177.8 90.17 0))
    (property "comment" "" (id 4) (at 177.8 90.17 0))
    (property "PN" "T491C226K025AT" (id 5) (at 177.8 90.17 0))
    (property "supplier" "TME" (id 6) (at 177.8 90.17 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Regulator_Linear:LM317_TO-220") (at 154.305 71.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U14" (id 0) (at 154.305 64.9732 0))
    (property "Value" "LM317_TO-220" (id 1) (at 154.305 67.2846 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 154.305 64.77 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf" (id 3) (at 154.305 71.12 0))
    (property "comment" "" (id 4) (at 154.305 71.12 0))
    (property "PN" "LM317BTG" (id 5) (at 154.305 71.12 0))
    (property "supplier" "TME" (id 6) (at 154.305 71.12 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:L_Core_Ferrite") (at 101.6 147.32 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L11" (id 0) (at 101.6 141.605 90))
    (property "Value" "68u" (id 1) (at 101.6 143.9164 90))
    (property "Footprint" "Inductor_SMD:L_Bourns_SRN6045TA" (id 2) (at 101.6 147.32 0))
    (property "Datasheet" "~" (id 3) (at 101.6 147.32 0))
    (property "comment" "" (id 4) (at 101.6 147.32 0))
    (property "PN" "SRN6045TA-680M" (id 5) (at 101.6 147.32 0))
    (property "supplier" "TME" (id 6) (at 101.6 147.32 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 142.24 74.93 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R57" (id 0) (at 146.05 74.295 0))
    (property "Value" "18k7" (id 1) (at 146.685 76.2 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 140.462 74.93 90))
    (property "Datasheet" "~" (id 3) (at 142.24 74.93 0))
    (property "comment" "" (id 4) (at 142.24 74.93 0))
    (property "PN" "SMDMM0204-18K7" (id 5) (at 142.24 74.93 0))
    (property "supplier" "TME" (id 6) (at 142.24 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 161.925 74.93 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R58" (id 0) (at 165.735 74.295 0))
    (property "Value" "220R" (id 1) (at 166.37 76.2 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 160.147 74.93 90))
    (property "Datasheet" "~" (id 3) (at 161.925 74.93 0))
    (property "comment" "" (id 4) (at 161.925 74.93 0))
    (property "PN" "MMA02040C2200" (id 5) (at 161.925 74.93 0))
    (property "supplier" "TME" (id 6) (at 161.925 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 186.69 90.805 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R63" (id 0) (at 189.865 89.535 0))
    (property "Value" "1k2" (id 1) (at 189.865 92.075 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 184.912 90.805 90))
    (property "Datasheet" "~" (id 3) (at 186.69 90.805 0))
    (property "comment" "" (id 4) (at 186.69 90.805 0))
    (property "PN" "MMA02040C1201" (id 5) (at 186.69 90.805 0))
    (property "supplier" "TME" (id 6) (at 186.69 90.805 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Regulator_Linear:LM7805_TO220") (at 139.065 50.165 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U13" (id 0) (at 139.065 44.0182 0))
    (property "Value" "LM7805_TO220" (id 1) (at 139.065 46.3296 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 139.065 44.45 0))
    (property "Datasheet" "https://www.onsemi.cn/PowerSolutions/document/MC7800-D.PDF" (id 3) (at 139.065 51.435 0))
    (property "comment" "" (id 4) (at 139.065 50.165 0))
    (property "PN" "L7805ABV" (id 5) (at 139.065 50.165 0))
    (property "supplier" "TME" (id 6) (at 139.065 50.165 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R") (at 154.305 90.805 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R62" (id 0) (at 158.115 90.17 0))
    (property "Value" "2k61" (id 1) (at 158.75 92.075 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 152.527 90.805 90))
    (property "Datasheet" "~" (id 3) (at 154.305 90.805 0))
    (property "link" "" (id 4) (at 154.305 90.805 0))
    (property "supplier" "MOUSER" (id 5) (at 154.305 90.805 0))
    (property "PN" "MMA02040C2611FB3" (id 6) (at 154.305 90.805 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 141.605 143.51 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R67" (id 0) (at 145.415 142.875 0))
    (property "Value" "18k7" (id 1) (at 146.05 144.78 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 139.827 143.51 90))
    (property "Datasheet" "~" (id 3) (at 141.605 143.51 0))
    (property "comment" "" (id 4) (at 141.605 143.51 0))
    (property "PN" "SMDMM0204-18K7" (id 5) (at 141.605 143.51 0))
    (property "supplier" "TME" (id 6) (at 141.605 143.51 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 194.31 90.805 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C61" (id 0) (at 197.3072 89.6366 0))
    (property "Value" "22u" (id 1) (at 197.3072 91.948 0))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (id 2) (at 193.3448 94.615 0))
    (property "Datasheet" "~" (id 3) (at 194.31 90.805 0))
    (property "comment" "" (id 4) (at 194.31 90.805 0))
    (property "PN" "T491C226K025AT" (id 5) (at 194.31 90.805 0))
    (property "supplier" "TME" (id 6) (at 194.31 90.805 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 161.29 139.065 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C66" (id 0) (at 164.2872 137.8966 0))
    (property "Value" "22u" (id 1) (at 164.2872 140.208 0))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (id 2) (at 160.3248 142.875 0))
    (property "Datasheet" "~" (id 3) (at 161.29 139.065 0))
    (property "comment" "" (id 4) (at 161.29 139.065 0))
    (property "PN" "T491C226K025AT" (id 5) (at 161.29 139.065 0))
    (property "supplier" "TME" (id 6) (at 161.29 139.065 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 177.8 82.55 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C58" (id 0) (at 180.7972 81.3816 0))
    (property "Value" "22u" (id 1) (at 180.7972 83.693 0))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (id 2) (at 178.7652 86.36 0))
    (property "Datasheet" "~" (id 3) (at 177.8 82.55 0))
    (property "comment" "" (id 4) (at 177.8 82.55 0))
    (property "PN" "T491C226K025AT" (id 5) (at 177.8 82.55 0))
    (property "supplier" "TME" (id 6) (at 177.8 82.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4007") (at 119.38 76.835 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D11" (id 0) (at 116.205 74.295 0))
    (property "Value" "1N5819" (id 1) (at 122.555 74.295 0))
    (property "Footprint" "Diode_SMD:D_MELF" (id 2) (at 119.38 72.39 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 119.38 76.835 0))
    (property "comment" "" (id 4) (at 119.38 76.835 0))
    (property "PN" "SM5819" (id 5) (at 119.38 76.835 0))
    (property "supplier" "TME" (id 6) (at 119.38 76.835 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 149.86 53.975 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C56" (id 0) (at 152.8572 52.8066 0))
    (property "Value" "22u" (id 1) (at 152.8572 55.118 0))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (id 2) (at 150.8252 57.785 0))
    (property "Datasheet" "~" (id 3) (at 149.86 53.975 0))
    (property "comment" "" (id 4) (at 149.86 53.975 0))
    (property "PN" "T491C226K025AT" (id 5) (at 149.86 53.975 0))
    (property "supplier" "TME" (id 6) (at 149.86 53.975 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Core_Ferrite") (at 100.965 95.25 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L8" (id 0) (at 100.965 89.535 90))
    (property "Value" "68u" (id 1) (at 100.965 91.8464 90))
    (property "Footprint" "Inductor_SMD:L_Bourns_SRN6045TA" (id 2) (at 100.965 95.25 0))
    (property "Datasheet" "~" (id 3) (at 100.965 95.25 0))
    (property "comment" "" (id 4) (at 100.965 95.25 0))
    (property "PN" "SRN6045TA-680M" (id 5) (at 100.965 95.25 0))
    (property "supplier" "TME" (id 6) (at 100.965 95.25 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Core_Ferrite") (at 100.33 76.835 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L7" (id 0) (at 100.33 71.12 90))
    (property "Value" "68u" (id 1) (at 100.33 73.4314 90))
    (property "Footprint" "Inductor_SMD:L_Bourns_SRN6045TA" (id 2) (at 100.33 76.835 0))
    (property "Datasheet" "~" (id 3) (at 100.33 76.835 0))
    (property "comment" "" (id 4) (at 100.33 76.835 0))
    (property "PN" "SRN6045TA-680M" (id 5) (at 100.33 76.835 0))
    (property "supplier" "TME" (id 6) (at 100.33 76.835 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 135.255 80.645 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C57" (id 0) (at 128.27 80.645 0))
    (property "Value" "1m2" (id 1) (at 128.905 82.55 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (id 2) (at 136.2202 84.455 0))
    (property "Datasheet" "~" (id 3) (at 135.255 80.645 0))
    (property "link" "" (id 4) (at 135.255 80.645 0))
    (property "supplier" "TME" (id 5) (at 135.255 80.645 0))
    (property "PN" "EEUFR1V122B" (id 6) (at 135.255 80.645 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 132.715 143.51 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C67" (id 0) (at 135.7122 142.3416 0))
    (property "Value" "1m2" (id 1) (at 135.7122 144.653 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (id 2) (at 133.6802 147.32 0))
    (property "Datasheet" "~" (id 3) (at 132.715 143.51 0))
    (property "link" "" (id 4) (at 132.715 143.51 0))
    (property "supplier" "TME" (id 5) (at 132.715 143.51 0))
    (property "PN" "EEUFR1V122B" (id 6) (at 132.715 143.51 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 106.045 138.43 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C65" (id 0) (at 111.125 140.97 0))
    (property "Value" "220n" (id 1) (at 111.125 142.875 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 105.0798 134.62 0))
    (property "Datasheet" "~" (id 3) (at 106.045 138.43 0))
    (property "comment" "" (id 4) (at 106.045 138.43 0))
    (property "PN" "VJ0805Y224KXATW1BC" (id 5) (at 106.045 138.43 0))
    (property "supplier" "TME" (id 6) (at 106.045 138.43 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 194.31 98.425 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R66" (id 0) (at 198.12 97.79 0))
    (property "Value" "240R" (id 1) (at 198.755 99.695 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 192.532 98.425 90))
    (property "Datasheet" "~" (id 3) (at 194.31 98.425 0))
    (property "comment" "" (id 4) (at 194.31 98.425 0))
    (property "PN" "MMA02040C2400" (id 5) (at 194.31 98.425 0))
    (property "supplier" "TME" (id 6) (at 194.31 98.425 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4007") (at 119.38 89.535 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D13" (id 0) (at 115.57 86.995 0))
    (property "Value" "1N5819" (id 1) (at 121.92 86.995 0))
    (property "Footprint" "Diode_SMD:D_MELF" (id 2) (at 119.38 85.09 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 119.38 89.535 0))
    (property "comment" "" (id 4) (at 119.38 89.535 0))
    (property "PN" "SM5819" (id 5) (at 119.38 89.535 0))
    (property "supplier" "TME" (id 6) (at 119.38 89.535 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 186.69 82.55 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R61" (id 0) (at 189.865 80.645 0))
    (property "Value" "1k2" (id 1) (at 189.865 83.185 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 184.912 82.55 90))
    (property "Datasheet" "~" (id 3) (at 186.69 82.55 0))
    (property "comment" "" (id 4) (at 186.69 82.55 0))
    (property "PN" "MMA02040C1201" (id 5) (at 186.69 82.55 0))
    (property "supplier" "TME" (id 6) (at 186.69 82.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Regulator_Linear:LM317_TO-220") (at 186.69 71.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U15" (id 0) (at 186.69 64.9732 0))
    (property "Value" "LM317_TO-220" (id 1) (at 186.69 67.2846 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 186.69 64.77 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm317.pdf" (id 3) (at 186.69 71.12 0))
    (property "comment" "" (id 4) (at 186.69 71.12 0))
    (property "PN" "LM317BTG" (id 5) (at 186.69 71.12 0))
    (property "supplier" "TME" (id 6) (at 186.69 71.12 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R") (at 142.24 98.425 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R64" (id 0) (at 146.05 97.79 0))
    (property "Value" "18k7" (id 1) (at 146.685 99.695 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 140.462 98.425 90))
    (property "Datasheet" "~" (id 3) (at 142.24 98.425 0))
    (property "comment" "" (id 4) (at 142.24 98.425 0))
    (property "PN" "SMDMM0204-18K7" (id 5) (at 142.24 98.425 0))
    (property "supplier" "TME" (id 6) (at 142.24 98.425 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 113.03 100.33 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C64" (id 0) (at 119.38 100.33 0))
    (property "Value" "220n" (id 1) (at 121.285 102.235 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 112.0648 96.52 0))
    (property "Datasheet" "~" (id 3) (at 113.03 100.33 0))
    (property "comment" "" (id 4) (at 113.03 100.33 0))
    (property "PN" "VJ0805Y224KXATW1BC" (id 5) (at 113.03 100.33 0))
    (property "supplier" "TME" (id 6) (at 113.03 100.33 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4007") (at 119.38 95.25 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D14" (id 0) (at 115.57 92.71 0))
    (property "Value" "1N5819" (id 1) (at 121.92 92.71 0))
    (property "Footprint" "Diode_SMD:D_MELF" (id 2) (at 119.38 90.805 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 119.38 95.25 0))
    (property "comment" "" (id 4) (at 119.38 95.25 0))
    (property "PN" "SM5819" (id 5) (at 119.38 95.25 0))
    (property "supplier" "TME" (id 6) (at 119.38 95.25 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Core_Ferrite") (at 100.33 128.905 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L10" (id 0) (at 100.33 123.19 90))
    (property "Value" "68u" (id 1) (at 100.33 125.5014 90))
    (property "Footprint" "Inductor_SMD:L_Bourns_SRN6045TA" (id 2) (at 100.33 128.905 0))
    (property "Datasheet" "~" (id 3) (at 100.33 128.905 0))
    (property "comment" "" (id 4) (at 100.33 128.905 0))
    (property "PN" "SRN6045TA-680M" (id 5) (at 100.33 128.905 0))
    (property "supplier" "TME" (id 6) (at 100.33 128.905 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 194.31 74.93 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R59" (id 0) (at 198.12 74.295 0))
    (property "Value" "240R" (id 1) (at 198.755 76.2 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 192.532 74.93 90))
    (property "Datasheet" "~" (id 3) (at 194.31 74.93 0))
    (property "comment" "" (id 4) (at 194.31 74.93 0))
    (property "PN" "MMA02040C2400" (id 5) (at 194.31 74.93 0))
    (property "supplier" "TME" (id 6) (at 194.31 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 194.31 82.55 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C59" (id 0) (at 197.3072 81.3816 0))
    (property "Value" "22u" (id 1) (at 197.3072 83.693 0))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (id 2) (at 195.2752 86.36 0))
    (property "Datasheet" "~" (id 3) (at 194.31 82.55 0))
    (property "comment" "" (id 4) (at 194.31 82.55 0))
    (property "PN" "T491C226K025AT" (id 5) (at 194.31 82.55 0))
    (property "supplier" "TME" (id 6) (at 194.31 82.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:1N4007") (at 119.38 141.605 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D18" (id 0) (at 115.57 139.065 0))
    (property "Value" "1N5819" (id 1) (at 121.92 139.065 0))
    (property "Footprint" "Diode_SMD:D_MELF" (id 2) (at 119.38 137.16 0))
    (property "Datasheet" "http://www.vishay.com/docs/88503/1n4001.pdf" (id 3) (at 119.38 141.605 0))
    (property "comment" "" (id 4) (at 119.38 141.605 0))
    (property "PN" "SM5819" (id 5) (at 119.38 141.605 0))
    (property "supplier" "TME" (id 6) (at 119.38 141.605 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Regulator_Linear:LM337_TO220") (at 186.69 102.235 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U17" (id 0) (at 186.69 106.0196 0))
    (property "Value" "LM337_TO220" (id 1) (at 186.69 108.331 0))
    (property "Footprint" "Package_TO_SOT_THT:TO-220-3_Vertical" (id 2) (at 186.69 107.315 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm337-n.pdf" (id 3) (at 186.69 102.235 0))
    (property "comment" "" (id 4) (at 186.69 102.235 0))
    (property "PN" "LM337TG" (id 5) (at 186.69 102.235 0))
    (property "supplier" "TME" (id 6) (at 186.69 102.235 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
)
