(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:CP" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "Device_CP" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 4) (at 0 0 0))
      (symbol "CP_0_1"
        (rectangle (start -2.286 0.508) (end 2.286 1.016)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.794)
            (xy -1.27 1.778)
          )
          (fill (type none))
        )
        (rectangle (start 2.286 -0.508) (end -2.286 -1.016)
          (fill (type outline))
        )
      )
      (symbol "CP_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:L_Core_Ferrite" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at -1.27 0 90))
      (property "Value" "Device_L_Core_Ferrite" (id 1) (at 2.794 0 90))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 4) (at 0 0 0))
      (symbol "L_Core_Ferrite_0_1"
        (arc (start 0 -2.54) (mid 0.635 -1.905) (end 0 -1.27)
          (fill (type none))
        )
        (arc (start 0 -1.27) (mid 0.635 -0.635) (end 0 0)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -2.794)
            (xy 1.016 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -1.778)
            (xy 1.016 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 -0.762)
            (xy 1.016 -0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 0.254)
            (xy 1.016 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.27)
            (xy 1.016 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 2.286)
            (xy 1.016 2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -2.286)
            (xy 1.524 -2.794)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -1.27)
            (xy 1.524 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 -0.254)
            (xy 1.524 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 0.762)
            (xy 1.524 0.254)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 1.778)
            (xy 1.524 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.524 2.794)
            (xy 1.524 2.286)
          )
          (fill (type none))
        )
        (arc (start 0 0) (mid 0.635 0.635) (end 0 1.27)
          (fill (type none))
        )
        (arc (start 0 1.27) (mid 0.635 1.905) (end 0 2.54)
          (fill (type none))
        )
      )
      (symbol "L_Core_Ferrite_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "jlib_1:LM43600" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -1.27 16.51 0))
      (property "Value" "jlib_1_LM43600" (id 1) (at 3.81 13.97 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "LM43600_0_0"
        (rectangle (start -10.16 12.7) (end 10.16 -15.24)
          (fill (type none))
        )
      )
      (symbol "LM43600_1_1"
        (pin input line (at 15.24 7.62 180) (length 5.08)
          (name "SW")
          (number "1")
        )
        (pin input line (at -15.24 -10.16 0) (length 5.08)
          (name "AGND")
          (number "10")
        )
        (pin input line (at -15.24 -2.54 0) (length 5.08)
          (name "SS/TRK")
          (number "11")
        )
        (pin input line (at -15.24 5.08 0) (length 5.08)
          (name "EN")
          (number "12")
        )
        (pin input line (at -15.24 10.16 0) (length 5.08)
          (name "VIN")
          (number "13")
        )
        (pin input line (at -15.24 7.62 0) (length 5.08)
          (name "VIN")
          (number "14")
        )
        (pin input line (at -15.24 -5.08 0) (length 5.08)
          (name "PGND")
          (number "15")
        )
        (pin input line (at -15.24 -7.62 0) (length 5.08)
          (name "PGND")
          (number "16")
        )
        (pin input line (at -15.24 -12.7 0) (length 5.08)
          (name "PAD")
          (number "17")
        )
        (pin input line (at 15.24 10.16 180) (length 5.08)
          (name "SW")
          (number "2")
        )
        (pin input line (at 15.24 2.54 180) (length 5.08)
          (name "CBOOT")
          (number "3")
        )
        (pin input line (at 15.24 -10.16 180) (length 5.08)
          (name "VCC")
          (number "4")
        )
        (pin input line (at 15.24 -2.54 180) (length 5.08)
          (name "BIAS")
          (number "5")
        )
        (pin input line (at -15.24 0 0) (length 5.08)
          (name "SYNC")
          (number "6")
        )
        (pin input line (at -15.24 2.54 0) (length 5.08)
          (name "RT")
          (number "7")
        )
        (pin input line (at 15.24 -7.62 180) (length 5.08)
          (name "PGOOD")
          (number "8")
        )
        (pin input line (at 15.24 -5.08 180) (length 5.08)
          (name "FB")
          (number "9")
        )
      )
    )
  )
  (junction (at 114.3 56.515) (diameter 0) (color 0 0 0 0))
  (junction (at 175.895 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 118.745) (diameter 0) (color 0 0 0 0))
  (junction (at 158.75 56.515) (diameter 0) (color 0 0 0 0))
  (junction (at 121.285 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 56.515) (diameter 0) (color 0 0 0 0))
  (junction (at 158.75 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 175.895 98.425) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 116.205) (diameter 0) (color 0 0 0 0))
  (junction (at 186.055 71.755) (diameter 0) (color 0 0 0 0))
  (junction (at 158.75 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 186.055 64.135) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 64.135) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 98.425) (diameter 0) (color 0 0 0 0))
  (junction (at 167.005 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 98.425) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 76.835) (diameter 0) (color 0 0 0 0))
  (junction (at 167.005 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 186.055 56.515) (diameter 0) (color 0 0 0 0))
  (junction (at 175.895 69.215) (diameter 0) (color 0 0 0 0))
  (junction (at 167.005 71.755) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 121.285) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 178.435 113.665) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 98.425) (diameter 0) (color 0 0 0 0))
  (junction (at 186.055 98.425) (diameter 0) (color 0 0 0 0))
  (junction (at 186.055 106.045) (diameter 0) (color 0 0 0 0))
  (junction (at 175.895 56.515) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 74.295) (diameter 0) (color 0 0 0 0))
  (junction (at 106.68 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 163.83 56.515) (diameter 0) (color 0 0 0 0))
  (junction (at 175.895 111.125) (diameter 0) (color 0 0 0 0))
  (junction (at 158.75 98.425) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 56.515) (diameter 0) (color 0 0 0 0))
  (junction (at 121.285 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 167.005 113.665) (diameter 0) (color 0 0 0 0))
  (junction (at 163.83 98.425) (diameter 0) (color 0 0 0 0))
  (junction (at 186.055 113.665) (diameter 0) (color 0 0 0 0))
  (junction (at 175.895 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 114.3 106.045) (diameter 0) (color 0 0 0 0))
  (junction (at 128.27 79.375) (diameter 0) (color 0 0 0 0))
  (junction (at 178.435 71.755) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 175.26 56.515) (xy 175.895 56.515)))
  (wire (pts (xy 178.435 64.135) (xy 178.435 71.755)))
  (wire (pts (xy 163.83 98.425) (xy 167.64 98.425)))
  (wire (pts (xy 88.9 98.425) (xy 88.9 56.515)))
  (wire (pts (xy 128.27 121.285) (xy 128.27 118.745)))
  (wire (pts (xy 175.895 80.01) (xy 175.895 69.215)))
  (wire (pts (xy 128.27 79.375) (xy 128.27 87.63)))
  (wire (pts (xy 175.895 56.515) (xy 186.055 56.515)))
  (wire (pts (xy 114.3 106.045) (xy 114.3 121.92)))
  (wire (pts (xy 106.68 129.54) (xy 106.68 121.285)))
  (wire (pts (xy 167.005 113.665) (xy 167.005 121.92)))
  (wire (pts (xy 124.46 61.595) (xy 128.27 61.595)))
  (wire (pts (xy 128.27 113.665) (xy 128.27 116.205)))
  (wire (pts (xy 175.895 129.54) (xy 186.055 129.54)))
  (wire (pts (xy 114.3 98.425) (xy 106.68 98.425)))
  (wire (pts (xy 167.005 71.755) (xy 178.435 71.755)))
  (wire (pts (xy 175.895 87.63) (xy 186.055 87.63)))
  (wire (pts (xy 158.75 98.425) (xy 163.83 98.425)))
  (wire (pts (xy 114.3 87.63) (xy 106.68 87.63)))
  (wire (pts (xy 158.75 56.515) (xy 163.83 56.515)))
  (wire (pts (xy 96.52 56.515) (xy 88.9 56.515)))
  (wire (pts (xy 121.285 129.54) (xy 114.3 129.54)))
  (wire (pts (xy 175.895 121.92) (xy 175.895 111.125)))
  (wire (pts (xy 175.895 69.215) (xy 175.895 56.515)))
  (wire (pts (xy 158.75 59.055) (xy 158.75 56.515)))
  (wire (pts (xy 128.27 129.54) (xy 158.75 129.54)))
  (wire (pts (xy 167.005 129.54) (xy 175.895 129.54)))
  (wire (pts (xy 167.005 71.755) (xy 167.005 80.01)))
  (wire (pts (xy 121.285 76.835) (xy 121.285 87.63)))
  (wire (pts (xy 128.27 118.745) (xy 128.27 116.205)))
  (wire (pts (xy 167.005 113.665) (xy 178.435 113.665)))
  (wire (pts (xy 114.3 129.54) (xy 106.68 129.54)))
  (wire (pts (xy 114.3 64.135) (xy 114.3 80.01)))
  (wire (pts (xy 175.895 98.425) (xy 186.055 98.425)))
  (wire (pts (xy 104.14 56.515) (xy 106.68 56.515)))
  (wire (pts (xy 124.46 64.135) (xy 124.46 61.595)))
  (wire (pts (xy 186.055 106.045) (xy 186.055 113.665)))
  (wire (pts (xy 158.75 126.365) (xy 158.75 129.54)))
  (wire (pts (xy 124.46 106.045) (xy 124.46 103.505)))
  (wire (pts (xy 186.055 64.135) (xy 186.055 71.755)))
  (wire (pts (xy 175.26 98.425) (xy 175.895 98.425)))
  (wire (pts (xy 114.3 106.045) (xy 124.46 106.045)))
  (wire (pts (xy 158.75 111.125) (xy 175.895 111.125)))
  (wire (pts (xy 163.83 56.515) (xy 167.64 56.515)))
  (wire (pts (xy 121.285 87.63) (xy 128.27 87.63)))
  (wire (pts (xy 121.285 111.125) (xy 128.27 111.125)))
  (wire (pts (xy 128.27 76.835) (xy 128.27 79.375)))
  (wire (pts (xy 186.055 113.665) (xy 186.055 121.92)))
  (wire (pts (xy 175.895 111.125) (xy 175.895 98.425)))
  (wire (pts (xy 128.27 100.965) (xy 128.27 98.425)))
  (wire (pts (xy 186.055 98.425) (xy 186.055 106.045)))
  (wire (pts (xy 114.3 56.515) (xy 106.68 56.515)))
  (wire (pts (xy 88.9 98.425) (xy 99.06 98.425)))
  (wire (pts (xy 186.055 71.755) (xy 186.055 80.01)))
  (wire (pts (xy 158.75 69.215) (xy 175.895 69.215)))
  (wire (pts (xy 128.27 129.54) (xy 128.27 121.285)))
  (wire (pts (xy 186.055 56.515) (xy 198.12 56.515)))
  (wire (pts (xy 128.27 98.425) (xy 114.3 98.425)))
  (wire (pts (xy 121.285 87.63) (xy 114.3 87.63)))
  (wire (pts (xy 158.75 100.965) (xy 158.75 98.425)))
  (wire (pts (xy 158.75 129.54) (xy 167.005 129.54)))
  (wire (pts (xy 121.285 69.215) (xy 128.27 69.215)))
  (wire (pts (xy 158.75 84.455) (xy 158.75 87.63)))
  (wire (pts (xy 94.615 87.63) (xy 106.68 87.63)))
  (wire (pts (xy 121.285 129.54) (xy 128.27 129.54)))
  (wire (pts (xy 158.75 71.755) (xy 167.005 71.755)))
  (wire (pts (xy 158.75 113.665) (xy 167.005 113.665)))
  (wire (pts (xy 106.68 98.425) (xy 106.68 113.665)))
  (wire (pts (xy 114.3 64.135) (xy 124.46 64.135)))
  (wire (pts (xy 167.005 87.63) (xy 175.895 87.63)))
  (wire (pts (xy 128.27 56.515) (xy 114.3 56.515)))
  (wire (pts (xy 121.285 118.745) (xy 121.285 129.54)))
  (wire (pts (xy 178.435 106.045) (xy 178.435 113.665)))
  (wire (pts (xy 128.27 59.055) (xy 128.27 56.515)))
  (wire (pts (xy 186.055 56.515) (xy 186.055 64.135)))
  (wire (pts (xy 94.615 129.54) (xy 94.615 87.63)))
  (wire (pts (xy 163.83 106.045) (xy 158.75 106.045)))
  (wire (pts (xy 163.83 64.135) (xy 158.75 64.135)))
  (wire (pts (xy 106.68 56.515) (xy 106.68 71.755)))
  (wire (pts (xy 124.46 103.505) (xy 128.27 103.505)))
  (wire (pts (xy 94.615 129.54) (xy 106.68 129.54)))
  (wire (pts (xy 128.27 71.755) (xy 128.27 74.295)))
  (wire (pts (xy 158.75 87.63) (xy 167.005 87.63)))
  (wire (pts (xy 106.68 87.63) (xy 106.68 79.375)))
  (wire (pts (xy 186.055 98.425) (xy 198.12 98.425)))
  (wire (pts (xy 128.27 74.295) (xy 128.27 76.835)))
  (wire (pts (xy 128.27 87.63) (xy 158.75 87.63)))
  (hierarchical_label "REG_GND" (shape input) (at 94.615 129.54 180))
  (hierarchical_label "REG_IN" (shape input) (at 88.9 56.515 180))
  (hierarchical_label "REG_5V" (shape input) (at 198.12 56.515 0))
  (hierarchical_label "REG_3V" (shape input) (at 198.12 98.425 0))
  (symbol (lib_id "Device:C") (at 175.895 83.82 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C41" (id 0) (at 178.816 82.6516 0))
    (property "Value" "2u2" (id 1) (at 178.816 84.963 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 176.8602 87.63 0))
    (property "Datasheet" "~" (id 3) (at 175.895 83.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 158.75 122.555 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C38" (id 0) (at 161.671 121.3866 0))
    (property "Value" "2u2" (id 1) (at 161.671 123.698 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 159.7152 126.365 0))
    (property "Datasheet" "~" (id 3) (at 158.75 122.555 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 186.055 125.73 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C46" (id 0) (at 189.0522 124.5616 0))
    (property "Value" "100u" (id 1) (at 189.0522 126.873 0))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D_Pad2.25x2.55mm_HandSolder" (id 2) (at 187.0202 129.54 0))
    (property "Datasheet" "~" (id 3) (at 186.055 125.73 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 158.75 80.645 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C37" (id 0) (at 161.671 79.4766 0))
    (property "Value" "2u2" (id 1) (at 161.671 81.788 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 159.7152 84.455 0))
    (property "Datasheet" "~" (id 3) (at 158.75 80.645 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 163.83 102.235 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C40" (id 0) (at 166.751 101.0666 0))
    (property "Value" "470n" (id 1) (at 166.751 103.378 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 164.7952 106.045 0))
    (property "Datasheet" "~" (id 3) (at 163.83 102.235 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 114.3 125.73 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R32" (id 0) (at 118.11 125.095 0))
    (property "Value" "56k" (id 1) (at 118.745 127 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 112.522 125.73 90))
    (property "Datasheet" "~" (id 3) (at 114.3 125.73 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 182.245 113.665 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C44" (id 0) (at 182.245 117.475 90))
    (property "Value" "33p" (id 1) (at 182.245 119.38 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 178.435 114.6302 0))
    (property "Datasheet" "~" (id 3) (at 182.245 113.665 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 182.245 71.755 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C43" (id 0) (at 182.245 75.565 90))
    (property "Value" "33p" (id 1) (at 182.245 77.47 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 178.435 72.7202 0))
    (property "Datasheet" "~" (id 3) (at 182.245 71.755 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "jlib_1:LM43600") (at 143.51 66.675 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U5" (id 0) (at 143.51 49.7332 0))
    (property "Value" "LM43600" (id 1) (at 143.51 52.0446 0))
    (property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm" (id 2) (at 143.51 66.675 0))
    (property "Datasheet" "" (id 3) (at 143.51 66.675 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:C") (at 106.68 75.565 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C33" (id 0) (at 109.601 74.3966 0))
    (property "Value" "2u2" (id 1) (at 109.601 76.708 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 107.6452 79.375 0))
    (property "Datasheet" "~" (id 3) (at 106.68 75.565 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 175.895 125.73 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C42" (id 0) (at 178.816 124.5616 0))
    (property "Value" "2u2" (id 1) (at 178.816 126.873 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 176.8602 129.54 0))
    (property "Datasheet" "~" (id 3) (at 175.895 125.73 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Core_Ferrite") (at 171.45 98.425 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L6" (id 0) (at 167.005 95.25 90))
    (property "Value" "22u" (id 1) (at 173.99 95.25 90))
    (property "Footprint" "Inductor_SMD:L_Coilcraft_LPS5030" (id 2) (at 171.45 98.425 0))
    (property "Datasheet" "~" (id 3) (at 171.45 98.425 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 114.3 102.235 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R31" (id 0) (at 118.11 101.6 0))
    (property "Value" "100k" (id 1) (at 118.745 103.505 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 112.522 102.235 90))
    (property "Datasheet" "~" (id 3) (at 114.3 102.235 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 163.83 60.325 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C39" (id 0) (at 166.751 59.1566 0))
    (property "Value" "470n" (id 1) (at 166.751 61.468 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 164.7952 64.135 0))
    (property "Datasheet" "~" (id 3) (at 163.83 60.325 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Core_Ferrite") (at 171.45 56.515 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L5" (id 0) (at 168.91 53.34 90))
    (property "Value" "33u" (id 1) (at 173.99 53.34 90))
    (property "Footprint" "Inductor_SMD:L_Coilcraft_LPS5030" (id 2) (at 171.45 56.515 0))
    (property "Datasheet" "~" (id 3) (at 171.45 56.515 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 114.3 83.82 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R30" (id 0) (at 118.11 83.185 0))
    (property "Value" "56k" (id 1) (at 118.745 85.09 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 112.522 83.82 90))
    (property "Datasheet" "~" (id 3) (at 114.3 83.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 167.005 125.73 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R34" (id 0) (at 170.815 125.095 0))
    (property "Value" "442k" (id 1) (at 171.45 127 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 165.227 125.73 90))
    (property "Datasheet" "~" (id 3) (at 167.005 125.73 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 100.33 56.515 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R27" (id 0) (at 97.155 53.975 90))
    (property "Value" "0R" (id 1) (at 102.235 53.975 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 100.33 58.293 90))
    (property "Datasheet" "~" (id 3) (at 100.33 56.515 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "jlib_1:LM43600") (at 143.51 108.585 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U6" (id 0) (at 143.51 91.6432 0))
    (property "Value" "LM43600" (id 1) (at 143.51 93.9546 0))
    (property "Footprint" "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm" (id 2) (at 143.51 108.585 0))
    (property "Datasheet" "" (id 3) (at 143.51 108.585 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R") (at 102.87 98.425 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R28" (id 0) (at 99.695 95.885 90))
    (property "Value" "0R" (id 1) (at 104.775 95.885 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 102.87 100.203 90))
    (property "Datasheet" "~" (id 3) (at 102.87 98.425 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 106.68 117.475 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C34" (id 0) (at 109.601 116.3066 0))
    (property "Value" "2u2" (id 1) (at 109.601 118.618 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 107.6452 121.285 0))
    (property "Datasheet" "~" (id 3) (at 106.68 117.475 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 121.285 114.935 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C36" (id 0) (at 124.206 113.7666 0))
    (property "Value" "2u2" (id 1) (at 124.206 116.078 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 122.2502 118.745 0))
    (property "Datasheet" "~" (id 3) (at 121.285 114.935 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 182.245 64.135 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R35" (id 0) (at 182.245 59.055 90))
    (property "Value" "1M" (id 1) (at 181.61 61.595 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 182.245 62.357 90))
    (property "Datasheet" "~" (id 3) (at 182.245 64.135 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP") (at 186.055 83.82 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C45" (id 0) (at 189.0522 82.6516 0))
    (property "Value" "100u" (id 1) (at 189.0522 84.963 0))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D_Pad2.25x2.55mm_HandSolder" (id 2) (at 187.0202 87.63 0))
    (property "Datasheet" "~" (id 3) (at 186.055 83.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 114.3 60.325 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R29" (id 0) (at 118.11 59.69 0))
    (property "Value" "100k" (id 1) (at 118.745 61.595 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 112.522 60.325 90))
    (property "Datasheet" "~" (id 3) (at 114.3 60.325 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 167.005 83.82 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R33" (id 0) (at 170.815 83.185 0))
    (property "Value" "255k" (id 1) (at 171.45 85.09 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 165.227 83.82 90))
    (property "Datasheet" "~" (id 3) (at 167.005 83.82 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 182.245 106.045 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R36" (id 0) (at 182.245 100.965 90))
    (property "Value" "1M" (id 1) (at 181.61 103.505 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 182.245 104.267 90))
    (property "Datasheet" "~" (id 3) (at 182.245 106.045 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 121.285 73.025 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C35" (id 0) (at 124.206 71.8566 0))
    (property "Value" "2u2" (id 1) (at 124.206 74.168 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 122.2502 76.835 0))
    (property "Datasheet" "~" (id 3) (at 121.285 73.025 0))
    (pin "1")
    (pin "2")
  )
)
