(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (grid_origin 112.6 -45)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer false)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerb/")
    )
  )
  (net 0 "")
  (net 1 "GNDREF")
  (net 2 "GND")
  (net 3 "Net-(C4-Pad1)")
  (net 4 "+12V")
  (net 5 "Net-(C18-Pad1)")
  (net 6 "/nvm_pmain_amp/OUT_P")
  (net 7 "/nvm_pmain_amp/OUT_N")
  (net 8 "Earth")
  (net 9 "Net-(C1-Pad1)")
  (net 10 "Net-(C32-Pad1)")
  (net 11 "Net-(C1-Pad2)")
  (net 12 "Net-(JP1-Pad2)")
  (net 13 "Net-(JP1-Pad3)")
  (net 14 "GNDA")
  (net 15 "Net-(C7-Pad1)")
  (net 16 "Net-(C30-Pad1)")
  (net 17 "+5V")
  (net 18 "+3V3")
  (net 19 "+3.3VADC")
  (net 20 "/nvm_pcb_pmain_digital/X1")
  (net 21 "/nvm_pcb_pmain_digital/X2")
  (net 22 "/nvm_pcb_pmain_digital/VREF_M")
  (net 23 "/nvm_pcb_pmain_digital/LED1")
  (net 24 "/nvm_pcb_pmain_digital/LED2")
  (net 25 "/nvm_pcb_pmain_digital/E_CS")
  (net 26 "/nvm_pcb_pmain_digital/E_SCK")
  (net 27 "/nvm_pcb_pmain_digital/E_MOSI")
  (net 28 "/nvm_pcb_pmain_digital/E_RST")
  (net 29 "/nvm_pcb_pmain_digital/E_MISO")
  (net 30 "/nvm_pcb_pmain_digital/AN3")
  (net 31 "/nvm_pcb_pmain_digital/AN2")
  (net 32 "/nvm_pcb_pmain_digital/AN1")
  (net 33 "/nvm_pcb_pmain_digital/K1")
  (net 34 "/nvm_pcb_pmain_digital/K3")
  (net 35 "/nvm_pcb_pmain_digital/K5")
  (net 36 "/nvm_pcb_pmain_digital/K7")
  (net 37 "/nvm_pcb_pmain_digital/K2")
  (net 38 "/nvm_pcb_pmain_digital/K4")
  (net 39 "/nvm_pcb_pmain_digital/K6")
  (net 40 "/nvm_pcb_pmain_digital/K8")
  (net 41 "/nvm_pcb_pmain_digital/DOT7")
  (net 42 "/nvm_pcb_pmain_digital/DOT5")
  (net 43 "/nvm_pcb_pmain_digital/DOT2")
  (net 44 "/nvm_pcb_pmain_digital/DOT8")
  (net 45 "/nvm_pcb_pmain_digital/DOT6")
  (net 46 "/nvm_pcb_pmain_digital/DOT3")
  (net 47 "/nvm_pcb_pmain_digital/DOT1")
  (net 48 "/nvm_pcb_pmain_digital/SWCLK")
  (net 49 "/nvm_pcb_pmain_digital/NRST")
  (net 50 "/nvm_pcb_pmain_digital/SWDIO")
  (net 51 "/nvm_pcb_pmain_digital/EE_CS")
  (net 52 "/nvm_pcb_pmain_digital/EE_MISO")
  (net 53 "/nvm_pcb_pmain_digital/EE_MOSI")
  (net 54 "/nvm_pcb_pmain_digital/EE_SCK")
  (net 55 "/nvm_pcb_pmain_digital/DO5")
  (net 56 "/nvm_pcb_pmain_digital/DO6")
  (net 57 "/nvm_pcb_pmain_digital/DO7")
  (net 58 "/nvm_pcb_pmain_digital/DO8")
  (net 59 "/nvm_pcb_pmain_digital/DO1")
  (net 60 "/nvm_pcb_pmain_digital/DO3")
  (net 61 "/nvm_pcb_pmain_digital/DO2")
  (net 62 "Net-(C8-Pad2)")
  (net 63 "Net-(C17-Pad1)")
  (net 64 "Net-(C19-Pad1)")
  (net 65 "Net-(C28-Pad1)")
  (net 66 "Net-(C8-Pad1)")
  (net 67 "Net-(C9-Pad2)")
  (net 68 "Net-(C10-Pad2)")
  (net 69 "Net-(F1-Pad2)")
  (net 70 "Net-(C14-Pad2)")
  (net 71 "Net-(F1-Pad1)")
  (net 72 "Net-(C15-Pad2)")
  (net 73 "Net-(C20-Pad1)")
  (net 74 "Net-(C21-Pad1)")
  (net 75 "Net-(C22-Pad1)")
  (net 76 "Net-(C23-Pad1)")
  (net 77 "Net-(C27-Pad1)")
  (net 78 "Net-(R1-Pad1)")
  (net 79 "Net-(R1-Pad2)")
  (net 80 "Net-(C27-Pad2)")
  (net 81 "Net-(C28-Pad2)")
  (net 82 "/nvm_pcb_pmain_digital/AB_CTRL")
  (net 83 "/nvm_pcb_pmain_digital/AB_RST")
  (net 84 "/nvm_pcb_pmain_digital/AB_TX")
  (net 85 "/nvm_pcb_pmain_digital/AB_RX")
  (net 86 "/nvm_pcb_pmain_digital/EIO1")
  (net 87 "/nvm_pcb_pmain_digital/EU2RX")
  (net 88 "/nvm_pcb_pmain_digital/EU1RX")
  (net 89 "/nvm_pcb_pmain_digital/EIO2")
  (net 90 "/nvm_pcb_pmain_digital/EU2TX")
  (net 91 "/nvm_pcb_pmain_digital/EU1TX")
  (net 92 "/nvm_pcb_pmain_digital/EX12")
  (net 93 "/nvm_pcb_pmain_digital/EX11")
  (net 94 "/nvm_pcb_pmain_digital/EX10")
  (net 95 "/nvm_pcb_pmain_digital/EX9")
  (net 96 "/nvm_pcb_pmain_digital/EX8")
  (net 97 "/nvm_pcb_pmain_digital/EX7")
  (net 98 "/nvm_pcb_pmain_digital/EX6")
  (net 99 "/nvm_pcb_pmain_digital/EX5")
  (net 100 "/nvm_pcb_pmain_digital/EX4")
  (net 101 "/nvm_pcb_pmain_digital/EX3")
  (net 102 "/nvm_pcb_pmain_digital/EX2")
  (net 103 "/nvm_pcb_pmain_digital/EX1")
  (net 104 "Net-(Q1-Pad1)")
  (net 105 "Net-(C29-Pad2)")
  (net 106 "/nvm_pcb_pmain_digital/ZCD_C")
  (net 107 "/nvm_pcb_pmain_digital/ZCD")
  (net 108 "Net-(C35-Pad1)")
  (net 109 "Net-(J6-Pad5)")
  (net 110 "Net-(J6-Pad6)")
  (net 111 "Net-(C37-Pad1)")
  (net 112 "+9VA")
  (net 113 "Net-(C39-Pad1)")
  (net 114 "/nvm_pcb_pmain_digital/MUTE")
  (net 115 "Net-(C43-Pad1)")
  (net 116 "Net-(C45-Pad2)")
  (net 117 "Net-(C57-Pad1)")
  (net 118 "Net-(C61-Pad2)")
  (net 119 "Net-(C13-Pad1)")
  (net 120 "Net-(C14-Pad1)")
  (net 121 "Net-(C62-Pad2)")
  (net 122 "Net-(C19-Pad2)")
  (net 123 "Net-(C63-Pad2)")
  (net 124 "Net-(C35-Pad2)")
  (net 125 "Net-(C36-Pad2)")
  (net 126 "Net-(C64-Pad2)")
  (net 127 "Net-(C59-Pad1)")
  (net 128 "/nvm_pmain_fpsu/FGND_A")
  (net 129 "Net-(D1-Pad2)")
  (net 130 "/nvm_pmain_fpsu/FGND_D")
  (net 131 "/nvm_pmain_fpsu/F5V_A")
  (net 132 "/nvm_pmain_fpsu/F5V_D")
  (net 133 "/nvm_pmain_fpsu/F+15V")
  (net 134 "/nvm_pmain_fpsu/F-15V")
  (net 135 "Net-(D2-Pad2)")
  (net 136 "Net-(D3-Pad1)")
  (net 137 "Net-(D4-Pad1)")
  (net 138 "Net-(D5-Pad3)")
  (net 139 "Net-(D5-Pad4)")
  (net 140 "unconnected-(J3-Pad2)")
  (net 141 "Net-(D7-Pad1)")
  (net 142 "Net-(D9-Pad1)")
  (net 143 "/nvm_pmain_fpsu/REC_S_HI")
  (net 144 "/nvm_pmain_fpsu/REC_S_LO")
  (net 145 "/nvm_pmain_fpsu/REC_S_MID")
  (net 146 "/nvm_pmain_fpsu/REC_N_HI")
  (net 147 "/nvm_pmain_fpsu/REC_N_LO")
  (net 148 "Net-(J3-Pad3)")
  (net 149 "unconnected-(J3-Pad4)")
  (net 150 "Net-(R13-Pad1)")
  (net 151 "unconnected-(J6-Pad11)")
  (net 152 "Net-(J8-Pad1)")
  (net 153 "Net-(J8-Pad2)")
  (net 154 "Net-(J8-Pad7)")
  (net 155 "unconnected-(U6-Pad6)")
  (net 156 "unconnected-(U6-Pad7)")
  (net 157 "unconnected-(U6-Pad8)")
  (net 158 "Net-(J8-Pad9)")
  (net 159 "Net-(J8-Pad11)")
  (net 160 "Net-(J8-Pad13)")
  (net 161 "Net-(J8-Pad15)")
  (net 162 "Net-(J9-Pad3)")
  (net 163 "Net-(J9-Pad4)")
  (net 164 "Net-(J9-Pad5)")
  (net 165 "Net-(C6-Pad1)")
  (net 166 "Net-(C9-Pad1)")
  (net 167 "Net-(C12-Pad1)")
  (net 168 "Net-(J9-Pad6)")
  (net 169 "Net-(J10-Pad1)")
  (net 170 "Net-(D8-Pad1)")
  (net 171 "Net-(J10-Pad2)")
  (net 172 "Net-(R23-Pad1)")
  (net 173 "Net-(J10-Pad3)")
  (net 174 "Net-(J10-Pad4)")
  (net 175 "Net-(R32-Pad2)")
  (net 176 "Net-(J10-Pad5)")
  (net 177 "Net-(J10-Pad6)")
  (net 178 "Net-(J10-Pad7)")
  (net 179 "Net-(J10-Pad8)")
  (net 180 "Net-(J10-Pad9)")
  (net 181 "Net-(J10-Pad10)")
  (net 182 "Net-(J10-Pad11)")
  (net 183 "Net-(J6-Pad7)")
  (net 184 "Net-(J6-Pad8)")
  (net 185 "Net-(J10-Pad12)")
  (net 186 "Net-(Q2-Pad1)")
  (net 187 "Net-(R2-Pad1)")
  (net 188 "Net-(R2-Pad2)")
  (net 189 "Net-(R7-Pad2)")
  (net 190 "Net-(J7-Pad3)")
  (net 191 "Net-(J7-Pad5)")
  (net 192 "Net-(R15-Pad2)")
  (net 193 "Net-(R18-Pad1)")
  (net 194 "Net-(R20-Pad1)")
  (net 195 "Net-(R22-Pad1)")
  (net 196 "Net-(R23-Pad2)")
  (net 197 "Net-(R24-Pad1)")
  (net 198 "Net-(J7-Pad4)")
  (net 199 "Net-(J7-Pad6)")
  (net 200 "Net-(J8-Pad3)")
  (net 201 "Net-(J8-Pad4)")
  (net 202 "Net-(J8-Pad5)")
  (net 203 "Net-(J8-Pad6)")
  (net 204 "Net-(R36-Pad2)")
  (net 205 "Net-(R46-Pad2)")
  (net 206 "Net-(R58-Pad2)")
  (net 207 "Net-(R62-Pad2)")
  (net 208 "unconnected-(U5-Pad16)")
  (net 209 "unconnected-(U5-Pad26)")
  (net 210 "unconnected-(U5-Pad27)")
  (net 211 "unconnected-(U5-Pad29)")
  (net 212 "unconnected-(U5-Pad30)")
  (net 213 "/nvm_pcb_pmain_digital/KC5")
  (net 214 "/nvm_pcb_pmain_digital/KC6")
  (net 215 "/nvm_pcb_pmain_digital/KC7")
  (net 216 "/nvm_pcb_pmain_digital/KC8")
  (net 217 "unconnected-(U9-Pad7)")
  (net 218 "unconnected-(U9-Pad8)")
  (net 219 "unconnected-(U9-Pad9)")
  (net 220 "unconnected-(U9-Pad15)")
  (net 221 "unconnected-(U9-Pad16)")
  (net 222 "unconnected-(U9-Pad18)")
  (net 223 "unconnected-(U9-Pad19)")
  (net 224 "unconnected-(U9-Pad27)")
  (net 225 "unconnected-(U9-Pad29)")
  (net 226 "unconnected-(U9-Pad30)")
  (net 227 "unconnected-(U9-Pad31)")
  (net 228 "unconnected-(U9-Pad32)")
  (net 229 "unconnected-(U9-Pad33)")
  (net 230 "unconnected-(U9-Pad37)")
  (net 231 "unconnected-(U9-Pad38)")
  (net 232 "unconnected-(U9-Pad39)")
  (net 233 "unconnected-(U9-Pad40)")
  (net 234 "unconnected-(U9-Pad41)")
  (net 235 "unconnected-(U9-Pad42)")
  (net 236 "unconnected-(U9-Pad43)")
  (net 237 "unconnected-(U9-Pad44)")
  (net 238 "unconnected-(U9-Pad45)")
  (net 239 "unconnected-(U9-Pad46)")
  (net 240 "unconnected-(U9-Pad47)")
  (net 241 "unconnected-(U9-Pad53)")
  (net 242 "/nvm_pcb_pmain_digital/S_DRIV")
  (net 243 "/nvm_pcb_pmain_digital/S_MUTE")
  (net 244 "unconnected-(U7-Pad6)")
  (net 245 "unconnected-(U7-Pad7)")
  (net 246 "Net-(C65-Pad1)")
  (net 247 "unconnected-(U7-Pad8)")
  (net 248 "Net-(C65-Pad2)")
  (net 249 "unconnected-(U8-Pad9)")
  (net 250 "Net-(C67-Pad1)")
  (net 251 "Net-(LS1-Pad2)")
  (net 252 "Net-(Q3-Pad1)")
  (net 253 "/nvm_pcb_pmain_digital/BEEP")
  (net 254 "/nvm_pmain_fpsu/F+8V")
  (net 255 "/nvm_pmain_fpsu/F-8V")
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 160 -141.5 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -4.2 180) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 204 -104.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 157 -99.5 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "PN" "EEAGA1E220H")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C7" (at 0 -4.1 180) (layer "F.SilkS"))
    (fp_text value "22u" (at 1.25 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L18.0mm_W6.0mm_P15.00mm_FKS3_FKP3" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 168 -144.5)
    (descr "C, Rect series, Radial, pin pitch=15.00mm, , length*width=18*6mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_3.pdf")
    (tags "C Rect series Radial pin pitch 15.00mm  length 18mm width 6mm Capacitor")
    (property "PN" "R75PI24704030J")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "link" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C2" (at -2.9 -1.5) (layer "F.SilkS"))
    (fp_text value "47n" (at 7.5 4.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 15 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L18.0mm_W6.0mm_P15.00mm_FKS3_FKP3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm_Mask4.11x4.36mm" (layer "F.Cu")
    (tedit 5A671CA1)
    (at 163 -120.5)
    (descr "HTSSOP32: plastic thin shrink small outline package; 32 leads; body width 6.1 mm; lead pitch 0.65 mm (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot487-1_po.pdf)")
    (tags "SSOP 0.65 PowerPAD")
    (property "PN" "TPA3116D2DAD")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr smd)
    (fp_text reference "U5" (at 0 -6.55) (layer "F.SilkS"))
    (fp_text value "TPS3116D2" (at 0 6.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd rect locked (at 0 -1.46) (size 1.07 1.16) (layers "F.Paste"))
    (pad "" smd rect locked (at -1.37 -1.46) (size 1.07 1.16) (layers "F.Paste"))
    (pad "" smd rect locked (at 0 0) (size 1.07 1.16) (layers "F.Paste"))
    (pad "" smd rect locked (at -1.37 1.46) (size 1.07 1.16) (layers "F.Paste"))
    (pad "" smd rect locked (at 0 0) (size 4.11 4.36) (layers "F.Mask"))
    (pad "" smd rect locked (at -1.37 0) (size 1.07 1.16) (layers "F.Paste"))
    (pad "" smd rect locked (at 1.37 -1.46) (size 1.07 1.16) (layers "F.Paste"))
    (pad "" smd rect locked (at 1.37 1.46) (size 1.07 1.16) (layers "F.Paste"))
    (pad "" smd rect locked (at 0 1.46) (size 1.07 1.16) (layers "F.Paste"))
    (pad "" smd rect locked (at 1.37 0) (size 1.07 1.16) (layers "F.Paste"))
    (pad "1" smd rect locked (at -3.65 -4.875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "MODSEL") (pintype "input"))
    (pad "2" smd rect locked (at -3.65 -4.225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(R13-Pad1)") (pinfunction "SDZ") (pintype "input"))
    (pad "3" smd rect locked (at -3.65 -3.575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(R13-Pad1)") (pinfunction "FAULTZ") (pintype "input"))
    (pad "4" smd rect locked (at -3.65 -2.925) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(C4-Pad1)") (pinfunction "RINP") (pintype "input"))
    (pad "5" smd rect locked (at -3.65 -2.275) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "Net-(C6-Pad1)") (pinfunction "RINN") (pintype "input"))
    (pad "6" smd rect locked (at -3.65 -1.625) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "Net-(R23-Pad1)") (pinfunction "PLIMIT") (pintype "input"))
    (pad "7" smd rect locked (at -3.65 -0.975) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 196 "Net-(R23-Pad2)") (pinfunction "GVDD") (pintype "input"))
    (pad "8" smd rect locked (at -3.65 -0.325) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 197 "Net-(R24-Pad1)") (pinfunction "GAIN/SLV") (pintype "input"))
    (pad "9" smd rect locked (at -3.65 0.325) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "10" smd rect locked (at -3.65 0.975) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "Net-(C9-Pad1)") (pinfunction "LINP") (pintype "input"))
    (pad "11" smd rect locked (at -3.65 1.625) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 119 "Net-(C13-Pad1)") (pinfunction "LINN") (pintype "input"))
    (pad "12" smd rect locked (at -3.65 2.275) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "/nvm_pcb_pmain_digital/MUTE") (pinfunction "MUTE") (pintype "input"))
    (pad "13" smd rect locked (at -3.65 2.925) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "AM2") (pintype "input"))
    (pad "14" smd rect locked (at -3.65 3.575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "AM1") (pintype "input"))
    (pad "15" smd rect locked (at -3.65 4.225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "AM0") (pintype "input"))
    (pad "16" smd rect locked (at -3.65 4.875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 208 "unconnected-(U5-Pad16)") (pinfunction "SYNC") (pintype "input"))
    (pad "17" smd rect locked (at 3.65 4.875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+12V") (pinfunction "AVCC") (pintype "input"))
    (pad "18" smd rect locked (at 3.65 4.225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+12V") (pinfunction "PVCC") (pintype "input"))
    (pad "19" smd rect locked (at 3.65 3.575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+12V") (pinfunction "PVCC") (pintype "input"))
    (pad "20" smd rect locked (at 3.65 2.925) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "Net-(C14-Pad2)") (pinfunction "BSNL") (pintype "input"))
    (pad "21" smd rect locked (at 3.65 2.275) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 120 "Net-(C14-Pad1)") (pinfunction "OUTNL") (pintype "input"))
    (pad "22" smd rect locked (at 3.65 1.625) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "23" smd rect locked (at 3.65 0.975) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "Net-(C8-Pad1)") (pinfunction "OUTPL") (pintype "input"))
    (pad "24" smd rect locked (at 3.65 0.325) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "Net-(C8-Pad2)") (pinfunction "BSPL") (pintype "input"))
    (pad "25" smd rect locked (at 3.65 -0.325) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "26" smd rect locked (at 3.65 -0.975) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 209 "unconnected-(U5-Pad26)") (pinfunction "BSNR") (pintype "input"))
    (pad "27" smd rect locked (at 3.65 -1.625) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 210 "unconnected-(U5-Pad27)") (pinfunction "OUTNR") (pintype "input"))
    (pad "28" smd rect locked (at 3.65 -2.275) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input"))
    (pad "29" smd rect locked (at 3.65 -2.925) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 211 "unconnected-(U5-Pad29)") (pinfunction "OUTPR") (pintype "input"))
    (pad "30" smd rect locked (at 3.65 -3.575) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 212 "unconnected-(U5-Pad30)") (pinfunction "BSPR") (pintype "input"))
    (pad "31" smd rect locked (at 3.65 -4.225) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+12V") (pinfunction "PVCC") (pintype "input"))
    (pad "32" smd rect locked (at 3.65 -4.875) (size 1.2 0.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+12V") (pinfunction "PVCC") (pintype "input"))
    (pad "33" smd rect locked (at 0 0) (size 5.2 11) (layers "F.Cu")
      (net 2 "GND") (pinfunction "PAD") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-32-1EP_6.1x11mm_P0.65mm_EP5.2x11mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 171 -86.5 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "PN" "EEAGA1E220H")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C5" (at 3.5 -3.75 180) (layer "F.SilkS"))
    (fp_text value "22u" (at 1.25 3.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 252.367677 -88 180)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (property "PN" "EEUFR1V122B")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "link" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C67" (at 2.5 -7.5 180) (layer "F.SilkS"))
    (fp_text value "1m2" (at 2.5 7.5 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 180) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 250 "Net-(C67-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 130 "/nvm_pmain_fpsu/FGND_D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Wide" (layer "F.Cu")
    (tedit 5A2795B7)
    (at 159.54 -105.27 180)
    (descr "TO-92 leads molded, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "PN" "L78L09ABZ")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "U3" (at -1.56 0.73) (layer "F.SilkS"))
    (fp_text value "L78L09" (at 2.54 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "+9VA") (pinfunction "VO") (pintype "power_out"))
    (pad "2" thru_hole circle locked (at 2.54 -2.54 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole circle locked (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "+12V") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 190.2 -79.1)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (property "PN" "ZL201-10G")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J11" (at 3.2 2.7) (layer "F.SilkS"))
    (fp_text value "Conn_01x05_Male" (at 0 12.49) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/nvm_pcb_pmain_digital/SWCLK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/nvm_pcb_pmain_digital/NRST") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 50 "/nvm_pcb_pmain_digital/SWDIO") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_KK-396_A-41791-0005_1x05_P3.96mm_Vertical" (layer "F.Cu")
    (tedit 61DC2F9F)
    (at 194.5 -172.42 -90)
    (descr "Molex KK 396 Interconnect System, old/engineering part number: A-41791-0005 example for new part number: 26-60-4050, 5 Pins (https://www.molex.com/pdm_docs/sd/026604020_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-396 vertical")
    (property "PN" "A3960WV-05P")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "remove pins 2 and 4")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J3" (at 7.92 -6.31 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x05_Male" (at 7.92 6.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 7.92 -4.41 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.07911392405)
      (net 8 "Earth") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle (at 8 -2.6 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 140 "unconnected-(J3-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 7.92 0 270) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 148 "Net-(J3-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle (at 15.8 -2.6 270) (size 0.6 0.6) (drill 0.3) (layers *.Cu *.Mask)
      (net 149 "unconnected-(J3-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 15.84 0 270) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 71 "Net-(F1-Pad1)") (pinfunction "Pin_5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-396_A-41791-0005_1x05_P3.96mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D3.50mm_Drill1.4mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 125.4 -49.5)
    (descr "wire loop with bead as test point, loop diameter 3.5mm, hole diameter 1.4mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "optional")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP2" (at 2.2 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D3.50mm_Drill1.4mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x07_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 121.7525 -66.88 180)
    (descr "Through hole IDC box header, 2x07, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x07 2.54mm double row")
    (property "PN" " T821-1-14-S1")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J6" (at -4.8475 21.62) (layer "F.SilkS"))
    (fp_text value "Conn_02x07_Odd_Even" (at 1.27 21.34) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 7.62 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 41 "/nvm_pcb_pmain_digital/DOT7") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/nvm_pcb_pmain_digital/DOT8") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/nvm_pcb_pmain_digital/DOT5") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 2.54 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/nvm_pcb_pmain_digital/DOT6") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 "Net-(J6-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.54 5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 "Net-(J6-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 183 "Net-(J6-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 2.54 7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 184 "Net-(J6-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/nvm_pcb_pmain_digital/DOT2") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle locked (at 2.54 10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/nvm_pcb_pmain_digital/DOT3") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle locked (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 151 "unconnected-(J6-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle locked (at 2.54 12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/nvm_pcb_pmain_digital/DOT1") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle locked (at 0 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle locked (at 2.54 15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "+5V") (pinfunction "Pin_14") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x07_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 240 -73.5 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "PN" "LM337TG")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "U17" (at 4 2) (layer "B.SilkS"))
    (fp_text value "LM337_TO220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 118 "Net-(C61-Pad2)") (pinfunction "ADJ") (pintype "input"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 134 "/nvm_pmain_fpsu/F-15V") (pinfunction "VI") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 255 "/nvm_pmain_fpsu/F-8V") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 151 -135.5 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-1U/50")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C6" (at -3.1 0) (layer "F.SilkS"))
    (fp_text value "1u" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 165 "Net-(C6-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open" (layer "F.Cu")
    (tedit 5D717D34)
    (at 187.25 -154 180)
    (descr "Fuseholder horizontal open, 5x20mm, 500V, 16A, Schurter 0031.8201, https://us.schurter.com/bundles/snceschurter/epim/_ProdPool_/newDS/en/typ_OGN.pdf")
    (tags "Fuseholder horizontal open 5x20 Schurter 0031.8201")
    (property "PN" "0031.8211")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "F1" (at -1.85 -1.5) (layer "F.SilkS"))
    (fp_text value "Fuse" (at 11.25 6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.25 4) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 11.25 0 180) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 71 "Net-(F1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 22.5 0 180) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 69 "Net-(F1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuseholder_Cylinder-5x20mm_Schurter_0031_8201_Horizontal_Open.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 203.6 -123)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H12" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 151 -110.5 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "PN" "EEAGA1E220H")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C3" (at 1.25 -3.75) (layer "F.SilkS"))
    (fp_text value "22u" (at 1.25 3.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 112 "+9VA") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 261 -47.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 151 -139.5 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-1U/50")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C4" (at -3.1 0) (layer "F.SilkS"))
    (fp_text value "1u" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 181 -94.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-220N/63-R")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C22" (at -2.9 0) (layer "F.SilkS"))
    (fp_text value "220n" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 75 "Net-(C22-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 116 -94.1 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "PN" "KP-2012YD")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D7" (at 0 -2.1 180) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 141 "Net-(D7-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 4 "+12V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 131.46 -79.58)
    (descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x05 2.54mm double row")
    (property "PN" "T821-1-10-S1")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J7" (at 1.27 -6.1) (layer "F.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.27 16.26) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 5.08 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 190 "Net-(J7-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 198 "Net-(J7-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 191 "Net-(J7-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 199 "Net-(J7-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 213 "/nvm_pcb_pmain_digital/KC5") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 214 "/nvm_pcb_pmain_digital/KC6") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 215 "/nvm_pcb_pmain_digital/KC7") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle locked (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 216 "/nvm_pcb_pmain_digital/KC8") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "jlib2:beeper12" (layer "F.Cu")
    (tedit 61DC2C52)
    (at 192 -59.7 -135)
    (property "PN" "LD-BZEN-1205")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "LS1" (at -6.646804 -0.707107 -45 unlocked) (layer "F.SilkS"))
    (fp_text value "Speaker" (at -0.777817 1.767767 -135 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -3.25 0 225) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 116 "Net-(C45-Pad2)") (pinfunction "1") (pintype "input"))
    (pad "2" thru_hole circle (at 3.25 0 225) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 251 "Net-(LS1-Pad2)") (pinfunction "2") (pintype "input"))
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 186 -102.5 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-1U/50")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C19" (at 0.4 3) (layer "F.SilkS"))
    (fp_text value "1u" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(C19-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 "Net-(C19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 163 -130.5)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Molex:Molex_KK-396_A-41791-0006_1x06_P3.96mm_Vertical" (layer "F.Cu")
    (tedit 5DC431B4)
    (at 233.88 -96.71 180)
    (descr "Molex KK 396 Interconnect System, old/engineering part number: A-41791-0006 example for new part number: 26-60-4060, 6 Pins (https://www.molex.com/pdm_docs/sd/026604020_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-396 vertical")
    (property "PN" "A3960WV-06P")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J4" (at 9.9 -6.31) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 9.9 6.1) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 9.9 -4.41) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.07911392405)
      (net 146 "/nvm_pmain_fpsu/REC_N_HI") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 3.96 0 180) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 147 "/nvm_pmain_fpsu/REC_N_LO") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 7.92 0 180) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 143 "/nvm_pmain_fpsu/REC_S_HI") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 11.88 0 180) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 145 "/nvm_pmain_fpsu/REC_S_MID") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 15.84 0 180) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 144 "/nvm_pmain_fpsu/REC_S_LO") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 19.8 0 180) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 145 "/nvm_pmain_fpsu/REC_S_MID") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-396_A-41791-0006_1x06_P3.96mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "j_lib:logo_rpg7x9" (layer "F.Cu")
    (tedit 61CE1C18)
    (at 259.4 -60.2)
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr board_only exclude_from_pos_files)
    (fp_text reference "LOGO1" (at -1.4 -1.8) (layer "F.SilkS") hide)
    (fp_text value "logo_generic" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 183 -75.5 -90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "PN" "KP-2012YD")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D9" (at 0.3 2.2) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0 270) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 142 "Net-(D9-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0 270) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 24 "/nvm_pcb_pmain_digital/LED2") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 193 -90.025)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "PN" "ZL201-10G")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "JP1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Jumper_3_Bridged12" (at 0 7.41) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "Net-(C27-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(JP1-Pad2)") (pinfunction "C") (pintype "input"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(JP1-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 181 -86.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-220N/63-R")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C20" (at -2.4 0) (layer "F.SilkS"))
    (fp_text value "220n" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 73 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 161.84 -77.5 90)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (property "PN" "ZL201-10G")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J10" (at 1.27 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_02x08_Odd_Even" (at 1.27 20.11 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 169 "Net-(J10-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 171 "Net-(J10-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 173 "Net-(J10-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 174 "Net-(J10-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 176 "Net-(J10-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 177 "Net-(J10-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 178 "Net-(J10-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 179 "Net-(J10-Pad8)") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 180 "Net-(J10-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 181 "Net-(J10-Pad10)") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 182 "Net-(J10-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 185 "Net-(J10-Pad12)") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "+3V3") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "+3V3") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "j_lib:NE18-2P" (layer "F.Cu")
    (tedit 61DC2C93)
    (at 155.5 -167.5 180)
    (property "PN" "NE182AEESN6AMP")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "SW1" (at -4.1 -9) (layer "F.SilkS"))
    (fp_text value "NE018" (at -8.5 -9.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 -7.5 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 0 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle (at -17.8 -5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 187 "Net-(R2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -24.8 -6.25 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 69 "Net-(F1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -17.8 5 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 78 "Net-(R1-Pad1)") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -24.8 6.25 180) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 148 "Net-(J3-Pad3)") (pinfunction "4") (pintype "passive"))
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 181 -98.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-22N/63")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C23" (at -2.9 0) (layer "F.SilkS"))
    (fp_text value "22n" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 76 "Net-(C23-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 204 -172.5 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H9" (at 0 -4.2 180) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 253 -73.555 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "PN" "LM317BTG")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "U15" (at 2.54 -5.055) (layer "F.SilkS"))
    (fp_text value "LM317_TO-220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 127 "Net-(C59-Pad1)") (pinfunction "ADJ") (pintype "input"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 254 "/nvm_pmain_fpsu/F+8V") (pinfunction "VO") (pintype "power_out"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 133 "/nvm_pmain_fpsu/F+15V") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 166 -104 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-1U/50")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C13" (at -2 0.4 180) (layer "F.SilkS"))
    (fp_text value "1u" (at 2.5 3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 "Net-(C13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_KK-254_AE-6410-06A_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B)
    (at 197.15 -47.72 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-06A example for new part number: 22-27-2061, 6 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "PN" "NS25-W6P")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J9" (at 15.05 1.28) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 6.35 4.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 -2.22) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.1436781609)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 18 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 162 "Net-(J9-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 163 "Net-(J9-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 10.16 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 164 "Net-(J9-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 12.7 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 168 "Net-(J9-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-06A_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 115 -47.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 204 -47.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P3.50mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 148 -126.847349 90)
    (descr "CP, Radial series, Radial, pin pitch=3.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 3.50mm  diameter 8mm Electrolytic Capacitor")
    (property "PN" "UPA1E471MPD")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "C26" (at -3.347349 1.6 180) (layer "F.SilkS"))
    (fp_text value "470u" (at 1.75 5.25 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.75 0 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 3.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P3.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_KK-396_A-41791-0003_1x03_P3.96mm_Vertical" (layer "F.Cu")
    (tedit 5DC431B4)
    (at 201.705 -138.54 90)
    (descr "Molex KK 396 Interconnect System, old/engineering part number: A-41791-0003 example for new part number: 26-60-4030, 3 Pins (https://www.molex.com/pdm_docs/sd/026604020_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-396 vertical")
    (property "PN" "A3960WV-03P")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J2" (at 3.96 -6.31 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x03_Male" (at 3.96 6.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.96 -4.41 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.07911392405)
      (net 7 "/nvm_pmain_amp/OUT_N") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 3.96 0 90) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 6 "/nvm_pmain_amp/OUT_P") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 7.92 0 90) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 8 "Earth") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-396_A-41791-0003_1x03_P3.96mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "j_lib:KPSB25" (layer "F.Cu")
    (tedit 61D780C3)
    (at 128 -134 -90)
    (property "PN" "KPSB25-12")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "U1" (at 27.5 12.9 unlocked) (layer "F.SilkS"))
    (fp_text value "KPSB25" (at 0 1 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -22.86 -10.16 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 187 "Net-(R2-Pad1)") (pinfunction "AC/L") (pintype "power_in"))
    (pad "2" thru_hole circle (at -22.86 10.16 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 78 "Net-(R1-Pad1)") (pinfunction "AC/N") (pintype "power_in"))
    (pad "3" thru_hole circle (at 22.86 0 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 135 "Net-(D2-Pad2)") (pinfunction "+Vout") (pintype "power_out"))
    (pad "4" thru_hole circle (at 22.86 -10.16 270) (size 3 3) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "-Vout") (pintype "power_out"))
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 115.8 -55.1)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "PN" "KP-2012YD")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D3" (at 1.3 2.1) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 136 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 17 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 146.2475 -83.39)
    (descr "Through hole IDC box header, 2x08, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x08 2.54mm double row")
    (property "PN" "T821-1-16-S1")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J8" (at 1.27 -6.1) (layer "F.SilkS"))
    (fp_text value "Conn_02x08_Odd_Even" (at 1.27 23.88) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 8.89 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 152 "Net-(J8-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 153 "Net-(J8-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 200 "Net-(J8-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 2.54 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 201 "Net-(J8-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 202 "Net-(J8-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.54 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 203 "Net-(J8-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole circle locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 "Net-(J8-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole circle locked (at 2.54 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "+5V") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole circle locked (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 158 "Net-(J8-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole circle locked (at 2.54 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "+3V3") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole circle locked (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 159 "Net-(J8-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole circle locked (at 2.54 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "+3V3") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole circle locked (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 160 "Net-(J8-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole circle locked (at 2.54 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole circle locked (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 161 "Net-(J8-Pad15)") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole circle locked (at 2.54 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 220.5 -72.5)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (property "PN" "EEUFR1V122B")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "link" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C57" (at 2.6 -7.5) (layer "F.SilkS"))
    (fp_text value "1m2" (at 2.5 7.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 117 "Net-(C57-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D3.50mm_Drill1.4mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 195 -79.3)
    (descr "wire loop with bead as test point, loop diameter 3.5mm, hole diameter 1.4mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "optional")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP1" (at 3.1 -1.2) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D3.50mm_Drill1.4mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 115 -104.5 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H10" (at 0 -4.2 180) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Molex:Molex_KK-396_A-41791-0002_1x02_P3.96mm_Vertical" (layer "F.Cu")
    (tedit 5DC431B4)
    (at 149 -144.5 90)
    (descr "Molex KK 396 Interconnect System, old/engineering part number: A-41791-0002 example for new part number: 26-60-4020, 2 Pins (https://www.molex.com/pdm_docs/sd/026604020_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-396 vertical")
    (property "PN" "A3960WV-02P")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J1" (at 7 -0.4 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x02_Male" (at 1.98 6.1 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.98 -4.41 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask) (roundrect_rratio 0.07911392405)
      (net 129 "Net-(D1-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 3.96 0 90) (size 3.16 4.1) (drill 1.7) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-396_A-41791-0002_1x02_P3.96mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 155.45 -86.5 180)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "PN" "T910W-100K")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "RV1" (at -2.54 -3.66) (layer "F.SilkS"))
    (fp_text value "100k" (at -2.54 3.67) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0.005) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 192 "Net-(R15-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(JP1-Pad3)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 180) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(JP1-Pad3)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D12.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF1)
    (at 207.5 -72.5)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=12.5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 12.5mm Electrolytic Capacitor")
    (property "PN" "EEUFR1V122B")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "link" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C62" (at 2.1 -7.5) (layer "F.SilkS"))
    (fp_text value "1m2" (at 2.5 7.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 121 "Net-(C62-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D12.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 237.54 -61.555 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "PN" "L7805ABV")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "U13" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "LM7805_TO220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 117 "Net-(C57-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 131 "/nvm_pmain_fpsu/F5V_A") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 167.7 -138.15)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=12.7mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 12.7mm 1W length 9.9mm diameter 3.6mm")
    (property "PN" "NFR2W-1K")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "link" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "R9" (at -1.6 -1.35) (layer "F.SilkS"))
    (fp_text value "1k" (at 6.35 2.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 12.7 0) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Earth") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P12.70mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 161.5 -93.5 180)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-220N/63-R")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C18" (at 2.5 -3) (layer "F.SilkS"))
    (fp_text value "220n" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(C18-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_KK-254_AE-6410-10A_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B)
    (at 231.84 -48.5)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-10A example for new part number: 22-27-2101, 10 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "PN" "NS25-W10P")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J5" (at 11.43 -4.12) (layer "F.SilkS"))
    (fp_text value "Conn_01x10_Male" (at 11.43 4.08) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 11.43 -2.22) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.1436781609)
      (net 133 "/nvm_pmain_fpsu/F+15V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 133 "/nvm_pmain_fpsu/F+15V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 5.08 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 254 "/nvm_pmain_fpsu/F+8V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 131 "/nvm_pmain_fpsu/F5V_A") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 10.16 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 12.7 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 255 "/nvm_pmain_fpsu/F-8V") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 15.24 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 134 "/nvm_pmain_fpsu/F-15V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 17.78 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 134 "/nvm_pmain_fpsu/F-15V") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 20.32 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 132 "/nvm_pmain_fpsu/F5V_D") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 22.86 0) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 130 "/nvm_pmain_fpsu/FGND_D") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-10A_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 224.54 -61.5 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "PN" "LM317BTG")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "U14" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "LM317_TO-220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 206 "Net-(R58-Pad2)") (pinfunction "ADJ") (pintype "input"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 133 "/nvm_pmain_fpsu/F+15V") (pinfunction "VO") (pintype "power_out"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 117 "Net-(C57-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "F.Cu")
    (tedit 5A3D4994)
    (at 190 -102.04 90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "PN" "T910W-10K")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "RV2" (at 3.46 0.005 180) (layer "F.SilkS"))
    (fp_text value "10k" (at -2.54 3.67 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0.005 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "Net-(C19-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at -2.54 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(C9-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at -5.08 0 90) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 261 -99.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H11" (at -0.2 5.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 186 -75.525 -90)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "PN" "KP-2012YD")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D8" (at 2.725 -1.2) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0 270) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 170 "Net-(D8-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0 270) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 23 "/nvm_pcb_pmain_digital/LED1") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 211.54 -61.5 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "PN" "LM337TG")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "U16" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "LM337_TO220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 207 "Net-(R62-Pad2)") (pinfunction "ADJ") (pintype "input"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 121 "Net-(C62-Pad2)") (pinfunction "VI") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 134 "/nvm_pmain_fpsu/F-15V") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 115 -172.5 180)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4.2 180) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0 180) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0 180) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 173.62 -47.1 -90)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "PN" "ZL201-10G")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J12" (at -2.4 8.02 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 0 15.03 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 6.35) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/nvm_pcb_pmain_digital/AN3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/nvm_pcb_pmain_digital/AN2") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/nvm_pcb_pmain_digital/AN1") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 171 -104 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-1U/50")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C9" (at -2 -0.1 180) (layer "F.SilkS"))
    (fp_text value "1u" (at 2.5 3 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 166 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 67 "Net-(C9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 115.8 -57.7)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "PN" "KP-2012YD")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D4" (at 1.3 -1.8) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 137 "Net-(D4-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 18 "+3V3") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 169 -126.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C25" (at 1.5 -3.1 180) (layer "F.SilkS"))
    (fp_text value "220n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tedit 5AC8BA0D)
    (at 251.54 -61.5 180)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "PN" "L7805ABV")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "U18" (at 2.54 -4.27) (layer "F.SilkS"))
    (fp_text value "LM7805_TO220" (at 2.54 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 250 "Net-(C67-Pad1)") (pinfunction "VI") (pintype "power_in"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 130 "/nvm_pmain_fpsu/FGND_D") (pinfunction "GND") (pintype "power_in"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 132 "/nvm_pmain_fpsu/F5V_D") (pinfunction "VO") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 163 -111.5)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "F.Cu")
    (tedit 5AE50EF0)
    (at 181 -90.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "MKS2-22N/63")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C21" (at -2.4 0) (layer "F.SilkS"))
    (fp_text value "22n" (at 2.5 3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 74 "Net-(C21-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 169 -114.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C24" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "220n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 195 -105.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2400")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R51" (at 0 -2.6 180) (layer "B.SilkS"))
    (fp_text value "240R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "/nvm_pcb_pmain_digital/MUTE") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 243 "/nvm_pcb_pmain_digital/S_MUTE") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 183 -81 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R49" (at -3 -0.1 180) (layer "B.SilkS"))
    (fp_text value "620R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 142 "Net-(D9-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 195 -99.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R29" (at -0.6 -2.6 180) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 104 "Net-(Q1-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 112 "+9VA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRN6045TA" (layer "B.Cu")
    (tedit 5B61DEEA)
    (at 228 -89.5 -90)
    (descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
    (tags "Semi-shielded Power Inductor")
    (property "PN" "SRN6045TA-680M")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "L7" (at 4.5 -1.1 180) (layer "B.SilkS"))
    (fp_text value "68u" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 143 "/nvm_pmain_fpsu/REC_S_HI") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "Net-(C63-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 166 -83.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R25" (at 0 -1.5) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GNDREF") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 195 "Net-(R22-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 121 -96.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "M24S4FF1004T30")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R33" (at 3.5 -3.9 180) (layer "B.SilkS"))
    (fp_text value "1M" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "Net-(C29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 171 -117.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C14" (at 2.5 -2.1 180) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 120 "Net-(C14-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 70 "Net-(C14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 249 -81 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1201")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R61" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "1k2" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 127 "Net-(C59-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 115 -81.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R43" (at 0 1.65 90) (layer "B.SilkS"))
    (fp_text value "620R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 110 "Net-(J6-Pad6)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 154.2 -51.25 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C51" (at -2.25 0.1 180) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 22 "/nvm_pcb_pmain_digital/VREF_M") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 196.8 -74.7 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C47" (at 2.3 -1.2 180) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.8625 0 90) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 121.5 -155.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3903")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R1" (at -2.5 -2.1 180) (layer "B.SilkS"))
    (fp_text value "39k" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 78 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "Net-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 124 -91.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C32" (at -2.5 0.4 180) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 10 "Net-(C32-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 138 -151.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3903")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R4" (at 1 1.9 180) (layer "B.SilkS"))
    (fp_text value "39k" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 188 "Net-(R2-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "Net-(D5-Pad4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 156.5 -65 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C46" (at 2.5 0.9 180) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 133.4 -139.7 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2400")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R7" (at 0 -2.2 180) (layer "B.SilkS"))
    (fp_text value "240R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 189 "Net-(R7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 159 -89.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R15" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 5 "Net-(C18-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 192 "Net-(R15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 166 -86.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R22" (at 0 1.5) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 195 "Net-(R22-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 13 "Net-(JP1-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_10.4x10.4_H4.8" (layer "B.Cu")
    (tedit 5990349B)
    (at 180.1 -117)
    (descr "Choke, SMD, 10.4x10.4mm 4.8mm height")
    (tags "Choke SMD")
    (property "PN" " PSDB1005NT100")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "L3" (at 0 6.35) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -6.35) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.15 0) (size 2.7 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 120 "Net-(C14-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.15 0) (size 2.7 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "Net-(C15-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_10.4x10.4_H4.8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF" (layer "B.Cu")
    (tedit 5905D864)
    (at 249 -99.5)
    (descr "Diode, MELF,,")
    (tags "Diode MELF ")
    (property "PN" "SM5819")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D16" (at 9.6 8) (layer "B.SilkS"))
    (fp_text value "1N5819" (at -0.25 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.4 0) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 250 "Net-(C67-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2.4 0) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 248 "Net-(C65-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 176.8 -73.5 -90)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V510J ")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN10" (at 3 -0.3 180) (layer "B.SilkS"))
    (fp_text value "51R" (at 0 -3.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 180 "Net-(J10-Pad9)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 181 "Net-(J10-Pad10)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 182 "Net-(J10-Pad11)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 185 "Net-(J10-Pad12)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 1.5 -2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 92 "/nvm_pcb_pmain_digital/EX12") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 1.5 -0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 93 "/nvm_pcb_pmain_digital/EX11") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 94 "/nvm_pcb_pmain_digital/EX10") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 95 "/nvm_pcb_pmain_digital/EX9") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 122.4 -142.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C1" (at -2.5 -0.8 180) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 9 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 11 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 142.84 -106.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1003")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R36" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "+12V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 204 "Net-(R36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 129 -103.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C31" (at 0.1 -1.5) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "+12V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 156.6 -47.1 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2401")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R55" (at 1.5 1.4) (layer "B.SilkS"))
    (fp_text value "2K4" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 32 "/nvm_pcb_pmain_digital/AN1") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/nvm_pcb_pmain_digital/VREF_M") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Coilcraft_LPS5030" (layer "B.Cu")
    (tedit 5C4CB0C4)
    (at 128 -88.5 -90)
    (descr "Shielded Power Inductor SMD, Coilcraft LPS5030, https://www.coilcraft.com/pdfs/lps5030.pdf, StepUp generated footprint")
    (tags "inductor")
    (property "PN" "LPS5030-333MRC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "L5" (at 0.5 14.4 180) (layer "B.SilkS"))
    (fp_text value "33u" (at 0 -3.8 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd custom locked (at -2.2275 0 270) (size 1.055 3.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 65 "Net-(C28-Pad1)") (pinfunction "1") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1.4675 -1.7)
            (xy 0.5275 -0.8445)
            (xy 0.5275 0.8445)
            (xy 1.4675 1.7)
            (xy 1.4675 2.755)
            (xy 0.5275 2.755)
            (xy -0.5275 1.7)
            (xy -0.5275 -1.7)
            (xy 0.5275 -2.755)
            (xy 1.4675 -2.755)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom locked (at 2.2275 0 270) (size 1.055 3.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 17 "+5V") (pinfunction "2") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5275 -1.7)
            (xy 0.5275 1.7)
            (xy -0.5275 2.755)
            (xy -1.4675 2.755)
            (xy -1.4675 1.7)
            (xy -0.5275 0.8445)
            (xy -0.5275 -0.8445)
            (xy -1.4675 -1.7)
            (xy -1.4675 -2.755)
            (xy -0.5275 -2.755)
          ) (width 0) (fill yes))
      ))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Coilcraft_LPS5030.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_HC49-SD" (layer "B.Cu")
    (tedit 5A1AD52C)
    (at 182.4 -58.9 -90)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (property "PN" "8.00M-SMDHC49R")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Y1" (at 1.9 3.8 180) (layer "B.SilkS"))
    (fp_text value "8MHz" (at 0 -3.55 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.25 0 270) (size 4.5 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 20 "/nvm_pcb_pmain_digital/X1") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.25 0 270) (size 4.5 2) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 21 "/nvm_pcb_pmain_digital/X2") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_HC49-SD.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 196.8 -70.2 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R47" (at 3.2 0.2 180) (layer "B.SilkS"))
    (fp_text value "24R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 116 "Net-(C45-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 220.5 -65.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2200")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R58" (at 0 1.65 180) (layer "B.SilkS"))
    (fp_text value "220R" (at 0 -1.7 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 133 "/nvm_pmain_fpsu/F+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 206 "Net-(R58-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 177 -90.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1803")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R17" (at -5.6 2) (layer "B.SilkS"))
    (fp_text value "180k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 74 "Net-(C21-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "B.Cu")
    (tedit 5EBA9318)
    (at 235 -68 180)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C226K025AT")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C60" (at 0 2.55) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -2.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.55 0 180) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.55 0 180) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 134 "/nvm_pmain_fpsu/F-15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 248.5 -91 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R67" (at -0.6 -2) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 250 "Net-(C67-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "/nvm_pmain_fpsu/FGND_D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 150 -96.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C43" (at -3.6 0) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "Net-(C43-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 232.5 -78.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2400")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R66" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "240R" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 118 "Net-(C61-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 255 "/nvm_pmain_fpsu/F-8V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 187.1 -122.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "C0805C684K5RAC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C15" (at -3.5 -0.1 180) (layer "B.SilkS"))
    (fp_text value "680n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 72 "Net-(C15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRN6045TA" (layer "B.Cu")
    (tedit 5B61DEEA)
    (at 214 -89.5 -90)
    (descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
    (tags "Semi-shielded Power Inductor")
    (property "PN" "SRN6045TA-680M")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "L8" (at 4.4 3 180) (layer "B.SilkS"))
    (fp_text value "68u" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 144 "/nvm_pmain_fpsu/REC_S_LO") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "Net-(C64-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRN6045TA" (layer "B.Cu")
    (tedit 5B61DEEA)
    (at 235 -89.5 -90)
    (descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
    (tags "Semi-shielded Power Inductor")
    (property "PN" "SRN6045TA-680M")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "L11" (at 4.5 1.4 180) (layer "B.SilkS"))
    (fp_text value "68u" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 147 "/nvm_pmain_fpsu/REC_N_LO") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 246 "Net-(C65-Pad1)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 147 -113.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1003")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R14" (at 0.9 -2) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 114 "/nvm_pcb_pmain_digital/MUTE") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 139.5 -91.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C39" (at -2.5 -0.1 180) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 113 "Net-(C39-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC" (layer "B.Cu")
    (tedit 5864295D)
    (at 128 -117.5 180)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (property "PN" "B540C-13-F")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D2" (at 2.9 -4.5) (layer "B.SilkS"))
    (fp_text value "B340" (at 0 -4.2) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.9) (layer "B.Fab"))
    (pad "1" smd rect locked (at -3.4 0 90) (size 3.3 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 0 90) (size 3.3 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 135 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 129 -93 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "C0805C684K5RAC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C28" (at -2.6 -2) (layer "B.SilkS"))
    (fp_text value "680n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 65 "Net-(C28-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 81 "Net-(C28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 190 -89.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1803")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R26" (at 3.5 0.4 180) (layer "B.SilkS"))
    (fp_text value "180k" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 77 "Net-(C27-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 1 "GNDREF") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 143 -93 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "C0805C684K5RAC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C35" (at -2.84 1.68) (layer "B.SilkS"))
    (fp_text value "680n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 108 "Net-(C35-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 124 "Net-(C35-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 138 -48.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "25LC640A-I/SN")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U11" (at 5 -2.1) (layer "B.SilkS"))
    (fp_text value "25LC640" (at 0 -3.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/nvm_pcb_pmain_digital/EE_CS") (pinfunction "~{CS}") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "/nvm_pcb_pmain_digital/EE_MISO") (pinfunction "MISO") (pintype "tri_state"))
    (pad "3" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pinfunction "~{WP}") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "/nvm_pcb_pmain_digital/EE_MOSI") (pinfunction "MOSI") (pintype "input"))
    (pad "6" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/nvm_pcb_pmain_digital/EE_SCK") (pinfunction "SCK") (pintype "input"))
    (pad "7" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pinfunction "~{HOLD}") (pintype "input"))
    (pad "8" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 224.6 -83.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C63" (at 3 1.5) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 123 "Net-(C63-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 191.6 -142.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG0033")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R12" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "3R3" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 167 "Net-(C12-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 142.5 -103.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C38" (at 3.6 -1) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "+12V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 125 -80.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R41" (at 3 -0.1 180) (layer "B.SilkS"))
    (fp_text value "620R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 183 "Net-(J6-Pad7)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 134.5 -155.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3903")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R2" (at 0 1.9 180) (layer "B.SilkS"))
    (fp_text value "39k" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 187 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 188 "Net-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "B.Cu")
    (tedit 5EBA9318)
    (at 257 -76.5 90)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C226K025AT")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C59" (at 2.5 3.1 180) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -2.55 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.55 0 90) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 127 "Net-(C59-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.55 0 90) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 116 -63.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R6" (at 0 2.1 180) (layer "B.SilkS"))
    (fp_text value "620R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 137 "Net-(D4-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 187.1 -134.1 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "C0805C684K5RAC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C10" (at -1.9 2.4 180) (layer "B.SilkS"))
    (fp_text value "680n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 68 "Net-(C10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 177 -86.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R16" (at 0 -2) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 12 "Net-(JP1-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 73 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 138 -103.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C37" (at -2.1 5.5) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 111 "Net-(C37-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 177 -94.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R18" (at 5.1 -2) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 193 "Net-(R18-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "Net-(C22-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D_Pad2.25x2.55mm_HandSolder" (layer "B.Cu")
    (tedit 5EBA9318)
    (at 136 -86.5 180)
    (descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C107K010AT")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C41" (at -4.1 -3) (layer "B.SilkS"))
    (fp_text value "100u" (at 0 -3.1) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -3.2 0 180) (size 2.25 2.55) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 3.2 0 180) (size 2.25 2.55) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 193.4 -64.4)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C45" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 116 "Net-(C45-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF" (layer "B.Cu")
    (tedit 5905D864)
    (at 211 -78.5 -90)
    (descr "Diode, MELF,,")
    (tags "Diode MELF ")
    (property "PN" "SM5819")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D14" (at 4 -0.1 180) (layer "B.SilkS"))
    (fp_text value "1N5819" (at -0.25 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.4 0 270) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "Net-(C64-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2.4 0 270) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "Net-(C62-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 115 -69.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1201")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R5" (at 0 2.1 180) (layer "B.SilkS"))
    (fp_text value "1k2" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 136 "Net-(D3-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 153 -116.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1003")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R24" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 197 "Net-(R24-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 196 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMC" (layer "B.Cu")
    (tedit 5864295D)
    (at 138 -119.5 90)
    (descr "Diode SMC (DO-214AB)")
    (tags "Diode SMC (DO-214AB)")
    (property "PN" "B540C-13-F")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D1" (at -5.5 -2.4 180) (layer "B.SilkS"))
    (fp_text value "B340" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.9 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -3.4 0) (size 3.3 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 3.4 0) (size 3.3 2.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 129 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMC.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 122 -91.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C33" (at 2 1.9 180) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 17 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 201.6 -129.7 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "C0805C684K5RAC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C11" (at 2.7 0.2 180) (layer "B.SilkS"))
    (fp_text value "680n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 6 "/nvm_pmain_amp/OUT_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 206.5 -69)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R64" (at 0 1.65 180) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "Net-(C62-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 128 -80.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R42" (at 3 -0.1 -180) (layer "B.SilkS"))
    (fp_text value "620R" (at 0 -1.7 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 184 "Net-(J6-Pad8)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 137.5 -91.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C40" (at 0 2.4 180) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 150 -99.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R45" (at 4.1 0) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "/nvm_pcb_pmain_digital/ZCD_C") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "Net-(C43-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 186.6 -57.7 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A330FXAAC")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C55" (at 1.8 2.5 180) (layer "B.SilkS"))
    (fp_text value "33p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 21 "/nvm_pcb_pmain_digital/X2") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 249 -77.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2400")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R59" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "240R" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 254 "/nvm_pmain_fpsu/F+8V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 127 "Net-(C59-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 217.4 -83.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C64" (at 3.8 0) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 126 "Net-(C64-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 177 -97.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1803")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R19" (at -3.9 0.5) (layer "B.SilkS"))
    (fp_text value "180k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 75 "Net-(C22-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 76 "Net-(C23-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF" (layer "B.Cu")
    (tedit 5905D864)
    (at 249 -95.5 180)
    (descr "Diode, MELF,,")
    (tags "Diode MELF ")
    (property "PN" "SM5819")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D18" (at -9.6 -5.5) (layer "B.SilkS"))
    (fp_text value "1N5819" (at -0.25 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.4 0 180) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 248 "Net-(C65-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2.4 0 180) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "/nvm_pmain_fpsu/FGND_D") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 157.2 -50.3 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C53" (at -4.7 1.6 180) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "+3.3VADC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.8625 0 270) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 127.6 -70.6 180)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V203J")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN6" (at 0 3.5) (layer "B.SilkS"))
    (fp_text value "20k" (at 0 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2 180) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 213 "/nvm_pcb_pmain_digital/KC5") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66 180) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 214 "/nvm_pcb_pmain_digital/KC6") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66 180) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 215 "/nvm_pcb_pmain_digital/KC7") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2 180) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 216 "/nvm_pcb_pmain_digital/KC8") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 1.5 -2 180) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 1.5 -0.66 180) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66 180) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2 180) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pinfunction "R1.2") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 226.5 -65.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2611FB3")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R60" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "2k61" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 206 "Net-(R58-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 177 -54.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C52" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "+3.3VADC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 182.4 -67.1 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R46" (at -2.2 1.8) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 205 "Net-(R46-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 130 -46.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R50" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 51 "/nvm_pcb_pmain_digital/EE_CS") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:SMDIP-4_W9.53mm" (layer "B.Cu")
    (tedit 5A02E8C5)
    (at 128.5 -133 -90)
    (descr "4-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)")
    (tags "SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil")
    (property "PN" "PC817X1NIP1B")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U2" (at -1.8 3.7 180) (layer "B.SilkS"))
    (fp_text value "PC817" (at 0 -3.6 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.765 1.27 270) (size 2 1.78) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 189 "Net-(R7-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at -4.765 -1.27 270) (size 2 1.78) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "Net-(C1-Pad1)") (pintype "passive"))
    (pad "3" smd rect locked (at 4.765 -1.27 270) (size 2 1.78) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "4" smd rect locked (at 4.765 1.27 270) (size 2 1.78) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "/nvm_pcb_pmain_digital/ZCD_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/SMDIP-4_W9.53mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 138.8 -74.9 -45)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V510J ")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN4" (at -2.687006 -1.697056 225) (layer "B.SilkS"))
    (fp_text value "51R" (at 0 -3.5 135) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 199 "Net-(J7-Pad6)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 191 "Net-(J7-Pad5)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 198 "Net-(J7-Pad4)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 190 "Net-(J7-Pad3)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 1.5 -2 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 33 "/nvm_pcb_pmain_digital/K1") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 1.5 -0.66 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 37 "/nvm_pcb_pmain_digital/K2") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 34 "/nvm_pcb_pmain_digital/K3") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 38 "/nvm_pcb_pmain_digital/K4") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "B.Cu")
    (tedit 5EBA9318)
    (at 249 -68)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C226K025AT")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C58" (at 0 2.55) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -2.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.55 0) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 133 "/nvm_pmain_fpsu/F+15V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.55 0) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 150.8 -47.1 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2401")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R54" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "2K4" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 31 "/nvm_pcb_pmain_digital/AN2") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/nvm_pcb_pmain_digital/VREF_M") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 153 -119.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2400")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.5) (layer "B.SilkS"))
    (fp_text value "240R" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 172 "Net-(R23-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 196 "Net-(R23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 196 -88.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6202")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R31" (at 3.5 0.4 180) (layer "B.SilkS"))
    (fp_text value "6k2" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 80 "Net-(C27-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 138.2 -67.3 -45)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V510J ")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN2" (at -2.687006 -1.131371 225) (layer "B.SilkS"))
    (fp_text value "51R" (at 0 -3.5 135) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 216 "/nvm_pcb_pmain_digital/KC8") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 215 "/nvm_pcb_pmain_digital/KC7") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 214 "/nvm_pcb_pmain_digital/KC6") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 213 "/nvm_pcb_pmain_digital/KC5") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 1.5 -2 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 35 "/nvm_pcb_pmain_digital/K5") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 1.5 -0.66 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 39 "/nvm_pcb_pmain_digital/K6") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 36 "/nvm_pcb_pmain_digital/K7") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2 315) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 40 "/nvm_pcb_pmain_digital/K8") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-7343-31_Kemet-D_Pad2.25x2.55mm_HandSolder" (layer "B.Cu")
    (tedit 5EBA9318)
    (at 120 -86.5 180)
    (descr "Tantalum Capacitor SMD Kemet-D (7343-31 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C107K010AT")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C34" (at -3.6 -3) (layer "B.SilkS"))
    (fp_text value "100u" (at 0 -3.1) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -3.2 0 180) (size 2.25 2.55) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 17 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 3.2 0 180) (size 2.25 2.55) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-7343-31_Kemet-D.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 121 -49.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C42" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 17 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (layer "B.Cu")
    (tedit 5A0AB76C)
    (at 150 -93.5 180)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (property "PN" "SN74LVC1G14DBVR")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U10" (at -3.6 0.5) (layer "B.SilkS"))
    (fp_text value "74LVC1G14" (at 0 -2.9) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.35 0.95 180) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "2" smd rect locked (at -1.35 0 180) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 115 "Net-(C43-Pad1)") (pintype "input"))
    (pad "3" smd rect locked (at -1.35 -0.95 180) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect locked (at 1.35 -0.95 180) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 107 "/nvm_pcb_pmain_digital/ZCD") (pintype "output"))
    (pad "5" smd rect locked (at 1.35 0.95 180) (size 1.56 0.65) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 115 -75.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R40" (at 0 2.1 180) (layer "B.SilkS"))
    (fp_text value "620R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 109 "Net-(J6-Pad5)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRN6045TA" (layer "B.Cu")
    (tedit 5B61DEEA)
    (at 242 -89.5 -90)
    (descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
    (tags "Semi-shielded Power Inductor")
    (property "PN" "SRN6045TA-680M")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "L10" (at 4.5 -1.6 180) (layer "B.SilkS"))
    (fp_text value "68u" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 146 "/nvm_pmain_fpsu/REC_N_HI") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 248 "Net-(C65-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 201.6 -116 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "C0805C684K5RAC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C16" (at 2.6 0.2) (layer "B.SilkS"))
    (fp_text value "680n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 7 "/nvm_pmain_amp/OUT_N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 191 -93.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C27" (at 0 -1.5) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 77 "Net-(C27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 80 "Net-(C27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 186.6 -62.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A330FXAAC")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C54" (at -1 -2.5 180) (layer "B.SilkS"))
    (fp_text value "33p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 20 "/nvm_pcb_pmain_digital/X1") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 138 -52.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C44" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 145 -47.1 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2401")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R53" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "2K4" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 30 "/nvm_pcb_pmain_digital/AN3") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 22 "/nvm_pcb_pmain_digital/VREF_M") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 193.2 -70.2 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R56" (at -3.2 -0.1 180) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 49 "/nvm_pcb_pmain_digital/NRST") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Bourns_SRN6045TA" (layer "B.Cu")
    (tedit 5B61DEEA)
    (at 221 -89.5 -90)
    (descr "http://www.bourns.com/docs/product-datasheets/srn6045ta.pdf")
    (tags "Semi-shielded Power Inductor")
    (property "PN" "SRN6045TA-680M")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "L9" (at 4.4 2.9 180) (layer "B.SilkS"))
    (fp_text value "68u" (at 0 -4.2 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 145 "/nvm_pmain_fpsu/REC_S_MID") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 2.075 0 270) (size 2.35 5.1) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRN6045TA.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 134.5 -96.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "M24S4FF1004T30")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R37" (at -3.5 0.1 180) (layer "B.SilkS"))
    (fp_text value "1M" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "Net-(C36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 124.5 -103.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C30" (at -2.1 5) (layer "B.SilkS"))
    (fp_text value "2u2" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 16 "Net-(C30-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_10.4x10.4_H4.8" (layer "B.Cu")
    (tedit 5990349B)
    (at 180.1 -128.5)
    (descr "Choke, SMD, 10.4x10.4mm 4.8mm height")
    (tags "Choke SMD")
    (property "PN" " PSDB1005NT100")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "L1" (at 0 -6) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -6.35) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.15 0) (size 2.7 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 66 "Net-(C8-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.15 0) (size 2.7 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "Net-(C10-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_10.4x10.4_H4.8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 243.5 -72 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1201")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R63" (at -3.5 -2.4) (layer "B.SilkS"))
    (fp_text value "1k2" (at 0 -1.7 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 118 "Net-(C61-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 132 -97 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A330FXAAC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C36" (at -2.5 -0.4 180) (layer "B.SilkS"))
    (fp_text value "33p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 125 "Net-(C36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF" (layer "B.Cu")
    (tedit 5905D864)
    (at 206 -78.5 90)
    (descr "Diode, MELF,,")
    (tags "Diode MELF ")
    (property "PN" "SM5819")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D12" (at 4 0.1 180) (layer "B.SilkS"))
    (fp_text value "1N5819" (at -0.25 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.4 0 90) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "Net-(C57-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2.4 0 90) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 126 "Net-(C64-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm" (layer "B.Cu")
    (tedit 5E1214D9)
    (at 140.42 -98.5 90)
    (descr "HTSSOP, 16 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "HTSSOP SO")
    (property "PN" "LM43600PWPR")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U7" (at 0 4.18 180) (layer "B.SilkS"))
    (fp_text value "LM43600" (at 0 -3.45 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at 0 0.58 90) (size 1.98 0.93) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0 -0.58 90) (size 1.98 0.93) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd rect locked (at 0 0 90) (size 2.46 2.31) (layers "B.Mask"))
    (pad "1" smd roundrect locked (at -2.8625 2.275 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(C35-Pad1)") (pinfunction "SW") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.8625 1.625 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(C35-Pad1)") (pinfunction "SW") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.8625 0.975 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(C35-Pad2)") (pinfunction "CBOOT") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.8625 0.325 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(C39-Pad1)") (pinfunction "VCC") (pintype "input"))
    (pad "5" smd roundrect locked (at -2.8625 -0.325 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pinfunction "BIAS") (pintype "input"))
    (pad "6" smd roundrect locked (at -2.8625 -0.975 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 244 "unconnected-(U7-Pad6)") (pinfunction "SYNC") (pintype "input"))
    (pad "7" smd roundrect locked (at -2.8625 -1.625 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 245 "unconnected-(U7-Pad7)") (pinfunction "RT") (pintype "input"))
    (pad "8" smd roundrect locked (at -2.8625 -2.275 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 247 "unconnected-(U7-Pad8)") (pinfunction "PGOOD") (pintype "input"))
    (pad "9" smd roundrect locked (at 2.8625 -2.275 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(C36-Pad2)") (pinfunction "FB") (pintype "input"))
    (pad "10" smd roundrect locked (at 2.8625 -1.625 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "AGND") (pintype "input"))
    (pad "11" smd roundrect locked (at 2.8625 -0.975 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 111 "Net-(C37-Pad1)") (pinfunction "SS/TRK") (pintype "input"))
    (pad "12" smd roundrect locked (at 2.8625 -0.325 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 204 "Net-(R36-Pad2)") (pinfunction "EN") (pintype "input"))
    (pad "13" smd roundrect locked (at 2.8625 0.325 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "+12V") (pinfunction "VIN") (pintype "input"))
    (pad "14" smd roundrect locked (at 2.8625 0.975 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "+12V") (pinfunction "VIN") (pintype "input"))
    (pad "15" smd roundrect locked (at 2.8625 1.625 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "PGND") (pintype "input"))
    (pad "16" smd roundrect locked (at 2.8625 2.275 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "PGND") (pintype "input"))
    (pad "17" smd rect locked (at 0 0 90) (size 3.4 5) (layers "B.Cu")
      (net 2 "GND") (pinfunction "PAD") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 162 -104.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R10" (at 1.5 2.6 180) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 112 "+9VA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "B.Cu")
    (tedit 5EBA9318)
    (at 240 -78.5 180)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C226K025AT")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C61" (at 0 2.55) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -2.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.55 0 180) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.55 0 180) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 118 "Net-(C61-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 177 -100.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2400")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R20" (at -0.4 -2) (layer "B.SilkS"))
    (fp_text value "240R" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 194 "Net-(R20-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 122 "Net-(C19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 137 -106.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3903")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R38" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "39k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 204 "Net-(R36-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 134.5 -102.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C4423FB300")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R39" (at -1.5 -2.4 180) (layer "B.SilkS"))
    (fp_text value "442k" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 125 "Net-(C36-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 116.8 -91.3)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2401")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R8" (at -0.7 -1.7) (layer "B.SilkS"))
    (fp_text value "2K4" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 141 "Net-(D7-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:TQFP-100_14x14mm_P0.5mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 166 -58.5 180)
    (descr "TQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TQFP QFP")
    (property "PN" "STM32F373VBT6")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U9" (at 0 9.35) (layer "B.SilkS"))
    (fp_text value "STM32F373VB" (at 0 -9.35) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -7.6625 6 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 94 "/nvm_pcb_pmain_digital/EX10") (pinfunction "PE2") (pintype "input"))
    (pad "2" smd roundrect locked (at -7.6625 5.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 93 "/nvm_pcb_pmain_digital/EX11") (pinfunction "PE3") (pintype "input"))
    (pad "3" smd roundrect locked (at -7.6625 5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 92 "/nvm_pcb_pmain_digital/EX12") (pinfunction "PE4") (pintype "input"))
    (pad "4" smd roundrect locked (at -7.6625 4.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 23 "/nvm_pcb_pmain_digital/LED1") (pinfunction "PE5") (pintype "input"))
    (pad "5" smd roundrect locked (at -7.6625 4 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 24 "/nvm_pcb_pmain_digital/LED2") (pinfunction "PE6") (pintype "input"))
    (pad "6" smd roundrect locked (at -7.6625 3.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pinfunction "VBAT") (pintype "input"))
    (pad "7" smd roundrect locked (at -7.6625 3 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 217 "unconnected-(U9-Pad7)") (pinfunction "PC13") (pintype "input"))
    (pad "8" smd roundrect locked (at -7.6625 2.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 218 "unconnected-(U9-Pad8)") (pinfunction "PC14/OSC32_IN") (pintype "input"))
    (pad "9" smd roundrect locked (at -7.6625 2 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 219 "unconnected-(U9-Pad9)") (pinfunction "PC15/OSC32_OUT") (pintype "input"))
    (pad "10" smd roundrect locked (at -7.6625 1.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 242 "/nvm_pcb_pmain_digital/S_DRIV") (pinfunction "PF9") (pintype "input"))
    (pad "11" smd roundrect locked (at -7.6625 1 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 243 "/nvm_pcb_pmain_digital/S_MUTE") (pinfunction "PF10") (pintype "input"))
    (pad "12" smd roundrect locked (at -7.6625 0.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 20 "/nvm_pcb_pmain_digital/X1") (pinfunction "PF0/OSC_IN") (pintype "input"))
    (pad "13" smd roundrect locked (at -7.6625 0 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 21 "/nvm_pcb_pmain_digital/X2") (pinfunction "PF1/OSC_OUT") (pintype "input"))
    (pad "14" smd roundrect locked (at -7.6625 -0.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 49 "/nvm_pcb_pmain_digital/NRST") (pinfunction "NRST") (pintype "input"))
    (pad "15" smd roundrect locked (at -7.6625 -1 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 220 "unconnected-(U9-Pad15)") (pinfunction "PC0") (pintype "input"))
    (pad "16" smd roundrect locked (at -7.6625 -1.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 221 "unconnected-(U9-Pad16)") (pinfunction "PC1") (pintype "input"))
    (pad "17" smd roundrect locked (at -7.6625 -2 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 253 "/nvm_pcb_pmain_digital/BEEP") (pinfunction "PC2") (pintype "input"))
    (pad "18" smd roundrect locked (at -7.6625 -2.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 222 "unconnected-(U9-Pad18)") (pinfunction "PC3") (pintype "input"))
    (pad "19" smd roundrect locked (at -7.6625 -3 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 223 "unconnected-(U9-Pad19)") (pinfunction "PF2") (pintype "input"))
    (pad "20" smd roundrect locked (at -7.6625 -3.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSSA/VREF-") (pintype "input"))
    (pad "21" smd roundrect locked (at -7.6625 -4 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "+3.3VADC") (pinfunction "VDDA") (pintype "input"))
    (pad "22" smd roundrect locked (at -7.6625 -4.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/nvm_pcb_pmain_digital/VREF_M") (pinfunction "VREF+") (pintype "input"))
    (pad "23" smd roundrect locked (at -7.6625 -5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 82 "/nvm_pcb_pmain_digital/AB_CTRL") (pinfunction "PA0") (pintype "input"))
    (pad "24" smd roundrect locked (at -7.6625 -5.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 83 "/nvm_pcb_pmain_digital/AB_RST") (pinfunction "PA1") (pintype "input"))
    (pad "25" smd roundrect locked (at -7.6625 -6 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 84 "/nvm_pcb_pmain_digital/AB_TX") (pinfunction "PA2") (pintype "input"))
    (pad "26" smd roundrect locked (at -6 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 85 "/nvm_pcb_pmain_digital/AB_RX") (pinfunction "PA3") (pintype "input"))
    (pad "27" smd roundrect locked (at -5.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 224 "unconnected-(U9-Pad27)") (pinfunction "PF4") (pintype "input"))
    (pad "28" smd roundrect locked (at -5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pinfunction "VDD") (pintype "input"))
    (pad "29" smd roundrect locked (at -4.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 225 "unconnected-(U9-Pad29)") (pinfunction "PA4") (pintype "input"))
    (pad "30" smd roundrect locked (at -4 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 226 "unconnected-(U9-Pad30)") (pinfunction "PA5") (pintype "input"))
    (pad "31" smd roundrect locked (at -3.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 227 "unconnected-(U9-Pad31)") (pinfunction "PA6") (pintype "input"))
    (pad "32" smd roundrect locked (at -3 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 228 "unconnected-(U9-Pad32)") (pinfunction "PA7") (pintype "input"))
    (pad "33" smd roundrect locked (at -2.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 229 "unconnected-(U9-Pad33)") (pinfunction "PC4") (pintype "input"))
    (pad "34" smd roundrect locked (at -2 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 30 "/nvm_pcb_pmain_digital/AN3") (pinfunction "PC5") (pintype "input"))
    (pad "35" smd roundrect locked (at -1.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 31 "/nvm_pcb_pmain_digital/AN2") (pinfunction "PB0") (pintype "input"))
    (pad "36" smd roundrect locked (at -1 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 32 "/nvm_pcb_pmain_digital/AN1") (pinfunction "PB1") (pintype "input"))
    (pad "37" smd roundrect locked (at -0.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 230 "unconnected-(U9-Pad37)") (pinfunction "PB2") (pintype "input"))
    (pad "38" smd roundrect locked (at 0 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 231 "unconnected-(U9-Pad38)") (pinfunction "PE7") (pintype "input"))
    (pad "39" smd roundrect locked (at 0.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 232 "unconnected-(U9-Pad39)") (pinfunction "PE8") (pintype "input"))
    (pad "40" smd roundrect locked (at 1 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 233 "unconnected-(U9-Pad40)") (pinfunction "PE9") (pintype "input"))
    (pad "41" smd roundrect locked (at 1.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 234 "unconnected-(U9-Pad41)") (pinfunction "PE10") (pintype "input"))
    (pad "42" smd roundrect locked (at 2 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 235 "unconnected-(U9-Pad42)") (pinfunction "PE11") (pintype "input"))
    (pad "43" smd roundrect locked (at 2.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 236 "unconnected-(U9-Pad43)") (pinfunction "PE12") (pintype "input"))
    (pad "44" smd roundrect locked (at 3 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 237 "unconnected-(U9-Pad44)") (pinfunction "PE13") (pintype "input"))
    (pad "45" smd roundrect locked (at 3.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 238 "unconnected-(U9-Pad45)") (pinfunction "PE14") (pintype "input"))
    (pad "46" smd roundrect locked (at 4 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 239 "unconnected-(U9-Pad46)") (pinfunction "PE15") (pintype "input"))
    (pad "47" smd roundrect locked (at 4.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 240 "unconnected-(U9-Pad47)") (pinfunction "PB10") (pintype "input"))
    (pad "48" smd roundrect locked (at 5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VREFSD-") (pintype "input"))
    (pad "49" smd roundrect locked (at 5.5 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSSSD") (pintype "input"))
    (pad "50" smd roundrect locked (at 6 -7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "+3.3VADC") (pinfunction "VDDSD12") (pintype "input"))
    (pad "51" smd roundrect locked (at 7.6625 -6 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "+3.3VADC") (pinfunction "VDDSD3") (pintype "input"))
    (pad "52" smd roundrect locked (at 7.6625 -5.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/nvm_pcb_pmain_digital/VREF_M") (pinfunction "VREFSD+") (pintype "input"))
    (pad "53" smd roundrect locked (at 7.6625 -5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 241 "unconnected-(U9-Pad53)") (pinfunction "PB14") (pintype "input"))
    (pad "54" smd roundrect locked (at 7.6625 -4.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 51 "/nvm_pcb_pmain_digital/EE_CS") (pinfunction "PB15") (pintype "input"))
    (pad "55" smd roundrect locked (at 7.6625 -4 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 54 "/nvm_pcb_pmain_digital/EE_SCK") (pinfunction "PD8") (pintype "input"))
    (pad "56" smd roundrect locked (at 7.6625 -3.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 53 "/nvm_pcb_pmain_digital/EE_MOSI") (pinfunction "PD9") (pintype "input"))
    (pad "57" smd roundrect locked (at 7.6625 -3 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 52 "/nvm_pcb_pmain_digital/EE_MISO") (pinfunction "PD10") (pintype "input"))
    (pad "58" smd roundrect locked (at 7.6625 -2.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "/nvm_pcb_pmain_digital/DO8") (pinfunction "PD11") (pintype "input"))
    (pad "59" smd roundrect locked (at 7.6625 -2 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/nvm_pcb_pmain_digital/DO7") (pinfunction "PD12") (pintype "input"))
    (pad "60" smd roundrect locked (at 7.6625 -1.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "/nvm_pcb_pmain_digital/DO6") (pinfunction "PD13") (pintype "input"))
    (pad "61" smd roundrect locked (at 7.6625 -1 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "/nvm_pcb_pmain_digital/DO5") (pinfunction "PD14") (pintype "input"))
    (pad "62" smd roundrect locked (at 7.6625 -0.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "/nvm_pcb_pmain_digital/DO3") (pinfunction "PD15") (pintype "input"))
    (pad "63" smd roundrect locked (at 7.6625 0 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "/nvm_pcb_pmain_digital/DO2") (pinfunction "PC6") (pintype "input"))
    (pad "64" smd roundrect locked (at 7.6625 0.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "/nvm_pcb_pmain_digital/DO1") (pinfunction "PC7") (pintype "input"))
    (pad "65" smd roundrect locked (at 7.6625 1 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 40 "/nvm_pcb_pmain_digital/K8") (pinfunction "PC8") (pintype "input"))
    (pad "66" smd roundrect locked (at 7.6625 1.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 36 "/nvm_pcb_pmain_digital/K7") (pinfunction "PC9") (pintype "input"))
    (pad "67" smd roundrect locked (at 7.6625 2 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 39 "/nvm_pcb_pmain_digital/K6") (pinfunction "PA8") (pintype "input"))
    (pad "68" smd roundrect locked (at 7.6625 2.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 35 "/nvm_pcb_pmain_digital/K5") (pinfunction "PA9") (pintype "input"))
    (pad "69" smd roundrect locked (at 7.6625 3 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 38 "/nvm_pcb_pmain_digital/K4") (pinfunction "PA10") (pintype "input"))
    (pad "70" smd roundrect locked (at 7.6625 3.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 34 "/nvm_pcb_pmain_digital/K3") (pinfunction "PA11") (pintype "input"))
    (pad "71" smd roundrect locked (at 7.6625 4 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 37 "/nvm_pcb_pmain_digital/K2") (pinfunction "PA12") (pintype "input"))
    (pad "72" smd roundrect locked (at 7.6625 4.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 50 "/nvm_pcb_pmain_digital/SWDIO") (pinfunction "PA13") (pintype "input"))
    (pad "73" smd roundrect locked (at 7.6625 5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 33 "/nvm_pcb_pmain_digital/K1") (pinfunction "PF6") (pintype "input"))
    (pad "74" smd roundrect locked (at 7.6625 5.5 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "input"))
    (pad "75" smd roundrect locked (at 7.6625 6 180) (size 1.475 0.3) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pinfunction "VDD") (pintype "input"))
    (pad "76" smd roundrect locked (at 6 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 48 "/nvm_pcb_pmain_digital/SWCLK") (pinfunction "PA14") (pintype "input"))
    (pad "77" smd roundrect locked (at 5.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 107 "/nvm_pcb_pmain_digital/ZCD") (pinfunction "PA15") (pintype "input"))
    (pad "78" smd roundrect locked (at 5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 26 "/nvm_pcb_pmain_digital/E_SCK") (pinfunction "PC10") (pintype "input"))
    (pad "79" smd roundrect locked (at 4.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 29 "/nvm_pcb_pmain_digital/E_MISO") (pinfunction "PC11") (pintype "input"))
    (pad "80" smd roundrect locked (at 4 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 27 "/nvm_pcb_pmain_digital/E_MOSI") (pinfunction "PC12") (pintype "input"))
    (pad "81" smd roundrect locked (at 3.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 28 "/nvm_pcb_pmain_digital/E_RST") (pinfunction "PD0") (pintype "input"))
    (pad "82" smd roundrect locked (at 3 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 25 "/nvm_pcb_pmain_digital/E_CS") (pinfunction "PD1") (pintype "input"))
    (pad "83" smd roundrect locked (at 2.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 89 "/nvm_pcb_pmain_digital/EIO2") (pinfunction "PD2") (pintype "input"))
    (pad "84" smd roundrect locked (at 2 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 86 "/nvm_pcb_pmain_digital/EIO1") (pinfunction "PD3") (pintype "input"))
    (pad "85" smd roundrect locked (at 1.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 103 "/nvm_pcb_pmain_digital/EX1") (pinfunction "PD4") (pintype "input"))
    (pad "86" smd roundrect locked (at 1 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 102 "/nvm_pcb_pmain_digital/EX2") (pinfunction "PD5") (pintype "input"))
    (pad "87" smd roundrect locked (at 0.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 101 "/nvm_pcb_pmain_digital/EX3") (pinfunction "PD6") (pintype "input"))
    (pad "88" smd roundrect locked (at 0 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 100 "/nvm_pcb_pmain_digital/EX4") (pinfunction "PD7") (pintype "input"))
    (pad "89" smd roundrect locked (at -0.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 99 "/nvm_pcb_pmain_digital/EX5") (pinfunction "PB3") (pintype "input"))
    (pad "90" smd roundrect locked (at -1 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 98 "/nvm_pcb_pmain_digital/EX6") (pinfunction "PB4") (pintype "input"))
    (pad "91" smd roundrect locked (at -1.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 97 "/nvm_pcb_pmain_digital/EX7") (pinfunction "PB5") (pintype "input"))
    (pad "92" smd roundrect locked (at -2 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 91 "/nvm_pcb_pmain_digital/EU1TX") (pinfunction "PB6") (pintype "input"))
    (pad "93" smd roundrect locked (at -2.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 88 "/nvm_pcb_pmain_digital/EU1RX") (pinfunction "PB7") (pintype "input"))
    (pad "94" smd roundrect locked (at -3 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 205 "Net-(R46-Pad2)") (pinfunction "BOOT0") (pintype "input"))
    (pad "95" smd roundrect locked (at -3.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 90 "/nvm_pcb_pmain_digital/EU2TX") (pinfunction "PB8") (pintype "input"))
    (pad "96" smd roundrect locked (at -4 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 87 "/nvm_pcb_pmain_digital/EU2RX") (pinfunction "PB9") (pintype "input"))
    (pad "97" smd roundrect locked (at -4.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 96 "/nvm_pcb_pmain_digital/EX8") (pinfunction "PE0") (pintype "input"))
    (pad "98" smd roundrect locked (at -5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 95 "/nvm_pcb_pmain_digital/EX9") (pinfunction "PE1") (pintype "input"))
    (pad "99" smd roundrect locked (at -5.5 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "input"))
    (pad "100" smd roundrect locked (at -6 7.6625 180) (size 0.3 1.475) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pinfunction "VDD") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-100_14x14mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 213 -65.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2611FB3")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R62" (at 0 -2) (layer "B.SilkS"))
    (fp_text value "2k61" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 207 "Net-(R62-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 171 -121.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C8" (at 2.5 1.6 180) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 66 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 62 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 147 -122.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1003")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R13" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 150 "Net-(R13-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF" (layer "B.Cu")
    (tedit 5905D8F5)
    (at 127.23 -141.5 180)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "PN" "TZMB4V7-GS08")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D6" (at 3.13 -2) (layer "B.SilkS"))
    (fp_text value "4V7" (at 0 -1.75) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.75 0 180) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "Net-(C1-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.75 0 180) (size 1.3 1.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "Net-(C1-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 171 -73.5 -90)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V510J ")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN9" (at 3 -0.6 180) (layer "B.SilkS"))
    (fp_text value "51R" (at 0 -3.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 176 "Net-(J10-Pad5)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 177 "Net-(J10-Pad6)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 178 "Net-(J10-Pad7)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 179 "Net-(J10-Pad8)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 1.5 -2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 96 "/nvm_pcb_pmain_digital/EX8") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 1.5 -0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 97 "/nvm_pcb_pmain_digital/EX7") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 98 "/nvm_pcb_pmain_digital/EX6") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 99 "/nvm_pcb_pmain_digital/EX5") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 186 -81 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R48" (at -3 -0.6 180) (layer "B.SilkS"))
    (fp_text value "620R" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 170 "Net-(D8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 238.6 -84.9)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y224KXATW1BC")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C65" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "220n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 246 "Net-(C65-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 248 "Net-(C65-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 118 -151 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3903")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R3" (at 0 1.9 180) (layer "B.SilkS"))
    (fp_text value "39k" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 79 "Net-(R1-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "Net-(D5-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 151.2 -51.25 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP1525T-I/TT")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U12" (at -2.25 0.6 180) (layer "B.SilkS"))
    (fp_text value "MCP1525-TT" (at 0 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 19 "+3.3VADC") (pinfunction "Vin") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 22 "/nvm_pcb_pmain_digital/VREF_M") (pinfunction "Vout") (pintype "power_out"))
    (pad "3" smd roundrect locked (at 0.9375 0 270) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Vss") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 129.5 -106.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1003")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R32" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 4 "+12V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 175 "Net-(R32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF" (layer "B.Cu")
    (tedit 5905D864)
    (at 221 -78.5 90)
    (descr "Diode, MELF,,")
    (tags "Diode MELF ")
    (property "PN" "SM5819")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D11" (at -1 3.1 180) (layer "B.SilkS"))
    (fp_text value "1N5819" (at -0.25 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.4 0 90) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "Net-(C57-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2.4 0 90) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "Net-(C63-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_10.4x10.4_H4.8" (layer "B.Cu")
    (tedit 5990349B)
    (at 194.1 -117)
    (descr "Choke, SMD, 10.4x10.4mm 4.8mm height")
    (tags "Choke SMD")
    (property "PN" " PSDB1005NT100")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "L4" (at 0 6.35) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -6.35) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.15 0) (size 2.7 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 72 "Net-(C15-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.15 0) (size 2.7 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 7 "/nvm_pmain_amp/OUT_N") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_10.4x10.4_H4.8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 153 -67.9)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V510J ")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN5" (at 3.6 -2.6) (layer "B.SilkS"))
    (fp_text value "51R" (at 0 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 161 "Net-(J8-Pad15)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 160 "Net-(J8-Pad13)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 159 "Net-(J8-Pad11)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "5" smd rect locked (at 1.5 -2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask"))
    (pad "6" smd rect locked (at 1.5 -0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 29 "/nvm_pcb_pmain_digital/E_MISO") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 27 "/nvm_pcb_pmain_digital/E_MOSI") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 26 "/nvm_pcb_pmain_digital/E_SCK") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 153 -74.1)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V510J ")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN3" (at 3.6 0.1) (layer "B.SilkS"))
    (fp_text value "51R" (at 0 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 154 "Net-(J8-Pad7)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 158 "Net-(J8-Pad9)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 203 "Net-(J8-Pad6)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 202 "Net-(J8-Pad5)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 1.5 -2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 88 "/nvm_pcb_pmain_digital/EU1RX") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 1.5 -0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 91 "/nvm_pcb_pmain_digital/EU1TX") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 25 "/nvm_pcb_pmain_digital/E_CS") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 28 "/nvm_pcb_pmain_digital/E_RST") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF" (layer "B.Cu")
    (tedit 5905D864)
    (at 216 -78.5 -90)
    (descr "Diode, MELF,,")
    (tags "Diode MELF ")
    (property "PN" "SM5819")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D13" (at 4 -0.1 180) (layer "B.SilkS"))
    (fp_text value "1N5819" (at -0.25 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.4 0 270) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 123 "Net-(C63-Pad2)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2.4 0 270) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 121 "Net-(C62-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5A02FF57)
    (at 195.8 -59.1 90)
    (descr "SOT-23, Standard")
    (tags "SOT-23")
    (property "PN" "BC847.215")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q3" (at 1.9 2.3 180) (layer "B.SilkS"))
    (fp_text value "BC847" (at 0 -2.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1 0.95 90) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 252 "Net-(Q3-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect locked (at -1 -0.95 90) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (pad "3" smd rect locked (at 1 0 90) (size 0.9 0.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 251 "Net-(LS1-Pad2)") (pinfunction "C") (pintype "passive"))
    (model "${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_Coilcraft_LPS5030" (layer "B.Cu")
    (tedit 5C4CB0C4)
    (at 144.5 -88.5 -90)
    (descr "Shielded Power Inductor SMD, Coilcraft LPS5030, https://www.coilcraft.com/pdfs/lps5030.pdf, StepUp generated footprint")
    (tags "inductor")
    (property "PN" "LPS5030-223MRC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "L6" (at -1 9.9 -180) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -3.8 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd custom locked (at -2.2275 0 270) (size 1.055 3.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 108 "Net-(C35-Pad1)") (pinfunction "1") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 1.4675 -1.7)
            (xy 0.5275 -0.8445)
            (xy 0.5275 0.8445)
            (xy 1.4675 1.7)
            (xy 1.4675 2.755)
            (xy 0.5275 2.755)
            (xy -0.5275 1.7)
            (xy -0.5275 -1.7)
            (xy 0.5275 -2.755)
            (xy 1.4675 -2.755)
          ) (width 0) (fill yes))
      ))
    (pad "2" smd custom locked (at 2.2275 0 270) (size 1.055 3.4) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pinfunction "2") (pintype "passive") (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
            (xy 0.5275 -1.7)
            (xy 0.5275 1.7)
            (xy -0.5275 2.755)
            (xy -1.4675 2.755)
            (xy -1.4675 1.7)
            (xy -0.5275 0.8445)
            (xy -0.5275 -0.8445)
            (xy -1.4675 -1.7)
            (xy -1.4675 -2.755)
            (xy -0.5275 -2.755)
          ) (width 0) (fill yes))
      ))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Coilcraft_LPS5030.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 196.5 -138.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y103KXAPW1BC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C17" (at 0.1 1.68) (layer "B.SilkS"))
    (fp_text value "10n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 63 "Net-(C17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 7 "/nvm_pmain_amp/OUT_N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (layer "B.Cu")
    (tedit 5D9F72B1)
    (at 126 -57.5 -90)
    (descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "74HCT244D.653")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U8" (at -1 8.4 180) (layer "B.SilkS"))
    (fp_text value "74HCT244" (at 0 -7.35 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -4.65 5.715 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "1OE") (pintype "input"))
    (pad "2" smd roundrect locked (at -4.65 4.445 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 59 "/nvm_pcb_pmain_digital/DO1") (pinfunction "1A0") (pintype "input"))
    (pad "3" smd roundrect locked (at -4.65 3.175 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 45 "/nvm_pcb_pmain_digital/DOT6") (pinfunction "2Y0") (pintype "tri_state"))
    (pad "4" smd roundrect locked (at -4.65 1.905 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 61 "/nvm_pcb_pmain_digital/DO2") (pinfunction "1A1") (pintype "input"))
    (pad "5" smd roundrect locked (at -4.65 0.635 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 41 "/nvm_pcb_pmain_digital/DOT7") (pinfunction "2Y1") (pintype "tri_state"))
    (pad "6" smd roundrect locked (at -4.65 -0.635 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 60 "/nvm_pcb_pmain_digital/DO3") (pinfunction "1A2") (pintype "input"))
    (pad "7" smd roundrect locked (at -4.65 -1.905 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 44 "/nvm_pcb_pmain_digital/DOT8") (pinfunction "2Y2") (pintype "tri_state"))
    (pad "8" smd roundrect locked (at -4.65 -3.175 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 55 "/nvm_pcb_pmain_digital/DO5") (pinfunction "1A3") (pintype "input"))
    (pad "9" smd roundrect locked (at -4.65 -4.445 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 249 "unconnected-(U8-Pad9)") (pinfunction "2Y3") (pintype "tri_state"))
    (pad "10" smd roundrect locked (at -4.65 -5.715 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "11" smd roundrect locked (at 4.65 -5.715 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "2A3") (pintype "input"))
    (pad "12" smd roundrect locked (at 4.65 -4.445 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 42 "/nvm_pcb_pmain_digital/DOT5") (pinfunction "1Y3") (pintype "tri_state"))
    (pad "13" smd roundrect locked (at 4.65 -3.175 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 58 "/nvm_pcb_pmain_digital/DO8") (pinfunction "2A2") (pintype "input"))
    (pad "14" smd roundrect locked (at 4.65 -1.905 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 46 "/nvm_pcb_pmain_digital/DOT3") (pinfunction "1Y2") (pintype "tri_state"))
    (pad "15" smd roundrect locked (at 4.65 -0.635 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 57 "/nvm_pcb_pmain_digital/DO7") (pinfunction "2A1") (pintype "input"))
    (pad "16" smd roundrect locked (at 4.65 0.635 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 43 "/nvm_pcb_pmain_digital/DOT2") (pinfunction "1Y1") (pintype "tri_state"))
    (pad "17" smd roundrect locked (at 4.65 1.905 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 56 "/nvm_pcb_pmain_digital/DO6") (pinfunction "2A0") (pintype "input"))
    (pad "18" smd roundrect locked (at 4.65 3.175 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 47 "/nvm_pcb_pmain_digital/DOT1") (pinfunction "1Y0") (pintype "tri_state"))
    (pad "19" smd roundrect locked (at 4.65 4.445 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "2OE") (pintype "input"))
    (pad "20" smd roundrect locked (at 4.65 5.715 270) (size 2.05 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "+5V") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "B.Cu")
    (tedit 5EBA9318)
    (at 249 -57)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C226K025AT")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C66" (at 0 2.55) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -2.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.55 0) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 132 "/nvm_pmain_fpsu/F5V_D") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.55 0) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 130 "/nvm_pmain_fpsu/FGND_D") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 176.6 -61.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C48" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 123.5 -106.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3903")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R34" (at 0 1.65) (layer "B.SilkS"))
    (fp_text value "39k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 175 "Net-(R32-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 200 -88.5 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC847.215")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q2" (at -3 -0.4 180) (layer "B.SilkS"))
    (fp_text value "BC847" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 186 "Net-(Q2-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect locked (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect locked (at 0.9375 0 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 104 "Net-(Q1-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 165 -73.5 -90)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V510J ")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN8" (at 3 -0.6 180) (layer "B.SilkS"))
    (fp_text value "51R" (at 0 -3.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 169 "Net-(J10-Pad1)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 171 "Net-(J10-Pad2)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 173 "Net-(J10-Pad3)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 174 "Net-(J10-Pad4)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 1.5 -2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 100 "/nvm_pcb_pmain_digital/EX4") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 1.5 -0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 101 "/nvm_pcb_pmain_digital/EX3") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 102 "/nvm_pcb_pmain_digital/EX2") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2 270) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 103 "/nvm_pcb_pmain_digital/EX1") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF" (layer "B.Cu")
    (tedit 5905D864)
    (at 241 -95.5)
    (descr "Diode, MELF,,")
    (tags "Diode MELF ")
    (property "PN" "SM5819")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D19" (at 14.1 5.5) (layer "B.SilkS"))
    (fp_text value "1N5819" (at -0.25 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.4 0) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 246 "Net-(C65-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2.4 0) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 130 "/nvm_pmain_fpsu/FGND_D") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 150 -102.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R44" (at 4.1 0.5) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 106 "/nvm_pcb_pmain_digital/ZCD_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 197 -54.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6202")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R52" (at 0.5 -2.4 180) (layer "B.SilkS"))
    (fp_text value "6k2" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 253 "/nvm_pcb_pmain_digital/BEEP") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 252 "Net-(Q3-Pad1)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_10.4x10.4_H4.8" (layer "B.Cu")
    (tedit 5990349B)
    (at 194.1 -128.5)
    (descr "Choke, SMD, 10.4x10.4mm 4.8mm height")
    (tags "Choke SMD")
    (property "PN" " PSDB1005NT100")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "L2" (at -0.4 -6) (layer "B.SilkS"))
    (fp_text value "10u" (at 0 -6.35) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.15 0) (size 2.7 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 68 "Net-(C10-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 4.15 0) (size 2.7 3.6) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 6 "/nvm_pmain_amp/OUT_P") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_10.4x10.4_H4.8.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:Diode_Bridge_Diotec_SO-DIL-Slim" (layer "B.Cu")
    (tedit 5A4F6E6E)
    (at 128 -148.5 90)
    (descr "SMD diode bridge Diotec SO-DIL Slim, see https://diotec.com/tl_files/diotec/files/pdf/datasheets/b40fs.pdf")
    (tags "DFS SO-DIL Slim")
    (property "PN" "DF10S-T")
    (property "Sheetfile" "rnvm_marge.kicad_sch")
    (property "Sheetname" "")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D5" (at -3.5 5.6) (layer "B.SilkS"))
    (fp_text value "DF10S" (at 0 -5.2 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0.065 270) (layer "B.Fab"))
    (pad "1" smd rect locked (at -4.37 2.55 90) (size 2 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 11 "Net-(C1-Pad2)") (pinfunction "+") (pintype "passive"))
    (pad "2" smd rect locked (at -4.37 -2.55 90) (size 2 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 9 "Net-(C1-Pad1)") (pinfunction "-") (pintype "passive"))
    (pad "3" smd rect locked (at 4.37 -2.55 90) (size 2 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 138 "Net-(D5-Pad3)") (pintype "passive"))
    (pad "4" smd rect locked (at 4.37 2.55 90) (size 2 1.5) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 139 "Net-(D5-Pad4)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/Diode_Bridge_Diotec_SO-DIL-Slim.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 206.5 -65.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2200")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R65" (at -5.6 3) (layer "B.SilkS"))
    (fp_text value "220R" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 207 "Net-(R62-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 134 "/nvm_pmain_fpsu/F-15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 118 -97 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A330FXAAC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C29" (at 1 -2.4 180) (layer "B.SilkS"))
    (fp_text value "33p" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 17 "+5V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 105 "Net-(C29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 196.6 -142.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y103KXAPW1BC")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C12" (at 0 1.68) (layer "B.SilkS"))
    (fp_text value "10n" (at 0 -1.68) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 167 "Net-(C12-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 6 "/nvm_pmain_amp/OUT_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0805_2012Metric_Pad1.05x1.20mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEF0)
    (at 147.4 -52.25 180)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "PN" "BLM21A102SPT")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB1" (at 0.3 1.25) (layer "B.SilkS"))
    (fp_text value "Ferrite_Bead_Small" (at 0 -1.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -1.15 0 180) (size 1.05 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2380952381)
      (net 19 "+3.3VADC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.15 0 180) (size 1.05 1.2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2380952381)
      (net 18 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "B.Cu")
    (tedit 5FA16958)
    (at 195 -94.5 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC847.215")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q1" (at 0 2.4 90) (layer "B.SilkS"))
    (fp_text value "BC847" (at 0 -2.4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 104 "Net-(Q1-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect locked (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(C27-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect locked (at 0.9375 0 90) (size 1.475 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 112 "+9VA") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 200 -93.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6202")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R30" (at 3.5 0.1 180) (layer "B.SilkS"))
    (fp_text value "6k2" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 186 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 242 "/nvm_pcb_pmain_digital/S_DRIV") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 191.5 -138.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG0033")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R21" (at 0.1 2) (layer "B.SilkS"))
    (fp_text value "3R3" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 63 "Net-(C17-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 174.8 -49.7)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C49" (at 1.3 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MELF" (layer "B.Cu")
    (tedit 5905D864)
    (at 241 -99.5 180)
    (descr "Diode, MELF,,")
    (tags "Diode MELF ")
    (property "PN" "SM5819")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D17" (at -14.1 -8) (layer "B.SilkS"))
    (fp_text value "1N5819" (at -0.25 -2.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5) (layer "B.Fab"))
    (pad "1" smd rect locked (at -2.4 0 180) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 250 "Net-(C67-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 2.4 0 180) (size 1.5 2.7) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 246 "Net-(C65-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 147 -119.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1003")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R27" (at -3.9 1) (layer "B.SilkS"))
    (fp_text value "100K" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 172 "Net-(R23-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 175 -66.5)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C50" (at 1.6 1.5) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 18 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect locked (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 121 -102.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2493FB300")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "link" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R35" (at -1 -2.9 180) (layer "B.SilkS"))
    (fp_text value "249k" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 105 "Net-(C29-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm" (layer "B.Cu")
    (tedit 5E1214D9)
    (at 127 -98.5 90)
    (descr "HTSSOP, 16 Pin (http://www.analog.com/media/en/technical-documentation/data-sheets/LTC7810.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "HTSSOP SO")
    (property "PN" "LM43600PWPR")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U6" (at -5 -0.9 180) (layer "B.SilkS"))
    (fp_text value "LM43600" (at 0 -3.45 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "" smd roundrect locked (at 0 -0.58 90) (size 1.98 0.93) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "" smd rect locked (at 0 0 90) (size 2.46 2.31) (layers "B.Mask"))
    (pad "" smd roundrect locked (at 0 0.58 90) (size 1.98 0.93) (layers "B.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -2.8625 2.275 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(C28-Pad1)") (pinfunction "SW") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.8625 1.625 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 65 "Net-(C28-Pad1)") (pinfunction "SW") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.8625 0.975 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(C28-Pad2)") (pinfunction "CBOOT") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.8625 0.325 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(C32-Pad1)") (pinfunction "VCC") (pintype "input"))
    (pad "5" smd roundrect locked (at -2.8625 -0.325 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 17 "+5V") (pinfunction "BIAS") (pintype "input"))
    (pad "6" smd roundrect locked (at -2.8625 -0.975 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 155 "unconnected-(U6-Pad6)") (pinfunction "SYNC") (pintype "input"))
    (pad "7" smd roundrect locked (at -2.8625 -1.625 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 156 "unconnected-(U6-Pad7)") (pinfunction "RT") (pintype "input"))
    (pad "8" smd roundrect locked (at -2.8625 -2.275 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 157 "unconnected-(U6-Pad8)") (pinfunction "PGOOD") (pintype "input"))
    (pad "9" smd roundrect locked (at 2.8625 -2.275 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 105 "Net-(C29-Pad2)") (pinfunction "FB") (pintype "input"))
    (pad "10" smd roundrect locked (at 2.8625 -1.625 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "AGND") (pintype "input"))
    (pad "11" smd roundrect locked (at 2.8625 -0.975 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C30-Pad1)") (pinfunction "SS/TRK") (pintype "input"))
    (pad "12" smd roundrect locked (at 2.8625 -0.325 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 175 "Net-(R32-Pad2)") (pinfunction "EN") (pintype "input"))
    (pad "13" smd roundrect locked (at 2.8625 0.325 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "+12V") (pinfunction "VIN") (pintype "input"))
    (pad "14" smd roundrect locked (at 2.8625 0.975 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "+12V") (pinfunction "VIN") (pintype "input"))
    (pad "15" smd roundrect locked (at 2.8625 1.625 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "PGND") (pintype "input"))
    (pad "16" smd roundrect locked (at 2.8625 2.275 90) (size 1.575 0.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "PGND") (pintype "input"))
    (pad "17" smd rect locked (at 0 0 90) (size 3.4 5) (layers "B.Cu")
      (net 2 "GND") (pinfunction "PAD") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/HTSSOP-16-1EP_4.4x5mm_P0.65mm_EP3.4x5mm_Mask2.46x2.31mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 162 -98.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R11" (at 2.5 -2.4 180) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 15 "Net-(C7-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 191 -51.5 90)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V510J ")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN7" (at 3 -0.9 180) (layer "B.SilkS"))
    (fp_text value "51R" (at 0 -3.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2 90) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 162 "Net-(J9-Pad3)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66 90) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 163 "Net-(J9-Pad4)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66 90) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 164 "Net-(J9-Pad5)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2 90) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 168 "Net-(J9-Pad6)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 1.5 -2 90) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 85 "/nvm_pcb_pmain_digital/AB_RX") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 1.5 -0.66 90) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 84 "/nvm_pcb_pmain_digital/AB_TX") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66 90) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 83 "/nvm_pcb_pmain_digital/AB_RST") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2 90) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 82 "/nvm_pcb_pmain_digital/AB_CTRL") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_Array_Convex_4x1206" (layer "B.Cu")
    (tedit 58E0A8BD)
    (at 153 -79.9)
    (descr "Chip Resistor Network, ROHM MNR34 (see mnr_g.pdf)")
    (tags "resistor array")
    (property "PN" "EXB-S8V510J ")
    (property "Sheetfile" "nvm_pcb_pmain_digital.kicad_sch")
    (property "Sheetname" "nvm_pcb_pmain_digital")
    (property "link" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN1" (at 3.6 0.4) (layer "B.SilkS"))
    (fp_text value "51R" (at 0 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 201 "Net-(J8-Pad4)") (pinfunction "R1.1") (pintype "passive"))
    (pad "2" smd rect locked (at -1.5 0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 200 "Net-(J8-Pad3)") (pinfunction "R2.1") (pintype "passive"))
    (pad "3" smd rect locked (at -1.5 -0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 153 "Net-(J8-Pad2)") (pinfunction "R3.1") (pintype "passive"))
    (pad "4" smd rect locked (at -1.5 -2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 152 "Net-(J8-Pad1)") (pinfunction "R4.1") (pintype "passive"))
    (pad "5" smd rect locked (at 1.5 -2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 86 "/nvm_pcb_pmain_digital/EIO1") (pinfunction "R4.2") (pintype "passive"))
    (pad "6" smd rect locked (at 1.5 -0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 89 "/nvm_pcb_pmain_digital/EIO2") (pinfunction "R3.2") (pintype "passive"))
    (pad "7" smd rect locked (at 1.5 0.66) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 87 "/nvm_pcb_pmain_digital/EU2RX") (pinfunction "R2.2") (pintype "passive"))
    (pad "8" smd rect locked (at 1.5 2) (size 0.9 0.9) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 90 "/nvm_pcb_pmain_digital/EU2TX") (pinfunction "R1.2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Array_Convex_4x1206.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 147 -116.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3903")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R28" (at -3.9 0.5) (layer "B.SilkS"))
    (fp_text value "39k" (at 0 -1.7) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 197 "Net-(R24-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "B.Cu")
    (tedit 5EBA9318)
    (at 235 -57)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C226K025AT")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C56" (at 0 2.55) (layer "B.SilkS"))
    (fp_text value "22u" (at 0 -2.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.55 0) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 131 "/nvm_pmain_fpsu/F5V_A") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.55 0) (size 2.25 2.35) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.1111111111)
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SO-14_3.9x8.65mm_P1.27mm" (layer "B.Cu")
    (tedit 5F427CE7)
    (at 168 -92.5 -90)
    (descr "SO, 14 Pin (https://www.st.com/resource/en/datasheet/l6491.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SO SO")
    (property "PN" "LM324AD")
    (property "Sheetfile" "nvm_pmain_amp.kicad_sch")
    (property "Sheetname" "nvm_pmain_amp")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U4" (at -4.5 -0.1 -180) (layer "B.SilkS"))
    (fp_text value "LM324" (at 0 -5.28 -270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "B.Fab"))
    (pad "1" smd roundrect locked (at -2.475 3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GNDREF") (pintype "output"))
    (pad "2" smd roundrect locked (at -2.475 2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 1 "GNDREF") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(C7-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 0 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 112 "+9VA") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect locked (at -2.475 -1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(C23-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect locked (at -2.475 -2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 194 "Net-(R20-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect locked (at -2.475 -3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 194 "Net-(R20-Pad1)") (pintype "output"))
    (pad "8" smd roundrect locked (at 2.475 -3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 193 "Net-(R18-Pad1)") (pintype "output"))
    (pad "9" smd roundrect locked (at 2.475 -2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 193 "Net-(R18-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect locked (at 2.475 -1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(C21-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect locked (at 2.475 0 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect locked (at 2.475 1.27 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 195 "Net-(R22-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect locked (at 2.475 2.54 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(C18-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect locked (at 2.475 3.81 270) (size 1.95 0.6) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(JP1-Pad3)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SO-14_3.9x8.65mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "B.Cu")
    (tedit 58FE61E9)
    (at 220.5 -69)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-18K7")
    (property "Sheetfile" "nvm_pmain_fpsu.kicad_sch")
    (property "Sheetname" "nvm_pmain_fpsu")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R57" (at 0 1.65 180) (layer "B.SilkS"))
    (fp_text value "18k7" (at 0 -1.7 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "B.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 117 "Net-(C57-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "B.Cu" "B.Paste" "B.Mask")
      (net 128 "/nvm_pmain_fpsu/FGND_A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 157 -176) (end 206.6 -176) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 155.1 -148) (end 198.1 -148) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 137.6 -133) (end 137.6 -146) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 148.6 -152) (end 142.6 -152) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 157 -174) (end 157 -176) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 263.6 -102.5) (end 206.6 -102.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 155.1 -149) (end 155.1 -148) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 141.6 -146) (end 141.6 -153) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 206.6 -102.5) (end 206.6 -176) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 137.6 -146) (end 141.6 -146) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 148.6 -153) (end 148.6 -152) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 120 -167) (end 120 -174) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 118.6 -132) (end 118.6 -133) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 141.6 -153) (end 148.6 -153) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 154 -175) (end 112.6 -175) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.6 -132) (end 118.6 -132) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 142.6 -152) (end 142.6 -145) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 112.6 -45) (end 263.6 -45) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 263.6 -45) (end 263.6 -102.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 154 -175) (end 154 -174) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 121 -174) (end 121 -166) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 138.6 -145) (end 138.6 -132) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 118.6 -133) (end 137.6 -133) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 121 -166) (end 113.5 -166) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 112.6 -175) (end 112.6 -45) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 113.5 -167) (end 113.5 -166) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 142.6 -145) (end 138.6 -145) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 113.5 -167) (end 120 -167) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 198.1 -148) (end 198.1 -149) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 198.1 -149) (end 155.1 -149) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 154 -174) (end 157 -174) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 120 -174) (end 121 -174) (layer "Edge.Cuts") (width 0.1))
  (gr_text "NVM\nMARGE PCB REV 1" (at 246 -99.8) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118 -45)
        (xy 112.6 -45)
        (xy 112.6 -50.5)
        (xy 118 -50.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 118 -101.5)
        (xy 112.6 -101.5)
        (xy 112.6 -107.5)
        (xy 118 -107.5)
      )
    )
  )
  (zone (net 18) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 172.5 -60.5)
        (xy 170.5 -60.5)
        (xy 170.5 -62.5)
        (xy 172.5 -62.5)
      )
    )
  )
  (zone (net 18) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 159 -63.5)
        (xy 159.8 -62.5)
        (xy 161.6 -62.5)
        (xy 161.6 -60.9)
        (xy 158.6 -60.9)
        (xy 157.2 -62.5)
        (xy 157.2 -66.9)
        (xy 159 -66.9)
      )
    )
  )
  (zone (net 128) (net_name "/nvm_pmain_fpsu/FGND_A") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.3) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 263.6 -53)
        (xy 256 -53)
        (xy 256 -45.5)
        (xy 209 -45)
        (xy 209 -53)
        (xy 204 -53)
        (xy 204 -83)
        (xy 207 -86)
        (xy 207 -98.6)
        (xy 210.2 -101.8)
        (xy 210.2 -102.4)
        (xy 256 -102.5)
        (xy 256 -95)
        (xy 263.6 -95)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 206.6 -109.5)
        (xy 199 -109.5)
        (xy 199 -98.5)
        (xy 203 -98.5)
        (xy 203 -86.5)
        (xy 200 -86.5)
        (xy 200 -52.5)
        (xy 199 -52.5)
        (xy 199 -45)
        (xy 112.6 -45)
        (xy 112.6 -127.5)
        (xy 140 -127.5)
        (xy 140 -140.5)
        (xy 145 -145.5)
        (xy 145 -151)
        (xy 154 -151)
        (xy 154 -146.5)
        (xy 196 -146.5)
        (xy 196 -149.5)
        (xy 206.6 -149.5)
      )
    )
  )
  (zone (net 18) (net_name "+3V3") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 174.5 -51.5)
        (xy 174.5 -51)
        (xy 173.5 -50)
        (xy 172.5 -50)
        (xy 169 -53.5)
        (xy 169 -54)
        (xy 170 -55)
        (xy 171 -55)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 163 -138.5)
        (xy 157 -138.5)
        (xy 157 -144.5)
        (xy 163 -144.5)
      )
    )
  )
  (zone (net 5) (net_name "Net-(C18-Pad1)") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 143.5 -94.75)
        (xy 144 -94.25)
        (xy 145 -94.25)
        (xy 145 -93)
        (xy 147.5 -90.5)
        (xy 147.5 -88.75)
        (xy 141.5 -88.75)
        (xy 141.5 -90.5)
        (xy 142.75 -91.75)
        (xy 142.75 -94)
        (xy 141.75 -94)
        (xy 141.75 -96.4)
        (xy 143.5 -96.4)
      )
    )
  )
  (zone (net 18) (net_name "+3V3") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 153 -85.5)
        (xy 153 -84.5)
        (xy 137 -84.5)
        (xy 137 -88)
        (xy 150 -88)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 130.5 -96.5)
        (xy 123.5 -96.5)
        (xy 123.5 -100.25)
        (xy 130.5 -100.25)
      )
    )
  )
  (zone (net 120) (net_name "Net-(C14-Pad1)") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 171.8 -118)
        (xy 168.8 -118)
        (xy 168.8 -118.6)
        (xy 169.4 -119.2)
        (xy 171.8 -119.2)
      )
    )
  )
  (zone (net 18) (net_name "+3V3") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 174.5 -50)
        (xy 157.5 -50)
        (xy 157.5 -64.75)
        (xy 155.75 -64.75)
        (xy 155.75 -67)
        (xy 174.5 -67)
      )
    )
  )
  (zone (net 17) (net_name "+5V") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 131 -83.5)
        (xy 120.5 -83.5)
        (xy 120.5 -81)
        (xy 118 -81)
        (xy 118 -84)
        (xy 119.5 -85.5)
        (xy 119.5 -88)
        (xy 131 -88)
      )
    )
  )
  (zone (net 66) (net_name "Net-(C8-Pad1)") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 171.8 -119.8)
        (xy 169.6 -119.8)
        (xy 169 -119.2)
        (xy 168.4 -119.2)
        (xy 168.4 -120.8)
        (xy 171.8 -120.8)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 144 -96.75)
        (xy 137 -96.75)
        (xy 137 -100.5)
        (xy 144 -100.5)
      )
    )
  )
  (zone (net 63) (net_name "Net-(C17-Pad1)") (layer "B.Cu") (hatch edge 0.508)
    (priority 2)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 130 -94.25)
        (xy 131 -93.25)
        (xy 131 -89)
        (xy 125 -89)
        (xy 125 -91.5)
        (xy 129 -91.5)
        (xy 129 -94)
        (xy 128.35 -94)
        (xy 128.35 -96.3)
        (xy 130 -96.3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.21) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 207.5 -60.1)
        (xy 216 -60.1)
        (xy 216 -61.1)
        (xy 218 -61.1)
        (xy 218 -60.1)
        (xy 226.5 -60.1)
        (xy 226.5 -61.1)
        (xy 229 -61.1)
        (xy 229 -45.1)
        (xy 209 -45.1)
        (xy 209 -52.6)
        (xy 204 -52.6)
        (xy 204 -63.6)
        (xy 207.5 -63.6)
      )
    )
  )
)
