(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "Nanovoltmeter - MEGGIE")
    (date "2022-05-15")
    (rev "1")
  )
  (lib_symbols
    (symbol "Connector:Conn_01x08_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 10.16 0))
      (property "Value" "Conn_01x08_Male" (id 1) (at 0 -12.7 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x08, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x08_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -10.16)
            (xy 0.8636 -10.16)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -7.62)
            (xy 0.8636 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 0.8636 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 5.08)
            (xy 0.8636 5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 7.62)
            (xy 0.8636 7.62)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -10.033) (end 0 -10.287)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -7.493) (end 0 -7.747)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -4.953) (end 0 -5.207)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (rectangle (start 0.8636 5.207) (end 0 4.953)
          (fill (type outline))
        )
        (rectangle (start 0.8636 7.747) (end 0 7.493)
          (fill (type outline))
        )
        (pin passive line (at 5.08 7.62 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 5.08 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at 5.08 -7.62 180) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 5.08 -10.16 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
      )
    )
    (symbol "Mechanical:MountingHole" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "H" (id 0) (at 0 5.08 0))
      (property "Value" "MountingHole" (id 1) (at 0 3.175 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "mounting hole" (id 4) (at 0 0 0))
      (property "ki_description" "Mounting Hole without connection" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "MountingHole*" (id 6) (at 0 0 0))
      (symbol "MountingHole_0_1"
        (circle (center 0 0) (radius 1.27)
          (fill (type none))
        )
      )
    )
    (symbol "Switch:SW_Push" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "SW" (id 0) (at 1.27 2.54 0))
      (property "Value" "SW_Push" (id 1) (at 0 -1.524 0))
      (property "Footprint" "" (id 2) (at 0 5.08 0))
      (property "Datasheet" "~" (id 3) (at 0 5.08 0))
      (property "ki_keywords" "switch normally-open pushbutton push-button" (id 4) (at 0 0 0))
      (property "ki_description" "Push button switch, generic, two pins" (id 5) (at 0 0 0))
      (symbol "SW_Push_0_1"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.27)
            (xy 0 3.048)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.27)
            (xy -2.54 1.27)
          )
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "j_lib:logo_generic" (in_bom yes) (on_board yes)
      (property "Reference" "LOGO" (id 0) (at 0 3.81 0))
      (property "Value" "logo_generic" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "logo_generic_0_1"
        (rectangle (start -3.81 2.54) (end 3.81 -2.54)
          (fill (type none))
        )
      )
    )
  )
  (junction (at 137.16 73.66) (diameter 0) (color 0 0 0 0))
  (junction (at 137.16 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 167.005 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 121.92 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 147.32 76.835) (diameter 0) (color 0 0 0 0))
  (junction (at 132.08 64.77) (diameter 0) (color 0 0 0 0))
  (junction (at 162.56 64.77) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 162.56 88.265) (diameter 0) (color 0 0 0 0))
  (junction (at 167.005 73.66) (diameter 0) (color 0 0 0 0))
  (junction (at 121.92 73.66) (diameter 0) (color 0 0 0 0))
  (junction (at 147.32 64.77) (diameter 0) (color 0 0 0 0))
  (junction (at 121.92 96.52) (diameter 0) (color 0 0 0 0))
  (junction (at 152.4 73.66) (diameter 0) (color 0 0 0 0))
  (junction (at 147.32 88.265) (diameter 0) (color 0 0 0 0))
  (junction (at 132.08 88.265) (diameter 0) (color 0 0 0 0))
  (junction (at 132.08 76.835) (diameter 0) (color 0 0 0 0))
  (junction (at 162.56 76.835) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 147.32 85.09) (xy 147.32 88.265)))
  (wire (pts (xy 137.16 62.865) (xy 137.16 73.66)))
  (wire (pts (xy 147.32 62.865) (xy 147.32 64.77)))
  (wire (pts (xy 162.56 64.77) (xy 177.165 64.77)))
  (wire (pts (xy 177.165 73.66) (xy 177.165 76.835)))
  (wire (pts (xy 132.08 96.52) (xy 132.08 100.33)))
  (wire (pts (xy 132.08 76.835) (xy 147.32 76.835)))
  (wire (pts (xy 113.665 88.265) (xy 132.08 88.265)))
  (wire (pts (xy 177.165 85.09) (xy 177.165 88.265)))
  (wire (pts (xy 137.16 73.66) (xy 137.16 85.09)))
  (wire (pts (xy 113.665 100.33) (xy 132.08 100.33)))
  (wire (pts (xy 152.4 62.865) (xy 152.4 73.66)))
  (wire (pts (xy 147.32 88.265) (xy 162.56 88.265)))
  (wire (pts (xy 132.08 85.09) (xy 132.08 88.265)))
  (wire (pts (xy 152.4 73.66) (xy 152.4 85.09)))
  (wire (pts (xy 162.56 88.265) (xy 177.165 88.265)))
  (wire (pts (xy 132.08 88.265) (xy 147.32 88.265)))
  (wire (pts (xy 121.92 96.52) (xy 121.92 104.14)))
  (wire (pts (xy 137.16 85.09) (xy 137.16 104.14)))
  (wire (pts (xy 147.32 64.77) (xy 162.56 64.77)))
  (wire (pts (xy 167.005 85.09) (xy 167.005 104.775)))
  (wire (pts (xy 132.08 64.77) (xy 147.32 64.77)))
  (wire (pts (xy 162.56 85.09) (xy 162.56 88.265)))
  (wire (pts (xy 121.92 73.66) (xy 121.92 85.09)))
  (wire (pts (xy 177.165 62.865) (xy 177.165 64.77)))
  (wire (pts (xy 162.56 73.66) (xy 162.56 76.835)))
  (wire (pts (xy 147.32 76.835) (xy 162.56 76.835)))
  (wire (pts (xy 167.005 73.66) (xy 167.005 85.09)))
  (wire (pts (xy 162.56 62.865) (xy 162.56 64.77)))
  (wire (pts (xy 162.56 76.835) (xy 177.165 76.835)))
  (wire (pts (xy 167.005 62.865) (xy 167.005 73.66)))
  (wire (pts (xy 132.08 73.66) (xy 132.08 76.835)))
  (wire (pts (xy 152.4 85.09) (xy 152.4 104.775)))
  (wire (pts (xy 114.3 76.835) (xy 132.08 76.835)))
  (wire (pts (xy 121.92 85.09) (xy 121.92 96.52)))
  (wire (pts (xy 147.32 73.66) (xy 147.32 76.835)))
  (wire (pts (xy 132.08 62.865) (xy 132.08 64.77)))
  (wire (pts (xy 121.92 62.865) (xy 121.92 73.66)))
  (wire (pts (xy 114.935 64.77) (xy 132.08 64.77)))
  (label "KC2" (at 137.16 104.14 0))
  (label "KR1" (at 114.935 64.77 0))
  (label "KC1" (at 66.675 77.47 0))
  (label "KC4" (at 167.005 104.775 0))
  (label "KC2" (at 66.675 80.01 0))
  (label "KC4" (at 66.675 85.09 0))
  (label "KR3" (at 66.675 72.39 0))
  (label "KR1" (at 66.675 67.31 0))
  (label "KC1" (at 121.92 104.14 0))
  (label "KC3" (at 66.675 82.55 0))
  (label "KC3" (at 152.4 104.775 0))
  (label "KR2" (at 114.3 76.835 0))
  (label "KR2" (at 66.675 69.85 0))
  (label "KR4" (at 66.675 74.93 0))
  (label "KR3" (at 113.665 88.265 0))
  (label "KR4" (at 113.665 100.33 0))
  (symbol (lib_id "Switch:SW_Push") (at 157.48 73.66 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW7" (id 0) (at 157.48 66.7725 0))
    (property "Value" "SW_Push" (id 1) (at 157.48 69.5476 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 157.48 68.58 0))
    (property "Datasheet" "~" (id 3) (at 157.48 68.58 0))
    (property "PN" "6450" (id 4) (at 157.48 73.66 0))
    (property "SUPPLIER" "TME" (id 5) (at 157.48 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 100.965 161.925 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H7" (id 0) (at 103.505 161.0165 0))
    (property "Value" "MountingHole" (id 1) (at 103.505 163.7916 0))
    (property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (id 2) (at 100.965 161.925 0))
    (property "Datasheet" "~" (id 3) (at 100.965 161.925 0))
    (property "Comment" "DNP" (id 4) (at 100.965 161.925 0))
  )
  (symbol (lib_id "Switch:SW_Push") (at 172.085 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW12" (id 0) (at 172.085 78.2025 0))
    (property "Value" "SW_Push" (id 1) (at 172.085 80.9776 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 172.085 80.01 0))
    (property "Datasheet" "~" (id 3) (at 172.085 80.01 0))
    (property "PN" "6450" (id 4) (at 172.085 85.09 0))
    (property "SUPPLIER" "TME" (id 5) (at 172.085 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 107.95 161.925 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H8" (id 0) (at 110.49 161.0165 0))
    (property "Value" "MountingHole" (id 1) (at 110.49 163.7916 0))
    (property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (id 2) (at 107.95 161.925 0))
    (property "Datasheet" "~" (id 3) (at 107.95 161.925 0))
    (property "Comment" "DNP" (id 4) (at 107.95 161.925 0))
  )
  (symbol (lib_id "Switch:SW_Push") (at 127 62.865 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW1" (id 0) (at 127 55.9775 0))
    (property "Value" "SW_Push" (id 1) (at 127 58.7526 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 127 57.785 0))
    (property "Datasheet" "~" (id 3) (at 127 57.785 0))
    (property "PN" "6450" (id 4) (at 127 62.865 0))
    (property "SUPPLIER" "TME" (id 5) (at 127 62.865 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_Push") (at 127 96.52 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW13" (id 0) (at 127 89.6325 0))
    (property "Value" "SW_Push" (id 1) (at 127 92.4076 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 127 91.44 0))
    (property "Datasheet" "~" (id 3) (at 127 91.44 0))
    (property "PN" "6450" (id 4) (at 127 96.52 0))
    (property "SUPPLIER" "TME" (id 5) (at 127 96.52 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 90.805 161.925 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H6" (id 0) (at 93.345 161.0165 0))
    (property "Value" "MountingHole" (id 1) (at 93.345 163.7916 0))
    (property "Footprint" "MountingHole:MountingHole_2.5mm_Pad" (id 2) (at 90.805 161.925 0))
    (property "Datasheet" "~" (id 3) (at 90.805 161.925 0))
    (property "Comment" "DNP" (id 4) (at 90.805 161.925 0))
  )
  (symbol (lib_id "Switch:SW_Push") (at 142.24 73.66 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW6" (id 0) (at 142.24 66.7725 0))
    (property "Value" "SW_Push" (id 1) (at 142.24 69.5476 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 142.24 68.58 0))
    (property "Datasheet" "~" (id 3) (at 142.24 68.58 0))
    (property "PN" "6450" (id 4) (at 142.24 73.66 0))
    (property "SUPPLIER" "TME" (id 5) (at 142.24 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_Push") (at 127 73.66 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW5" (id 0) (at 127 66.7725 0))
    (property "Value" "SW_Push" (id 1) (at 127 69.5476 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 127 68.58 0))
    (property "Datasheet" "~" (id 3) (at 127 68.58 0))
    (property "PN" "6450" (id 4) (at 127 73.66 0))
    (property "SUPPLIER" "TME" (id 5) (at 127 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 100.965 156.845 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H3" (id 0) (at 103.505 155.9365 0))
    (property "Value" "MountingHole" (id 1) (at 103.505 158.7116 0))
    (property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (id 2) (at 100.965 156.845 0))
    (property "Datasheet" "~" (id 3) (at 100.965 156.845 0))
    (property "Comment" "DNP" (id 4) (at 100.965 156.845 0))
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 90.805 156.845 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H2" (id 0) (at 93.345 155.9365 0))
    (property "Value" "MountingHole" (id 1) (at 93.345 158.7116 0))
    (property "Footprint" "MountingHole:MountingHole_2.5mm_Pad" (id 2) (at 90.805 156.845 0))
    (property "Datasheet" "~" (id 3) (at 90.805 156.845 0))
    (property "Comment" "DNP" (id 4) (at 90.805 156.845 0))
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 107.95 156.845 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H4" (id 0) (at 110.49 155.9365 0))
    (property "Value" "MountingHole" (id 1) (at 110.49 158.7116 0))
    (property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (id 2) (at 107.95 156.845 0))
    (property "Datasheet" "~" (id 3) (at 107.95 156.845 0))
    (property "Comment" "DNP" (id 4) (at 107.95 156.845 0))
  )
  (symbol (lib_id "Switch:SW_Push") (at 142.24 85.09 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW10" (id 0) (at 142.24 78.2025 0))
    (property "Value" "SW_Push" (id 1) (at 142.24 80.9776 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 142.24 80.01 0))
    (property "Datasheet" "~" (id 3) (at 142.24 80.01 0))
    (property "PN" "6450" (id 4) (at 142.24 85.09 0))
    (property "SUPPLIER" "TME" (id 5) (at 142.24 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_Push") (at 172.085 73.66 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW8" (id 0) (at 172.085 66.7725 0))
    (property "Value" "SW_Push" (id 1) (at 172.085 69.5476 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 172.085 68.58 0))
    (property "Datasheet" "~" (id 3) (at 172.085 68.58 0))
    (property "PN" "6450" (id 4) (at 172.085 73.66 0))
    (property "SUPPLIER" "TME" (id 5) (at 172.085 73.66 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_Push") (at 127 85.09 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW9" (id 0) (at 127 78.2025 0))
    (property "Value" "SW_Push" (id 1) (at 127 80.9776 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 127 80.01 0))
    (property "Datasheet" "~" (id 3) (at 127 80.01 0))
    (property "PN" "6450" (id 4) (at 127 85.09 0))
    (property "SUPPLIER" "TME" (id 5) (at 127 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_Push") (at 157.48 85.09 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "SW11" (id 0) (at 157.48 78.2025 0))
    (property "Value" "SW_Push" (id 1) (at 157.48 80.9776 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 157.48 80.01 0))
    (property "Datasheet" "~" (id 3) (at 157.48 80.01 0))
    (property "PN" "6450" (id 4) (at 157.48 85.09 0))
    (property "SUPPLIER" "TME" (id 5) (at 157.48 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_Push") (at 157.48 62.865 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW3" (id 0) (at 157.48 55.9775 0))
    (property "Value" "SW_Push" (id 1) (at 157.48 58.7526 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 157.48 57.785 0))
    (property "Datasheet" "~" (id 3) (at 157.48 57.785 0))
    (property "PN" "6450" (id 4) (at 157.48 62.865 0))
    (property "SUPPLIER" "TME" (id 5) (at 157.48 62.865 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 83.82 156.845 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H1" (id 0) (at 86.36 155.9365 0))
    (property "Value" "MountingHole" (id 1) (at 86.36 158.7116 0))
    (property "Footprint" "MountingHole:MountingHole_2.5mm_Pad" (id 2) (at 83.82 156.845 0))
    (property "Datasheet" "~" (id 3) (at 83.82 156.845 0))
    (property "Comment" "DNP" (id 4) (at 83.82 156.845 0))
  )
  (symbol (lib_id "Connector:Conn_01x08_Male") (at 61.595 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J1" (id 0) (at 62.23 63.2673 0))
    (property "Value" "Conn_01x08_Male" (id 1) (at 62.23 66.0424 0))
    (property "Footprint" "Connector_Molex:Molex_KK-254_AE-6410-08A_1x08_P2.54mm_Vertical" (id 2) (at 61.595 74.93 0))
    (property "Datasheet" "~" (id 3) (at 61.595 74.93 0))
    (property "Comment" "DNP" (id 4) (at 61.595 74.93 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "j_lib:logo_generic") (at 125.73 161.29 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "LOGO1" (id 0) (at 130.2512 161.769 0))
    (property "Value" "logo_generic" (id 1) (at 125.73 165.1 0))
    (property "Footprint" "j_lib:logo_rpg7x9" (id 2) (at 125.73 161.29 0))
    (property "Datasheet" "" (id 3) (at 125.73 161.29 0))
    (property "Comment" "DNP" (id 4) (at 125.73 161.29 0))
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 83.82 161.925 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H5" (id 0) (at 86.36 161.0165 0))
    (property "Value" "MountingHole" (id 1) (at 86.36 163.7916 0))
    (property "Footprint" "MountingHole:MountingHole_2.5mm_Pad" (id 2) (at 83.82 161.925 0))
    (property "Datasheet" "~" (id 3) (at 83.82 161.925 0))
    (property "Comment" "DNP" (id 4) (at 83.82 161.925 0))
  )
  (symbol (lib_id "Switch:SW_Push") (at 142.24 62.865 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW2" (id 0) (at 142.24 55.9775 0))
    (property "Value" "SW_Push" (id 1) (at 142.24 58.7526 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 142.24 57.785 0))
    (property "Datasheet" "~" (id 3) (at 142.24 57.785 0))
    (property "PN" "6450" (id 4) (at 142.24 62.865 0))
    (property "SUPPLIER" "TME" (id 5) (at 142.24 62.865 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Switch:SW_Push") (at 172.085 62.865 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "SW4" (id 0) (at 172.085 55.9775 0))
    (property "Value" "SW_Push" (id 1) (at 172.085 58.7526 0))
    (property "Footprint" "j_lib:MQ_6450" (id 2) (at 172.085 57.785 0))
    (property "Datasheet" "~" (id 3) (at 172.085 57.785 0))
    (property "PN" "6450" (id 4) (at 172.085 62.865 0))
    (property "SUPPLIER" "TME" (id 5) (at 172.085 62.865 0))
    (pin "1")
    (pin "2")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "H1") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_2.5mm_Pad")
    )
    (path
      (reference "H2") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_2.5mm_Pad")
    )
    (path
      (reference "H3") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad")
    )
    (path
      (reference "H4") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad")
    )
    (path
      (reference "H5") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_2.5mm_Pad")
    )
    (path
      (reference "H6") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_2.5mm_Pad")
    )
    (path
      (reference "H7") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad")
    )
    (path
      (reference "H8") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad")
    )
    (path
      (reference "J1") (unit 1) (value "Conn_01x08_Male") (footprint "Connector_Molex:Molex_KK-254_AE-6410-08A_1x08_P2.54mm_Vertical")
    )
    (path
      (reference "LOGO1") (unit 1) (value "logo_generic") (footprint "j_lib:logo_rpg7x9")
    )
    (path
      (reference "SW1") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW2") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW3") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW4") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW5") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW6") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW7") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW8") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW9") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW10") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW11") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW12") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
    (path
      (reference "SW13") (unit 1) (value "SW_Push") (footprint "j_lib:MQ_6450")
    )
  )
)
