(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.69)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (1 "In1.Cu" signal)
    (2 "In2.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 0.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In1.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 2" (type "prepreg") (thickness 0.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "In2.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 3" (type "core") (thickness 0.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "+15V")
  (net 2 "GND")
  (net 3 "GNDS")
  (net 4 "-15V")
  (net 5 "+5V")
  (net 6 "/RE_P")
  (net 7 "+3V3")
  (net 8 "Net-(C19-Pad1)")
  (net 9 "Net-(C19-Pad2)")
  (net 10 "Net-(FB3-Pad2)")
  (net 11 "Net-(FB4-Pad2)")
  (net 12 "Net-(FB5-Pad2)")
  (net 13 "Net-(FB6-Pad2)")
  (net 14 "Net-(FB7-Pad2)")
  (net 15 "Net-(FB8-Pad2)")
  (net 16 "Net-(FB9-Pad2)")
  (net 17 "Net-(FB10-Pad2)")
  (net 18 "Net-(FB11-Pad2)")
  (net 19 "Net-(D1-Pad2)")
  (net 20 "Net-(FB1-Pad1)")
  (net 21 "Net-(FB1-Pad2)")
  (net 22 "/LNAMP/L_IN")
  (net 23 "Net-(FB2-Pad2)")
  (net 24 "Net-(J1-Pad1)")
  (net 25 "Net-(J1-Pad2)")
  (net 26 "Net-(J1-Pad3)")
  (net 27 "Net-(J1-Pad4)")
  (net 28 "/MA_G1")
  (net 29 "/MS_A2")
  (net 30 "/MA_G10")
  (net 31 "/MS_A1")
  (net 32 "/MA_G100")
  (net 33 "/MS_A0")
  (net 34 "/JA_DOUT")
  (net 35 "Net-(C2-Pad1)")
  (net 36 "/JA_DIN")
  (net 37 "Net-(C3-Pad1)")
  (net 38 "/COMP")
  (net 39 "/JA_CS")
  (net 40 "Net-(C12-Pad2)")
  (net 41 "/JA_SCK")
  (net 42 "Net-(C235-Pad1)")
  (net 43 "Net-(C235-Pad2)")
  (net 44 "/VREF_EXT")
  (net 45 "/OUT")
  (net 46 "/R1B")
  (net 47 "/R1A")
  (net 48 "/R2B")
  (net 49 "/CP_9M")
  (net 50 "/R2A")
  (net 51 "Net-(K3-Pad1)")
  (net 52 "/RE3")
  (net 53 "unconnected-(J4-Pad7)")
  (net 54 "/RE4")
  (net 55 "Net-(Q1-Pad1)")
  (net 56 "Net-(Q2-Pad1)")
  (net 57 "unconnected-(J4-Pad9)")
  (net 58 "/VR28N")
  (net 59 "unconnected-(J4-Pad11)")
  (net 60 "/VR28P")
  (net 61 "unconnected-(J4-Pad14)")
  (net 62 "/VREF7")
  (net 63 "/CP_07V")
  (net 64 "/CP_70M")
  (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT")
  (net 66 "GND1")
  (net 67 "/LNAMP/L_OUT")
  (net 68 "/LNAMP/VTRIM")
  (net 69 "/LNAMP/ITRIM")
  (net 70 "/JAMP_OUT")
  (net 71 "/BOOT")
  (net 72 "/MAMP_IN")
  (net 73 "unconnected-(U6-Pad1)")
  (net 74 "unconnected-(U6-Pad5)")
  (net 75 "unconnected-(U6-Pad8)")
  (net 76 "-9V")
  (net 77 "+9V")
  (net 78 "Net-(FB12-Pad2)")
  (net 79 "Net-(FB13-Pad2)")
  (net 80 "Net-(FB14-Pad2)")
  (net 81 "Net-(FB15-Pad2)")
  (net 82 "Net-(FB16-Pad2)")
  (net 83 "Net-(FB17-Pad2)")
  (net 84 "Net-(FB18-Pad2)")
  (net 85 "Net-(FB19-Pad2)")
  (net 86 "Net-(FB20-Pad2)")
  (net 87 "Net-(FB21-Pad2)")
  (net 88 "Net-(FB22-Pad2)")
  (net 89 "Net-(FB23-Pad2)")
  (net 90 "Net-(FB24-Pad2)")
  (net 91 "Net-(FB25-Pad2)")
  (net 92 "Net-(FB26-Pad2)")
  (net 93 "Net-(FB27-Pad2)")
  (net 94 "Net-(FB28-Pad2)")
  (net 95 "Net-(FB29-Pad2)")
  (net 96 "Net-(FB30-Pad2)")
  (net 97 "Net-(FB31-Pad2)")
  (net 98 "Net-(FB32-Pad2)")
  (net 99 "Net-(FB33-Pad2)")
  (net 100 "Net-(FB34-Pad2)")
  (net 101 "Net-(FB35-Pad2)")
  (net 102 "Net-(FB36-Pad2)")
  (net 103 "Net-(FB37-Pad2)")
  (net 104 "Net-(FB38-Pad2)")
  (net 105 "Net-(FB39-Pad2)")
  (net 106 "Net-(FB40-Pad2)")
  (net 107 "Net-(FB41-Pad2)")
  (net 108 "Net-(FB42-Pad2)")
  (net 109 "Net-(FB43-Pad2)")
  (net 110 "Net-(FB44-Pad2)")
  (net 111 "Net-(FB45-Pad2)")
  (net 112 "Net-(FB46-Pad2)")
  (net 113 "Net-(FB47-Pad2)")
  (net 114 "Net-(FB48-Pad2)")
  (net 115 "Net-(FB49-Pad2)")
  (net 116 "Net-(FB50-Pad2)")
  (net 117 "Net-(FB51-Pad2)")
  (net 118 "Net-(FB52-Pad2)")
  (net 119 "Net-(FB53-Pad2)")
  (net 120 "Net-(FB54-Pad2)")
  (net 121 "Net-(FB55-Pad2)")
  (net 122 "Net-(FB56-Pad2)")
  (net 123 "Net-(FB57-Pad2)")
  (net 124 "Net-(FB58-Pad2)")
  (net 125 "Net-(FB59-Pad2)")
  (net 126 "Net-(FB60-Pad2)")
  (net 127 "Net-(FB61-Pad2)")
  (net 128 "Net-(FB62-Pad2)")
  (net 129 "Net-(FB63-Pad2)")
  (net 130 "Net-(FB64-Pad2)")
  (net 131 "Net-(FB65-Pad2)")
  (net 132 "Net-(FB66-Pad2)")
  (net 133 "Net-(FB67-Pad2)")
  (net 134 "Net-(FB68-Pad2)")
  (net 135 "Net-(FB69-Pad2)")
  (net 136 "Net-(FB70-Pad2)")
  (net 137 "Net-(FB71-Pad2)")
  (net 138 "Net-(FB72-Pad2)")
  (net 139 "Net-(FB73-Pad2)")
  (net 140 "Net-(FB74-Pad2)")
  (net 141 "Net-(FB75-Pad2)")
  (net 142 "Net-(FB76-Pad2)")
  (net 143 "Net-(FB77-Pad2)")
  (net 144 "Net-(FB78-Pad2)")
  (net 145 "Net-(FB79-Pad2)")
  (net 146 "Net-(FB80-Pad2)")
  (net 147 "Net-(FB81-Pad2)")
  (net 148 "Net-(FB82-Pad2)")
  (net 149 "Net-(FB83-Pad2)")
  (net 150 "Net-(FB84-Pad2)")
  (net 151 "Net-(FB85-Pad2)")
  (net 152 "Net-(FB86-Pad2)")
  (net 153 "Net-(FB87-Pad2)")
  (net 154 "Net-(FB88-Pad2)")
  (net 155 "Net-(FB89-Pad2)")
  (net 156 "Net-(FB90-Pad2)")
  (net 157 "Net-(FB91-Pad2)")
  (net 158 "Net-(FB92-Pad2)")
  (net 159 "Net-(FB93-Pad2)")
  (net 160 "Net-(FB94-Pad2)")
  (net 161 "Net-(FB95-Pad2)")
  (net 162 "Net-(FB96-Pad2)")
  (net 163 "Net-(FB97-Pad2)")
  (net 164 "Net-(FB98-Pad2)")
  (net 165 "Net-(FB99-Pad2)")
  (net 166 "Net-(FB100-Pad2)")
  (net 167 "Net-(FB101-Pad2)")
  (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT")
  (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT")
  (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT")
  (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT")
  (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT")
  (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT")
  (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT")
  (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT")
  (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT")
  (net 177 "Net-(C240-Pad1)")
  (net 178 "Net-(C40-Pad2)")
  (net 179 "Net-(C40-Pad1)")
  (net 180 "Net-(C60-Pad1)")
  (net 181 "Net-(C60-Pad2)")
  (net 182 "Net-(C61-Pad1)")
  (net 183 "Net-(C61-Pad2)")
  (net 184 "Net-(C80-Pad1)")
  (net 185 "Net-(C80-Pad2)")
  (net 186 "Net-(C81-Pad1)")
  (net 187 "Net-(C81-Pad2)")
  (net 188 "Net-(C59-Pad2)")
  (net 189 "Net-(C59-Pad1)")
  (net 190 "Net-(C41-Pad2)")
  (net 191 "Net-(C41-Pad1)")
  (net 192 "Net-(C39-Pad2)")
  (net 193 "Net-(C39-Pad1)")
  (net 194 "Net-(C38-Pad2)")
  (net 195 "Net-(C38-Pad1)")
  (net 196 "Net-(C21-Pad2)")
  (net 197 "Net-(C21-Pad1)")
  (net 198 "Net-(C20-Pad2)")
  (net 199 "Net-(C20-Pad1)")
  (net 200 "Net-(C18-Pad2)")
  (net 201 "Net-(C18-Pad1)")
  (net 202 "Net-(C17-Pad2)")
  (net 203 "Net-(C17-Pad1)")
  (net 204 "/nvm_amp_main/OUT")
  (net 205 "unconnected-(U123-Pad1)")
  (net 206 "unconnected-(U123-Pad5)")
  (net 207 "unconnected-(U123-Pad8)")
  (net 208 "Net-(C243-Pad1)")
  (net 209 "Net-(J2-Pad1)")
  (net 210 "Net-(C239-Pad1)")
  (net 211 "Net-(C239-Pad2)")
  (net 212 "Net-(C242-Pad1)")
  (net 213 "Net-(J2-Pad2)")
  (net 214 "Net-(J2-Pad3)")
  (net 215 "Net-(J2-Pad4)")
  (net 216 "Net-(J2-Pad5)")
  (net 217 "Net-(C7-Pad1)")
  (net 218 "Net-(C22-Pad2)")
  (net 219 "Net-(C22-Pad1)")
  (net 220 "Net-(C23-Pad2)")
  (net 221 "Net-(C23-Pad1)")
  (net 222 "Net-(C24-Pad2)")
  (net 223 "Net-(C24-Pad1)")
  (net 224 "Net-(C25-Pad2)")
  (net 225 "Net-(C25-Pad1)")
  (net 226 "Net-(C26-Pad2)")
  (net 227 "Net-(C26-Pad1)")
  (net 228 "Net-(C42-Pad2)")
  (net 229 "Net-(C42-Pad1)")
  (net 230 "Net-(C43-Pad2)")
  (net 231 "Net-(C43-Pad1)")
  (net 232 "Net-(C44-Pad2)")
  (net 233 "Net-(C44-Pad1)")
  (net 234 "Net-(C45-Pad2)")
  (net 235 "Net-(C45-Pad1)")
  (net 236 "Net-(C46-Pad2)")
  (net 237 "Net-(C46-Pad1)")
  (net 238 "Net-(C62-Pad2)")
  (net 239 "Net-(C62-Pad1)")
  (net 240 "Net-(C63-Pad2)")
  (net 241 "Net-(C63-Pad1)")
  (net 242 "Net-(C64-Pad2)")
  (net 243 "Net-(C64-Pad1)")
  (net 244 "Net-(C65-Pad2)")
  (net 245 "Net-(C65-Pad1)")
  (net 246 "Net-(C66-Pad2)")
  (net 247 "Net-(C66-Pad1)")
  (net 248 "Net-(C82-Pad2)")
  (net 249 "Net-(C82-Pad1)")
  (net 250 "Net-(C83-Pad2)")
  (net 251 "Net-(C83-Pad1)")
  (net 252 "Net-(C84-Pad2)")
  (net 253 "Net-(C84-Pad1)")
  (net 254 "Net-(C85-Pad2)")
  (net 255 "Net-(C85-Pad1)")
  (net 256 "Net-(C86-Pad2)")
  (net 257 "Net-(C86-Pad1)")
  (net 258 "Net-(C112-Pad2)")
  (net 259 "Net-(C112-Pad1)")
  (net 260 "Net-(C113-Pad2)")
  (net 261 "Net-(C113-Pad1)")
  (net 262 "Net-(C114-Pad2)")
  (net 263 "Net-(C114-Pad1)")
  (net 264 "Net-(C115-Pad2)")
  (net 265 "Net-(C115-Pad1)")
  (net 266 "Net-(C116-Pad2)")
  (net 267 "Net-(C116-Pad1)")
  (net 268 "Net-(C133-Pad2)")
  (net 269 "Net-(C133-Pad1)")
  (net 270 "Net-(C134-Pad2)")
  (net 271 "Net-(C134-Pad1)")
  (net 272 "Net-(C135-Pad2)")
  (net 273 "Net-(C135-Pad1)")
  (net 274 "Net-(C136-Pad2)")
  (net 275 "Net-(C136-Pad1)")
  (net 276 "Net-(C154-Pad2)")
  (net 277 "Net-(C154-Pad1)")
  (net 278 "Net-(C155-Pad2)")
  (net 279 "Net-(C155-Pad1)")
  (net 280 "Net-(C156-Pad2)")
  (net 281 "Net-(C156-Pad1)")
  (net 282 "Net-(C175-Pad2)")
  (net 283 "Net-(C175-Pad1)")
  (net 284 "Net-(C176-Pad2)")
  (net 285 "Net-(C176-Pad1)")
  (net 286 "Net-(C196-Pad2)")
  (net 287 "Net-(C196-Pad1)")
  (net 288 "unconnected-(U2-Pad1)")
  (net 289 "unconnected-(U2-Pad5)")
  (net 290 "unconnected-(U2-Pad8)")
  (net 291 "Net-(K1-Pad3)")
  (net 292 "Net-(J2-Pad6)")
  (net 293 "Net-(K4-Pad1)")
  (net 294 "Net-(C222-Pad1)")
  (net 295 "Net-(C225-Pad1)")
  (net 296 "Net-(C226-Pad1)")
  (net 297 "Net-(R1-Pad1)")
  (net 298 "Net-(R2-Pad1)")
  (net 299 "Net-(R7-Pad1)")
  (net 300 "Net-(R7-Pad2)")
  (net 301 "Net-(R8-Pad2)")
  (net 302 "Net-(R11-Pad1)")
  (net 303 "Net-(R17-Pad2)")
  (net 304 "Net-(Q3-Pad1)")
  (net 305 "Net-(Q4-Pad1)")
  (net 306 "/LNAMP/IN")
  (net 307 "Net-(R58-Pad2)")
  (net 308 "Net-(R90-Pad2)")
  (net 309 "Net-(R122-Pad2)")
  (net 310 "Net-(R154-Pad2)")
  (net 311 "Net-(R156-Pad2)")
  (net 312 "Net-(R21-Pad2)")
  (net 313 "Net-(R188-Pad2)")
  (net 314 "Net-(R220-Pad2)")
  (net 315 "Net-(R252-Pad2)")
  (net 316 "Net-(R284-Pad2)")
  (net 317 "Net-(R316-Pad2)")
  (net 318 "Net-(R348-Pad2)")
  (net 319 "Net-(R349-Pad2)")
  (net 320 "Net-(R351-Pad2)")
  (net 321 "Net-(R352-Pad2)")
  (net 322 "Net-(R353-Pad2)")
  (net 323 "Net-(R361-Pad1)")
  (net 324 "Net-(R362-Pad2)")
  (net 325 "Net-(R363-Pad1)")
  (net 326 "Net-(R364-Pad1)")
  (net 327 "Net-(R366-Pad2)")
  (net 328 "Net-(R368-Pad2)")
  (net 329 "Net-(R355-Pad2)")
  (net 330 "Net-(R370-Pad2)")
  (net 331 "Net-(R373-Pad1)")
  (net 332 "Net-(R376-Pad1)")
  (net 333 "Net-(R358-Pad2)")
  (net 334 "unconnected-(U5-Pad1)")
  (net 335 "unconnected-(U5-Pad5)")
  (net 336 "Net-(R369-Pad1)")
  (net 337 "unconnected-(U5-Pad8)")
  (net 338 "unconnected-(U7-Pad1)")
  (net 339 "unconnected-(U7-Pad5)")
  (net 340 "unconnected-(U7-Pad8)")
  (net 341 "Net-(C47-Pad1)")
  (net 342 "Net-(C47-Pad2)")
  (net 343 "Net-(C67-Pad1)")
  (net 344 "Net-(C67-Pad2)")
  (net 345 "Net-(C68-Pad1)")
  (net 346 "Net-(C68-Pad2)")
  (net 347 "Net-(C87-Pad1)")
  (net 348 "Net-(C87-Pad2)")
  (net 349 "Net-(C88-Pad1)")
  (net 350 "Net-(C88-Pad2)")
  (net 351 "Net-(C89-Pad1)")
  (net 352 "Net-(C89-Pad2)")
  (net 353 "Net-(C117-Pad1)")
  (net 354 "Net-(C117-Pad2)")
  (net 355 "Net-(C118-Pad1)")
  (net 356 "Net-(C118-Pad2)")
  (net 357 "Net-(C119-Pad1)")
  (net 358 "Net-(C119-Pad2)")
  (net 359 "Net-(C120-Pad1)")
  (net 360 "Net-(C120-Pad2)")
  (net 361 "Net-(C121-Pad1)")
  (net 362 "Net-(C121-Pad2)")
  (net 363 "Net-(C137-Pad1)")
  (net 364 "Net-(C137-Pad2)")
  (net 365 "Net-(C138-Pad1)")
  (net 366 "Net-(C138-Pad2)")
  (net 367 "Net-(C139-Pad1)")
  (net 368 "Net-(C139-Pad2)")
  (net 369 "Net-(C140-Pad1)")
  (net 370 "Net-(C140-Pad2)")
  (net 371 "Net-(C141-Pad1)")
  (net 372 "Net-(C141-Pad2)")
  (net 373 "Net-(C142-Pad1)")
  (net 374 "Net-(C142-Pad2)")
  (net 375 "Net-(C157-Pad1)")
  (net 376 "Net-(C157-Pad2)")
  (net 377 "Net-(C158-Pad1)")
  (net 378 "Net-(C158-Pad2)")
  (net 379 "Net-(C159-Pad1)")
  (net 380 "Net-(C159-Pad2)")
  (net 381 "Net-(C160-Pad1)")
  (net 382 "Net-(C160-Pad2)")
  (net 383 "Net-(C161-Pad1)")
  (net 384 "Net-(C161-Pad2)")
  (net 385 "Net-(C162-Pad1)")
  (net 386 "Net-(C162-Pad2)")
  (net 387 "Net-(C163-Pad1)")
  (net 388 "Net-(C163-Pad2)")
  (net 389 "Net-(C177-Pad1)")
  (net 390 "Net-(C177-Pad2)")
  (net 391 "Net-(C178-Pad1)")
  (net 392 "Net-(C178-Pad2)")
  (net 393 "Net-(C179-Pad1)")
  (net 394 "Net-(C179-Pad2)")
  (net 395 "Net-(C180-Pad1)")
  (net 396 "Net-(C180-Pad2)")
  (net 397 "Net-(C181-Pad1)")
  (net 398 "Net-(C181-Pad2)")
  (net 399 "Net-(C182-Pad1)")
  (net 400 "Net-(C182-Pad2)")
  (net 401 "Net-(C183-Pad1)")
  (net 402 "Net-(C183-Pad2)")
  (net 403 "Net-(C184-Pad1)")
  (net 404 "Net-(C184-Pad2)")
  (net 405 "Net-(C197-Pad1)")
  (net 406 "Net-(C197-Pad2)")
  (net 407 "Net-(C198-Pad1)")
  (net 408 "Net-(C198-Pad2)")
  (net 409 "Net-(C199-Pad1)")
  (net 410 "Net-(C199-Pad2)")
  (net 411 "Net-(C200-Pad1)")
  (net 412 "Net-(C200-Pad2)")
  (net 413 "Net-(C201-Pad1)")
  (net 414 "Net-(C201-Pad2)")
  (net 415 "Net-(C202-Pad1)")
  (net 416 "Net-(C202-Pad2)")
  (net 417 "Net-(C203-Pad1)")
  (net 418 "Net-(C203-Pad2)")
  (net 419 "Net-(C204-Pad1)")
  (net 420 "Net-(C204-Pad2)")
  (net 421 "Net-(C205-Pad1)")
  (net 422 "Net-(C205-Pad2)")
  (net 423 "Net-(C217-Pad1)")
  (net 424 "Net-(C217-Pad2)")
  (net 425 "Net-(C218-Pad1)")
  (net 426 "Net-(C218-Pad2)")
  (net 427 "Net-(C219-Pad1)")
  (net 428 "Net-(C219-Pad2)")
  (net 429 "Net-(C220-Pad1)")
  (net 430 "Net-(C220-Pad2)")
  (net 431 "Net-(C221-Pad1)")
  (net 432 "Net-(C221-Pad2)")
  (net 433 "Net-(C222-Pad2)")
  (net 434 "Net-(C223-Pad1)")
  (net 435 "Net-(C223-Pad2)")
  (net 436 "Net-(C224-Pad1)")
  (net 437 "Net-(C224-Pad2)")
  (net 438 "Net-(C225-Pad2)")
  (net 439 "Net-(C226-Pad2)")
  (net 440 "unconnected-(U120-Pad12)")
  (net 441 "unconnected-(U120-Pad13)")
  (net 442 "unconnected-(U120-Pad14)")
  (net 443 "unconnected-(U120-Pad15)")
  (net 444 "unconnected-(U122-Pad1)")
  (net 445 "unconnected-(U122-Pad5)")
  (net 446 "unconnected-(U122-Pad8)")
  (net 447 "unconnected-(U124-Pad1)")
  (net 448 "unconnected-(U124-Pad5)")
  (net 449 "unconnected-(U124-Pad8)")
  (net 450 "unconnected-(U125-Pad9)")
  (net 451 "unconnected-(U125-Pad10)")
  (net 452 "unconnected-(U125-Pad11)")
  (net 453 "unconnected-(U127-Pad1)")
  (net 454 "unconnected-(U127-Pad5)")
  (net 455 "unconnected-(U127-Pad8)")
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 28.3075 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R168" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 265 "Net-(C115-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 25.65 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB8" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(FB8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 118.825 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB39" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "Net-(FB39-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.7275 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R185" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 362 "Net-(C121-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.5375 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C180" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 395 "Net-(C180-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 396 "Net-(C180-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.875 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R63" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 192 "Net-(C39-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.25 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C26" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 227 "Net-(C26-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 226 "Net-(C26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.5375 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R108" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 243 "Net-(C64-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.425 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C84" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 253 "Net-(C84-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 252 "Net-(C84-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 63.125 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U72" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 370 "Net-(C140-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(FB59-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 369 "Net-(C140-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.575 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R148" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 350 "Net-(C88-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 97.5 19.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C8" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "-15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 38.925 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB48" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(FB48-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.775 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R150" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 350 "Net-(C88-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 349 "Net-(C88-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.505 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R166" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 262 "Net-(C114-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 263 "Net-(C114-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.9275 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R160" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 258 "Net-(C112-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 259 "Net-(C112-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 84.3275 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U31" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 188 "Net-(C59-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(FB22-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 189 "Net-(C59-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.925 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C63" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 241 "Net-(C63-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 240 "Net-(C63-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.225 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C223" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 434 "Net-(C223-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 435 "Net-(C223-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.925 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R309" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 418 "Net-(C203-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 417 "Net-(C203-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.2375 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R335" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 433 "Net-(C222-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 294 "Net-(C222-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 46.2 11.4)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C237" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "-15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 70.875 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U95" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 402 "Net-(C183-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 146 "Net-(FB80-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 401 "Net-(C183-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.175 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C162" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 385 "Net-(C162-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 386 "Net-(C162-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 81.5 3)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "optional")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP2" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 60 "/VR28P") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 29.5 7 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC857.215")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q4" (at -2 -2.1) (layer "F.SilkS"))
    (fp_text value "BC857" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 305 "Net-(Q4-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "Net-(C239-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 129.725 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U27" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 234 "Net-(C45-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(FB19-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 235 "Net-(C45-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 79.1375 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R270" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 395 "Net-(C180-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.4325 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R34" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 9 "Net-(C19-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.25 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R39" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 198 "Net-(C20-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 199 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.725 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C42" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 229 "Net-(C42-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 228 "Net-(C42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.6275 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R124" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 185 "Net-(C80-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 23.25 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U12" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 198 "Net-(C20-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(FB5-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 199 "Net-(C20-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.875 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C113" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 261 "Net-(C113-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 260 "Net-(C113-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.775 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C81" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 186 "Net-(C81-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 187 "Net-(C81-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 47.025 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R243" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 384 "Net-(C161-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.125 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C139" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 367 "Net-(C139-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 368 "Net-(C139-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 39.105 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R165" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 263 "Net-(C114-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.925 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R106" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 240 "Net-(C63-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 241 "Net-(C63-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 26.73 89.6375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C37" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 29.675 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U52" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 310 "Net-(R154-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113 35.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08056M20")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R353" (at -1.9 0.3 180) (layer "F.SilkS"))
    (fp_text value "6M2" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 319 "Net-(R349-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 322 "Net-(R353-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.105 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R98" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 183 "Net-(C61-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 78.925 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB79" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "Net-(FB79-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.9075 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R265" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 392 "Net-(C178-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 391 "Net-(C178-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 25.65 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB11" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(FB11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 142.925 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U105" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 418 "Net-(C203-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "Net-(FB89-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 417 "Net-(C203-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 118.8375 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB37" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "Net-(FB37-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.405 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R229" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 281 "Net-(C156-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.4 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R49" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 222 "Net-(C24-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.025 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R146" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 347 "Net-(C87-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (tedit 5E476F32)
    (at 111.5 30.5 180)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "PN" "LTC1664IGN")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U120" (at -4.9 -1) (layer "F.SilkS"))
    (fp_text value "LTC1664IGN" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 -1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 320 "Net-(R351-Pad2)") (pinfunction "OUTA") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 321 "Net-(R352-Pad2)") (pinfunction "OUTB") (pintype "output"))
    (pad "4" smd roundrect (at -2.8625 -0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 322 "Net-(R353-Pad2)") (pinfunction "OUTC") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 329 "Net-(R355-Pad2)") (pinfunction "OUTD") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/VR28P") (pinfunction "REF") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/JA_CS") (pinfunction "~{CS}/LD") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/JA_SCK") (pinfunction "SCK") (pintype "input"))
    (pad "9" smd roundrect (at 2.8625 2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/JA_DIN") (pinfunction "DIN") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/JA_DOUT") (pinfunction "DOUT") (pintype "output"))
    (pad "11" smd roundrect (at 2.8625 0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "+3V3") (pinfunction "~{CLR}") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 440 "unconnected-(U120-Pad12)") (pinfunction "NC") (pintype "no_connect"))
    (pad "13" smd roundrect (at 2.8625 -0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 441 "unconnected-(U120-Pad13)") (pinfunction "NC") (pintype "no_connect"))
    (pad "14" smd roundrect (at 2.8625 -0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 442 "unconnected-(U120-Pad14)") (pinfunction "NC") (pintype "no_connect"))
    (pad "15" smd roundrect (at 2.8625 -1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 443 "unconnected-(U120-Pad15)") (pinfunction "NC") (pintype "no_connect"))
    (pad "16" smd roundrect (at 2.8625 -2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 47.0075 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R231" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 376 "Net-(C157-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 41.8275 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB71" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(FB71-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.4375 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C85" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 255 "Net-(C85-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 254 "Net-(C85-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.405 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R324" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 428 "Net-(C219-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 12.4 57.8 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C173" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.7375 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R173" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 354 "Net-(C117-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.775 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R129" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 187 "Net-(C81-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 186 "Net-(C81-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.275 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R214" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 372 "Net-(C141-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.9075 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C178" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 391 "Net-(C178-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 392 "Net-(C178-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 28.3275 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R186" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 361 "Net-(C121-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 89.925 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U37" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 244 "Net-(C65-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(FB28-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 245 "Net-(C65-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.3275 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R190" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 268 "Net-(C133-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.405 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C82" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 249 "Net-(C82-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 248 "Net-(C82-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.725 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R275" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 400 "Net-(C182-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 124.075 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U21" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 192 "Net-(C39-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(FB13-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 193 "Net-(C39-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 39.1375 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R174" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 353 "Net-(C117-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.8075 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R135" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 250 "Net-(C83-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 251 "Net-(C83-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 97.6275 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U118" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 439 "Net-(C226-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 167 "Net-(FB101-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 296 "Net-(C226-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 80.13 89.6375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C57" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.525 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C118" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 355 "Net-(C118-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 356 "Net-(C118-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 79.53 47.2375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C111" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 28.5075 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB45" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "Net-(FB45-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142 89.9 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C79" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 108.4275 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB32" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(FB32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 41 17 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "TL061ID")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U124" (at 1 -3.1 90) (layer "F.SilkS"))
    (fp_text value "TL061" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 447 "unconnected-(U124-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(C235-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(C235-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 448 "unconnected-(U124-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 204 "/nvm_amp_main/OUT") (pintype "output"))
    (pad "7" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 449 "unconnected-(U124-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 36.525 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U61" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 358 "Net-(C119-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(FB49-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 357 "Net-(C119-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124 26.5875 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080512K0")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R349" (at -2.1125 -1.4 180) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 58 "/VR28N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 319 "Net-(R349-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.1275 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R92" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 188 "Net-(C59-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 16.4 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U53" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 311 "Net-(R156-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 30.875 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U55" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 260 "Net-(C113-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "Net-(FB43-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 261 "Net-(C113-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 52.225 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB69" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 135 "Net-(FB69-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 118.825 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB36" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(FB36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.4525 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 202 "Net-(C17-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 15.2525 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB7" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(FB7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.53 89.6375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C78" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.025 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R137" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 253 "Net-(C84-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.6275 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C217" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 423 "Net-(C217-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 424 "Net-(C217-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 78.925 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB76" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "Net-(FB76-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.175 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R128" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 186 "Net-(C81-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.6075 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C220" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 429 "Net-(C220-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 430 "Net-(C220-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.7075 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R167" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 264 "Net-(C115-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.525 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R172" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 266 "Net-(C116-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 267 "Net-(C116-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 58.5875 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R188" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 313 "Net-(R188-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 54.9275 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R191" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 269 "Net-(C133-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 79.105 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R261" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 389 "Net-(C177-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.305 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R196" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 272 "Net-(C135-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.525 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C181" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 397 "Net-(C181-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 398 "Net-(C181-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 92.305 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB24" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(FB24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 65.725 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R203" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 363 "Net-(C137-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.7275 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R314" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 421 "Net-(C205-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.45 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R46" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 220 "Net-(C23-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.325 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R79" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 233 "Net-(C44-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 39 27 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080524K0")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R375" (at -2.8 0) (layer "F.SilkS"))
    (fp_text value "24k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 72 "/MAMP_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 212 "Net-(C242-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 142.925 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U104" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 416 "Net-(C202-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 154 "Net-(FB88-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 415 "Net-(C202-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.425 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R339" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 437 "Net-(C224-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.405 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R132" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 248 "Net-(C82-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 249 "Net-(C82-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.5275 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R219" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 374 "Net-(C142-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 373 "Net-(C142-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.7275 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R120" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 345 "Net-(C68-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 121.7275 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB21" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(FB21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 132.1375 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB17" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(FB17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.5375 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R302" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 413 "Net-(C201-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tedit 5905D8F5)
    (at 12 7 90)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "PN" "LL43-GS08")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D1" (at 0 -2 90) (layer "F.SilkS"))
    (fp_text value "LL43" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/RE_P") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.75 0 90) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.6275 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C226" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 296 "Net-(C226-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 439 "Net-(C226-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.925 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R81" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 234 "Net-(C45-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 137.3275 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U98" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 286 "Net-(C196-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 148 "Net-(FB82-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 287 "Net-(C196-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 59.475 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R189" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 313 "Net-(R188-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 39.93 89.6375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C36" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 81.875 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB23" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(FB23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.8275 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R153" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 352 "Net-(C89-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 351 "Net-(C89-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.425 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C87" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 347 "Net-(C87-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 348 "Net-(C87-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 23.2625 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U17" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 224 "Net-(C25-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(FB10-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 225 "Net-(C25-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.125 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C140" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 369 "Net-(C140-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 370 "Net-(C140-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 2.5 97.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 65.725 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R209" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 367 "Net-(C139-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 23.25 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U18" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 226 "Net-(C26-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(FB11-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 227 "Net-(C26-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.4375 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R333" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 433 "Net-(C222-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.725 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R272" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 398 "Net-(C181-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.475 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C134" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 271 "Net-(C134-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 270 "Net-(C134-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.5275 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R88" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 341 "Net-(C47-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 102.5 34.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "TLV333IDR")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U7" (at -4.4 2.4) (layer "F.SilkS"))
    (fp_text value "TLV333" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 338 "unconnected-(U7-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/VR28P") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 303 "Net-(R17-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 339 "unconnected-(U7-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/VR28P") (pintype "output"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 340 "unconnected-(U7-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.505 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C177" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 389 "Net-(C177-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 390 "Net-(C177-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.925 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C200" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 411 "Net-(C200-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 412 "Net-(C200-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 39.125 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R171" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 267 "Net-(C116-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.2625 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R54" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 224 "Net-(C25-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 225 "Net-(C25-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.725 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R179" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 358 "Net-(C119-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.9275 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R187" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 362 "Net-(C121-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 361 "Net-(C121-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.875 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R163" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 260 "Net-(C113-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 261 "Net-(C113-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 79.125 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R267" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 393 "Net-(C179-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.275 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R118" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 344 "Net-(C67-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 343 "Net-(C67-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 17.6525 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U9" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 202 "Net-(C17-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(FB2-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 203 "Net-(C17-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.575 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R127" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 187 "Net-(C81-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.7275 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R281" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 404 "Net-(C184-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 25.65 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB5" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(FB5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.925 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C65" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 245 "Net-(C65-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 244 "Net-(C65-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.1075 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R295" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 410 "Net-(C199-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 15.2525 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB2" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(FB2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 129.7375 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U25" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 230 "Net-(C43-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(FB17-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 231 "Net-(C43-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 5 12 180)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "293D106X9025C2TE3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C12" (at -4.9 -0.1) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 180) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 6 "/RE_P") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 180) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 40 "Net-(C12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 83.075 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U30" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 308 "Net-(R90-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.1375 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R301" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 414 "Net-(C201-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 31.5 4 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C240" (at 3.3 -0.6) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 177 "Net-(C240-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.7275 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R158" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 258 "Net-(C112-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 129.725 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U24" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 228 "Net-(C42-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(FB16-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 229 "Net-(C42-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.575 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C225" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 295 "Net-(C225-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 438 "Net-(C225-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.875 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R184" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 360 "Net-(C120-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 359 "Net-(C120-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 63.125 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U69" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 364 "Net-(C137-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "Net-(FB56-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 363 "Net-(C137-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 4.5 30.5)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "74LVC125AS14-13")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "Has to have 5V VDD limit!")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U4" (at 4.3 -4.1) (layer "F.SilkS"))
    (fp_text value "74LVC125" (at 0 5.28) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C12-Pad2)") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 214 "Net-(J2-Pad3)") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/R1A") (pintype "tri_state"))
    (pad "4" smd roundrect (at -2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C12-Pad2)") (pintype "input"))
    (pad "5" smd roundrect (at -2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 215 "Net-(J2-Pad4)") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/R1B") (pintype "tri_state"))
    (pad "7" smd roundrect (at -2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C12-Pad2)") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/R2A") (pintype "tri_state"))
    (pad "9" smd roundrect (at 2.475 2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 216 "Net-(J2-Pad5)") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C12-Pad2)") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/R2B") (pintype "tri_state"))
    (pad "12" smd roundrect (at 2.475 -1.27) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 292 "Net-(J2-Pad6)") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 -2.54) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C12-Pad2)") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -3.81) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/RE_P") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3275 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R288" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 286 "Net-(C196-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 287 "Net-(C196-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 137.275 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U106" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 420 "Net-(C204-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 156 "Net-(FB90-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 419 "Net-(C204-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.9075 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R69" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 190 "Net-(C41-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 30.9075 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U57" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 264 "Net-(C115-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 111 "Net-(FB45-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 265 "Net-(C115-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.105 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R292" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 408 "Net-(C198-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.3275 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R121" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 346 "Net-(C68-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 345 "Net-(C68-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.1275 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C38" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 195 "Net-(C38-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 194 "Net-(C38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.8375 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R334" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 294 "Net-(C222-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 39.125 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R177" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 355 "Net-(C118-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.075 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R289" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 406 "Net-(C197-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 121.7075 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB15" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(FB15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 39.2 3 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080524K0")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R371" (at -2 1.4 180) (layer "F.SilkS"))
    (fp_text value "24k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 210 "Net-(C239-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 211 "Net-(C239-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.525 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R181" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 358 "Net-(C119-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 357 "Net-(C119-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 38.905 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB44" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "Net-(FB44-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.575 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C218" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 425 "Net-(C218-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 426 "Net-(C218-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.375 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R321" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 426 "Net-(C218-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.225 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R341" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 437 "Net-(C224-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 436 "Net-(C224-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 3 56)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 65.725 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R212" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 369 "Net-(C140-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85 31.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08058M20")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R359" (at -0.5 -1.4) (layer "F.SilkS"))
    (fp_text value "8M2" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 68 "/LNAMP/VTRIM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 25.85 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R38" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 199 "Net-(C20-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3075 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C199" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 409 "Net-(C199-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 410 "Net-(C199-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 76 3)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "optional")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP1" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 62 "/VREF7") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 23.25 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U15" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 220 "Net-(C23-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "Net-(FB8-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 221 "Net-(C23-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 134.9075 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB85" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 151 "Net-(FB85-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.4375 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R238" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 379 "Net-(C159-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.5375 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C117" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 353 "Net-(C117-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 354 "Net-(C117-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3275 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C196" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 287 "Net-(C196-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 286 "Net-(C196-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 124.1275 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U20" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 194 "Net-(C38-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(FB12-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 195 "Net-(C38-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 18.4125 34)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080524K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R5" (at 0 1.4) (layer "F.SilkS"))
    (fp_text value "24k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 21 "Net-(FB1-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 35 "Net-(C2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.175 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C155" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 279 "Net-(C155-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 278 "Net-(C155-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 57.5275 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U74" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 374 "Net-(C142-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(FB61-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 373 "Net-(C142-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 132.125 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB19" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(FB19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.475 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R85" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 237 "Net-(C46-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 54.9275 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R218" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 373 "Net-(C142-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.175 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R248" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 386 "Net-(C162-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 385 "Net-(C162-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 36.525 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U58" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 266 "Net-(C116-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(FB46-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 267 "Net-(C116-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 97.575 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U117" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 438 "Net-(C225-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 166 "Net-(FB100-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 295 "Net-(C225-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.625 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R136" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 252 "Net-(C84-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.8375 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R239" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 380 "Net-(C159-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 379 "Net-(C159-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 31.9875 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R154" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 310 "Net-(R154-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.25 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R48" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 220 "Net-(C23-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 221 "Net-(C23-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 55.1275 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB61" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(FB61-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.525 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C179" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 393 "Net-(C179-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 394 "Net-(C179-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.9275 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R87" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 342 "Net-(C47-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 110.8275 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U42" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 185 "Net-(C80-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "Net-(FB32-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 184 "Net-(C80-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.225 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R338" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 435 "Net-(C223-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 434 "Net-(C223-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111.8875 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R122" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 309 "Net-(R122-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.3375 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R205" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 366 "Net-(C138-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 145.325 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB86" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 152 "Net-(FB86-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.1375 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R107" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 242 "Net-(C64-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 75.4 35.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C233" (at -1.3 -2.1 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "-15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.8275 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R126" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 185 "Net-(C80-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 184 "Net-(C80-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.8275 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C80" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 184 "Net-(C80-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 185 "Net-(C80-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.505 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R293" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 407 "Net-(C198-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.505 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R262" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 390 "Net-(C177-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 389 "Net-(C177-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 26.5 7 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08056K20")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R379" (at 0 1.5 90) (layer "F.SilkS"))
    (fp_text value "6k2" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 4 "-15V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 305 "Net-(Q4-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.425 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R147" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 348 "Net-(C87-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 347 "Net-(C87-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.505 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C114" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 263 "Net-(C114-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 262 "Net-(C114-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 76.525 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U91" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 394 "Net-(C179-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "Net-(FB76-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 393 "Net-(C179-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 46.8 25.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C1" (at 2.1 -1.3 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 136.075 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U97" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 316 "Net-(R284-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.8 21.4 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08053K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R11" (at 1.9 -0.05 180) (layer "F.SilkS"))
    (fp_text value "3k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 302 "Net-(R11-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 5 "+5V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 2.5 19.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08053K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R16" (at 0 1.4) (layer "F.SilkS"))
    (fp_text value "3k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 209 "Net-(J2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 55 "Net-(Q1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 35.5 7 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC847.215")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q3" (at 0.4 2.3 180) (layer "F.SilkS"))
    (fp_text value "BC847" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 304 "Net-(Q3-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 210 "Net-(C239-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 121.7275 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB12" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(FB12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.9075 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C115" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 265 "Net-(C115-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 264 "Net-(C115-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.2375 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C222" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 294 "Net-(C222-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 433 "Net-(C222-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 15 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R32" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 201 "Net-(C18-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.925 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R78" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 232 "Net-(C44-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 53.33 89.6375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C195" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.125 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R110" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 244 "Net-(C65-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 121.675 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB13" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "Net-(FB13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.105 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R198" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 272 "Net-(C135-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 273 "Net-(C135-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 52.2375 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB67" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(FB67-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 30 14.75 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "TL431ACDBZR")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U128" (at 0.9 2.2 -90) (layer "F.SilkS"))
    (fp_text value "TL431DBZ" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 331 "Net-(R373-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 332 "Net-(R376-Pad1)") (pinfunction "REF") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 305 "Net-(Q4-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 144.78 48.2375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C231" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 36.505 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U56" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 262 "Net-(C114-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "Net-(FB44-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 263 "Net-(C114-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.2275 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C163" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 387 "Net-(C163-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 388 "Net-(C163-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 103.225 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U116" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 437 "Net-(C224-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 165 "Net-(FB99-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 436 "Net-(C224-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.275 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R258" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 285 "Net-(C176-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.2275 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R224" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 276 "Net-(C154-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 277 "Net-(C154-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100 7.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08053K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R2" (at -2.6 0) (layer "F.SilkS"))
    (fp_text value "3k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 298 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 297 "Net-(R1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 38.925 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB49" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "Net-(FB49-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 111 35.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08056K20")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R352" (at -1.9 -0.4 180) (layer "F.SilkS"))
    (fp_text value "6k2" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 318 "Net-(R348-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 321 "Net-(R352-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.1275 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R286" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 286 "Net-(C196-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 49.825 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U80" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 378 "Net-(C158-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "Net-(FB66-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 377 "Net-(C158-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.0375 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R140" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 255 "Net-(C85-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 91.5 36.0875)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08050000")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R360" (at 0 -1.2875) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 3 "GNDS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.33 47.0375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C99" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.1275 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R313" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 422 "Net-(C205-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 78.905 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB74" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 140 "Net-(FB74-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 84.275 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U32" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 181 "Net-(C60-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "Net-(FB23-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 180 "Net-(C60-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.5075 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C136" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 275 "Net-(C136-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 274 "Net-(C136-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 47.0275 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R249" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 388 "Net-(C163-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6525 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C22" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 219 "Net-(C22-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 218 "Net-(C22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 92.3375 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB27" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(FB27-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.825 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R242" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 382 "Net-(C160-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 381 "Net-(C160-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.7075 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R102" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 239 "Net-(C62-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.475 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R216" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 372 "Net-(C141-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 371 "Net-(C141-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 15 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R50" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 223 "Net-(C24-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 112.775 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R123" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 309 "Net-(R122-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3075 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R297" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 410 "Net-(C199-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 409 "Net-(C199-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 134.875 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB83" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "Net-(FB83-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.6275 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R347" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 439 "Net-(C226-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 296 "Net-(C226-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 115 35.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08056K20")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R355" (at -1.9 1.6 180) (layer "F.SilkS"))
    (fp_text value "6k2" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 319 "Net-(R349-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 329 "Net-(R355-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 49.8375 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U81" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 380 "Net-(C159-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(FB67-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 379 "Net-(C159-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_SMD:Relay_DPDT_Omron_G6K-2F-Y" (layer "F.Cu")
    (tedit 5A565DE2)
    (at 8.5 45.5)
    (descr "Omron G6K-2F-Y relay package http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf")
    (tags "Omron G6K-2F-Y relay")
    (property "PN" "G6KU-2P-Y DC5 ")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "K2" (at -2.9 5.9) (layer "F.SilkS"))
    (fp_text value "G6KU-2" (at -0.04 6.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.01 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.5 -3.8) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/R2B") (pintype "passive"))
    (pad "2" smd rect (at -3.5 -0.6) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GNDS") (pintype "passive"))
    (pad "3" smd rect (at -3.5 1.6) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GNDS") (pintype "passive"))
    (pad "4" smd rect (at -3.5 3.8) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "Net-(K1-Pad3)") (pintype "passive"))
    (pad "5" smd rect (at 3.5 3.8) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(FB1-Pad1)") (pintype "passive"))
    (pad "6" smd rect (at 3.5 1.6) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "/LNAMP/IN") (pintype "passive"))
    (pad "7" smd rect (at 3.5 -0.6) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/CP_9M") (pintype "passive"))
    (pad "8" smd rect (at 3.5 -3.8) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/R2A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_SMD.3dshapes/Relay_DPDT_Omron_G6K-2F-Y.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.4625 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R52" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 224 "Net-(C25-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.525 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R178" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 356 "Net-(C118-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 355 "Net-(C118-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.6075 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R329" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 430 "Net-(C220-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 429 "Net-(C220-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.9275 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C175" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 283 "Net-(C175-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 282 "Net-(C175-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 7 19.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08053K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R25" (at 0.8 1.4 180) (layer "F.SilkS"))
    (fp_text value "3k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 213 "Net-(J2-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 56 "Net-(Q2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.825 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C158" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 377 "Net-(C158-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 378 "Net-(C158-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 81.9275 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB31" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(FB31-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.275 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R97" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 181 "Net-(C60-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 180 "Net-(C60-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 108.375 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB33" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(FB33-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.3275 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R217" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 374 "Net-(C142-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 68.475 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB80" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 146 "Net-(FB80-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124 23.0875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R357" (at -2.1875 0.1 180) (layer "F.SilkS"))
    (fp_text value "40k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 69 "/LNAMP/ITRIM") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 319 "Net-(R349-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.2075 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C157" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 375 "Net-(C157-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 376 "Net-(C157-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 41.8075 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB65" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "Net-(FB65-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 132.125 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB16" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(FB16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.705 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C40" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 179 "Net-(C40-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 178 "Net-(C40-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 65.525 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB56" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "Net-(FB56-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.9375 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C201" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 413 "Net-(C201-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 414 "Net-(C201-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.275 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R312" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 420 "Net-(C204-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 419 "Net-(C204-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.875 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R259" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 284 "Net-(C176-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 285 "Net-(C176-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.7075 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R263" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 392 "Net-(C178-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 34.6 11 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080512K0")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R369" (at 0 -1.2 90) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 336 "Net-(R369-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 304 "Net-(Q3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.5 22.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R361" (at 0.1 1.5) (layer "F.SilkS"))
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 323 "Net-(R361-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 70 "/JAMP_OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6325 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C19" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C19-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C19-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 47.025 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R234" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 378 "Net-(C158-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.825 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R340" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 436 "Net-(C224-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.705 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R164" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 262 "Net-(C114-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 142.925 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U102" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 412 "Net-(C200-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 152 "Net-(FB86-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 411 "Net-(C200-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.825 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R245" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 384 "Net-(C161-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 383 "Net-(C161-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 70.875 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U88" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 284 "Net-(C176-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "Net-(FB73-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 285 "Net-(C176-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.525 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R111" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 245 "Net-(C65-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 125.1875 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R58" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 307 "Net-(R58-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 41.575 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R247" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 385 "Net-(C162-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 97.6275 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U109" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 424 "Net-(C217-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 158 "Net-(FB92-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 423 "Net-(C217-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 25.6625 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB10" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(FB10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.525 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R305" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 415 "Net-(C202-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 94.975 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R343" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 295 "Net-(C225-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.7275 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R93" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 189 "Net-(C59-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 22.2 12 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C246" (at 0.5 2.2 -180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "-15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 35 2 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW0805240R")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R378" (at -2.9 0.6) (layer "F.SilkS"))
    (fp_text value "240R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 211 "Net-(C239-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 208 "Net-(C243-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 118.805 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB34" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(FB34-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.3275 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C68" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 345 "Net-(C68-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 346 "Net-(C68-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.675 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R161" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 260 "Net-(C113-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.73 47.2375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C230" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 63.105 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U67" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 272 "Net-(C135-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "Net-(FB54-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 273 "Net-(C135-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.6275 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R151" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 352 "Net-(C89-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.125 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R213" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 370 "Net-(C140-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 369 "Net-(C140-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 25.63 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB6" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(FB6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 17.6525 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U14" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 218 "Net-(C22-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "Net-(FB7-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 219 "Net-(C22-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 44.175 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U84" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 386 "Net-(C162-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(FB70-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 385 "Net-(C162-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 105.625 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB98" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "Net-(FB98-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 41.6075 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R232" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 375 "Net-(C157-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.2275 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C154" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 277 "Net-(C154-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 276 "Net-(C154-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.7375 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R269" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 396 "Net-(C180-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 57.5075 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U68" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 274 "Net-(C136-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(FB55-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 275 "Net-(C136-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.125 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R307" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 418 "Net-(C203-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "j_lib:logo_rpg7x9" (layer "F.Cu")
    (tedit 61CE1C18)
    (at 72.721042 28.982469)
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr board_only exclude_from_pos_files)
    (fp_text reference "LOGO1" (at -0.4 5.6) (layer "F.SilkS") hide)
    (fp_text value "logo_generic" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.9375 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C64" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 243 "Net-(C64-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 242 "Net-(C64-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 94.975 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R322" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 425 "Net-(C218-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 93.33 89.6375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C58" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.7075 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R296" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 409 "Net-(C199-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.3075 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R199" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 274 "Net-(C136-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 95.2075 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB95" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 161 "Net-(FB95-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 71.9875 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R252" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 315 "Net-(R252-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 57.475 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U66" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 270 "Net-(C134-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(FB53-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 271 "Net-(C134-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.125 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R298" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 412 "Net-(C200-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.925 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R306" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 416 "Net-(C202-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 415 "Net-(C202-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.525 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C182" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 399 "Net-(C182-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 400 "Net-(C182-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 68.5275 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB72" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "Net-(FB72-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3275 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R315" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 422 "Net-(C205-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 421 "Net-(C205-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.43 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R40" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 196 "Net-(C21-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.8275 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C89" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 351 "Net-(C89-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 352 "Net-(C89-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 146.5 91.5)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 109 35.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08056M20")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R351" (at -2 -1.7 180) (layer "F.SilkS"))
    (fp_text value "6M2" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 318 "Net-(R348-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 320 "Net-(R351-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 32.5 11 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080530K0")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R373" (at 0 1.1 90) (layer "F.SilkS"))
    (fp_text value "30k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 331 "Net-(R373-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 336 "Net-(R369-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 41.575 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R226" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 279 "Net-(C155-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 134.9275 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB91" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 157 "Net-(FB91-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.875 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R280" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 402 "Net-(C183-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 401 "Net-(C183-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 41.8275 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB62" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(FB62-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 79.125 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R276" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 399 "Net-(C182-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87 8)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW0805620R")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R8" (at -0.7 -1.5) (layer "F.SilkS"))
    (fp_text value "620R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 299 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 301 "Net-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 142.2 23.5)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "optional")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP6" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 69 "/LNAMP/ITRIM") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.1275 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R89" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 342 "Net-(C47-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 341 "Net-(C47-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 30.875 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U62" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 360 "Net-(C120-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(FB50-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 359 "Net-(C120-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.5375 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R175" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 354 "Net-(C117-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 353 "Net-(C117-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 25.85 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R56" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 227 "Net-(C26-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.5 24.75)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R363" (at 2 -0.1 90) (layer "F.SilkS"))
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 325 "Net-(R363-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 323 "Net-(R361-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.925 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R112" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 244 "Net-(C65-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 245 "Net-(C65-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 116.425 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U49" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 348 "Net-(C87-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "Net-(FB39-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 347 "Net-(C87-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 110.8275 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U51" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 352 "Net-(C89-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "Net-(FB41-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 351 "Net-(C89-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 12.93 81.6375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C174" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 124.1275 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U29" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 342 "Net-(C47-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(FB21-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 341 "Net-(C47-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100 5.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080512K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R3" (at 2.7 -0.7) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 60 "/VR28P") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 298 "Net-(R2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.075 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R86" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 236 "Net-(C46-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 237 "Net-(C46-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.4075 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R327" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 430 "Net-(C220-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.725 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R170" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 266 "Net-(C116-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 76.5375 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U92" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 396 "Net-(C180-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "Net-(FB77-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 395 "Net-(C180-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 134.9275 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB82" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 148 "Net-(FB82-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 97 23.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA202IDR")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U5" (at 3.1 2.9) (layer "F.SilkS"))
    (fp_text value "OPA202" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 334 "unconnected-(U5-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/VREF7") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 217 "Net-(C7-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 335 "unconnected-(U5-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/VREF7") (pintype "output"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 337 "unconnected-(U5-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.2075 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R134" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 251 "Net-(C83-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 28.275 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R162" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 261 "Net-(C113-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.425 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R144" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 256 "Net-(C86-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 257 "Net-(C86-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 81 35)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA202IDR")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U122" (at -4 -3.2) (layer "F.SilkS"))
    (fp_text value "OPA202" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 444 "unconnected-(U122-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/LNAMP/L_OUT") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GNDS") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 445 "unconnected-(U122-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/JAMP_OUT") (pintype "output"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 446 "unconnected-(U122-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 16.5 30)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040E2001BB100")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R374" (at 1.75 -1.5) (layer "F.SilkS"))
    (fp_text value "2k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 330 "Net-(R370-Pad2)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.275 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C60" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 180 "Net-(C60-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 181 "Net-(C60-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 45.2875 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R220" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 314 "Net-(R220-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 116.4375 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U47" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 254 "Net-(C85-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "Net-(FB37-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 255 "Net-(C85-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 34 24.5 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "TL081HIDR")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U127" (at 0.4 -4.1 180) (layer "F.SilkS"))
    (fp_text value "TL081H" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 453 "unconnected-(U127-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 331 "Net-(R373-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 212 "Net-(C242-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 454 "unconnected-(U127-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 331 "Net-(R373-Pad1)") (pintype "output"))
    (pad "7" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 455 "unconnected-(U127-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.9075 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R169" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 264 "Net-(C115-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 265 "Net-(C115-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 89.925 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U35" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 240 "Net-(C63-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(FB26-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 241 "Net-(C63-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.9275 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R256" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 282 "Net-(C175-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 283 "Net-(C175-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.8 20.2 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080524R0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R23" (at 0.8 1.3) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 293 "Net-(K4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 51 "Net-(K3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 28.475 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB50" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(FB50-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 110.775 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U43" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 187 "Net-(C81-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "Net-(FB33-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 186 "Net-(C81-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.2275 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R125" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 184 "Net-(C80-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 47 31 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA145ID")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U2" (at 0 -3.4 90) (layer "F.SilkS"))
    (fp_text value "OPA145" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 288 "unconnected-(U2-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/BOOT") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(C3-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 289 "unconnected-(U2-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/BOOT") (pintype "output"))
    (pad "7" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 290 "unconnected-(U2-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 65.7375 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R206" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 365 "Net-(C138-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 15.2 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB9" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(FB9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.3275 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C205" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 421 "Net-(C205-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 422 "Net-(C205-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.125 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R104" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 240 "Net-(C63-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89 32.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08050000")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R12" (at 2.1 0.1 180) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 3 "GNDS") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 56 8.8 90)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "293D106X9025C2TE3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C16" (at -4.5 0 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.55 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 90) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 90) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 4 "-15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.8075 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C83" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 251 "Net-(C83-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 250 "Net-(C83-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.1275 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R62" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 194 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 195 "Net-(C38-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 68.5275 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB81" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 147 "Net-(FB81-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87 10.3 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080515K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "15k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 38 "/COMP") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 299 "Net-(R7-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 116.405 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U44" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 248 "Net-(C82-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(FB34-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 249 "Net-(C82-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.825 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R331" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 431 "Net-(C221-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 49.825 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U83" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 384 "Net-(C161-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 135 "Net-(FB69-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 383 "Net-(C161-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 33.75 14.75 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "TL431ACDBZR")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U126" (at 0.1 -2.25 90) (layer "F.SilkS"))
    (fp_text value "TL431DBZ" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 304 "Net-(Q3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 336 "Net-(R369-Pad1)") (pinfunction "REF") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 331 "Net-(R373-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 44.2275 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U76" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 276 "Net-(C154-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(FB62-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 277 "Net-(C154-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.375 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R342" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 438 "Net-(C225-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 95.175 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB93" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 159 "Net-(FB93-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 26.13 47.2375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C132" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.1075 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R101" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 238 "Net-(C62-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 30.9275 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U63" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 362 "Net-(C121-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(FB51-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 361 "Net-(C121-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 119 24.0875)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA2202IDR")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U119" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "OPA2202" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "/LNAMP/VTRIM") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 318 "Net-(R348-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GNDS") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GNDS") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 319 "Net-(R349-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "/LNAMP/ITRIM") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.525 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R308" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 417 "Net-(C203-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 81.9275 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB22" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "Net-(FB22-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 40.8 22.6 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805Y333KXACW1BC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C235" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "33n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 42 "Net-(C235-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 43 "Net-(C235-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.4275 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R345" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 439 "Net-(C226-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 56.5 31 -90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "DG408DY-E3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U3" (at -0.5 -5.9 180) (layer "F.SilkS"))
    (fp_text value "DG408" (at 0 5.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/MS_A0") (pinfunction "A0") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 302 "Net-(R11-Pad1)") (pinfunction "EN") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "4" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "GNDS") (pinfunction "S1") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/JAMP_OUT") (pinfunction "S2") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/VREF7") (pinfunction "S3") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -2.475 3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/CP_07V") (pinfunction "S4") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -2.475 4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/MAMP_IN") (pinfunction "D") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 2.475 4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(C3-Pad1)") (pinfunction "S8") (pintype "bidirectional"))
    (pad "10" smd roundrect (at 2.475 3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/BOOT") (pinfunction "S7") (pintype "bidirectional"))
    (pad "11" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/CP_9M") (pinfunction "S6") (pintype "bidirectional"))
    (pad "12" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/CP_70M") (pinfunction "S5") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "15" smd roundrect (at 2.475 -3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "/MS_A2") (pinfunction "A2") (pintype "input"))
    (pad "16" smd roundrect (at 2.475 -4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/MS_A1") (pinfunction "A1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6525 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C17" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 203 "Net-(C17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 202 "Net-(C17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 91.5 97.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 45.5 3.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 4.3 -0.1) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 17 16)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C236" (at 0.2 -1.5 180) (layer "F.SilkS"))
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 204 "/nvm_amp_main/OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 43 "Net-(C235-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 147.25 23.5)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "optional")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP5" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 68 "/LNAMP/VTRIM") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 31.5625 2 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C243" (at 3.3625 -1.8) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 208 "Net-(C243-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 71.4 8.8 -90)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "293D106X9025C2TE3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C11" (at 4.4 0 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.55 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 270) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 270) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 101 30.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C6" (at 2.4 1) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.4525 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R43" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 218 "Net-(C22-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 7.5 23.6)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC847.215")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q2" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "BC847" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(Q2-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C12-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/RE4") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 14 34)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (attr smd)
    (fp_text reference "FB1" (at 0 1.3) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead_Small" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "Net-(FB1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(FB1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 60 8.8 90)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "293D106X9025C2TE3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C15" (at -4.5 0.1 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.55 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 90) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 90) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.905 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R66" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 178 "Net-(C40-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 97.575 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U110" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 426 "Net-(C218-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 159 "Net-(FB93-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 425 "Net-(C218-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 28.5275 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB51" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(FB51-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.25 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C23" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 221 "Net-(C23-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 220 "Net-(C23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.175 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R149" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 349 "Net-(C88-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.525 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R268" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 394 "Net-(C179-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 393 "Net-(C179-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SMB" (layer "F.Cu")
    (tedit 58645DF3)
    (at 5.5 7 180)
    (descr "Diode SMB (DO-214AA)")
    (tags "Diode SMB (DO-214AA)")
    (property "PN" "SM6T6V8A")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D2" (at -2.5 2.9) (layer "F.SilkS"))
    (fp_text value "SM6T6V8A" (at 0 3.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3) (layer "F.Fab"))
    (pad "1" smd rect (at -2.15 0 180) (size 2.5 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "/RE_P") (pinfunction "A1") (pintype "passive"))
    (pad "2" smd rect (at 2.15 0 180) (size 2.5 2.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 40 "Net-(C12-Pad2)") (pinfunction "A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMB.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 76.525 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U93" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 398 "Net-(C181-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 144 "Net-(FB78-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 397 "Net-(C181-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.675 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R278" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 402 "Net-(C183-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.205 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C219" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 427 "Net-(C219-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 428 "Net-(C219-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 47.005 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R228" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 280 "Net-(C156-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.075 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C46" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 237 "Net-(C46-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 236 "Net-(C46-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 65.505 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB54" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "Net-(FB54-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 84.3075 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U34" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 238 "Net-(C62-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(FB25-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 239 "Net-(C62-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 56.275 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U64" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 313 "Net-(R188-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R51" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 222 "Net-(C24-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 223 "Net-(C24-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.125 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R113" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 246 "Net-(C66-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.325 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R211" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 370 "Net-(C140-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 44.2275 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U85" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 388 "Net-(C163-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(FB71-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 387 "Net-(C163-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 97.6075 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U112" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 430 "Net-(C220-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 161 "Net-(FB95-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 429 "Net-(C220-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 47.025 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R240" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 382 "Net-(C160-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_SMD:Relay_DPDT_Omron_G6K-2F-Y" (layer "F.Cu")
    (tedit 5A565DE2)
    (at 7.7 65.4)
    (descr "Omron G6K-2F-Y relay package http://omronfs.omron.com/en_US/ecb/products/pdf/en-g6k.pdf")
    (tags "Omron G6K-2F-Y relay")
    (property "PN" "G6KU-2P-Y DC5 ")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "K1" (at 3.1 6) (layer "F.SilkS"))
    (fp_text value "G6KU-2" (at -0.04 6.3) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.01 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.5 -3.8) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/R1B") (pintype "passive"))
    (pad "2" smd rect (at -3.5 -0.6) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(J1-Pad4)") (pintype "passive"))
    (pad "3" smd rect (at -3.5 1.6) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 291 "Net-(K1-Pad3)") (pintype "passive"))
    (pad "4" smd rect (at -3.5 3.8) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(J1-Pad2)") (pintype "passive"))
    (pad "5" smd rect (at 3.5 3.8) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(J1-Pad1)") (pintype "passive"))
    (pad "6" smd rect (at 3.5 1.6) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "Net-(FB1-Pad1)") (pintype "passive"))
    (pad "7" smd rect (at 3.5 -0.6) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "Net-(J1-Pad3)") (pintype "passive"))
    (pad "8" smd rect (at 3.5 -3.8) (size 1.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/R1A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_SMD.3dshapes/Relay_DPDT_Omron_G6K-2F-Y.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 108.4275 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB41" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "Net-(FB41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 39.125 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R180" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 357 "Net-(C119-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 55.1075 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB55" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(FB55-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.275 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C67" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 343 "Net-(C67-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 344 "Net-(C67-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.075 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R95" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 181 "Net-(C60-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.075 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R65" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 192 "Net-(C39-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 193 "Net-(C39-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 55.075 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB60" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(FB60-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 134.5 24.5 90)
    (descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "LM324AD")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U121" (at -2.7 5.5 180) (layer "F.SilkS"))
    (fp_text value "LM324A" (at 0 5.28 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 326 "Net-(R364-Pad1)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 323 "Net-(R361-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 326 "Net-(R364-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at -2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 333 "Net-(R358-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at -2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 333 "Net-(R358-Pad2)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 324 "Net-(R362-Pad2)") (pintype "output"))
    (pad "9" smd roundrect (at 2.475 2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 324 "Net-(R362-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 326 "Net-(R364-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 0 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "12" smd roundrect (at 2.475 -1.27 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 326 "Net-(R364-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 -2.54 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 327 "Net-(R366-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -3.81 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 327 "Net-(R366-Pad2)") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.475 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R64" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 193 "Net-(C39-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.505 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R99" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 182 "Net-(C61-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.9275 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R60" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 194 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.25 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C20" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 199 "Net-(C20-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 198 "Net-(C20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 15.0525 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R29" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 203 "Net-(C17-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 68.475 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB73" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "Net-(FB73-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.805 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R230" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 280 "Net-(C156-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 281 "Net-(C156-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.905 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R294" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 408 "Net-(C198-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 407 "Net-(C198-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 101.5 19.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C5" (at -1.1 1.5) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.1275 58.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R119" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 346 "Net-(C68-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100 9.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080512K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R1" (at 2.7 0.8) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 297 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 58 "/VR28N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.825 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C161" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 383 "Net-(C161-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 384 "Net-(C161-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 36.525 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U60" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 356 "Net-(C118-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(FB48-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 355 "Net-(C118-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87 5.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW0805620R")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R7" (at 0 1.5) (layer "F.SilkS"))
    (fp_text value "620R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 299 "Net-(R7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 300 "Net-(R7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.005 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R131" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 249 "Net-(C82-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 105 23.5 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA202IDR")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U6" (at -4.4 -0.7) (layer "F.SilkS"))
    (fp_text value "OPA202" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "unconnected-(U6-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 312 "Net-(R21-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "unconnected-(U6-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/VR28N") (pintype "output"))
    (pad "7" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "unconnected-(U6-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 116.425 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U46" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 252 "Net-(C84-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(FB36-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 253 "Net-(C84-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 93.5 7.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "LM393AD")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U1" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "LM393" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 300 "Net-(R7-Pad2)") (pintype "open_collector"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/BOOT") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 298 "Net-(R2-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/BOOT") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 297 "Net-(R1-Pad1)") (pinfunction "_") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 301 "Net-(R8-Pad2)") (pintype "open_collector"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 105.5 27.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C14" (at 2.6 0.8) (layer "F.SilkS"))
    (fp_text value "2u2" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 7 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 67.6 8.8 -90)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "293D106X9025C2TE3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C10" (at 4.4 0.1 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.55 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 270) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 270) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 76 8)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "optional")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP4" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 "GNDS") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.805 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C156" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 281 "Net-(C156-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 280 "Net-(C156-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.925 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R300" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 412 "Net-(C200-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 411 "Net-(C200-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.5 22.5 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R354" (at -1.5 2 180) (layer "F.SilkS"))
    (fp_text value "40k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 68 "/LNAMP/VTRIM") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 318 "Net-(R348-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.0075 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R328" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 429 "Net-(C220-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.6275 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R320" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 424 "Net-(C217-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 423 "Net-(C217-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 121.675 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB20" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(FB20-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 132.125 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB18" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(FB18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.725 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R80" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 232 "Net-(C44-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 233 "Net-(C44-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 87.075 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R116" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 344 "Net-(C67-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6325 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R36" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 9 "Net-(C19-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 8 "Net-(C19-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 32.875 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R155" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 310 "Net-(R154-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 63.1375 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U70" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 366 "Net-(C138-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "Net-(FB57-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 365 "Net-(C138-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.5075 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R70" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 191 "Net-(C41-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.525 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R299" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 411 "Net-(C200-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 65.525 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB58" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(FB58-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.7375 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C43" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 231 "Net-(C43-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 230 "Net-(C43-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 132.105 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB14" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(FB14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C24" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 223 "Net-(C24-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 222 "Net-(C24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.325 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R208" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 368 "Net-(C139-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 99.575 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R317" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 317 "Net-(R316-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 105.625 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB99" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 165 "Net-(FB99-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 85.3875 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R90" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 308 "Net-(R90-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 76.505 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U89" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 390 "Net-(C177-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 140 "Net-(FB74-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 389 "Net-(C177-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.705 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R68" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 178 "Net-(C40-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 179 "Net-(C40-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 33.5 18.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C238" (at -0.4 -1.4 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.905 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C198" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 407 "Net-(C198-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 408 "Net-(C198-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 91 20.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C7" (at -2.7 0.4) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 217 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.25 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R57" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 226 "Net-(C26-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 227 "Net-(C26-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 70.9075 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U90" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 392 "Net-(C178-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "Net-(FB75-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 391 "Net-(C178-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.0275 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R319" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 423 "Net-(C217-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.7275 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R254" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 282 "Net-(C175-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 89.9375 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U36" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 242 "Net-(C64-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(FB27-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 243 "Net-(C64-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81 31.5 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A15K4BTDF")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R365" (at 1.2 1.4) (layer "F.SilkS"))
    (fp_text value "15k53" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 70 "/JAMP_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.725 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R176" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 356 "Net-(C118-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 25.83 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R41" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 197 "Net-(C21-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 103.205 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U111" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 428 "Net-(C219-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 160 "Net-(FB94-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 427 "Net-(C219-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 81.875 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB30" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(FB30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 89.925 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U38" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 246 "Net-(C66-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(FB29-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 247 "Net-(C66-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.9275 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R283" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 404 "Net-(C184-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 403 "Net-(C184-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.5 11 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080512K0")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R376" (at 0 -1.1 90) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 332 "Net-(R376-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 331 "Net-(R373-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.23 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R42" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 196 "Net-(C21-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 197 "Net-(C21-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.675 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R96" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 180 "Net-(C60-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 145.325 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB89" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "Net-(FB89-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.625 78.8375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R145" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 348 "Net-(C87-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 91 23)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW0805620R")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R19" (at -1.2 1.6) (layer "F.SilkS"))
    (fp_text value "620R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 217 "Net-(C7-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 44 "/VREF_EXT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 49.805 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U78" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 280 "Net-(C156-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "Net-(FB64-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 281 "Net-(C156-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.805 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R325" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 427 "Net-(C219-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 41.775 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB63" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "Net-(FB63-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.925 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R115" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 246 "Net-(C66-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 247 "Net-(C66-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 110.8075 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U45" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 250 "Net-(C83-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "Net-(FB35-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 251 "Net-(C83-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.4375 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R141" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 254 "Net-(C85-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 255 "Net-(C85-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.125 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R210" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 368 "Net-(C139-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 367 "Net-(C139-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 129.705 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U22" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 178 "Net-(C40-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(FB14-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 179 "Net-(C40-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 95.0275 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R346" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 296 "Net-(C226-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C18" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 201 "Net-(C18-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 200 "Net-(C18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.225 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C221" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 431 "Net-(C221-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 432 "Net-(C221-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.73 47.0375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C216" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.105 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C135" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 273 "Net-(C135-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 272 "Net-(C135-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.575 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R323" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 426 "Net-(C218-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 425 "Net-(C218-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 86.275 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R91" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 308 "Net-(R90-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 169 "/LNAMP/LNAMP_2L2/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 81.5 8)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "optional")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP3" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 58 "/VR28N") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.905 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R100" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 183 "Net-(C61-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 182 "Net-(C61-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.6375 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R139" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 254 "Net-(C85-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.705 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R260" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 390 "Net-(C177-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.1275 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C47" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 341 "Net-(C47-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 342 "Net-(C47-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 122.875 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U19" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 307 "Net-(R58-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.3275 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R94" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 188 "Net-(C59-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 189 "Net-(C59-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 139.275 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R285" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 316 "Net-(R284-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 145.3375 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB87" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 153 "Net-(FB87-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 63.125 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U71" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 368 "Net-(C139-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(FB58-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 367 "Net-(C139-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.2075 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R233" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 376 "Net-(C157-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 375 "Net-(C157-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.5 18 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08053K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R4" (at 2.4 0.8) (layer "F.SilkS"))
    (fp_text value "3k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 7 "+3V3") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 38 "/COMP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.675 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R311" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 419 "Net-(C204-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.4275 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R318" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 424 "Net-(C217-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.9275 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C121" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 361 "Net-(C121-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 362 "Net-(C121-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.2275 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R251" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 388 "Net-(C163-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 387 "Net-(C163-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 28.5275 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB42" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(FB42-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.4 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R31" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 200 "Net-(C18-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 137.3275 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U107" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 422 "Net-(C205-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 157 "Net-(FB91-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 421 "Net-(C205-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 95.175 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB100" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 166 "Net-(FB100-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.7275 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R287" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 287 "Net-(C196-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.325 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R82" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 235 "Net-(C45-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.275 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R193" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 270 "Net-(C134-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 36.5375 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U59" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 354 "Net-(C117-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(FB47-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 353 "Net-(C117-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.275 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R279" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 401 "Net-(C183-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 41.775 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB70" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(FB70-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 105.625 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB96" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 162 "Net-(FB96-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 28.475 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB43" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "Net-(FB43-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 23 22.5)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "DG442DYZ")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U125" (at 2.3 -5.5) (layer "F.SilkS"))
    (fp_text value "DG442" (at 0 5.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/MA_G10") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(C235-Pad2)") (pintype "passive"))
    (pad "3" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 328 "Net-(R368-Pad2)") (pintype "passive"))
    (pad "4" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(C235-Pad2)") (pintype "passive"))
    (pad "7" smd roundrect (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 330 "Net-(R370-Pad2)") (pintype "passive"))
    (pad "8" smd roundrect (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/MA_G100") (pintype "input"))
    (pad "9" smd roundrect (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 450 "unconnected-(U125-Pad9)") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 451 "unconnected-(U125-Pad10)") (pintype "passive"))
    (pad "11" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 452 "unconnected-(U125-Pad11)") (pintype "passive"))
    (pad "12" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "VL") (pintype "power_in"))
    (pad "13" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "14" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 204 "/nvm_amp_main/OUT") (pintype "passive"))
    (pad "15" smd roundrect (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(C235-Pad2)") (pintype "passive"))
    (pad "16" smd roundrect (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/MA_G1") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.925 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R72" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 228 "Net-(C42-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 54.875 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R215" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 371 "Net-(C141-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 103.2375 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U114" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 433 "Net-(C222-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 163 "Net-(FB97-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 294 "Net-(C222-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 44.175 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U77" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 278 "Net-(C155-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "Net-(FB63-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 279 "Net-(C155-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.605 71.025 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R130" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 248 "Net-(C82-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.725 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C44" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 233 "Net-(C44-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 232 "Net-(C44-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.3375 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R76" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 231 "Net-(C43-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.275 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R291" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 406 "Net-(C197-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 405 "Net-(C197-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.1375 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R207" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 366 "Net-(C138-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 365 "Net-(C138-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 134.875 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB90" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 156 "Net-(FB90-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.5275 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R192" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 268 "Net-(C133-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 269 "Net-(C133-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.9375 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R303" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 414 "Net-(C201-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 413 "Net-(C201-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 25.8625 51.075 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R53" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 225 "Net-(C25-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 78.9375 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB77" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "Net-(FB77-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.1075 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R71" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 190 "Net-(C41-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 191 "Net-(C41-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 92.325 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB28" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "Net-(FB28-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 108.4075 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB35" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "Net-(FB35-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 92.325 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB26" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(FB26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 15 19.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040E2003BB300 ")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R368" (at -0.1 -2.1 180) (layer "F.SilkS"))
    (fp_text value "200k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 204 "/nvm_amp_main/OUT") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 328 "Net-(R368-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.3275 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R255" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 283 "Net-(C175-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.875 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R84" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 236 "Net-(C46-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.425 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R241" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 381 "Net-(C160-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 49 25.2 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C4" (at -1.7 1.2 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "-15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 41.4 11.4)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C234" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6525 64 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R45" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 218 "Net-(C22-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 219 "Net-(C22-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.225 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C224" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 436 "Net-(C224-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 437 "Net-(C224-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.075 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R59" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 307 "Net-(R58-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 70.9275 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U96" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 404 "Net-(C184-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 147 "Net-(FB81-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 403 "Net-(C184-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 38.925 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB46" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "Net-(FB46-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 121.5275 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R61" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 195 "Net-(C38-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 106.13 47.2375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C100" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 92.325 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB29" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(FB29-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 84.3275 59.2 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U40" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 346 "Net-(C68-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(FB31-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 345 "Net-(C68-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 25.85 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R47" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 221 "Net-(C23-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 124.075 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U28" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 236 "Net-(C46-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(FB20-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 237 "Net-(C46-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 54.875 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R194" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 271 "Net-(C134-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 66.73 89.6375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C194" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 42.975 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U75" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 314 "Net-(R220-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 127.5875 27)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08050000")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R364" (at 1.0125 1.6) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 326 "Net-(R364-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 325 "Net-(R363-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.45 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R55" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 226 "Net-(C26-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 118.825 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB38" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "Net-(FB38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 110.775 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U50" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 350 "Net-(C88-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "Net-(FB40-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 349 "Net-(C88-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 41.6275 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R223" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 277 "Net-(C154-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.925 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C203" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 417 "Net-(C203-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 418 "Net-(C203-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 15.2 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB3" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(FB3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.525 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R277" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 400 "Net-(C182-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 399 "Net-(C182-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 20.45 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R37" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 198 "Net-(C20-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 28.5 11 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080530K0")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R377" (at 0.2 1.5 90) (layer "F.SilkS"))
    (fp_text value "30k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 305 "Net-(Q4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 332 "Net-(R376-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 38.9375 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB47" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "Net-(FB47-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 96.375 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U108" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 317 "Net-(R316-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 134.675 86.70625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R290" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 405 "Net-(C197-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.875 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C183" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 401 "Net-(C183-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 402 "Net-(C183-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 146.5 32)
    (descr "Mounting Hole 2.7mm, no annular")
    (tags "mounting hole 2.7mm no annular")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 2.7 2.7) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 105.605 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB94" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 160 "Net-(FB94-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.5 34)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080524K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R6" (at 0.1 1.4) (layer "F.SilkS"))
    (fp_text value "24k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 35 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 37 "Net-(C3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.7375 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R77" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 230 "Net-(C43-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 231 "Net-(C43-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 84.275 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U39" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 344 "Net-(C67-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(FB30-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 343 "Net-(C67-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.825 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R236" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 378 "Net-(C158-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 377 "Net-(C158-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.875 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C120" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 359 "Net-(C120-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 360 "Net-(C120-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.475 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R195" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 270 "Net-(C134-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 271 "Net-(C134-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 145.305 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB84" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 150 "Net-(FB84-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 57.475 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U73" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 372 "Net-(C141-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(FB60-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 371 "Net-(C141-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 46.175 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R221" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 314 "Net-(R220-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.125 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R304" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 416 "Net-(C202-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 79.125 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R273" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 397 "Net-(C181-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.1375 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C138" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 365 "Net-(C138-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 366 "Net-(C138-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 145.325 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB88" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 154 "Net-(FB88-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 32.5 7 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08056K20")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R367" (at 2 0 180) (layer "F.SilkS"))
    (fp_text value "6k2" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 304 "Net-(Q3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.3275 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C59" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 189 "Net-(C59-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 188 "Net-(C59-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.1075 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C41" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 191 "Net-(C41-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 190 "Net-(C41-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.23 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C21" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 197 "Net-(C21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 196 "Net-(C21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 95.2275 58.8 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB101" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 167 "Net-(FB101-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.825 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C160" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 381 "Net-(C160-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 382 "Net-(C160-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 52.225 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB68" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(FB68-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.93 47.2375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C110" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.525 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C119" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 357 "Net-(C119-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 358 "Net-(C119-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.425 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R244" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 383 "Net-(C161-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.525 58.025)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R274" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 398 "Net-(C181-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 397 "Net-(C181-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 33.675 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R182" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 360 "Net-(C120-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 171 "/LNAMP/LNAMP_2L4/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.425 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C86" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 257 "Net-(C86-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 256 "Net-(C86-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 140.075 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R310" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 420 "Net-(C204-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 175 "/LNAMP/LNAMP_2L8/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.925 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C66" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 247 "Net-(C66-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 246 "Net-(C66-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 17.6 74.875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U16" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 222 "Net-(C24-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(FB9-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 223 "Net-(C24-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.3075 70.0125)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C62" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 239 "Net-(C62-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 238 "Net-(C62-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.525 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R105" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 241 "Net-(C63-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 124.075 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C39" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 193 "Net-(C39-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 192 "Net-(C39-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.125 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C137" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 363 "Net-(C137-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 364 "Net-(C137-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 4.4 77)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "PN" "ZL262-8SG")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Male" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "Net-(J1-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "Net-(J1-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 63.8 8.8 -90)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "293D106X9025C2TE3")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C9" (at 4.5 0.1 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.55 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.55 0 270) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 5 "+5V") (pintype "passive"))
    (pad "2" smd roundrect (at 2.55 0 270) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 63.125 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R204" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 364 "Net-(C137-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 363 "Net-(C137-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 69.675 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U86" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 315 "Net-(R252-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 60.325 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R202" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 364 "Net-(C137-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 172 "/LNAMP/LNAMP_2L5/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 66.13 47.2375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C215" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 15 25 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040E2002BB100")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R370" (at 3 0) (layer "F.SilkS"))
    (fp_text value "19k8" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 328 "Net-(R368-Pad2)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 330 "Net-(R370-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.93 89.8375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C152" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 105.6375 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB97" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 163 "Net-(FB97-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 36.525 83.25 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C116" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 267 "Net-(C116-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 266 "Net-(C116-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 2.5 23.6)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC847.215")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q1" (at 0 -2.2) (layer "F.SilkS"))
    (fp_text value "BC847" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "Net-(Q1-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "Net-(C12-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "/RE3") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 35 4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW0805240R")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R372" (at -2.6 -1) (layer "F.SilkS"))
    (fp_text value "240R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 210 "Net-(C239-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 177 "Net-(C240-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 76.5375 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R271" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 396 "Net-(C180-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 395 "Net-(C180-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 116.425 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U48" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 256 "Net-(C86-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "Net-(FB38-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 257 "Net-(C86-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 28.3275 55.3875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R159" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 259 "Net-(C112-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 35.5 18.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C241" (at -0.3 1.3 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "-15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 86.5 35.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C232" (at 1.8 -2.1 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 24.6 12 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C244" (at -2.5 0.1 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.905 67.625 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C61" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 182 "Net-(C61-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 183 "Net-(C61-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 126.9375 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R75" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 230 "Net-(C43-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 168 "/LNAMP/LNAMP_2L1/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 17.6325 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U11" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C19-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(FB4-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "Net-(C19-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 55.1275 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB52" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(FB52-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 55.075 82.30625 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB53" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(FB53-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.725 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R74" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 228 "Net-(C42-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 229 "Net-(C42-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.305 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R67" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 179 "Net-(C40-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 95.2275 50.9875 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB92" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 158 "Net-(FB92-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 98.6875 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R316" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 317 "Net-(R316-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 4 16)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C13" (at 2.9 0) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 40 "Net-(C12-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 6 "/RE_P") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 15.0325 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R35" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 8 "Net-(C19-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.875 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C176" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 285 "Net-(C176-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 284 "Net-(C176-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 49.8375 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C159" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 379 "Net-(C159-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 380 "Net-(C159-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 28.275 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R183" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 359 "Net-(C120-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.5275 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C133" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 269 "Net-(C133-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 268 "Net-(C133-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.5 26.0875 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080512K0")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R348" (at 0.8875 -2.1 180) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 58 "/VR28N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 318 "Net-(R348-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 41.6275 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R250" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 387 "Net-(C163-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.5075 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R201" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 274 "Net-(C136-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 275 "Net-(C136-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 70.9275 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C184" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 403 "Net-(C184-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 404 "Net-(C184-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 44.175 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R227" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 278 "Net-(C155-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 279 "Net-(C155-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 89.905 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U33" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 183 "Net-(C61-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "Net-(FB24-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 182 "Net-(C61-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0411_L9.9mm_D3.6mm_P20.32mm_Horizontal" (layer "F.Cu")
    (tedit 5AE5139B)
    (at 143.871338 38.385503 175)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=20.32mm, 1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 20.32mm 1W length 9.9mm diameter 3.6mm")
    (property "PN" "MOX-400231007FE ")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R350" (at 16.16205 1.482529 265) (layer "F.SilkS"))
    (fp_text value "1G" (at 10.16 2.92 175) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 10.16 0 175) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 175) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" thru_hole oval (at 20.32 0 175) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 69 "/LNAMP/ITRIM") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P20.32mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 23.23 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U13" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 196 "Net-(C21-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "Net-(FB6-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 197 "Net-(C21-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.93 89.8875 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C153" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.205 65.825)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R326" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 428 "Net-(C219-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 427 "Net-(C219-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 103.225 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U115" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 435 "Net-(C223-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "Net-(FB98-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 434 "Net-(C223-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 78.925 63.225 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB78" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 144 "Net-(FB78-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 39.53 47.2375 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C131" (at 0 -1.68 90) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 97.575 79.675 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R344" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 438 "Net-(C225-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 295 "Net-(C225-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 47.0375 55.475 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R237" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 380 "Net-(C159-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.725 75.4375 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C45" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 235 "Net-(C45-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 234 "Net-(C45-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 137.3075 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U101" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 410 "Net-(C199-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 151 "Net-(FB85-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 409 "Net-(C199-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 65.525 78.8375 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB59" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(FB59-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81.675 78.875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R117" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 343 "Net-(C67-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 132.325 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R73" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 229 "Net-(C42-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6 87.50625 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R33" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 200 "Net-(C18-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 201 "Net-(C18-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.425 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R330" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 432 "Net-(C221-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 52.425 82.25 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R235" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 377 "Net-(C158-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 76.525 78.4375 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U94" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 400 "Net-(C182-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "Net-(FB79-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 399 "Net-(C182-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 84.3075 71.8125 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R103" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 238 "Net-(C62-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 239 "Net-(C62-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.725 86.65 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R266" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 394 "Net-(C179-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 105.825 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R337" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 434 "Net-(C223-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 30.9275 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U54" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 258 "Net-(C112-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(FB42-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 259 "Net-(C112-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 52.205 71.025 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB64" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "Net-(FB64-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 89.9375 50.275)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R109" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 242 "Net-(C64-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 243 "Net-(C64-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 44.2075 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U79" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 376 "Net-(C157-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "Net-(FB65-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 375 "Net-(C157-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 103.225 86.25 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U113" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 432 "Net-(C221-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 162 "Net-(FB96-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 431 "Net-(C221-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 18.7125 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R156" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 311 "Net-(R156-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 100.425 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R336" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 435 "Net-(C223-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 176 "/LNAMP/LNAMP_2L9/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 47.0275 50.9875 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R222" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 276 "Net-(C154-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 81 28.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW080524R0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 204 "/nvm_amp_main/OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 45 "/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 73.675 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R257" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 284 "Net-(C176-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 17.6525 56.1875 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R30" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 202 "Net-(C17-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 203 "Net-(C17-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 142.905 70.625 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U100" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 408 "Net-(C198-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 150 "Net-(FB84-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 407 "Net-(C198-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 119.025 58.825 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R143" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 257 "Net-(C86-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 49.825 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U82" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 382 "Net-(C160-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(FB68-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 381 "Net-(C160-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.475 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C141" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 371 "Net-(C141-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 372 "Net-(C141-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 137.275 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U99" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 406 "Net-(C197-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "Net-(FB83-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 405 "Net-(C197-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 17.6 82.70625 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U10" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 200 "Net-(C18-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(FB3-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 201 "Net-(C18-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.3275 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R282" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 403 "Net-(C184-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 54.9075 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R200" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 275 "Net-(C136-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 110.775 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C88" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 349 "Net-(C88-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 350 "Net-(C88-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 30.9275 54.3875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C112" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 259 "Net-(C112-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 258 "Net-(C112-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 68.3075 71.0125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R264" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 391 "Net-(C178-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 50.6 11.4)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C239" (at 0 1.3) (layer "F.SilkS"))
    (fp_text value "2u2" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 210 "Net-(C239-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 211 "Net-(C239-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.6075 66.6125 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R133" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 250 "Net-(C83-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 70.9275 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U87" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 282 "Net-(C175-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "Net-(FB72-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 283 "Net-(C175-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 109.575 47.2)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U41" (at 0 -2.4) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 309 "Net-(R122-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "GND1") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 81.9075 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB25" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(FB25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 52.225 86.65 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB66" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 132 "Net-(FB66-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 15.2325 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB4" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(FB4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 19.6 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R157" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 311 "Net-(R156-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 65 "/LNAMP/LNAMP_2L/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 12.2 53.4 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-5R6")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R356" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "5R6" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 306 "/LNAMP/IN") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 103.225 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R332" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 432 "Net-(C221-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 431 "Net-(C221-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 57.5275 51.3875 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U65" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 268 "Net-(C133-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(FB52-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 269 "Net-(C133-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 46.975 74.475 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R246" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 386 "Net-(C162-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 124.1075 67.0125 -90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U23" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 190 "Net-(C41-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(FB15-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 191 "Net-(C41-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 270) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 46.975 82.30625 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R225" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 278 "Net-(C155-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 173 "/LNAMP/LNAMP_2L6/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 113.625 63.225 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "ERA-6AED203V ")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R142" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "20k" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 256 "Net-(C86-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 170 "/LNAMP/LNAMP_2L3/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 108.375 74.475 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB40" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "Net-(FB40-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 142.9375 55.075 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U103" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 414 "Net-(C201-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 153 "Net-(FB87-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 413 "Net-(C201-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 23.2625 52.075 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C25" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 225 "Net-(C25-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 224 "Net-(C25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.275 85.70625)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L1")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C197" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 405 "Net-(C197-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 406 "Net-(C197-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 47 17 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "AD8628ARZ")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U123" (at 2.5 3.9 180) (layer "F.SilkS"))
    (fp_text value "AD8628" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 205 "unconnected-(U123-Pad1)") (pinfunction "NC") (pintype "no_connect"))
    (pad "2" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "Net-(C235-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "/MAMP_IN") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "Net-(C239-Pad2)") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 206 "unconnected-(U123-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "Net-(C235-Pad1)") (pintype "output"))
    (pad "7" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 210 "Net-(C239-Pad1)") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 207 "unconnected-(U123-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 57.5275 62.2)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C142" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 373 "Net-(C142-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 374 "Net-(C142-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 129.725 73.6375)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R83" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 234 "Net-(C45-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 235 "Net-(C45-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 92.525 74.4375 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L6")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R114" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 247 "Net-(C66-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137.275 77.875)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L7")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C204" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 419 "Net-(C204-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 420 "Net-(C204-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 68.5075 66.6125 -90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L2")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB75" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 141 "Net-(FB75-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 72.875 47.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "RN73C2A5K11BTD")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R253" (at 0 -1.65 -270) (layer "F.SilkS") hide)
    (fp_text value "5k1" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 315 "Net-(R252-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 174 "/LNAMP/LNAMP_2L7/LNAMP_1L/OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5" (layer "F.Cu")
    (tedit 5F6F9B37)
    (at 129.725 62.825 90)
    (descr "SOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AA), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP6V51T-E/OT")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U26" (at 0 -2.4 90) (layer "F.SilkS") hide)
    (fp_text value "MCP6V51" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 232 "Net-(C44-Pad2)") (pintype "output"))
    (pad "2" smd roundrect (at -1.1375 0 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pinfunction "V-") (pintype "power_in"))
    (pad "3" smd roundrect (at -1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(FB18-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at 1.1375 0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 233 "Net-(C44-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "5" smd roundrect (at 1.1375 -0.95 90) (size 1.325 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 116.425 81.45)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1002ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L3")
    (property "comment" " ")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R138" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "10k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 252 "Net-(C84-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 253 "Net-(C84-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 108.2275 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R152" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 351 "Net-(C89-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 65.705 66.625 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L4")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R197" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 273 "Net-(C135-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 15.0525 63.2 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRT0805-FX-1000ELF")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L5")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R44" (at 0 -1.65 90) (layer "F.SilkS") hide)
    (fp_text value "100R" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 219 "Net-(C22-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 138.3875 44.4 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "279-RN73C2A40K2BTD ")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "R284" (at 0 -1.65) (layer "F.SilkS") hide)
    (fp_text value "40k" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 67 "/LNAMP/L_OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 316 "Net-(R284-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 142.925 59.825 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L9")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C202" (at 0 -1.68) (layer "F.SilkS") hide)
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 415 "Net-(C202-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 416 "Net-(C202-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 65.5375 55.475 90)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "PN" "BLM18RK601SN1D")
    (property "Sheetfile" "lnamp_l1.kicad_sch")
    (property "Sheetname" "LNAMP_1L8")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB57" (at 0 -1.43 90) (layer "F.SilkS") hide)
    (fp_text value "FerriteBead_Small" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab") hide)
    (pad "1" smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "Net-(FB57-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 105 30 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP1700T-3302E")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U8" (at -1.7 -2.1 180) (layer "F.SilkS"))
    (fp_text value "MCP1700-33" (at 0 2.5 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "+3V3") (pinfunction "VO") (pintype "power_out"))
    (pad "3" smd roundrect (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "+5V") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 135.5925 50.4375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C150" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 66.41 28.5)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "YR1B18K2CC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R14" (at 4.29 0.1) (layer "B.SilkS"))
    (fp_text value "18k20" (at 1.27 -2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.37) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "Net-(K3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "/VREF7") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 144.73 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C149" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 99.455 28)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "YR1B4K99CC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R26" (at 1.445 -1.8) (layer "B.SilkS"))
    (fp_text value "5k" (at 1.27 -2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.37) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 312 "Net-(R21-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 58 "/VR28N") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 91.5 25.5 180)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "PN" "ZL262-8SG")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J5" (at 0 2.33) (layer "B.SilkS"))
    (fp_text value "Conn_01x04_Male" (at 0 -9.95) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -3.81 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/VREF_EXT") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/OUT") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "GNDS") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 78.13 59.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C129" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 144.53 59.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C148" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 51.53 59.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C98" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 22.732233 34 45)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "FKP2-470P/630-R")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 3 225) (layer "B.SilkS"))
    (fp_text value "470p" (at 2.5 -3 225) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 225) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 35 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 124 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C52" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 141.33 79.4375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C144" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 55.93 50.6375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C74" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 60.2 29.8375 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C247" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "-15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 104.93 59.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C55" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 80.5 12.5 -90)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (property "PN" "ZL262-8SG")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J4" (at 1.27 2.33 90) (layer "B.SilkS"))
    (fp_text value "Conn_02x08_Odd_Even" (at 1.27 -20.11 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -8.89) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "/MA_G1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "/MS_A2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "/MA_G10") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "/MS_A1") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/MA_G100") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "/MS_A0") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 53 "unconnected-(J4-Pad7)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "/JA_DOUT") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 57 "unconnected-(J4-Pad9)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "/JA_DIN") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 59 "unconnected-(J4-Pad11)") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "/COMP") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/JA_CS") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 61 "unconnected-(J4-Pad14)") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/JA_SCK") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 29.13 50.4375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C211" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 59.33 49.5275)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C69" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 105.13 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C54" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 19.33 49.0375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C101" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 15.93 72.8375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C107" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 64.93 59.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C76" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 87.08 27 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "PTF56200R00FZEB")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R24" (at -0.02 -1.5) (layer "B.SilkS"))
    (fp_text value "200R0" (at 5.08 -2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "/CP_70M") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 91.73 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C193" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 97.4 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C189" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 29.33 73.0375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C212" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 118.13 59.8375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C171" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 35.232233 34 45)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "FKP2-470P/630-R")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 3 225) (layer "B.SilkS"))
    (fp_text value "470p" (at 2.5 -3 225) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 225) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 45) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 131.53 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C33" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 15.9925 50.1475)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C106" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 32.5925 49.4375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C206" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 72.53 74.2375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C123" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 97.045 35 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "YR1B18K2CC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R17" (at -2.455 -0.1) (layer "B.SilkS"))
    (fp_text value "18k20" (at 1.27 -2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.37) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "/VREF7") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 303 "Net-(R17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 112.4675 49.6375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C164" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 55.93 73.2375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C77" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 42.53 73.0375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C96" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 125.93 49.8375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C29" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 78.33 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C128" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 21.73 80.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C104" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 111.5 23.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C228" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "-15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 87.08 19 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "PTF5620K000FZEB ")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R15" (at 0.08 -1.5) (layer "B.SilkS"))
    (fp_text value "20k00" (at 5.08 -2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 62 "/VREF7") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "/CP_07V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 34.93 80.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C209" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 94.5 28)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "YR1B4K99CC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R21" (at 0.2 -1.8) (layer "B.SilkS"))
    (fp_text value "5k" (at 1.27 -2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.37) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 60 "/VR28P") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 312 "Net-(R21-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 138.93 49.4375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C145" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 45.93 74.0375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C91" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 69.33 73.4375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C130" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 82.73 50.6375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C190" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 137.2 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C73" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 28.5 2.5 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "PN" "ZL262-4SG")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J2" (at 0 2.33 90) (layer "B.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 -20.11 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -8.89) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 209 "Net-(J2-Pad1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 213 "Net-(J2-Pad2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 214 "Net-(J2-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 215 "Net-(J2-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 216 "Net-(J2-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 292 "Net-(J2-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(D1-Pad2)") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 "Net-(C12-Pad2)") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 84.2625 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C94" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 59.13 74.2375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C71" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 10.2 53.3 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "PN" "R82IC2220Z350K")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C229" (at 2.5 3 90) (layer "B.SilkS"))
    (fp_text value "22n" (at 2.5 -3 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "/LNAMP/L_IN") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 66 "GND1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 107.5 22.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C227" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 74.93 79.8375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C124" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 105.2 28.8 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08053K0")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R27" (at -2.1 0 180) (layer "B.SilkS"))
    (fp_text value "3k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 58 "/VR28N") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 3 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 95.8 73.4)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C56" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 133.5 45 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08053K0")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R362" (at 2.4 0.1 180) (layer "B.SilkS"))
    (fp_text value "3k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 324 "Net-(R362-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 128.13 58.8375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C27" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 61.53 58.0375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C72" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 70.7375 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C168" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 85.93 74.2375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C187" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 48.13 58.0375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C93" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 69.33 50.5475)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C127" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 87.08 23 180)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "PTF562K0000BZEK")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R20" (at -0.12 -1.7) (layer "B.SilkS"))
    (fp_text value "2k00" (at 5.08 -2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 5.08 0) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 63 "/CP_07V") (pintype "passive"))
    (pad "2" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 64 "/CP_70M") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 7.6 47.8 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW0805240R")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R13" (at 1.1 -1.9 180) (layer "B.SilkS"))
    (fp_text value "240R" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 291 "Net-(K1-Pad3)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 3 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 25.13 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C109" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 74.93 58.4375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C125" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 60 34.4 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C245" (at 0 1.68 90) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.68 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 1 "+15V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0375 0 270) (size 1.175 1.45) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 118.33 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C170" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 17.6 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C147" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 109.33 73.2375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C172" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 61.53 79.8375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C70" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 122.53 73.0375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C35" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 114.73 79.4375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C165" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 30.8 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C105" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 125.73 74.0375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C28" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 21.73 57.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C103" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 101.73 79.4375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C49" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 91.53 59.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C192" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 88.33 58.4375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C188" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 99.4 74)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C50" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 51.6675 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C97" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 59FED5CC)
    (at 70.5 2.5 90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "PN" "ZL262-4SG")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J3" (at 0 2.33 90) (layer "B.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 -20.11 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -8.89) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+15V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+15V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 "+9V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "+5V") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "-9V") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "-15V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "-15V") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 82.73 73.4375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C191" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 114.93 58.8375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C166" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPST_StandexMeder_SIL_Form1A" (layer "B.Cu")
    (tedit 5A54B0D5)
    (at 57.835 23.5175)
    (descr "Standex-Meder SIL-relais, Form 1A, see https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_SIL.pdf")
    (tags "Standex Meder SIL reed relais")
    (property "PN" "Pickering 107-1-A-5")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "Could be different type")
    (property "supplier" "Own stock")
    (attr through_hole)
    (fp_text reference "K3" (at 3.665 3.3825) (layer "B.SilkS"))
    (fp_text value "SILxx-1Axx-71x" (at 7.65 -3.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 7.75 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 51 "Net-(K3-Pad1)") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "/RE_P") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 52 "/RE3") (pintype "passive"))
    (pad "7" thru_hole circle (at 15.24 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 49 "/CP_9M") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_StandexMeder_SIL_Form1A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 48.13 80.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C92" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 101.73 58.4375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C51" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 38.13 59.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C213" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 26 49.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08053K0")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R358" (at 2.4 1.1 180) (layer "B.SilkS"))
    (fp_text value "3k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 333 "Net-(R358-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 66.455 32)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "CMF5523R200BEEK")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R18" (at 4.345 0.1) (layer "B.SilkS"))
    (fp_text value "24R" (at 1.27 -2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.37) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 49 "/CP_9M") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 141.33 58.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C143" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 95.93 50.6375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C53" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 57.4 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C126" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 38.3925 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C214" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 135.53 73.2375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C151" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 42.53 50.4375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C95" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 25.13 59.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C108" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 94.455 31.5)
    (descr "Resistor, Axial_DIN0207 series, Axial, Vertical, pin pitch=2.54mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Vertical pin pitch 2.54mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "YR1B12K1CC")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R22" (at 4.445 0) (layer "B.SilkS"))
    (fp_text value "12k1" (at 1.27 -2.37) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.37) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 303 "Net-(R17-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "B.Cu")
    (tedit 5F68FEEE)
    (at 79 50.5 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "PN" "CRCW08053K0")
    (property "Sheetfile" "lnamp.kicad_sch")
    (property "Sheetname" "LNAMP")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R366" (at 2.4 0 180) (layer "B.SilkS"))
    (fp_text value "3k" (at 0 -1.65 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 66 "GND1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.243902439)
      (net 327 "Net-(R366-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 34.7925 57.6375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C208" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 86.13 49.6375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C185" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 32.53 74.0375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C207" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W3.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 29.5 27 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*3.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 3.5mm Capacitor")
    (property "Sheetfile" "nvm_amp_main.kicad_sch")
    (property "Sheetname" "nvm_amp_main")
    (property "comment" "DNP")
    (attr through_hole)
    (fp_text reference "C242" (at 2.3 3.1) (layer "B.SilkS"))
    (fp_text value "DNP" (at 2.5 -3 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 270) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 212 "Net-(C242-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W3.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 64.93 78.2375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L3")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C75" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 72.73 49.4375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L5")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C122" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 19.33 74.0375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C102" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 112.53 74.2375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C167" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 109.13 50.6375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L7")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C169" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 128.13 79.4375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C30" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 44.2 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L9")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C210" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 131.33 59.8375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C32" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 122.53 50.4375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C34" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 138.93 74.0375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L6")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C146" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 45.93 49.5275)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L4")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C90" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 88.33 79.8375 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L8")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C186" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 110.6 53.6 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L1")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C31" (at 0 1.43) (layer "B.SilkS"))
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab"))
    (pad "1" smd roundrect (at -0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0 180) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 76 "-9V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Relay_THT:Relay_SPST_StandexMeder_SIL_Form1A" (layer "B.Cu")
    (tedit 5A54B0D5)
    (at 57.835 17.0175)
    (descr "Standex-Meder SIL-relais, Form 1A, see https://standexelectronics.com/wp-content/uploads/datasheet_reed_relay_SIL.pdf")
    (tags "Standex Meder SIL reed relais")
    (property "PN" "Pickering 107-1-A-5")
    (property "Sheetfile" "rnvm_bart.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "Could be different type")
    (property "supplier" "Own stock")
    (attr through_hole)
    (fp_text reference "K4" (at 1.865 -3.3175) (layer "B.SilkS"))
    (fp_text value "SILxx-1Axx-71x" (at 7.65 -3.55) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 7.75 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 293 "Net-(K4-Pad1)") (pintype "passive"))
    (pad "3" thru_hole circle (at 5.08 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 6 "/RE_P") (pintype "passive"))
    (pad "5" thru_hole circle (at 10.16 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 54 "/RE4") (pintype "passive"))
    (pad "7" thru_hole circle (at 15.24 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Relay_THT.3dshapes/Relay_SPST_StandexMeder_SIL_Form1A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (layer "B.Cu")
    (tedit 5F68FEEF)
    (at 99.33 49.6375)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL10B104KB8NNND")
    (property "Sheetfile" "lnamp_l2.kicad_sch")
    (property "Sheetname" "LNAMP_2L2")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C48" (at 0 1.43) (layer "B.SilkS") hide)
    (fp_text value "100n" (at 0 -1.43) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "B.Fab") hide)
    (pad "1" smd roundrect (at -0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 77 "+9V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.8625 0) (size 1.075 0.95) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 0 3.5) (end 6.5 3.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 87.5 3.5) (end 105 3.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 6.5 3.5) (end 6.5 0.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105 20) (end 150 20) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 87.5 0.5) (end 87.5 3.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 0 100) (end 0 3.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 0 100) (end 94.5 100) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 6.5 0.5) (end 87.5 0.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 150 94.5) (end 94.5 94.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 105 3.5) (end 105 20) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 94.5 94.5) (end 94.5 100) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 150 94.5) (end 150 20) (layer "Edge.Cuts") (width 0.1))
  (gr_text "NVM\nBART PCB 2\nREV 2" (at 19 9.5) (layer "F.SilkS"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149 94) (xy 9 94))
    (height -16)
    (gr_text "140,0000 mm" (at 79 108.85) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.35) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149 94) (xy 149 29.5))
    (height 8)
    (gr_text "64,5000 mm" (at 155.85 61.75 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.35) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 118 38) (xy 0.5 38))
    (height 11.499999)
    (gr_text "117,5000 mm" (at 59.25 25.350001) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.35) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 9 94) (xy 9 74))
    (height -14)
    (gr_text "20,0000 mm" (at -6.15 84 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.35) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 146.5 32) (xy 146.5 91.5))
    (height -7)
    (gr_text "59,5000 mm" (at 152.35 61.75 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.35) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 3 56) (xy 3 38))
    (height -5.5)
    (gr_text "18,0000 mm" (at -3.65 47 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.35) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 149 29.5) (xy 118 29.5))
    (height 3)
    (gr_text "31,0000 mm" (at 133.5 25.35) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.35) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 9 74) (xy 0.5 74))
    (height -36)
    (gr_text "8,5000 mm" (at 4.75 108.85) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.35) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 2 74) (xy 2 38))
    (height -7)
    (gr_text "36,0000 mm" (at -6.15 56 90) (layer "Dwgs.User"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.35) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 10.5 77)
        (xy 9 77)
        (xy 9 74)
        (xy 3.5 74)
        (xy 3.5 72.5)
        (xy 10.5 72.5)
      )
    )
  )
  (zone (net 40) (net_name "Net-(C12-Pad2)") (layers "F.Cu" "In1.Cu" "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 30 5.5)
        (xy 17.5 5.5)
        (xy 17.5 12.5)
        (xy 10 12.5)
        (xy 10 28.5)
        (xy 8 28.5)
        (xy 8 35)
        (xy 0.5 35)
        (xy 0.5 4)
        (xy 7 4)
        (xy 7 1)
        (xy 30 1)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 149.5 89)
        (xy 149.5 94)
        (xy 144 94)
        (xy 94.5 94)
        (xy 93.5 94)
        (xy 87.957888 93.990067)
        (xy 87.99994 99.490657)
        (xy 6 99.5)
        (xy 6 94)
        (xy 0.5 94)
        (xy 0.5 35.5)
        (xy 8.5 35.5)
        (xy 8.5 29)
        (xy 10.5 29)
        (xy 10.5 13)
        (xy 18 13)
        (xy 18 6)
        (xy 30.5 6)
        (xy 30.5 1)
        (xy 42 1)
        (xy 42 7)
        (xy 49 7)
        (xy 49 1)
        (xy 87 1)
        (xy 87 4)
        (xy 104.5 4)
        (xy 104.5 20.5)
        (xy 139.5 20.5)
        (xy 149.5 20.5)
      )
    )
  )
  (zone (net 66) (net_name "GND1") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 143 91.5)
        (xy 23.5 91.5)
        (xy 23.5 90)
        (xy 143 90)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "In1.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 87 4)
        (xy 104.5 4)
        (xy 104.5 20.5)
        (xy 149.5 20.5)
        (xy 149.5 94)
        (xy 94 94)
        (xy 94 99.5)
        (xy 0.5 99.5)
        (xy 0.5 35.5)
        (xy 8.5 35.5)
        (xy 8.5 29)
        (xy 10.5 29)
        (xy 10.5 13)
        (xy 18 13)
        (xy 18 6)
        (xy 30.5 6)
        (xy 30.5 1)
        (xy 87 1)
      )
    )
  )
  (zone (net 3) (net_name "GNDS") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 87 4)
        (xy 104.5 4)
        (xy 104.5 20.5)
        (xy 149.5 20.5)
        (xy 149.5 43.5)
        (xy 96 43.5)
        (xy 96 35.1)
        (xy 91 35.1)
        (xy 91 43.5)
        (xy 0.5 43.5)
        (xy 0.5 35.5)
        (xy 8.5 35.5)
        (xy 8.5 29)
        (xy 10.5 29)
        (xy 10.5 13)
        (xy 18 13)
        (xy 18 6)
        (xy 30.5 6)
        (xy 30.5 1)
        (xy 87 1)
      )
    )
  )
  (zone (net 66) (net_name "GND1") (layer "In2.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 149.5 94)
        (xy 0.5 94)
        (xy 0.5 44)
        (xy 91.5 44)
        (xy 91.5 36)
        (xy 95.5 36)
        (xy 95.5 44)
        (xy 149.5 44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 71 39.5)
        (xy 58 39.5)
        (xy 58 38)
        (xy 71 38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 55.5 39.5)
        (xy 6 39.5)
        (xy 6 38)
        (xy 55.5 38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 127 31)
        (xy 119.5 31)
        (xy 119.5 39.5)
        (xy 72.5 39.5)
        (xy 72.5 38)
        (xy 118 38)
        (xy 118 29.5)
        (xy 127 29.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 149 94)
        (xy 9 94)
        (xy 9 76.5)
        (xy 9 74)
        (xy 0.5 74)
        (xy 0.5 38)
        (xy 2 38)
        (xy 2 53.5)
        (xy 5.5 53.5)
        (xy 5.5 58.5)
        (xy 2 58.5)
        (xy 2 72.5)
        (xy 10.5 72.5)
        (xy 10.5 92.5)
        (xy 144 92.5)
        (xy 144 89)
        (xy 147.5 89)
        (xy 147.5 35)
        (xy 144 35.014397)
        (xy 144 31)
        (xy 130.9 31)
        (xy 130.9 29.5)
        (xy 149 29.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 10.5 77)
        (xy 9 77)
        (xy 9 74)
        (xy 3.5 74)
        (xy 3.5 72.5)
        (xy 10.5 72.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 8 39.5)
        (xy 2 39.5)
        (xy 2 53.5)
        (xy 5.5 53.5)
        (xy 5.5 58.5)
        (xy 2 58.5)
        (xy 2 74)
        (xy 0.5 74)
        (xy 0.5 38)
        (xy 8 38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.21))
    (polygon
      (pts
        (xy 9 78.5)
        (xy 10.5 78.5)
        (xy 10.5 92.5)
        (xy 144 92.5)
        (xy 144 89)
        (xy 147.5 89)
        (xy 147.5 35)
        (xy 144 35)
        (xy 144 31)
        (xy 119.5 31)
        (xy 119.5 39.5)
        (xy 12 39.5)
        (xy 12 38)
        (xy 118 38)
        (xy 118 29.5)
        (xy 149 29.5)
        (xy 149 94)
        (xy 9 94)
      )
    )
  )
)
