(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer false)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "GNDS")
  (net 3 "+24V")
  (net 4 "+15V")
  (net 5 "+6V")
  (net 6 "-6V")
  (net 7 "-15V")
  (net 8 "-24V")
  (net 9 "/MA_G1")
  (net 10 "/MS_A2")
  (net 11 "/MA_G10")
  (net 12 "/MS_A1")
  (net 13 "/MA_G100")
  (net 14 "/MS_A0")
  (net 15 "/JA_C1")
  (net 16 "/JA_DOUT")
  (net 17 "/JA_C2")
  (net 18 "/JA_DIN")
  (net 19 "/JA_C3")
  (net 20 "/COMP")
  (net 21 "/JA_CS")
  (net 22 "/JA_SCK")
  (net 23 "GNDA")
  (net 24 "Net-(C2-Pad2)")
  (net 25 "Net-(C4-Pad2)")
  (net 26 "Net-(C2-Pad1)")
  (net 27 "Net-(C5-Pad2)")
  (net 28 "Net-(C4-Pad1)")
  (net 29 "Net-(C6-Pad2)")
  (net 30 "/nvm_pcb_analog_ada/INT_IN")
  (net 31 "Net-(C8-Pad1)")
  (net 32 "/nvm_pcb_analog_ada/VA1V2")
  (net 33 "/nvm_pcb_analog_ada/INT_OUT")
  (net 34 "+3.3VA")
  (net 35 "/nvm_pcb_analog_ada/VADC")
  (net 36 "+5VD")
  (net 37 "Net-(C9-Pad1)")
  (net 38 "Net-(D3-Pad1)")
  (net 39 "+5VA")
  (net 40 "/nvm_analog_adfpga/TDO")
  (net 41 "/nvm_analog_adfpga/TDI")
  (net 42 "/nvm_analog_adfpga/TCK")
  (net 43 "/nvm_analog_adfpga/TMS")
  (net 44 "/RE3")
  (net 45 "/RE4")
  (net 46 "/R1A")
  (net 47 "/R1B")
  (net 48 "/R2A")
  (net 49 "/R2B")
  (net 50 "Net-(C11-Pad2)")
  (net 51 "VREF+")
  (net 52 "VREF-")
  (net 53 "Net-(C23-Pad2)")
  (net 54 "/nvm_analog_adfpga/FC0")
  (net 55 "/nvm_pcb_analog_ada/RES_ADC_IN")
  (net 56 "Net-(C17-Pad1)")
  (net 57 "/nvm_analog_adfpga/FC9")
  (net 58 "Net-(C46-Pad2)")
  (net 59 "Net-(Q1-Pad1)")
  (net 60 "/nvm_analog_adfpga/FC6")
  (net 61 "/nvm_analog_adfpga/FC5")
  (net 62 "/nvm_pcb_analog_ada/COM_OUT")
  (net 63 "/nvm_analog_adfpga/FC3")
  (net 64 "/nvm_analog_adfpga/FC2")
  (net 65 "/nvm_analog_adfpga/FC1")
  (net 66 "/nvm_pcb_analog_ada/AD_IN")
  (net 67 "Net-(Q2-Pad1)")
  (net 68 "Net-(R1-Pad1)")
  (net 69 "+8V")
  (net 70 "-8V")
  (net 71 "/nvm_pcb_analog_ada/LOC_AD")
  (net 72 "Net-(RN1-Pad5)")
  (net 73 "Net-(RN1-Pad6)")
  (net 74 "Net-(RN1-Pad7)")
  (net 75 "Net-(RN3-Pad1)")
  (net 76 "VREF7")
  (net 77 "/nvm_analog_adfpga/TDAT")
  (net 78 "/nvm_analog_adfpga/TSCK")
  (net 79 "/nvm_analog_adfpga/TCS")
  (net 80 "/nvm_analog_adfpga/FPGA_RX")
  (net 81 "/nvm_analog_adfpga/FPGA_STB")
  (net 82 "/nvm_analog_adfpga/FPGA_CTRL")
  (net 83 "/nvm_analog_adfpga/FPGA_TX")
  (net 84 "Net-(D1-Pad1)")
  (net 85 "Net-(C19-Pad1)")
  (net 86 "Net-(C21-Pad1)")
  (net 87 "Net-(C25-Pad2)")
  (net 88 "Net-(D2-Pad2)")
  (net 89 "Net-(D9-Pad1)")
  (net 90 "/nvm_pcb_analog_ada/VREF25")
  (net 91 "Net-(J1-Pad3)")
  (net 92 "Net-(J1-Pad4)")
  (net 93 "Net-(J1-Pad5)")
  (net 94 "unconnected-(X1-Pad1)")
  (net 95 "Net-(J1-Pad6)")
  (net 96 "unconnected-(J3-Pad13)")
  (net 97 "Net-(C30-Pad2)")
  (net 98 "/FEN_B")
  (net 99 "/FEN_A")
  (net 100 "/FEN_C")
  (net 101 "/AMP_OUT")
  (net 102 "Net-(R59-Pad1)")
  (net 103 "unconnected-(U2-Pad7)")
  (net 104 "unconnected-(U2-Pad10)")
  (net 105 "unconnected-(U4-Pad1)")
  (net 106 "unconnected-(U4-Pad5)")
  (net 107 "unconnected-(U4-Pad8)")
  (net 108 "Net-(C33-Pad2)")
  (net 109 "Net-(C37-Pad2)")
  (net 110 "Net-(C39-Pad1)")
  (net 111 "Net-(C39-Pad2)")
  (net 112 "/nvm_analog_adfpga/FPGA_CLK")
  (net 113 "/nvm_pcb_analog_ada/GUARD")
  (net 114 "Net-(D6-Pad1)")
  (net 115 "3VFPGA")
  (net 116 "Net-(C45-Pad2)")
  (net 117 "Net-(C47-Pad2)")
  (net 118 "Net-(TP2-Pad1)")
  (net 119 "Net-(TP3-Pad1)")
  (net 120 "Net-(TP4-Pad1)")
  (net 121 "Net-(TP5-Pad1)")
  (net 122 "Net-(TP6-Pad1)")
  (net 123 "Net-(TP7-Pad1)")
  (net 124 "Net-(TP8-Pad1)")
  (net 125 "Net-(TP9-Pad1)")
  (net 126 "Net-(TP10-Pad1)")
  (net 127 "Net-(TP11-Pad1)")
  (net 128 "Net-(TP12-Pad1)")
  (net 129 "Net-(D6-Pad2)")
  (net 130 "Net-(C32-Pad1)")
  (net 131 "Net-(D7-Pad1)")
  (net 132 "Net-(D8-Pad1)")
  (net 133 "Net-(D8-Pad2)")
  (net 134 "Net-(D7-Pad2)")
  (net 135 "Net-(D10-Pad1)")
  (net 136 "Net-(FB3-Pad2)")
  (net 137 "Net-(FB4-Pad1)")
  (net 138 "Net-(Q2-Pad3)")
  (net 139 "Net-(Q4-Pad1)")
  (net 140 "Net-(Q5-Pad2)")
  (net 141 "Net-(Q6-Pad1)")
  (net 142 "Net-(Q7-Pad1)")
  (net 143 "Net-(Q8-Pad1)")
  (net 144 "Net-(Q8-Pad3)")
  (net 145 "Net-(R2-Pad1)")
  (net 146 "Net-(D9-Pad2)")
  (net 147 "/PSWB")
  (net 148 "Net-(R18-Pad2)")
  (net 149 "Net-(R25-Pad2)")
  (net 150 "Net-(R26-Pad2)")
  (net 151 "Net-(R32-Pad2)")
  (net 152 "Net-(R36-Pad2)")
  (net 153 "/PSWA")
  (net 154 "Net-(R53-Pad1)")
  (net 155 "Net-(R54-Pad1)")
  (net 156 "Net-(R55-Pad1)")
  (net 157 "Net-(R56-Pad1)")
  (net 158 "Net-(R57-Pad1)")
  (net 159 "Net-(R25-Pad1)")
  (net 160 "Net-(R58-Pad1)")
  (net 161 "/AZSW")
  (net 162 "Net-(R60-Pad1)")
  (net 163 "Net-(R61-Pad1)")
  (net 164 "Net-(R62-Pad1)")
  (net 165 "Net-(R63-Pad1)")
  (net 166 "Net-(R64-Pad1)")
  (net 167 "Net-(R65-Pad1)")
  (net 168 "Net-(R66-Pad1)")
  (net 169 "Net-(R67-Pad1)")
  (net 170 "Net-(R68-Pad1)")
  (net 171 "Net-(R69-Pad1)")
  (net 172 "Net-(R70-Pad1)")
  (net 173 "Net-(R71-Pad1)")
  (net 174 "Net-(R72-Pad1)")
  (net 175 "Net-(R73-Pad1)")
  (net 176 "Net-(R74-Pad1)")
  (net 177 "Net-(R75-Pad1)")
  (net 178 "Net-(R76-Pad1)")
  (net 179 "Net-(R77-Pad1)")
  (net 180 "Net-(R78-Pad1)")
  (net 181 "Net-(R79-Pad1)")
  (net 182 "Net-(R80-Pad1)")
  (net 183 "Net-(R81-Pad1)")
  (net 184 "Net-(R82-Pad1)")
  (net 185 "Net-(R83-Pad1)")
  (net 186 "Net-(R84-Pad1)")
  (net 187 "Net-(R85-Pad1)")
  (net 188 "Net-(R86-Pad1)")
  (net 189 "Net-(R87-Pad1)")
  (net 190 "Net-(U1-Pad14)")
  (net 191 "unconnected-(U5-Pad1)")
  (net 192 "unconnected-(U5-Pad5)")
  (net 193 "unconnected-(U5-Pad8)")
  (net 194 "unconnected-(U6-Pad5)")
  (net 195 "unconnected-(U6-Pad6)")
  (net 196 "unconnected-(U7-Pad1)")
  (net 197 "unconnected-(U7-Pad5)")
  (net 198 "unconnected-(U7-Pad8)")
  (net 199 "unconnected-(U8-Pad1)")
  (net 200 "unconnected-(U8-Pad5)")
  (net 201 "unconnected-(U8-Pad8)")
  (net 202 "unconnected-(U9-Pad1)")
  (net 203 "unconnected-(U9-Pad8)")
  (net 204 "unconnected-(U15-Pad1)")
  (net 205 "unconnected-(U15-Pad5)")
  (net 206 "unconnected-(U9-Pad5)")
  (net 207 "unconnected-(U15-Pad8)")
  (net 208 "unconnected-(U16-Pad1)")
  (net 209 "unconnected-(U16-Pad5)")
  (net 210 "unconnected-(U16-Pad8)")
  (net 211 "unconnected-(U17-Pad1)")
  (net 212 "unconnected-(U17-Pad5)")
  (net 213 "unconnected-(U17-Pad8)")
  (net 214 "unconnected-(U20-Pad4)")
  (net 215 "unconnected-(U20-Pad7)")
  (net 216 "unconnected-(U20-Pad14)")
  (net 217 "unconnected-(U20-Pad21)")
  (net 218 "unconnected-(U20-Pad30)")
  (net 219 "unconnected-(U20-Pad31)")
  (net 220 "unconnected-(U20-Pad32)")
  (net 221 "unconnected-(U20-Pad34)")
  (net 222 "unconnected-(U20-Pad43)")
  (net 223 "unconnected-(U20-Pad45)")
  (net 224 "unconnected-(U20-Pad47)")
  (net 225 "unconnected-(U20-Pad48)")
  (net 226 "unconnected-(U20-Pad49)")
  (net 227 "unconnected-(U20-Pad76)")
  (net 228 "unconnected-(U20-Pad77)")
  (net 229 "unconnected-(U20-Pad78)")
  (net 230 "unconnected-(U20-Pad81)")
  (net 231 "unconnected-(U20-Pad82)")
  (net 232 "unconnected-(U20-Pad83)")
  (net 233 "unconnected-(U20-Pad84)")
  (net 234 "unconnected-(U20-Pad85)")
  (net 235 "unconnected-(U20-Pad86)")
  (net 236 "unconnected-(U20-Pad87)")
  (net 237 "unconnected-(U20-Pad89)")
  (net 238 "unconnected-(U20-Pad99)")
  (net 239 "Net-(C38-Pad2)")
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 131.5 -19.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R33" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "VREF-") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(R26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 132.5 -48.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R47" (at -4 0) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(D6-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm" (layer "F.Cu")
    (tedit 5DC5FE75)
    (at 137.5 -57.5 -90)
    (descr "MSOP, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (property "PN" "LT5400BIMS8E-2#PBF ")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN3" (at -4.8 -2.4 180) (layer "F.SilkS"))
    (fp_text value "LT5400-1" (at 0 2.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "" smd roundrect locked (at 0.42 0.47 270) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.42 0.47 270) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.42 -0.47 270) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.42 -0.47 270) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -2.15 -0.975 270) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(RN3-Pad1)") (pinfunction "R1A") (pintype "passive"))
    (pad "2" smd roundrect locked (at -2.15 -0.325 270) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(RN3-Pad1)") (pinfunction "R2A") (pintype "passive"))
    (pad "3" smd roundrect locked (at -2.15 0.325 270) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "VREF7") (pinfunction "R3A") (pintype "passive"))
    (pad "4" smd roundrect locked (at -2.15 0.975 270) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "VREF7") (pinfunction "R4A") (pintype "passive"))
    (pad "5" smd roundrect locked (at 2.15 0.975 270) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDS") (pinfunction "R4B") (pintype "passive"))
    (pad "6" smd roundrect locked (at 2.15 0.325 270) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "VREF+") (pinfunction "R3B") (pintype "passive"))
    (pad "7" smd roundrect locked (at 2.15 -0.325 270) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "VREF-") (pinfunction "R2B") (pintype "passive"))
    (pad "8" smd roundrect locked (at 2.15 -0.975 270) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "VREF+") (pinfunction "R1B") (pintype "passive"))
    (pad "9" smd rect locked (at 0 0 270) (size 1.68 1.88) (layers "F.Cu" "F.Mask")
      (net 2 "GNDS") (pinfunction "EP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 140.7 -39.9)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C22" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 35 "/nvm_pcb_analog_ada/VADC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 165.3 -26.7)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C2" (at -3.2 0) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 26 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 24 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 80.5 -84.96 90)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (property "PN" "ZL201-10G")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J3" (at 4.94 5.4 180) (layer "F.SilkS"))
    (fp_text value "Conn_02x08_Odd_Even" (at 1.27 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "/MS_A2") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/MA_G1") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "/MS_A1") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "/MA_G10") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "/MS_A0") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "/MA_G100") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "/JA_DOUT") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "/JA_C1") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "/JA_DIN") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "/JA_C2") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval locked (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "/COMP") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval locked (at 2.54 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "/JA_C3") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval locked (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 96 "unconnected-(J3-Pad13)") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval locked (at 2.54 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "/JA_CS") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval locked (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval locked (at 2.54 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "/JA_SCK") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 56.9 -68.4 -135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C42" (at -3.323402 -0.070711 45) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.679999 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 225) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 225) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "3VFPGA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 100.5 -57.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "TL071ACDR")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U5" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "TL071" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 191 "unconnected-(U5-Pad1)") (pinfunction "NULL") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(C4-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDS") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 192 "unconnected-(U5-Pad5)") (pinfunction "NULL") (pintype "input"))
    (pad "6" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C5-Pad2)") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 193 "unconnected-(U5-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 83.7 -4.1 90)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP3" (at 0.7 2.5 90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 119 "Net-(TP3-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 39.1 -50.6 45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C41" (at 0.777817 1.767767 45) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.679999 45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 45) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 45) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 45) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "3VFPGA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 108.5 -26.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1201")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R28" (at 1.4 -1.8) (layer "F.SilkS"))
    (fp_text value "1k2" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "Net-(R25-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 45.5 -96.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 17.5 -59)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R88" (at -4 0.1) (layer "F.SilkS"))
    (fp_text value "620R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "Net-(D8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tedit 5905D8F5)
    (at 166.6 -89.05 180)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "PN" "LL4148-GS18")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D2" (at 0 2) (layer "F.SilkS"))
    (fp_text value "LL4148" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "+8V") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -68.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R58" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 160 "Net-(R58-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/MS_A0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 136.5 -27.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "MCP3201-CI/SN")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U10" (at 4.8 0.4) (layer "F.SilkS"))
    (fp_text value "MCP3201" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/nvm_pcb_analog_ada/VREF25") (pinfunction "Vref") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/nvm_pcb_analog_ada/RES_ADC_IN") (pinfunction "IN+") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDS") (pinfunction "IN-") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "Vss") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/nvm_analog_adfpga/FC6") (pinfunction "~{CS}/SHDN") (pintype "input"))
    (pad "6" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/nvm_analog_adfpga/FC5") (pinfunction "Dout") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/nvm_analog_adfpga/FC0") (pinfunction "CLK") (pintype "input"))
    (pad "8" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/nvm_pcb_analog_ada/VADC") (pinfunction "Vdd") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.7mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 142.5 -69.5)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H11" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 98.9 -27.1 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A221JXACW1BC")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C31" (at -2.6 -0.8 180) (layer "F.SilkS"))
    (fp_text value "220p" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 33 "/nvm_pcb_analog_ada/INT_OUT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 30 "/nvm_pcb_analog_ada/INT_IN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_KK-254_AE-6410-10A_1x10_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B)
    (at 166 -97 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-10A example for new part number: 22-27-2101, 10 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "PN" "NS25-W10P")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J2" (at 25.3 2.4) (layer "F.SilkS"))
    (fp_text value "Conn_01x10_Male" (at 11.43 4.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 11.43 -2.22) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.1436781609)
      (net 3 "+24V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 69 "+8V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 39 "+5VA") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 10.16 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 12.7 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 70 "-8V") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 15.24 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 7 "-15V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 17.78 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 8 "-24V") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval locked (at 20.32 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 36 "+5VD") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval locked (at 22.86 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-10A_1x10_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -38.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R73" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 175 "Net-(R73-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/nvm_pcb_analog_ada/COM_OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (layer "F.Cu")
    (tedit 5A0AB76C)
    (at 42.3 -81.3 90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5 hand-soldering")
    (property "PN" "TC77-3.3MCTTR")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U21" (at 0.8 -2.9 180) (layer "F.SilkS"))
    (fp_text value "tc77-SOT23-5" (at 0 2.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.35 -0.95 90) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/nvm_analog_adfpga/TCS") (pinfunction "CS") (pintype "input"))
    (pad "2" smd rect locked (at -1.35 0 90) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pinfunction "VSS") (pintype "power_in"))
    (pad "3" smd rect locked (at -1.35 0.95 90) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/nvm_analog_adfpga/TSCK") (pinfunction "SCK") (pintype "input"))
    (pad "4" smd rect locked (at 1.35 0.95 90) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/nvm_analog_adfpga/TDAT") (pinfunction "SIO") (pintype "bidirectional"))
    (pad "5" smd rect locked (at 1.35 -0.95 90) (size 1.56 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "3VFPGA") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 52.1625 -48.5 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C50" (at 1.4 2.4625 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "3VFPGA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 95 -67.7 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1602")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R2" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "16k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 145 "Net-(R2-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 121.5 -50.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-0R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R32" (at 3.8 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/nvm_pcb_analog_ada/AD_IN") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 151 "Net-(R32-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 25.5 -71.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R77" (at 4 0 90) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 179 "Net-(R77-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/R1B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_IDC:IDC-Header_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EAC9A07)
    (at 111.955 -83.7475 90)
    (descr "Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
    (tags "Through hole vertical IDC box header THT 2x03 2.54mm double row")
    (property "PN" "75869-331LF")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J7" (at 7.3525 5.345 180) (layer "F.SilkS"))
    (fp_text value "Conn_02x03_Odd_Even" (at 1.27 11.18 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.1470588235)
      (net 40 "/nvm_analog_adfpga/TDO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 43 "/nvm_analog_adfpga/TMS") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole circle locked (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "/nvm_analog_adfpga/TDI") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole circle locked (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 115 "3VFPGA") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole circle locked (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "/nvm_analog_adfpga/TCK") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 172 -63.2)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC847.215")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q3" (at 0.1 2.4) (layer "F.SilkS"))
    (fp_text value "BC847" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "Net-(Q2-Pad3)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "Net-(C9-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 120.9625 -20.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C26" (at 3.0625 0) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 87 "Net-(C25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 138.5 -15.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA192ID")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U9" (at 4.2 -3 90) (layer "F.SilkS"))
    (fp_text value "OPA192" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 202 "unconnected-(U9-Pad1)") (pinfunction "VOS") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 150 "Net-(R26-Pad2)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDS") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "Net-(C32-Pad1)") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 206 "unconnected-(U9-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/nvm_pcb_analog_ada/LOC_AD") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "+3.3VA") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 203 "unconnected-(U9-Pad8)") (pinfunction "VOS") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 102.5 -45.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C21" (at -2.6 0.2 180) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 86 "Net-(C21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 138.1 -83.1 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C38" (at 2.828427 0 225) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 135) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 7 "-15V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 135) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 239 "Net-(C38-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 99.5 -45.5 90)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491B106K025AT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C34" (at -0.2 -3 180) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.35 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.5375 0 90) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 86 "Net-(C21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5375 0 90) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 135.2 -94.7 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2402")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R38" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "Net-(Q7-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 144 "Net-(Q8-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tedit 5905D8F5)
    (at 132.5 -51.5 180)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "PN" "TZMB5V6-GS08")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D6" (at 3.6 0.2) (layer "F.SilkS"))
    (fp_text value "5V6" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "Net-(D6-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "Net-(D6-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -64.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R60" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 162 "Net-(R60-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/JA_DOUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric_Pad1.22x1.90mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 56.5 -74.5 -90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "PN" "BLM31A260SPT")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB7" (at -1 -2.6 180) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead_Small" (at 0 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.6625 0 270) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 58 "Net-(C46-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.6625 0 270) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 115 "3VFPGA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 34.5 -71.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R74" (at 4 0 90) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 176 "Net-(R74-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 44 "/RE3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 124.9625 -36.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R19" (at 0 2.3375 180) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "Net-(C17-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -70.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R57" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 158 "Net-(R57-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/MA_G100") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 29.5 -53)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP8" (at -1.6 2.3) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 124 "Net-(TP8-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tedit 5905D8F5)
    (at 138.5 -19.5 180)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "PN" "TZMB5V6-GS08")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D4" (at 3.6 0) (layer "F.SilkS"))
    (fp_text value "5V6" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "+3.3VA") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "Net-(C32-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 166.6 -74.05 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-12R")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "12R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "+6V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(D2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 149.3 -70.4 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3601")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R43" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "3k6" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 54 -84.1 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C44" (at 0.9 -2.4) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 36 "+5VD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 149.3 -80.1 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3601")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R42" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "3k6" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 159.5 -33.5 180)
    (descr "SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "ISO7341CDWR")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U2" (at 2.6 -6.2) (layer "F.SilkS"))
    (fp_text value "ISO7341C" (at 0 6.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -4.65 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "Net-(C2-Pad1)") (pinfunction "VCC1") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -4.65 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C2-Pad2)") (pinfunction "GND1") (pintype "power_in"))
    (pad "3" smd roundrect locked (at -4.65 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "Net-(J1-Pad3)") (pinfunction "INA") (pintype "input"))
    (pad "4" smd roundrect locked (at -4.65 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "Net-(J1-Pad4)") (pinfunction "INB") (pintype "input"))
    (pad "5" smd roundrect locked (at -4.65 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "Net-(J1-Pad5)") (pinfunction "INC") (pintype "input"))
    (pad "6" smd roundrect locked (at -4.65 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 95 "Net-(J1-Pad6)") (pinfunction "OUTD") (pintype "output"))
    (pad "7" smd roundrect locked (at -4.65 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 103 "unconnected-(U2-Pad7)") (pinfunction "EN1") (pintype "input"))
    (pad "8" smd roundrect locked (at -4.65 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "Net-(C2-Pad2)") (pinfunction "GND1") (pintype "passive"))
    (pad "9" smd roundrect locked (at 4.65 4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND2") (pintype "passive"))
    (pad "10" smd roundrect locked (at 4.65 3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 104 "unconnected-(U2-Pad10)") (pinfunction "EN2") (pintype "input"))
    (pad "11" smd roundrect locked (at 4.65 1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/nvm_analog_adfpga/FPGA_TX") (pinfunction "IND") (pintype "input"))
    (pad "12" smd roundrect locked (at 4.65 0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/nvm_analog_adfpga/FPGA_CTRL") (pinfunction "OUTC") (pintype "output"))
    (pad "13" smd roundrect locked (at 4.65 -0.635 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/nvm_analog_adfpga/FPGA_STB") (pinfunction "OUTB") (pintype "output"))
    (pad "14" smd roundrect locked (at 4.65 -1.905 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "/nvm_analog_adfpga/FPGA_RX") (pinfunction "OUTA") (pintype "output"))
    (pad "15" smd roundrect locked (at 4.65 -3.175 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND2") (pintype "power_in"))
    (pad "16" smd roundrect locked (at 4.65 -4.445 180) (size 2.05 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCC2") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 151.5 -66.6 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "Net-(Q5-Pad2)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "/PSWB") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 163.7 -63.4)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC857.215")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q5" (at 0 2.4) (layer "F.SilkS"))
    (fp_text value "BC857" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 140 "Net-(Q5-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "Net-(Q4-Pad1)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 164.5 -50.5)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TGNDA1" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 17.5 -56.1)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R90" (at -4 0) (layer "F.SilkS"))
    (fp_text value "620R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "Net-(D10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 102.5 -50.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C33" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 86 "Net-(C21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 108 "Net-(C33-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric_Pad1.22x1.90mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 131.9 -31.5 180)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "PN" "BLM31A260SPT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB1" (at 3.8 0.6) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead_Small" (at 0 1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.6625 0 180) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 35 "/nvm_pcb_analog_ada/VADC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.6625 0 180) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 34 "+3.3VA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 160 -70.1 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2402")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R16" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 139 "Net-(Q4-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "-8V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 120.55 -70.5 180)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C226K025AT")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C15" (at -5.55 1.2) (layer "F.SilkS"))
    (fp_text value "22u" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.55 0 180) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 39 "+5VA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.55 0 180) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 149.3 -76.9 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3601")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R44" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "3k6" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 156.5 -56.5)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TVR+1" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 51 "VREF+") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 132.5 -44.5 180)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC847.215")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q9" (at 2 -1.4) (layer "F.SilkS"))
    (fp_text value "BC847" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 -0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 114 "Net-(D6-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect locked (at -0.9375 0.95 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "VREF+") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect locked (at 0.9375 0 180) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+15V") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 100.1 -16.3)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "T_CM1" (at -1 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 62 "/nvm_pcb_analog_ada/COM_OUT") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 131.5 -13.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1201")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R26" (at 0.4 -2) (layer "F.SilkS"))
    (fp_text value "1k2" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/nvm_pcb_analog_ada/LOC_AD") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(R26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 41 -70.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C47" (at 3.3 0) (layer "F.SilkS"))
    (fp_text value "2u2" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 117 "Net-(C47-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 109.5 -67.5)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "DG412DYZ")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "U1" (at 4.8 -5.2) (layer "F.SilkS"))
    (fp_text value "DG412xY" (at 0 5.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "/FEN_B") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "3" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "4" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "6" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "7" smd roundrect locked (at -2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 190 "Net-(U1-Pad14)") (pintype "passive"))
    (pad "8" smd roundrect locked (at -2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "/FEN_A") (pintype "input"))
    (pad "9" smd roundrect locked (at 2.475 4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "/FEN_C") (pintype "input"))
    (pad "10" smd roundrect locked (at 2.475 3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(C4-Pad2)") (pintype "passive"))
    (pad "11" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "12" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "+5VA") (pinfunction "VL") (pintype "power_in"))
    (pad "13" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "14" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 190 "Net-(U1-Pad14)") (pintype "passive"))
    (pad "15" smd roundrect locked (at 2.475 -3.175) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "16" smd roundrect locked (at 2.475 -4.445) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 98 "/FEN_B") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -36.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R87" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 189 "Net-(R87-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/nvm_analog_adfpga/FC6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 102.5 -27.1 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A221JXACW1BC")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C28" (at -2.6 -0.8 180) (layer "F.SilkS"))
    (fp_text value "220p" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 33 "/nvm_pcb_analog_ada/INT_OUT") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 30 "/nvm_pcb_analog_ada/INT_IN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 63.7 -38.4)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2401")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R21" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "2k4" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "3VFPGA") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/nvm_pcb_analog_ada/COM_OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 135.1 -34.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C36" (at 0.2 -1.4 270) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 32 "/nvm_pcb_analog_ada/VA1V2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -40.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R72" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 174 "Net-(R72-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/nvm_analog_adfpga/FC1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 120.9625 -22.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C20" (at 3.0625 -0.2) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 85 "Net-(C19-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 112.5375 -12.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C16" (at 0 1.6) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 7 "-15V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 4 "+15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 22.5 -56.5)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "PN" "KP-2012YD")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D10" (at 0 2) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 135 "Net-(D10-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 115 "3VFPGA") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 91.5 -100.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at -6.1 0.3) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Diode_SMD:D_SOD-123" (layer "F.Cu")
    (tedit 58645DC7)
    (at 123.7 -11.8)
    (descr "SOD-123")
    (tags "SOD-123")
    (property "PN" "BAT42W-7-F")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D5" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "BAT42" (at 0 2.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect (at -1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect (at 1.65 0) (size 0.9 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "Net-(C32-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 32 -47.5 90)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "TP10" (at -2.2 -0.9 180) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0 0 90) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 126 "Net-(TP10-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 103 -2.5)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP1" (at 1.2 -2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -66.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R59" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 102 "Net-(R59-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 161 "/AZSW") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 169.6 -74.05 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1203")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R11" (at 0.85 -2 90) (layer "F.SilkS"))
    (fp_text value "120k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -22.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R79" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 181 "Net-(R79-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/nvm_analog_adfpga/FPGA_RX") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 39.5 -77.1 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-0R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R52" (at -3.8 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "Net-(C47-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "3VFPGA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -32.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R85" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 187 "Net-(R85-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/nvm_analog_adfpga/FC0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 95 -73.2 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1602")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R1" (at 0 1.8 -270) (layer "F.SilkS"))
    (fp_text value "16k" (at 0 1.7 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "Net-(R1-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "/AMP_OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 134.8 -97.7)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC847.215")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q8" (at 0 -2.4) (layer "F.SilkS"))
    (fp_text value "BC847" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "Net-(Q8-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 144 "Net-(Q8-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 136.5 -31.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C27" (at -3.2 -0.6) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 35 "/nvm_pcb_analog_ada/VADC") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 120.9625 -35.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C18" (at 2.2625 -0.2 90) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 56 "Net-(C17-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 167.7 -63.3)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC847.215")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q2" (at -0.6 2.4) (layer "F.SilkS"))
    (fp_text value "BC847" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "Net-(Q2-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "Net-(Q2-Pad3)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 144.5 -18 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R30" (at 0.1 -2.6 180) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/nvm_pcb_analog_ada/RES_ADC_IN") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/nvm_pcb_analog_ada/LOC_AD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 56.5 -79.1 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C45" (at 1.2 2.4 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 116 "Net-(C45-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 110.5 -53.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C6" (at -2.8 -0.2) (layer "F.SilkS"))
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 66 "/nvm_pcb_analog_ada/AD_IN") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 29 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 120.9625 -17.5 180)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491B106K025AT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C25" (at 0 -2.35) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.5375 0 180) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5375 0 180) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 87 "Net-(C25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 167.6 -83.05 -90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "PN" "BCP56-16.115")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q1" (at 5.4 -2.8 180) (layer "F.SilkS"))
    (fp_text value "BCP56" (at 0 4.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.15 -2.3 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(Q1-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect locked (at -3.15 0 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "+8V") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect locked (at -3.15 2.3 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "Net-(D2-Pad2)") (pinfunction "E") (pintype "passive"))
    (pad "4" smd rect locked (at 3.15 0 270) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "+8V") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm" (layer "F.Cu")
    (tedit 5DC5FE75)
    (at 120.5 -54.5 180)
    (descr "MSOP, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (property "PN" "LT5400BIMS8E-1#PBF ")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN1" (at -4.6 -1) (layer "F.SilkS"))
    (fp_text value "LT5400-2" (at 0 2.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect locked (at 0.42 0.47 180) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.42 -0.47 180) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.42 0.47 180) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.42 -0.47 180) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -2.15 -0.975 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 151 "Net-(R32-Pad2)") (pinfunction "R1A") (pintype "passive"))
    (pad "2" smd roundrect locked (at -2.15 -0.325 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 151 "Net-(R32-Pad2)") (pinfunction "R2A") (pintype "passive"))
    (pad "3" smd roundrect locked (at -2.15 0.325 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "VREF+") (pinfunction "R3A") (pintype "passive"))
    (pad "4" smd roundrect locked (at -2.15 0.975 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "VREF-") (pinfunction "R4A") (pintype "passive"))
    (pad "5" smd roundrect locked (at 2.15 0.975 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(RN1-Pad5)") (pinfunction "R4B") (pintype "passive"))
    (pad "6" smd roundrect locked (at 2.15 0.325 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(RN1-Pad6)") (pinfunction "R3B") (pintype "passive"))
    (pad "7" smd roundrect locked (at 2.15 -0.325 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(RN1-Pad7)") (pinfunction "R2B") (pintype "passive"))
    (pad "8" smd roundrect locked (at 2.15 -0.975 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/nvm_pcb_analog_ada/AD_IN") (pinfunction "R1B") (pintype "passive"))
    (pad "9" smd rect locked (at 0 0 180) (size 1.68 1.88) (layers "F.Cu" "F.Mask")
      (net 23 "GNDA") (pinfunction "EP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 86.5 -1.7 90)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP4" (at 0.7 2.5 90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 120 "Net-(TP4-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 138.5375 -21.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C32" (at 3.3625 0) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 130 "Net-(C32-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 34 "+3.3VA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 141.1 -37.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R37" (at -3.8 0.6) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/nvm_analog_adfpga/FC9") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/nvm_pcb_analog_ada/VADC") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 105.5 -32.5)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "T_INI1" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 30 "/nvm_pcb_analog_ada/INT_IN") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 106.5 -17.3 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R22" (at -4 0.2 90) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "Net-(R18-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 151.5 -64.1 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "Net-(Q2-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "/PSWB") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 28.5 -97.5 -90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "PN" "ZL201-10G")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J5" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 44 "/RE3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 45 "/RE4") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 46 "/R1A") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 47 "/R1B") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 48 "/R2A") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 49 "/R2B") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "+5VD") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "j_lib:logo_rpg7x9" (layer "F.Cu")
    (tedit 61CE1C18)
    (at 163.6 -7.6)
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr board_only exclude_from_pos_files)
    (fp_text reference "LOGO1" (at 0.956014 12.7) (layer "F.SilkS") hide)
    (fp_text value "logo_generic" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 109.5 -43.5 -90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "SN74LV4053AD")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U11" (at 0 -5.9 -270) (layer "F.SilkS"))
    (fp_text value "LV4053" (at 0 5.9 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(FB4-Pad1)") (pinfunction "B1") (pintype "bidirectional"))
    (pad "2" smd roundrect locked (at -2.475 -3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(FB3-Pad2)") (pinfunction "B0") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(FB4-Pad1)") (pinfunction "C1") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(RN1-Pad5)") (pinfunction "C") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(FB3-Pad2)") (pinfunction "C0") (pintype "bidirectional"))
    (pad "6" smd roundrect locked (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "INH") (pintype "input"))
    (pad "7" smd roundrect locked (at -2.475 3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 108 "Net-(C33-Pad2)") (pinfunction "VEE") (pintype "power_in"))
    (pad "8" smd roundrect locked (at -2.475 4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "VSS") (pintype "power_in"))
    (pad "9" smd roundrect locked (at 2.475 4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/nvm_analog_adfpga/FC3") (pinfunction "S3") (pintype "input"))
    (pad "10" smd roundrect locked (at 2.475 3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/nvm_analog_adfpga/FC2") (pinfunction "S2") (pintype "input"))
    (pad "11" smd roundrect locked (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/nvm_analog_adfpga/FC1") (pinfunction "S1") (pintype "input"))
    (pad "12" smd roundrect locked (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "Net-(FB3-Pad2)") (pinfunction "A0") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "Net-(FB4-Pad1)") (pinfunction "A1") (pintype "bidirectional"))
    (pad "14" smd roundrect locked (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(RN1-Pad6)") (pinfunction "A") (pintype "bidirectional"))
    (pad "15" smd roundrect locked (at 2.475 -3.175 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(RN1-Pad7)") (pinfunction "B") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at 2.475 -4.445 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "Net-(C21-Pad1)") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -54.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R65" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 167 "Net-(R65-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/JA_CS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric_Pad1.22x1.90mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 98.5 -51.5 90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "PN" "BLM31A260SPT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB2" (at -3 -2.4 180) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead_Small" (at 0 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.6625 0 90) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 86 "Net-(C21-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.6625 0 90) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 39 "+5VA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 103.5 -17.3 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R18" (at 4 -0.2 90) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/nvm_pcb_analog_ada/COM_OUT") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "Net-(R18-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 54.1625 -72.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C51" (at -2.6 0.5375 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "3VFPGA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 40.8625 -73.7 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "DNP")
    (attr smd)
    (fp_text reference "U19" (at -0.4 -2.5625 180) (layer "F.SilkS"))
    (fp_text value "DNP-MCP1700-12" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(C47-Pad2)") (pinfunction "VO") (pintype "power_out"))
    (pad "3" smd roundrect locked (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric_Pad1.22x1.90mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 108.5 -36.5 90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "PN" "BLM31A260SPT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB3" (at 0.6 -3.2 180) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead_Small" (at 0 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.6625 0 90) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 30 "/nvm_pcb_analog_ada/INT_IN") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.6625 0 90) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 136 "Net-(FB3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 39.1 -68.4 -45)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C40" (at -0.919239 2.474874 225) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.679999 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 315) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 315) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "3VFPGA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 36.1625 -54.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C52" (at 0 1.8) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "3VFPGA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 91.5 -74.5)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "PN" "ZL201-10G")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Male" (at 0 9.95) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 "VREF7") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 101 "/AMP_OUT") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GNDS") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 142.5 -44.5)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC857.215")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q10" (at 1.4 2.8) (layer "F.SilkS"))
    (fp_text value "BC857" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 134 "Net-(D7-Pad2)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect locked (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "VREF-") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect locked (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "-15V") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:TQFP-100_14x14mm_P0.5mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 48.1625 -59.5)
    (descr "TQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TQFP QFP")
    (property "PN" "XO21200HC4TG100C")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U20" (at 10.1375 -0.8) (layer "F.SilkS"))
    (fp_text value "LCMXO2-1200xx-xTG100" (at 0 9.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -7.6625 -6) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 176 "Net-(R74-Pad1)") (pinfunction "PL2C/BANK3/T/L_GPLLT_IN") (pintype "bidirectional"))
    (pad "2" smd roundrect locked (at -7.6625 -5.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 177 "Net-(R75-Pad1)") (pinfunction "PL2D/BANK3/C/L_GPLLC_IN") (pintype "bidirectional"))
    (pad "3" smd roundrect locked (at -7.6625 -5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 178 "Net-(R76-Pad1)") (pinfunction "PL3A/BANK3/T/PCLKT3_2") (pintype "bidirectional"))
    (pad "4" smd roundrect locked (at -7.6625 -4.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 214 "unconnected-(U20-Pad4)") (pinfunction "PL3B/BANK3/C/PCLKC3_2") (pintype "bidirectional"))
    (pad "5" smd roundrect locked (at -7.6625 -4) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCCIO3") (pintype "power_in"))
    (pad "6" smd roundrect locked (at -7.6625 -3.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd roundrect locked (at -7.6625 -3) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 215 "unconnected-(U20-Pad7)") (pinfunction "PL3C/BANK3/T") (pintype "bidirectional"))
    (pad "8" smd roundrect locked (at -7.6625 -2.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 179 "Net-(R77-Pad1)") (pinfunction "PL3D/BANK3/C") (pintype "bidirectional"))
    (pad "9" smd roundrect locked (at -7.6625 -2) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 180 "Net-(R78-Pad1)") (pinfunction "PL4A/BANK3/T") (pintype "bidirectional"))
    (pad "10" smd roundrect locked (at -7.6625 -1.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 182 "Net-(R80-Pad1)") (pinfunction "PL4B/BANK3/C") (pintype "bidirectional"))
    (pad "11" smd roundrect locked (at -7.6625 -1) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCCIO3") (pintype "power_in"))
    (pad "12" smd roundrect locked (at -7.6625 -0.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 146 "Net-(D9-Pad2)") (pinfunction "PL5A/BANK3/T/PCLKT3_1") (pintype "bidirectional"))
    (pad "13" smd roundrect locked (at -7.6625 0) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "Net-(D8-Pad2)") (pinfunction "PL5B/BANK3/C/PCLKC3_1") (pintype "bidirectional"))
    (pad "14" smd roundrect locked (at -7.6625 0.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 216 "unconnected-(U20-Pad14)") (pinfunction "PL5C/BANK3/T") (pintype "bidirectional"))
    (pad "15" smd roundrect locked (at -7.6625 1) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "Net-(TP5-Pad1)") (pinfunction "PL5D/BANK3/C") (pintype "bidirectional"))
    (pad "16" smd roundrect locked (at -7.6625 1.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 122 "Net-(TP6-Pad1)") (pinfunction "PL8A/BANK3/T") (pintype "bidirectional"))
    (pad "17" smd roundrect locked (at -7.6625 2) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 123 "Net-(TP7-Pad1)") (pinfunction "PL8B/BANK3/C") (pintype "bidirectional"))
    (pad "18" smd roundrect locked (at -7.6625 2.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "Net-(TP8-Pad1)") (pinfunction "PL8C/BANK3/T") (pintype "bidirectional"))
    (pad "19" smd roundrect locked (at -7.6625 3) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 125 "Net-(TP9-Pad1)") (pinfunction "PL8D/BANK3/C") (pintype "bidirectional"))
    (pad "20" smd roundrect locked (at -7.6625 3.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 126 "Net-(TP10-Pad1)") (pinfunction "PL9A/BANK3/T/PCLKT3_0") (pintype "bidirectional"))
    (pad "21" smd roundrect locked (at -7.6625 4) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 217 "unconnected-(U20-Pad21)") (pinfunction "PL9B/BANK3/C/PCLKC3_0") (pintype "bidirectional"))
    (pad "22" smd roundrect locked (at -7.6625 4.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "23" smd roundrect locked (at -7.6625 5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCCIO3") (pintype "power_in"))
    (pad "24" smd roundrect locked (at -7.6625 5.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "Net-(TP11-Pad1)") (pinfunction "PL10C/BANK3/T") (pintype "bidirectional"))
    (pad "25" smd roundrect locked (at -7.6625 6) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 128 "Net-(TP12-Pad1)") (pinfunction "PL10D/BANK3/C") (pintype "bidirectional"))
    (pad "26" smd roundrect locked (at -6 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCCIO2") (pintype "power_in"))
    (pad "27" smd roundrect locked (at -5.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 118 "Net-(TP2-Pad1)") (pinfunction "PB4C/BANK2/T/CSSPIN") (pintype "bidirectional"))
    (pad "28" smd roundrect locked (at -5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "Net-(TP3-Pad1)") (pinfunction "PB4D/BANK2/C") (pintype "bidirectional"))
    (pad "29" smd roundrect locked (at -4.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "Net-(TP4-Pad1)") (pinfunction "PB6A/BANK2/T") (pintype "bidirectional"))
    (pad "30" smd roundrect locked (at -4 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 218 "unconnected-(U20-Pad30)") (pinfunction "PB6B/BANK2/C") (pintype "bidirectional"))
    (pad "31" smd roundrect locked (at -3.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 219 "unconnected-(U20-Pad31)") (pinfunction "PB6C/BANK2/T/MCLK/CCLK") (pintype "bidirectional"))
    (pad "32" smd roundrect locked (at -3 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 220 "unconnected-(U20-Pad32)") (pinfunction "PB6D/BANK2/C/SO/SPISO") (pintype "bidirectional"))
    (pad "33" smd roundrect locked (at -2.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "34" smd roundrect locked (at -2 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 221 "unconnected-(U20-Pad34)") (pinfunction "PB9A/BANK2/T/PCLKT2_0") (pintype "bidirectional"))
    (pad "35" smd roundrect locked (at -1.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 181 "Net-(R79-Pad1)") (pinfunction "PB9B/BANK2/C/PCLKC2_0") (pintype "bidirectional"))
    (pad "36" smd roundrect locked (at -1 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 183 "Net-(R81-Pad1)") (pinfunction "PB11C/BANK2/T") (pintype "bidirectional"))
    (pad "37" smd roundrect locked (at -0.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 184 "Net-(R82-Pad1)") (pinfunction "PB11D/BANK2/C") (pintype "bidirectional"))
    (pad "38" smd roundrect locked (at 0 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 185 "Net-(R83-Pad1)") (pinfunction "PB11A/BANK2/T/PCLKT2_1") (pintype "bidirectional"))
    (pad "39" smd roundrect locked (at 0.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 186 "Net-(R84-Pad1)") (pinfunction "PB11B/BANK2/C/PCLKC2_1") (pintype "bidirectional"))
    (pad "40" smd roundrect locked (at 1 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 187 "Net-(R85-Pad1)") (pinfunction "PB15A/BANK2/T") (pintype "bidirectional"))
    (pad "41" smd roundrect locked (at 1.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 188 "Net-(R86-Pad1)") (pinfunction "PB15B/BANK2/C") (pintype "bidirectional"))
    (pad "42" smd roundrect locked (at 2 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 189 "Net-(R87-Pad1)") (pinfunction "PB18A/BANK2/T") (pintype "bidirectional"))
    (pad "43" smd roundrect locked (at 2.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 222 "unconnected-(U20-Pad43)") (pinfunction "PB18B/BANK2/C") (pintype "bidirectional"))
    (pad "44" smd roundrect locked (at 3 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "45" smd roundrect locked (at 3.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 223 "unconnected-(U20-Pad45)") (pinfunction "PB18C/BANK2/T") (pintype "bidirectional"))
    (pad "46" smd roundrect locked (at 4 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCCIO2") (pintype "power_in"))
    (pad "47" smd roundrect locked (at 4.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 224 "unconnected-(U20-Pad47)") (pinfunction "PB18D/BANK2/C") (pintype "bidirectional"))
    (pad "48" smd roundrect locked (at 5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 225 "unconnected-(U20-Pad48)") (pinfunction "PB20C/BANK2/T/SN") (pintype "bidirectional"))
    (pad "49" smd roundrect locked (at 5.5 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 226 "unconnected-(U20-Pad49)") (pinfunction "PB20D/BANK2/C/SI/SISPI") (pintype "bidirectional"))
    (pad "50" smd roundrect locked (at 6 7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(C47-Pad2)") (pinfunction "VCC") (pintype "power_in"))
    (pad "51" smd roundrect locked (at 7.6625 6) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 175 "Net-(R73-Pad1)") (pinfunction "PR10D/BANK1/C/DQ1") (pintype "bidirectional"))
    (pad "52" smd roundrect locked (at 7.6625 5.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 174 "Net-(R72-Pad1)") (pinfunction "PR10C/BANK1/T/DQ1") (pintype "bidirectional"))
    (pad "53" smd roundrect locked (at 7.6625 5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 173 "Net-(R71-Pad1)") (pinfunction "PR9D/BANK1/C/DQ1") (pintype "bidirectional"))
    (pad "54" smd roundrect locked (at 7.6625 4.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 172 "Net-(R70-Pad1)") (pinfunction "PR9C/BANK1/T/DQ1") (pintype "bidirectional"))
    (pad "55" smd roundrect locked (at 7.6625 4) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCCIO1") (pintype "power_in"))
    (pad "56" smd roundrect locked (at 7.6625 3.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "57" smd roundrect locked (at 7.6625 3) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 171 "Net-(R69-Pad1)") (pinfunction "PR9B/BANK1/C/DQ1") (pintype "bidirectional"))
    (pad "58" smd roundrect locked (at 7.6625 2.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 170 "Net-(R68-Pad1)") (pinfunction "PR9A/BANK1/T/DQ1") (pintype "bidirectional"))
    (pad "59" smd roundrect locked (at 7.6625 2) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 169 "Net-(R67-Pad1)") (pinfunction "PR8D/BANK1/C/DQ1") (pintype "bidirectional"))
    (pad "60" smd roundrect locked (at 7.6625 1.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 168 "Net-(R66-Pad1)") (pinfunction "PR8C/BANK1/T/DQ1") (pintype "bidirectional"))
    (pad "61" smd roundrect locked (at 7.6625 1) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 167 "Net-(R65-Pad1)") (pinfunction "PR8A/BANK1/DQS1") (pintype "bidirectional"))
    (pad "62" smd roundrect locked (at 7.6625 0.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 166 "Net-(R64-Pad1)") (pinfunction "PR5D/BANK1/C/PCLKC1_0/DQ0") (pintype "bidirectional"))
    (pad "63" smd roundrect locked (at 7.6625 0) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 165 "Net-(R63-Pad1)") (pinfunction "PR5C/BANK1/T/PCLKT1_0/DQ0") (pintype "bidirectional"))
    (pad "64" smd roundrect locked (at 7.6625 -0.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 164 "Net-(R62-Pad1)") (pinfunction "PR5B/BANK1/C/DQS0N") (pintype "bidirectional"))
    (pad "65" smd roundrect locked (at 7.6625 -1) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 163 "Net-(R61-Pad1)") (pinfunction "PR5A/BANK1/T/DQS0") (pintype "bidirectional"))
    (pad "66" smd roundrect locked (at 7.6625 -1.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 162 "Net-(R60-Pad1)") (pinfunction "PR4D/BANK1/C/DQ0") (pintype "bidirectional"))
    (pad "67" smd roundrect locked (at 7.6625 -2) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "Net-(R59-Pad1)") (pinfunction "PR4C/BANK1/T/DQ0") (pintype "bidirectional"))
    (pad "68" smd roundrect locked (at 7.6625 -2.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 160 "Net-(R58-Pad1)") (pinfunction "PR4B/BANK1/C/DQ0") (pintype "bidirectional"))
    (pad "69" smd roundrect locked (at 7.6625 -3) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 158 "Net-(R57-Pad1)") (pinfunction "PR4A/BANK1/T/DQ0") (pintype "bidirectional"))
    (pad "70" smd roundrect locked (at 7.6625 -3.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 157 "Net-(R56-Pad1)") (pinfunction "PR3B/BANK1/C/DQ0") (pintype "bidirectional"))
    (pad "71" smd roundrect locked (at 7.6625 -4) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 156 "Net-(R55-Pad1)") (pinfunction "PR3A/BANK1/T/DQ0") (pintype "bidirectional"))
    (pad "72" smd roundrect locked (at 7.6625 -4.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "73" smd roundrect locked (at 7.6625 -5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCCIO1") (pintype "power_in"))
    (pad "74" smd roundrect locked (at 7.6625 -5.5) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 155 "Net-(R54-Pad1)") (pinfunction "PR2B/BANK1/C/DQ0") (pintype "bidirectional"))
    (pad "75" smd roundrect locked (at 7.6625 -6) (size 1.475 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 154 "Net-(R53-Pad1)") (pinfunction "PR2A/BANK1/T/DQ0") (pintype "bidirectional"))
    (pad "76" smd roundrect locked (at 6 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 227 "unconnected-(U20-Pad76)") (pinfunction "PT17D/BANK0/C/DONE") (pintype "bidirectional"))
    (pad "77" smd roundrect locked (at 5.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 228 "unconnected-(U20-Pad77)") (pinfunction "PT17C/BANK0/T/INITN") (pintype "bidirectional"))
    (pad "78" smd roundrect locked (at 5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 229 "unconnected-(U20-Pad78)") (pinfunction "PT16C/BANK0") (pintype "bidirectional"))
    (pad "79" smd roundrect locked (at 4.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "80" smd roundrect locked (at 4 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCCIO0") (pintype "power_in"))
    (pad "81" smd roundrect locked (at 3.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 230 "unconnected-(U20-Pad81)") (pinfunction "PT15D/BANK0/C/PROGRAMN") (pintype "bidirectional"))
    (pad "82" smd roundrect locked (at 3 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 231 "unconnected-(U20-Pad82)") (pinfunction "PT15C/BANK0/T/JTAGENB") (pintype "bidirectional"))
    (pad "83" smd roundrect locked (at 2.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 232 "unconnected-(U20-Pad83)") (pinfunction "PT15B/BANK0/C/LVDS") (pintype "bidirectional"))
    (pad "84" smd roundrect locked (at 2 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 233 "unconnected-(U20-Pad84)") (pinfunction "PT15A/BANK0/T/LVDS") (pintype "bidirectional"))
    (pad "85" smd roundrect locked (at 1.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 234 "unconnected-(U20-Pad85)") (pinfunction "PT12D/BANK0/C/SDA/PCLKC0_0") (pintype "bidirectional"))
    (pad "86" smd roundrect locked (at 1 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 235 "unconnected-(U20-Pad86)") (pinfunction "PT12C/BANK0/T/SCL/PCLKT0_0") (pintype "bidirectional"))
    (pad "87" smd roundrect locked (at 0.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 236 "unconnected-(U20-Pad87)") (pinfunction "PT12B/BANK0/C/PCLKC0_1/LVDS") (pintype "bidirectional"))
    (pad "88" smd roundrect locked (at 0 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 112 "/nvm_analog_adfpga/FPGA_CLK") (pinfunction "PT12A/BANK0/T/PCLKT0_1/LVDS") (pintype "bidirectional"))
    (pad "89" smd roundrect locked (at -0.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 237 "unconnected-(U20-Pad89)") (pinfunction "NC") (pintype "no_connect"))
    (pad "90" smd roundrect locked (at -1 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 43 "/nvm_analog_adfpga/TMS") (pinfunction "PT11D/BANK0/C/TMS") (pintype "bidirectional"))
    (pad "91" smd roundrect locked (at -1.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/nvm_analog_adfpga/TCK") (pinfunction "PT11C/BANK0/T/TCK") (pintype "bidirectional"))
    (pad "92" smd roundrect locked (at -2 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "93" smd roundrect locked (at -2.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 115 "3VFPGA") (pinfunction "VCCIO0") (pintype "power_in"))
    (pad "94" smd roundrect locked (at -3 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 41 "/nvm_analog_adfpga/TDI") (pinfunction "PT10D/BANK0/C/TDI") (pintype "bidirectional"))
    (pad "95" smd roundrect locked (at -3.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/nvm_analog_adfpga/TDO") (pinfunction "PT10C/BANK0/T/TDO") (pintype "bidirectional"))
    (pad "96" smd roundrect locked (at -4 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/nvm_analog_adfpga/TDAT") (pinfunction "PT10B/BANK0/C/LVDS") (pintype "bidirectional"))
    (pad "97" smd roundrect locked (at -4.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "/nvm_analog_adfpga/TSCK") (pinfunction "PT10A/BANK0/T/LVDS") (pintype "bidirectional"))
    (pad "98" smd roundrect locked (at -5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 79 "/nvm_analog_adfpga/TCS") (pinfunction "PT9B/BANK0/C/LVDS") (pintype "bidirectional"))
    (pad "99" smd roundrect locked (at -5.5 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 238 "unconnected-(U20-Pad99)") (pinfunction "PT9A/BANK0/T/LVDS") (pintype "bidirectional"))
    (pad "100" smd roundrect locked (at -6 -7.6625) (size 0.3 1.475) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 117 "Net-(C47-Pad2)") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-100_14x14mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 144.5 -13.5)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "T_LADC1" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 71 "/nvm_pcb_analog_ada/LOC_AD") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 112.5 -30.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA140AIDR")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U7" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "OPA140" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 196 "unconnected-(U7-Pad1)") (pinfunction "VOS") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/nvm_pcb_analog_ada/INT_IN") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDS") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "Net-(C23-Pad2)") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 197 "unconnected-(U7-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 159 "Net-(R25-Pad1)") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "Net-(C17-Pad1)") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 198 "unconnected-(U7-Pad8)") (pinfunction "VOS") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 149.3 -73.7 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3601")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R41" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "3k6" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "Net-(C38-Pad2)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 138.5 -11.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C8201")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R35" (at 0 2) (layer "F.SilkS"))
    (fp_text value "8k2" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "-15V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 130 "Net-(C32-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 164.5 -56.5)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TVR-1" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 52 "VREF-") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 22.5 -71.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R78" (at 4 0 270) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 180 "Net-(R78-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/R2A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -44.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R70" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 172 "Net-(R70-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/nvm_analog_adfpga/FC3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm" (layer "F.Cu")
    (tedit 5DC5FE75)
    (at 120.5 -46.5 180)
    (descr "MSOP, 8 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/4440fb.pdf#page=13), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "MSOP SO")
    (property "PN" "LT5400BIMS8E-1#PBF ")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "RN2" (at -4.6 -1) (layer "F.SilkS"))
    (fp_text value "LT5400-2" (at 0 2.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect locked (at -0.42 0.47 180) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at -0.42 -0.47 180) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.42 0.47 180) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect locked (at 0.42 -0.47 180) (size 0.68 0.76) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd roundrect locked (at -2.15 -0.975 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 152 "Net-(R36-Pad2)") (pinfunction "R1A") (pintype "passive"))
    (pad "2" smd roundrect locked (at -2.15 -0.325 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 152 "Net-(R36-Pad2)") (pinfunction "R2A") (pintype "passive"))
    (pad "3" smd roundrect locked (at -2.15 0.325 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 51 "VREF+") (pinfunction "R3A") (pintype "passive"))
    (pad "4" smd roundrect locked (at -2.15 0.975 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 52 "VREF-") (pinfunction "R4A") (pintype "passive"))
    (pad "5" smd roundrect locked (at 2.15 0.975 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 72 "Net-(RN1-Pad5)") (pinfunction "R4B") (pintype "passive"))
    (pad "6" smd roundrect locked (at 2.15 0.325 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "Net-(RN1-Pad6)") (pinfunction "R3B") (pintype "passive"))
    (pad "7" smd roundrect locked (at 2.15 -0.325 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "Net-(RN1-Pad7)") (pinfunction "R2B") (pintype "passive"))
    (pad "8" smd roundrect locked (at 2.15 -0.975 180) (size 1.45 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/nvm_pcb_analog_ada/AD_IN") (pinfunction "R1B") (pintype "passive"))
    (pad "9" smd rect locked (at 0 0 180) (size 1.68 1.88) (layers "F.Cu" "F.Mask")
      (net 23 "GNDA") (pinfunction "EP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-8-1EP_3x3mm_P0.65mm_EP1.68x1.88mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 137.5 -43.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C8201")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R51" (at 2.8 1 180) (layer "F.SilkS"))
    (fp_text value "8k2" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GNDS") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "VREF-") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 120.5 -64 180)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C226K025AT")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C13" (at -5.4 -0.9) (layer "F.SilkS"))
    (fp_text value "22u" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.55 0 180) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.55 0 180) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 132.5 -57.5 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA202IDR")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U16" (at -4.4 0.2 180) (layer "F.SilkS"))
    (fp_text value "OPA202" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 208 "unconnected-(U16-Pad1)") (pinfunction "VOS") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "VREF7") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "Net-(C39-Pad1)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 209 "unconnected-(U16-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect locked (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 129 "Net-(D6-Pad2)") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 210 "unconnected-(U16-Pad8)") (pinfunction "VOS") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 36.1625 -63.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C48" (at -3.4625 -0.4) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "3VFPGA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 37.5 -42.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H14" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -60.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R62" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 164 "Net-(R62-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "/JA_DIN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 92 -31.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H10" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.7mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 128.5 -91.5)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H12" (at 0 -3.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask))
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 22.5 -59)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "PN" "KP-2012YD")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D8" (at 2.8 -1.1) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 132 "Net-(D8-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 133 "Net-(D8-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 142.5 -48.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R48" (at -2 -1.8) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "-15V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "Net-(D7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 17.5 -62)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R89" (at -4 -0.1) (layer "F.SilkS"))
    (fp_text value "620R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "Net-(D9-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tedit 5905D8F5)
    (at 142.5 -51.5 180)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "PN" "TZMB5V6-GS08")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D7" (at -0.4 1.6) (layer "F.SilkS"))
    (fp_text value "5V6" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "Net-(D7-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.75 0 180) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "Net-(D7-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 172.5 -2.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 86.9 -50.9)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H13" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 132 -65.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-12R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R50" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "12R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "Net-(C39-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 114.5 -26.6 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R25" (at -3.2 0.4 180) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 159 "Net-(R25-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 149 "Net-(R25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 170.2 -69.9)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C2402")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R7" (at 0.8 2) (layer "F.SilkS"))
    (fp_text value "24k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "+8V") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 138 "Net-(Q2-Pad3)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -62.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R61" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 163 "Net-(R61-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "/PSWA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 26.5 -58)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP5" (at 1.8 -2.1) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 121 "Net-(TP5-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 157.6 -83.05 -90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "PN" "BCP53-16,115")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q6" (at 3.4 3.8 180) (layer "F.SilkS"))
    (fp_text value "BCP53" (at 0 4.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -3.15 -2.3 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "Net-(Q6-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect locked (at -3.15 0 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "-8V") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect locked (at -3.15 2.3 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(D3-Pad1)") (pinfunction "E") (pintype "passive"))
    (pad "4" smd rect locked (at 3.15 0 270) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "-8V") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 131.5 -16.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R31" (at 3.8 -1.2) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 150 "Net-(R26-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/nvm_pcb_analog_ada/INT_OUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 120.9625 -29.7 180)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491B106K025AT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C23" (at 2.8625 0 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.5375 0 180) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5375 0 180) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 53 "Net-(C23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 130.5 -27.5 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C29" (at 0 -1.68 90) (layer "F.SilkS"))
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GNDS") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 90) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 55 "/nvm_pcb_analog_ada/RES_ADC_IN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric_Pad1.22x1.90mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 107.5 -50.5)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "PN" "BLM31A260SPT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB5" (at 0 -1.4) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead_Small" (at 0 1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.6625 0) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 108 "Net-(C33-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.6625 0) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 171.345 -19.055 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6200")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "620R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(C2-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "Net-(D1-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 106.5 -53.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "VJ0805A102JXACW1BC")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C7" (at 1.6 1.4) (layer "F.SilkS"))
    (fp_text value "1n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 29 "Net-(C6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 2 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -76.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R54" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 155 "Net-(R54-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "/MS_A2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 91.5 -2.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 112.5 -16.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "LM311DR")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U6" (at 5 1.6) (layer "F.SilkS"))
    (fp_text value "LM311" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "passive"))
    (pad "2" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 148 "Net-(R18-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/nvm_pcb_analog_ada/INT_OUT") (pinfunction "-") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 194 "unconnected-(U6-Pad5)") (pinfunction "BAL") (pintype "input"))
    (pad "6" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 195 "unconnected-(U6-Pad6)") (pinfunction "STRB") (pintype "input"))
    (pad "7" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/nvm_pcb_analog_ada/COM_OUT") (pintype "open_collector"))
    (pad "8" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 70.5 -97.5 -90)
    (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x08 2.54mm single row")
    (property "PN" "ZL201-10G")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 0 20.11 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.89) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "+24V") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "+15V") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "+6V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "+5VA") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "-6V") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "-15V") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "-24V") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 109.5 -57.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA140AIDR")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U4" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "OPA140" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "unconnected-(U4-Pad1)") (pinfunction "NULL") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/nvm_pcb_analog_ada/AD_IN") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(C6-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 106 "unconnected-(U4-Pad5)") (pinfunction "NULL") (pintype "input"))
    (pad "6" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/nvm_pcb_analog_ada/AD_IN") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "unconnected-(U4-Pad8)") (pinfunction "NC") (pintype "no_connect"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:MSOP-10_3x3mm_P0.5mm" (layer "F.Cu")
    (tedit 5A02F25C)
    (at 140.1 -34.5)
    (descr "10-Lead Plastic Micro Small Outline Package (MS) [MSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.5")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "DNP")
    (attr smd)
    (fp_text reference "U12" (at 4.6 0) (layer "F.SilkS"))
    (fp_text value "DNP-MCP33151" (at 0 2.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -2.2 -1) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/nvm_pcb_analog_ada/VREF25") (pinfunction "VREF") (pintype "input"))
    (pad "2" smd rect locked (at -2.2 -0.5) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/nvm_pcb_analog_ada/VA1V2") (pinfunction "AVDD") (pintype "input"))
    (pad "3" smd rect locked (at -2.2 0) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/nvm_pcb_analog_ada/RES_ADC_IN") (pinfunction "IN+") (pintype "input"))
    (pad "4" smd rect locked (at -2.2 0.5) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GNDS") (pinfunction "IN-") (pintype "input"))
    (pad "5" smd rect locked (at -2.2 1) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pinfunction "GND") (pintype "input"))
    (pad "6" smd rect locked (at 2.2 1) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/nvm_analog_adfpga/FC6") (pinfunction "CNVST") (pintype "input"))
    (pad "7" smd rect locked (at 2.2 0.5) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/nvm_analog_adfpga/FC5") (pinfunction "SDO") (pintype "input"))
    (pad "8" smd rect locked (at 2.2 0) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/nvm_analog_adfpga/FC0") (pinfunction "SCLK") (pintype "input"))
    (pad "9" smd rect locked (at 2.2 -0.5) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/nvm_analog_adfpga/FC9") (pinfunction "SDI") (pintype "input"))
    (pad "10" smd rect locked (at 2.2 -1) (size 1.4 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/nvm_pcb_analog_ada/VADC") (pinfunction "DVIO") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/MSOP-10_3x3mm_P0.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 131.3 -35.1 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C35" (at 3.2 -0.4) (layer "F.SilkS"))
    (fp_text value "2u2" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 34 "+3.3VA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 172.6 -82.05 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1200")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R9" (at 2.95 0.1) (layer "F.SilkS"))
    (fp_text value "120R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "Net-(Q1-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(C9-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 120 -77)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "T_V1" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 76 "VREF7") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 162.6 -82.05 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1200")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R14" (at -3.2 -1.6 180) (layer "F.SilkS"))
    (fp_text value "120R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "Net-(Q6-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(C11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 2.5 -2.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 124.9625 -18.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R29" (at 0 2.3375 180) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "Net-(C25-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "-15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -74.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R55" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 156 "Net-(R55-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/MA_G10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 19.5 -71.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R80" (at 4 0.2 270) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 182 "Net-(R80-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/R2B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -48.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R68" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 170 "Net-(R68-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 100 "/FEN_C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 131.5 -38.5)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP1700T-3302E")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U13" (at 0 -2.5) (layer "F.SilkS"))
    (fp_text value "MCP1700-33" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "+3.3VA") (pinfunction "VO") (pintype "power_out"))
    (pad "3" smd roundrect locked (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "+5VA") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 53.3 -78.9 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "MCP1700T-3302E")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U18" (at 2.4 -0.9 180) (layer "F.SilkS"))
    (fp_text value "MCP1700-33" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "Net-(C46-Pad2)") (pinfunction "VO") (pintype "power_out"))
    (pad "3" smd roundrect locked (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "Net-(C45-Pad2)") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric_Pad1.22x1.90mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 56.5 -83.6 -90)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "PN" "BLM31A260SPT")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB6" (at 0 -2.6 180) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead_Small" (at 0 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.6625 0 270) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 36 "+5VD") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.6625 0 270) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 116 "Net-(C45-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 31.5 -71.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R75" (at 4 0 90) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 177 "Net-(R75-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 45 "/RE4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -72.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R56" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 157 "Net-(R56-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 12 "/MS_A1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 152.7 -27.1 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C1" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "3VFPGA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 104.2 -85.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R40" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 143 "Net-(Q8-Pad1)") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 153 "/PSWA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -34.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R86" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 188 "Net-(R86-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/nvm_analog_adfpga/FC5") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -24.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R81" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 183 "Net-(R81-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/nvm_analog_adfpga/FPGA_STB") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 124.9625 -30.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R27" (at 0.2 2.3375 180) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "Net-(C23-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "-15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 80.5 -1.7 90)
    (descr "wire loop with bead as test point, loop diameter2.6mm, hole diameter 1.6mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP2" (at 0.7 2.5 90) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5 90) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 3 3) (drill 1.6) (layers *.Cu *.Mask)
      (net 118 "Net-(TP2-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 53.2 -75.7)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B225KPFNNNE")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C46" (at -3.1 -0.8) (layer "F.SilkS"))
    (fp_text value "2u2" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 58 "Net-(C46-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 159.6 -74.05 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1203")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "120k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(C11-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 29.5 -56.5)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP6" (at 1.6 -2.2 unlocked) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 122 "Net-(TP6-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 148.5 -58.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R45" (at 3.2 0.4 180) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "Net-(C37-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "VREF+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -42.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R71" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 173 "Net-(R71-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/nvm_analog_adfpga/FC2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -56.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R64" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 166 "Net-(R64-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/COMP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 142.4 -90.8 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C3003")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R39" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "300k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "Net-(Q7-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 97.5 -2.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -4.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 101.3 -78 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "DG419DY-E3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U3" (at 0 -3.4) (layer "F.SilkS"))
    (fp_text value "DG419xY" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "Net-(C6-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 190 "Net-(U1-Pad14)") (pintype "passive"))
    (pad "3" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "+5VA") (pinfunction "VL") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 161 "/AZSW") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "Net-(R2-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 149.5 -48.5 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA202IDR")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U15" (at 4 -4.6 180) (layer "F.SilkS"))
    (fp_text value "OPA202" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 204 "unconnected-(U15-Pad1)") (pinfunction "VOS") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/nvm_pcb_analog_ada/VREF25") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 109 "Net-(C37-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 205 "unconnected-(U15-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect locked (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/nvm_pcb_analog_ada/VREF25") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 207 "unconnected-(U15-Pad8)") (pinfunction "VOS") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 120.9625 -38.5)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491B106K025AT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C17" (at 3.9375 -1) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 56 "Net-(C17-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 95.1 -52.9 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R24" (at -0.8 -2.8 180) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GNDS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 32 -50 90)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "TP9" (at 1.7 -0.1 180) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0 0 90) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 125 "Net-(TP9-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 26.5 -54.5)
    (descr "wire loop with bead as test point, loop diameter 1.8mm, hole diameter 1.0mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TP7" (at -0.8 2.4) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 123 "Net-(TP7-Pad1)") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 172.6 -88.05 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R8" (at -3.15 0) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "+8V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "Net-(C9-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 34.5 -47.5 -90)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "TP12" (at 2 -0.2 180) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0 0 270) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 128 "Net-(TP12-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 120.925 -32.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C24" (at 3.225 -0.2) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 53 "Net-(C23-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 100.5 -21.9)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "T_INO1" (at -2.2 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 33 "/nvm_pcb_analog_ada/INT_OUT") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-6032-28_Kemet-C_Pad2.25x2.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 120.5 -60)
    (descr "Tantalum Capacitor SMD Kemet-C (6032-28 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491C226K025AT")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C14" (at 5.4 -1.1) (layer "F.SilkS"))
    (fp_text value "22u" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.55 0) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 2.55 0) (size 2.25 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1111111111)
      (net 7 "-15V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-6032-28_Kemet-C.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 54.1625 -48.4625 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C49" (at 2.5625 -1.9375 180) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 117 "Net-(C47-Pad2)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 270) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 148 -86.7 -90)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "PN" "BCP53-16,115")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q7" (at 0 -4.5 90) (layer "F.SilkS"))
    (fp_text value "BCP53" (at 0 4.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 142 "Net-(Q7-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd rect (at -3.15 0 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "Net-(C38-Pad2)") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at -3.15 2.3 270) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pinfunction "E") (pintype "passive"))
    (pad "4" smd rect (at 3.15 0 270) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 239 "Net-(C38-Pad2)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 28.5 -71.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R76" (at 4 0 90) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 178 "Net-(R76-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/R1A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -50.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R67" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 169 "Net-(R67-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "/FEN_A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_MiniMELF" (layer "F.Cu")
    (tedit 5905D8F5)
    (at 156.6 -89.05)
    (descr "Diode Mini-MELF (SOD-80)")
    (tags "Diode Mini-MELF (SOD-80)")
    (property "PN" "LL4148-GS18")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D3" (at 0 -2) (layer "F.SilkS"))
    (fp_text value "LL4148" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -2) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.75 0) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(D3-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 1.75 0) (size 1.3 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "-8V") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_MiniMELF.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 136.1 -38.5)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "DNP")
    (attr smd)
    (fp_text reference "U14" (at -1.1 -2.5) (layer "F.SilkS"))
    (fp_text value "DNP-MCP1700-18" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd roundrect locked (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/nvm_pcb_analog_ada/VA1V2") (pinfunction "VO") (pintype "power_out"))
    (pad "3" smd roundrect locked (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/nvm_pcb_analog_ada/VADC") (pinfunction "VI") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "TestPoint:TestPoint_Pad_1.5x1.5mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 34.5 -50 -90)
    (descr "SMD rectangular pad as test Point, square 1.5mm side length")
    (tags "test point SMD pad rectangle square")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "TP11" (at 0.9 -2.8 180) (layer "F.SilkS") hide)
    (fp_text value "TestPoint" (at 0 1.75 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.65 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at 0 0 270) (size 1.5 1.5) (layers "F.Cu" "F.Mask")
      (net 127 "Net-(TP11-Pad1)") (pinfunction "1") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 2.5 -100.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0.1 5.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 100.1 -32.3)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-0R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GNDS") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 113 "/nvm_pcb_analog_ada/GUARD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 92.5 -57.5 180)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1602")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "16k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 27 "Net-(C5-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 180) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(C8-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 116.5 -36.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "DNP")
    (attr smd)
    (fp_text reference "R34" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "DNP" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "Net-(C30-Pad2)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 162.6 -88.05 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C1202")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R15" (at -3 -0.6 180) (layer "F.SilkS"))
    (fp_text value "12k" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "-8V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "Net-(C11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -52.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R66" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 168 "Net-(R66-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "/JA_SCK") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 165.5 -23.7)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491B106K025AT")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C3" (at 0 2.4) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 26 "Net-(C2-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 24 "Net-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 112.4625 -35.5)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "DNP")
    (attr smd)
    (fp_text reference "C30" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "DNP" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 30 "/nvm_pcb_analog_ada/INT_IN") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 97 "Net-(C30-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 22.5 -61.5)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "PN" "KP-2012YD")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D9" (at 3 -0.8) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 89 "Net-(D9-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 146 "Net-(D9-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -78.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R53" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 154 "Net-(R53-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/MA_G1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -58.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R63" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 165 "Net-(R63-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 147 "/PSWB") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 142.5 -57.5 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA202IDR")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U17" (at -4.6 -2 180) (layer "F.SilkS"))
    (fp_text value "OPA202" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 211 "unconnected-(U17-Pad1)") (pinfunction "VOS") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 75 "Net-(RN3-Pad1)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GNDS") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "-15V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 212 "unconnected-(U17-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect locked (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 131 "Net-(D7-Pad1)") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "+15V") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 213 "unconnected-(U17-Pad8)") (pinfunction "VOS") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 56.9 -50.6 135)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B104KBCNNNC")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C43" (at 0.636396 2.333452 45) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.679999 135) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 135) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 135) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 135) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 115 "3VFPGA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 152.5 -58.5 -90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "MMA02040C6201")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R46" (at -3 0 180) (layer "F.SilkS"))
    (fp_text value "6k2" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 270) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "Net-(C37-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 165.9 -18.9 180)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED handsolder")
    (property "PN" "KP-2012YD")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "D1" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "LED" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 84 "Net-(D1-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.025 0 180) (size 1.15 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2173913043)
      (net 26 "Net-(C2-Pad1)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_KK-254_AE-6410-06A_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 5EA53D3B)
    (at 171.52 -25.5 90)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-06A example for new part number: 22-27-2061, 6 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "PN" "NS25-W6P")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "J1" (at 15 -0.02 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x06_Male" (at 6.35 4.08 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 6.35 -2.22 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.1436781609)
      (net 24 "Net-(C2-Pad2)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 26 "Net-(C2-Pad1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 5.08 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 91 "Net-(J1-Pad3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 92 "Net-(J1-Pad4)") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 10.16 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 93 "Net-(J1-Pad5)") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 12.7 0 90) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 95 "Net-(J1-Pad6)") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-06A_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3528-21_Kemet-B" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 120.9625 -25.3)
    (descr "Tantalum Capacitor SMD Kemet-B (3528-21 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "PN" "T491B106K025AT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C19" (at -3.2625 0.6 90) (layer "F.SilkS"))
    (fp_text value "10u" (at 0 2.35) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 85 "Net-(C19-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.5375 0) (size 1.325 2.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1886792453)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3528-21_Kemet-B.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Oscillator:Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm" (layer "F.Cu")
    (tedit 58CD3345)
    (at 50.1625 -72.5 180)
    (descr "SMD Crystal Oscillator Seiko Epson SG-8002LB https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal oscillator")
    (property "PN" "5032CAN320M")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "X1" (at 3.8625 1.8) (layer "F.SilkS"))
    (fp_text value "SG-5032CAN" (at 0 2.85) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.27 1.1 180) (size 1.6 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "unconnected-(X1-Pad1)") (pinfunction "~{ST}") (pintype "input"))
    (pad "2" smd rect locked (at 1.27 1.1 180) (size 1.6 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "GNDA") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect locked (at 1.27 -1.1 180) (size 1.6 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "/nvm_analog_adfpga/FPGA_CLK") (pinfunction "OUT") (pintype "output"))
    (pad "4" smd rect locked (at -1.27 -1.1 180) (size 1.6 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "3VFPGA") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 156.6 -74.05 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-12R")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R17" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "12R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 6 "-6V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "Net-(D3-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -46.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R69" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 171 "Net-(R69-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "/FEN_B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEEF)
    (at 149.5 -54.5 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "PN" "CL21B105KAFNNNG")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "C37" (at 0 -1.68) (layer "F.SilkS"))
    (fp_text value "1u" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.0375 0 180) (size 1.175 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2127659574)
      (net 109 "Net-(C37-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 124.9625 -24.5 90)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R20" (at 0.2 2.3375 180) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "+15V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0 90) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "Net-(C19-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Inductor_SMD:L_1206_3216Metric_Pad1.22x1.90mm_HandSolder" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 113.5 -50.5 180)
    (descr "Inductor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor handsolder")
    (property "PN" "BLM31A260SPT")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "FB4" (at -2.8 1.6) (layer "F.SilkS"))
    (fp_text value "Ferrite_Bead_Small" (at 0 1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -1.6625 0 180) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 137 "Net-(FB4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect locked (at 1.6625 0 180) (size 1.225 1.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.2040816327)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 97.5 -100.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 5.9 -0.1) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "TestPoint:TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 156.5 -50.5)
    (descr "wire loop with bead as test point, loop diameter2.548mm, hole diameter 1.5mm")
    (tags "test point wire loop bead")
    (property "PN" "optional")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "aliexpress")
    (attr through_hole)
    (fp_text reference "TGNDS1" (at 0.7 2.5) (layer "F.SilkS"))
    (fp_text value "TestPoint" (at 0 -2.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.7 2.5) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 3 3) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 "GNDS") (pinfunction "1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/TestPoint.3dshapes/TestPoint_Loop_D2.54mm_Drill1.5mm_Beaded.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 112.5 -22.5)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PN" "OPA140AIDR")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr smd)
    (fp_text reference "U8" (at -4.8 2.2) (layer "F.SilkS"))
    (fp_text value "OPA140" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect locked (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 199 "unconnected-(U8-Pad1)") (pinfunction "VOS") (pintype "input"))
    (pad "2" smd roundrect locked (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/nvm_pcb_analog_ada/INT_IN") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect locked (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 149 "Net-(R25-Pad2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect locked (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "Net-(C25-Pad2)") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect locked (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 200 "unconnected-(U8-Pad5)") (pinfunction "NC") (pintype "no_connect"))
    (pad "6" smd roundrect locked (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/nvm_pcb_analog_ada/INT_OUT") (pintype "output"))
    (pad "7" smd roundrect locked (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "Net-(C19-Pad1)") (pinfunction "V+") (pintype "power_in"))
    (pad "8" smd roundrect locked (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 201 "unconnected-(U8-Pad8)") (pinfunction "VOS") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (tedit 5FA16958)
    (at 164.3 -70.5 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PN" "BC857.215")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "Q4" (at -2.5 0 180) (layer "F.SilkS"))
    (fp_text value "BC857" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "Net-(Q4-Pad1)") (pinfunction "B") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "GNDA") (pinfunction "E") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "Net-(C11-Pad2)") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -30.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R84" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 186 "Net-(R84-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/nvm_analog_adfpga/FC9") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 172.5 -100.5)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "DNP")
    (attr exclude_from_pos_files)
    (fp_text reference "H9" (at 0 5.1) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 4.2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 121.5 -42.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-0R")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R36" (at 3.6 0) (layer "F.SilkS"))
    (fp_text value "0R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/nvm_pcb_analog_ada/AD_IN") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 152 "Net-(R36-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 92.5 -63.7)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "CSRV0204FTDG1602")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "16k" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 69.5 -26.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R82" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 184 "Net-(R82-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/nvm_analog_adfpga/FPGA_CTRL") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_MiniMELF_MMA-0204" (layer "F.Cu")
    (tedit 58FE61E9)
    (at 75.5 -28.5)
    (descr "Resistor, MiniMELF, MMA-0204, http://www.vishay.com/docs/28713/melfprof.pdf")
    (tags "MiniMELF Resistor")
    (property "PN" "SMDMM0204-24R")
    (property "Sheetfile" "nvm_pcb_analog_adfpga.kicad_sch")
    (property "Sheetname" "nvm_analog_adfpga")
    (property "comment" "")
    (property "supplier" "TME")
    (attr smd)
    (fp_text reference "R83" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "24R" (at 0 1.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 185 "Net-(R83-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 1.5 0) (size 1.5 1.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/nvm_analog_adfpga/FPGA_TX") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_MiniMELF_MMA-0204.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P2.50mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 172.6 -78.05 -90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (property "PN" "ECE-A1AKS221")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "C9" (at 1.25 5.25 90) (layer "B.SilkS"))
    (fp_text value "220u" (at 1.25 -5.25 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 37 "Net-(C9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W4.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 98 -68.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*4.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 4.5mm Capacitor")
    (property "PN" "MKS2-1U/50")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C5" (at 2.5 3.5) (layer "B.SilkS"))
    (fp_text value "1u" (at 2.5 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 "Net-(C5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "j_lib:LM399" (layer "B.Cu")
    (tedit 61A8CCCA)
    (at 135.5 -80.5)
    (property "PN" "ADR1399KHZ")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "Alternative: LM399 ")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "VR1" (at 0 -6) (layer "B.SilkS"))
    (fp_text value "ADR1399" (at 0 6) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 -1.5 270) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 239 "Net-(C38-Pad2)") (pinfunction "HP") (pintype "power_in"))
    (pad "2" thru_hole circle locked (at 1.5 0 270) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 7 "-15V") (pinfunction "HM") (pintype "power_in"))
    (pad "3" thru_hole circle locked (at 0 1.5 270) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 110 "Net-(C39-Pad1)") (pinfunction "RP") (pintype "power_in"))
    (pad "4" thru_hole circle locked (at -1.5 0 270) (size 1.6 1.6) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 "GNDS") (pinfunction "RM") (pintype "power_in"))
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W4.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 130.5 -63 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*4.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 4.5mm Capacitor")
    (property "PN" "MKS2-1U/50")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C39" (at 2.5 3.5 90) (layer "B.SilkS"))
    (fp_text value "1u" (at 2.5 -3.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(C39-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 111 "Net-(C39-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W4.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 98 -63.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*4.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 4.5mm Capacitor")
    (property "PN" "MKS2-1U/50")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C8" (at 2.5 3.5) (layer "B.SilkS"))
    (fp_text value "1u" (at 2.5 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 31 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal" (layer "B.Cu")
    (tedit 5AE5139B)
    (at 137.5 -63.5 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=15.24mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 15.24mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "PN" "YR1B2K49CC")
    (property "Sheetfile" "nvm_pcb_analog_ada.kicad_sch")
    (property "Sheetname" "nvm_pcb_analog_ada")
    (property "comment" "7k for LM399")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "R49" (at 7.62 2.37 90) (layer "B.SilkS"))
    (fp_text value "2k49" (at 7.62 -2.37 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 7.62 0 90) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 110 "Net-(C39-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 15.24 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 51 "VREF+") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P15.24mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P2.50mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 166.6 -67.05)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (property "PN" "ECE-A1AKS221")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "C10" (at 1.25 5.25) (layer "B.SilkS"))
    (fp_text value "220u" (at 1.25 -5.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "+6V") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P2.50mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 162.6 -75.55 90)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (property "PN" "ECE-A1AKS221")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "C11" (at 1.25 5.25 90) (layer "B.SilkS"))
    (fp_text value "220u" (at 1.25 -5.25 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0 90) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 50 "Net-(C11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P2.50mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 159.6 -67.05 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 8mm Electrolytic Capacitor")
    (property "PN" "ECE-A1AKS221")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "MOUSER")
    (attr through_hole)
    (fp_text reference "C12" (at 1.25 5.25) (layer "B.SilkS"))
    (fp_text value "220u" (at 1.25 -5.25) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab"))
    (pad "1" thru_hole rect locked (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "GNDA") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "-6V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.0mm_W4.5mm_P5.00mm" (layer "B.Cu")
    (tedit 5AE50EF0)
    (at 98 -73.5)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7*4.5mm^2, Capacitor")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7mm width 4.5mm Capacitor")
    (property "PN" "MKS2-1U/50")
    (property "Sheetfile" "rnvm_homer.kicad_sch")
    (property "Sheetname" "")
    (property "comment" "")
    (property "supplier" "TME")
    (attr through_hole)
    (fp_text reference "C4" (at 2.5 3.5) (layer "B.SilkS"))
    (fp_text value "1u" (at 2.5 -3.5) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "B.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(C4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(C4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.0mm_W4.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 158.5 -16.5) (end 160.5 -16.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 160.5 -16.5) (end 160.5 -43.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 175 0) (end 175 -103) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 0 -103) (end 0 0) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 0 0) (end 175 0) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 160.5 -43.5) (end 158.5 -43.5) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 175 -103) (end 0 -103) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 158.5 -43.5) (end 158.5 -16.5) (layer "Edge.Cuts") (width 0.1))
  (gr_text "NVM\nHOMER PCB REV 2" (at 129.4 -2.8) (layer "F.SilkS"))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -12.5)
        (xy 19 -12.5)
        (xy 19 -14)
        (xy 20.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -6.5)
        (xy 19 -6.5)
        (xy 19 -8)
        (xy 20.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -18.5)
        (xy 7 -18.5)
        (xy 7 -20)
        (xy 8.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -6.5)
        (xy 31 -6.5)
        (xy 31 -8)
        (xy 32.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -30.5)
        (xy 33 -30.5)
        (xy 33 -32)
        (xy 34.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -46.5)
        (xy 13 -46.5)
        (xy 13 -48)
        (xy 14.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -6.5)
        (xy 17 -6.5)
        (xy 17 -8)
        (xy 18.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.5 -2.5)
        (xy 61 -2.5)
        (xy 61 -4)
        (xy 62.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 6 0)
        (xy 0 0)
        (xy 0 -6)
        (xy 6 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -22.5)
        (xy 35 -22.5)
        (xy 35 -24)
        (xy 36.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.5 -6.5)
        (xy 57 -6.5)
        (xy 57 -8)
        (xy 58.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -6.5)
        (xy 53 -6.5)
        (xy 53 -8)
        (xy 54.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -16.5)
        (xy 49 -16.5)
        (xy 49 -18)
        (xy 50.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.5 -6.5)
        (xy 73 -6.5)
        (xy 73 -8)
        (xy 74.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -22.5)
        (xy 33 -22.5)
        (xy 33 -24)
        (xy 34.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -28.5)
        (xy 17 -28.5)
        (xy 17 -30)
        (xy 18.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -2.5)
        (xy 19 -2.5)
        (xy 19 -4)
        (xy 20.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -8.5)
        (xy 43 -8.5)
        (xy 43 -10)
        (xy 44.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -34.5)
        (xy 25 -34.5)
        (xy 25 -36)
        (xy 26.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -8.5)
        (xy 17 -8.5)
        (xy 17 -10)
        (xy 18.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -40.5)
        (xy 17 -40.5)
        (xy 17 -42)
        (xy 18.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -14.5)
        (xy 13 -14.5)
        (xy 13 -16)
        (xy 14.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -20.5)
        (xy 15 -20.5)
        (xy 15 -22)
        (xy 16.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -6.5)
        (xy 35 -6.5)
        (xy 35 -8)
        (xy 36.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -30.5)
        (xy 19 -30.5)
        (xy 19 -32)
        (xy 20.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -2.5)
        (xy 17 -2.5)
        (xy 17 -4)
        (xy 18.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -14.5)
        (xy 25 -14.5)
        (xy 25 -16)
        (xy 26.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -8.5)
        (xy 29 -8.5)
        (xy 29 -10)
        (xy 30.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -26.5)
        (xy 37 -26.5)
        (xy 37 -28)
        (xy 38.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -26.5)
        (xy 25 -26.5)
        (xy 25 -28)
        (xy 26.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -12.5)
        (xy 29 -12.5)
        (xy 29 -14)
        (xy 30.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -14.5)
        (xy 15 -14.5)
        (xy 15 -16)
        (xy 16.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -2.5)
        (xy 21 -2.5)
        (xy 21 -4)
        (xy 22.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -4.5)
        (xy 39 -4.5)
        (xy 39 -6)
        (xy 40.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.5 -12.5)
        (xy 69 -12.5)
        (xy 69 -14)
        (xy 70.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.5 -8.5)
        (xy 57 -8.5)
        (xy 57 -10)
        (xy 58.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -12.5)
        (xy 51 -12.5)
        (xy 51 -14)
        (xy 52.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -10.5)
        (xy 11 -10.5)
        (xy 11 -12)
        (xy 12.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.5 -10.5)
        (xy 73 -10.5)
        (xy 73 -12)
        (xy 74.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -42.5)
        (xy 9 -42.5)
        (xy 9 -44)
        (xy 10.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -24.5)
        (xy 21 -24.5)
        (xy 21 -26)
        (xy 22.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -20.5)
        (xy 35 -20.5)
        (xy 35 -22)
        (xy 36.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -20.5)
        (xy 53 -20.5)
        (xy 53 -22)
        (xy 54.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -8.5)
        (xy 31 -8.5)
        (xy 31 -10)
        (xy 32.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -28.5)
        (xy 9 -28.5)
        (xy 9 -30)
        (xy 10.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -20.5)
        (xy 25 -20.5)
        (xy 25 -22)
        (xy 26.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -8.5)
        (xy 23 -8.5)
        (xy 23 -10)
        (xy 24.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -2.5)
        (xy 9 -2.5)
        (xy 9 -4)
        (xy 10.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -14.5)
        (xy 49 -14.5)
        (xy 49 -16)
        (xy 50.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -4.5)
        (xy 27 -4.5)
        (xy 27 -6)
        (xy 28.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -32.5)
        (xy 41 -32.5)
        (xy 41 -34)
        (xy 42.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -44.5)
        (xy 27 -44.5)
        (xy 27 -46)
        (xy 28.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -48.5)
        (xy 27 -48.5)
        (xy 27 -50)
        (xy 28.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -28.5)
        (xy 33 -28.5)
        (xy 33 -30)
        (xy 34.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -26.5)
        (xy 39 -26.5)
        (xy 39 -28)
        (xy 40.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -10.5)
        (xy 35 -10.5)
        (xy 35 -12)
        (xy 36.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -8.5)
        (xy 27 -8.5)
        (xy 27 -10)
        (xy 28.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -40.5)
        (xy 9 -40.5)
        (xy 9 -42)
        (xy 10.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -24.5)
        (xy 25 -24.5)
        (xy 25 -26)
        (xy 26.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -16.5)
        (xy 51 -16.5)
        (xy 51 -18)
        (xy 52.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -16.5)
        (xy 7 -16.5)
        (xy 7 -18)
        (xy 8.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -12.5)
        (xy 45 -12.5)
        (xy 45 -14)
        (xy 46.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -4.5)
        (xy 41 -4.5)
        (xy 41 -6)
        (xy 42.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -2.5)
        (xy 43 -2.5)
        (xy 43 -4)
        (xy 44.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -34.5)
        (xy 21 -34.5)
        (xy 21 -36)
        (xy 22.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -6.5)
        (xy 7 -6.5)
        (xy 7 -8)
        (xy 8.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -4.5)
        (xy 29 -4.5)
        (xy 29 -6)
        (xy 30.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -12.5)
        (xy 47 -12.5)
        (xy 47 -14)
        (xy 48.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -20.5)
        (xy 37 -20.5)
        (xy 37 -22)
        (xy 38.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -32.5)
        (xy 15 -32.5)
        (xy 15 -34)
        (xy 16.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -16.5)
        (xy 11 -16.5)
        (xy 11 -18)
        (xy 12.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -18.5)
        (xy 35 -18.5)
        (xy 35 -20)
        (xy 36.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -10.5)
        (xy 41 -10.5)
        (xy 41 -12)
        (xy 42.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -20.5)
        (xy 41 -20.5)
        (xy 41 -22)
        (xy 42.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.5 -10.5)
        (xy 71 -10.5)
        (xy 71 -12)
        (xy 72.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -38.5)
        (xy 29 -38.5)
        (xy 29 -40)
        (xy 30.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -32.5)
        (xy 39 -32.5)
        (xy 39 -34)
        (xy 40.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -42.5)
        (xy 27 -42.5)
        (xy 27 -44)
        (xy 28.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -20.5)
        (xy 45 -20.5)
        (xy 45 -22)
        (xy 46.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -36.5)
        (xy 15 -36.5)
        (xy 15 -38)
        (xy 16.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -26.5)
        (xy 9 -26.5)
        (xy 9 -28)
        (xy 10.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -10.5)
        (xy 13 -10.5)
        (xy 13 -12)
        (xy 14.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.5 -2.5)
        (xy 63 -2.5)
        (xy 63 -4)
        (xy 64.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -36.5)
        (xy 35 -36.5)
        (xy 35 -38)
        (xy 36.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.5 -6.5)
        (xy 69 -6.5)
        (xy 69 -8)
        (xy 70.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -2.5)
        (xy 33 -2.5)
        (xy 33 -4)
        (xy 34.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -24.5)
        (xy 37 -24.5)
        (xy 37 -26)
        (xy 38.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -16.5)
        (xy 47 -16.5)
        (xy 47 -18)
        (xy 48.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -36.5)
        (xy 9 -36.5)
        (xy 9 -38)
        (xy 10.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -26.5)
        (xy 15 -26.5)
        (xy 15 -28)
        (xy 16.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -34.5)
        (xy 23 -34.5)
        (xy 23 -36)
        (xy 24.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -30.5)
        (xy 15 -30.5)
        (xy 15 -32)
        (xy 16.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -44.5)
        (xy 23 -44.5)
        (xy 23 -46)
        (xy 24.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.5 -12.5)
        (xy 55 -12.5)
        (xy 55 -14)
        (xy 56.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -20.5)
        (xy 11 -20.5)
        (xy 11 -22)
        (xy 12.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -16.5)
        (xy 29 -16.5)
        (xy 29 -18)
        (xy 30.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -10.5)
        (xy 37 -10.5)
        (xy 37 -12)
        (xy 38.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -18.5)
        (xy 31 -18.5)
        (xy 31 -20)
        (xy 32.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -20.5)
        (xy 49 -20.5)
        (xy 49 -22)
        (xy 50.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -20.5)
        (xy 29 -20.5)
        (xy 29 -22)
        (xy 30.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -28.5)
        (xy 35 -28.5)
        (xy 35 -30)
        (xy 36.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -12.5)
        (xy 7 -12.5)
        (xy 7 -14)
        (xy 8.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -12.5)
        (xy 15 -12.5)
        (xy 15 -14)
        (xy 16.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -26.5)
        (xy 35 -26.5)
        (xy 35 -28)
        (xy 36.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.5 -6.5)
        (xy 55 -6.5)
        (xy 55 -8)
        (xy 56.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.5 -4.5)
        (xy 69 -4.5)
        (xy 69 -6)
        (xy 70.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -38.5)
        (xy 23 -38.5)
        (xy 23 -40)
        (xy 24.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -20.5)
        (xy 21 -20.5)
        (xy 21 -22)
        (xy 22.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -28.5)
        (xy 29 -28.5)
        (xy 29 -30)
        (xy 30.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -24.5)
        (xy 33 -24.5)
        (xy 33 -26)
        (xy 34.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -36.5)
        (xy 21 -36.5)
        (xy 21 -38)
        (xy 22.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -16.5)
        (xy 9 -16.5)
        (xy 9 -18)
        (xy 10.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -16.5)
        (xy 53 -16.5)
        (xy 53 -18)
        (xy 54.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.5 -2.5)
        (xy 55 -2.5)
        (xy 55 -4)
        (xy 56.5 -4)
      )
    )
  )
  (zone (net 23) (net_name "GNDA") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 175 -48.5)
        (xy 156.5 -48.5)
        (xy 156.5 0)
        (xy 0 0)
        (xy 0 -103)
        (xy 175 -103)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -44.5)
        (xy 25 -44.5)
        (xy 25 -46)
        (xy 26.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -16.5)
        (xy 39 -16.5)
        (xy 39 -18)
        (xy 40.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -4.5)
        (xy 33 -4.5)
        (xy 33 -6)
        (xy 34.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.5 -2.5)
        (xy 75 -2.5)
        (xy 75 -4)
        (xy 76.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -2.5)
        (xy 53 -2.5)
        (xy 53 -4)
        (xy 54.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -28.5)
        (xy 41 -28.5)
        (xy 41 -30)
        (xy 42.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -2.5)
        (xy 15 -2.5)
        (xy 15 -4)
        (xy 16.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -6.5)
        (xy 41 -6.5)
        (xy 41 -8)
        (xy 42.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -36.5)
        (xy 37 -36.5)
        (xy 37 -38)
        (xy 38.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -16.5)
        (xy 15 -16.5)
        (xy 15 -18)
        (xy 16.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -6.5)
        (xy 27 -6.5)
        (xy 27 -8)
        (xy 28.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -34.5)
        (xy 31 -34.5)
        (xy 31 -36)
        (xy 32.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -40.5)
        (xy 21 -40.5)
        (xy 21 -42)
        (xy 22.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -46.5)
        (xy 7 -46.5)
        (xy 7 -48)
        (xy 8.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -10.5)
        (xy 47 -10.5)
        (xy 47 -12)
        (xy 48.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -26.5)
        (xy 41 -26.5)
        (xy 41 -28)
        (xy 42.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -8.5)
        (xy 39 -8.5)
        (xy 39 -10)
        (xy 40.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -6.5)
        (xy 43 -6.5)
        (xy 43 -8)
        (xy 44.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -18.5)
        (xy 21 -18.5)
        (xy 21 -20)
        (xy 22.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -40.5)
        (xy 19 -40.5)
        (xy 19 -42)
        (xy 20.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -22.5)
        (xy 53 -22.5)
        (xy 53 -24)
        (xy 54.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -36.5)
        (xy 29 -36.5)
        (xy 29 -38)
        (xy 30.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -2.5)
        (xy 31 -2.5)
        (xy 31 -4)
        (xy 32.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.5 -6.5)
        (xy 63 -6.5)
        (xy 63 -8)
        (xy 64.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -14.5)
        (xy 19 -14.5)
        (xy 19 -16)
        (xy 20.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -2.5)
        (xy 25 -2.5)
        (xy 25 -4)
        (xy 26.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -48.5)
        (xy 19 -48.5)
        (xy 19 -50)
        (xy 20.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -12.5)
        (xy 11 -12.5)
        (xy 11 -14)
        (xy 12.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -4.5)
        (xy 47 -4.5)
        (xy 47 -6)
        (xy 48.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -48.5)
        (xy 17 -48.5)
        (xy 17 -50)
        (xy 18.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.5 -4.5)
        (xy 65 -4.5)
        (xy 65 -6)
        (xy 66.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.5 -2.5)
        (xy 59 -2.5)
        (xy 59 -4)
        (xy 60.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.5 -4.5)
        (xy 63 -4.5)
        (xy 63 -6)
        (xy 64.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -18.5)
        (xy 45 -18.5)
        (xy 45 -20)
        (xy 46.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.5 -12.5)
        (xy 77 -12.5)
        (xy 77 -14)
        (xy 78.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -18.5)
        (xy 29 -18.5)
        (xy 29 -20)
        (xy 30.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -10.5)
        (xy 15 -10.5)
        (xy 15 -12)
        (xy 16.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -34.5)
        (xy 11 -34.5)
        (xy 11 -36)
        (xy 12.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -2.5)
        (xy 35 -2.5)
        (xy 35 -4)
        (xy 36.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -26.5)
        (xy 17 -26.5)
        (xy 17 -28)
        (xy 18.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -8.5)
        (xy 33 -8.5)
        (xy 33 -10)
        (xy 34.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -36.5)
        (xy 31 -36.5)
        (xy 31 -38)
        (xy 32.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -42.5)
        (xy 11 -42.5)
        (xy 11 -44)
        (xy 12.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -30.5)
        (xy 39 -30.5)
        (xy 39 -32)
        (xy 40.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -10.5)
        (xy 7 -10.5)
        (xy 7 -12)
        (xy 8.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -12.5)
        (xy 41 -12.5)
        (xy 41 -14)
        (xy 42.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -44.5)
        (xy 7 -44.5)
        (xy 7 -46)
        (xy 8.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -34.5)
        (xy 37 -34.5)
        (xy 37 -36)
        (xy 38.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -8.5)
        (xy 13 -8.5)
        (xy 13 -10)
        (xy 14.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -18.5)
        (xy 27 -18.5)
        (xy 27 -20)
        (xy 28.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -48.5)
        (xy 15 -48.5)
        (xy 15 -50)
        (xy 16.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -34.5)
        (xy 39 -34.5)
        (xy 39 -36)
        (xy 40.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101 0)
        (xy 88 0)
        (xy 88 -6)
        (xy 101 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -6.5)
        (xy 9 -6.5)
        (xy 9 -8)
        (xy 10.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -8.5)
        (xy 53 -8.5)
        (xy 53 -10)
        (xy 54.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -2.5)
        (xy 11 -2.5)
        (xy 11 -4)
        (xy 12.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -22.5)
        (xy 21 -22.5)
        (xy 21 -24)
        (xy 22.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.5 -6.5)
        (xy 67 -6.5)
        (xy 67 -8)
        (xy 68.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -26.5)
        (xy 27 -26.5)
        (xy 27 -28)
        (xy 28.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -18.5)
        (xy 43 -18.5)
        (xy 43 -20)
        (xy 44.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -16.5)
        (xy 33 -16.5)
        (xy 33 -18)
        (xy 34.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -4.5)
        (xy 53 -4.5)
        (xy 53 -6)
        (xy 54.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -26.5)
        (xy 31 -26.5)
        (xy 31 -28)
        (xy 32.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -24.5)
        (xy 17 -24.5)
        (xy 17 -26)
        (xy 18.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -10.5)
        (xy 49 -10.5)
        (xy 49 -12)
        (xy 50.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -36.5)
        (xy 27 -36.5)
        (xy 27 -38)
        (xy 28.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -6.5)
        (xy 11 -6.5)
        (xy 11 -8)
        (xy 12.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -10.5)
        (xy 39 -10.5)
        (xy 39 -12)
        (xy 40.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -32.5)
        (xy 21 -32.5)
        (xy 21 -34)
        (xy 22.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.5 -8.5)
        (xy 65 -8.5)
        (xy 65 -10)
        (xy 66.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -42.5)
        (xy 21 -42.5)
        (xy 21 -44)
        (xy 22.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -12.5)
        (xy 35 -12.5)
        (xy 35 -14)
        (xy 36.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -14.5)
        (xy 7 -14.5)
        (xy 7 -16)
        (xy 8.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -4.5)
        (xy 45 -4.5)
        (xy 45 -6)
        (xy 46.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -2.5)
        (xy 47 -2.5)
        (xy 47 -4)
        (xy 48.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -48.5)
        (xy 9 -48.5)
        (xy 9 -50)
        (xy 10.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -24.5)
        (xy 31 -24.5)
        (xy 31 -26)
        (xy 32.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -22.5)
        (xy 27 -22.5)
        (xy 27 -24)
        (xy 28.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -14.5)
        (xy 51 -14.5)
        (xy 51 -16)
        (xy 52.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -46.5)
        (xy 11 -46.5)
        (xy 11 -48)
        (xy 12.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -40.5)
        (xy 23 -40.5)
        (xy 23 -42)
        (xy 24.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -28.5)
        (xy 21 -28.5)
        (xy 21 -30)
        (xy 22.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -10.5)
        (xy 29 -10.5)
        (xy 29 -12)
        (xy 30.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -16.5)
        (xy 23 -16.5)
        (xy 23 -18)
        (xy 24.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -32.5)
        (xy 37 -32.5)
        (xy 37 -34)
        (xy 38.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -4.5)
        (xy 7 -4.5)
        (xy 7 -6)
        (xy 8.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -24.5)
        (xy 53 -24.5)
        (xy 53 -26)
        (xy 54.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.5 -8.5)
        (xy 75 -8.5)
        (xy 75 -10)
        (xy 76.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -26.5)
        (xy 13 -26.5)
        (xy 13 -28)
        (xy 14.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -26.5)
        (xy 21 -26.5)
        (xy 21 -28)
        (xy 22.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.5 -10.5)
        (xy 65 -10.5)
        (xy 65 -12)
        (xy 66.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -12.5)
        (xy 27 -12.5)
        (xy 27 -14)
        (xy 28.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -20.5)
        (xy 31 -20.5)
        (xy 31 -22)
        (xy 32.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.5 -12.5)
        (xy 71 -12.5)
        (xy 71 -14)
        (xy 72.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.5 -2.5)
        (xy 67 -2.5)
        (xy 67 -4)
        (xy 68.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -24.5)
        (xy 51 -24.5)
        (xy 51 -26)
        (xy 52.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -4.5)
        (xy 23 -4.5)
        (xy 23 -6)
        (xy 24.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.5 -2.5)
        (xy 65 -2.5)
        (xy 65 -4)
        (xy 66.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -22.5)
        (xy 29 -22.5)
        (xy 29 -24)
        (xy 30.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -10.5)
        (xy 33 -10.5)
        (xy 33 -12)
        (xy 34.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -8.5)
        (xy 7 -8.5)
        (xy 7 -10)
        (xy 8.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.5 -6.5)
        (xy 75 -6.5)
        (xy 75 -8)
        (xy 76.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -34.5)
        (xy 35 -34.5)
        (xy 35 -36)
        (xy 36.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -22.5)
        (xy 9 -22.5)
        (xy 9 -24)
        (xy 10.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.5 -6.5)
        (xy 77 -6.5)
        (xy 77 -8)
        (xy 78.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -10.5)
        (xy 31 -10.5)
        (xy 31 -12)
        (xy 32.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.5 -8.5)
        (xy 69 -8.5)
        (xy 69 -10)
        (xy 70.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -32.5)
        (xy 35 -32.5)
        (xy 35 -34)
        (xy 36.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -14.5)
        (xy 27 -14.5)
        (xy 27 -16)
        (xy 28.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -12.5)
        (xy 49 -12.5)
        (xy 49 -14)
        (xy 50.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -6.5)
        (xy 23 -6.5)
        (xy 23 -8)
        (xy 24.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -14.5)
        (xy 23 -14.5)
        (xy 23 -16)
        (xy 24.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -24.5)
        (xy 35 -24.5)
        (xy 35 -26)
        (xy 36.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -14.5)
        (xy 31 -14.5)
        (xy 31 -16)
        (xy 32.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -30.5)
        (xy 41 -30.5)
        (xy 41 -32)
        (xy 42.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -42.5)
        (xy 23 -42.5)
        (xy 23 -44)
        (xy 24.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -18.5)
        (xy 37 -18.5)
        (xy 37 -20)
        (xy 38.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.5 -10.5)
        (xy 55 -10.5)
        (xy 55 -12)
        (xy 56.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -30.5)
        (xy 21 -30.5)
        (xy 21 -32)
        (xy 22.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -10.5)
        (xy 9 -10.5)
        (xy 9 -12)
        (xy 10.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -24.5)
        (xy 43 -24.5)
        (xy 43 -26)
        (xy 44.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -38.5)
        (xy 7 -38.5)
        (xy 7 -40)
        (xy 8.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -28.5)
        (xy 31 -28.5)
        (xy 31 -30)
        (xy 32.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -8.5)
        (xy 51 -8.5)
        (xy 51 -10)
        (xy 52.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -40.5)
        (xy 25 -40.5)
        (xy 25 -42)
        (xy 26.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -38.5)
        (xy 13 -38.5)
        (xy 13 -40)
        (xy 14.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -30.5)
        (xy 9 -30.5)
        (xy 9 -32)
        (xy 10.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -44.5)
        (xy 9 -44.5)
        (xy 9 -46)
        (xy 10.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -40.5)
        (xy 7 -40.5)
        (xy 7 -42)
        (xy 8.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -6.5)
        (xy 47 -6.5)
        (xy 47 -8)
        (xy 48.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -2.5)
        (xy 13 -2.5)
        (xy 13 -4)
        (xy 14.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -6.5)
        (xy 15 -6.5)
        (xy 15 -8)
        (xy 16.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -8.5)
        (xy 35 -8.5)
        (xy 35 -10)
        (xy 36.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -18.5)
        (xy 51 -18.5)
        (xy 51 -20)
        (xy 52.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -20.5)
        (xy 9 -20.5)
        (xy 9 -22)
        (xy 10.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -20.5)
        (xy 19 -20.5)
        (xy 19 -22)
        (xy 20.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.5 -10.5)
        (xy 57 -10.5)
        (xy 57 -12)
        (xy 58.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -34.5)
        (xy 7 -34.5)
        (xy 7 -36)
        (xy 8.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -14.5)
        (xy 21 -14.5)
        (xy 21 -16)
        (xy 22.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -16.5)
        (xy 27 -16.5)
        (xy 27 -18)
        (xy 28.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -48.5)
        (xy 7 -48.5)
        (xy 7 -50)
        (xy 8.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -8.5)
        (xy 37 -8.5)
        (xy 37 -10)
        (xy 38.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -24.5)
        (xy 41 -24.5)
        (xy 41 -26)
        (xy 42.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -8.5)
        (xy 19 -8.5)
        (xy 19 -10)
        (xy 20.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -24.5)
        (xy 29 -24.5)
        (xy 29 -26)
        (xy 30.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -2.5)
        (xy 51 -2.5)
        (xy 51 -4)
        (xy 52.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.5 -8.5)
        (xy 73 -8.5)
        (xy 73 -10)
        (xy 74.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -30.5)
        (xy 11 -30.5)
        (xy 11 -32)
        (xy 12.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -18.5)
        (xy 13 -18.5)
        (xy 13 -20)
        (xy 14.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.5 -12.5)
        (xy 63 -12.5)
        (xy 63 -14)
        (xy 64.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -32.5)
        (xy 23 -32.5)
        (xy 23 -34)
        (xy 24.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.5 -4.5)
        (xy 61 -4.5)
        (xy 61 -6)
        (xy 62.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.5 -12.5)
        (xy 59 -12.5)
        (xy 59 -14)
        (xy 60.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -16.5)
        (xy 21 -16.5)
        (xy 21 -18)
        (xy 22.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -36.5)
        (xy 19 -36.5)
        (xy 19 -38)
        (xy 20.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -8.5)
        (xy 25 -8.5)
        (xy 25 -10)
        (xy 26.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.5 -2.5)
        (xy 71 -2.5)
        (xy 71 -4)
        (xy 72.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -4.5)
        (xy 21 -4.5)
        (xy 21 -6)
        (xy 22.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -20.5)
        (xy 27 -20.5)
        (xy 27 -22)
        (xy 28.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.5 -10.5)
        (xy 75 -10.5)
        (xy 75 -12)
        (xy 76.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.5 -12.5)
        (xy 67 -12.5)
        (xy 67 -14)
        (xy 68.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -12.5)
        (xy 33 -12.5)
        (xy 33 -14)
        (xy 34.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -18.5)
        (xy 23 -18.5)
        (xy 23 -20)
        (xy 24.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -34.5)
        (xy 41 -34.5)
        (xy 41 -36)
        (xy 42.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -48.5)
        (xy 29 -48.5)
        (xy 29 -50)
        (xy 30.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -4.5)
        (xy 9 -4.5)
        (xy 9 -6)
        (xy 10.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -24.5)
        (xy 27 -24.5)
        (xy 27 -26)
        (xy 28.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -4.5)
        (xy 17 -4.5)
        (xy 17 -6)
        (xy 18.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -6.5)
        (xy 49 -6.5)
        (xy 49 -8)
        (xy 50.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -12.5)
        (xy 37 -12.5)
        (xy 37 -14)
        (xy 38.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.5 -8.5)
        (xy 55 -8.5)
        (xy 55 -10)
        (xy 56.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -46.5)
        (xy 21 -46.5)
        (xy 21 -48)
        (xy 22.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.5 -4.5)
        (xy 73 -4.5)
        (xy 73 -6)
        (xy 74.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -6.5)
        (xy 29 -6.5)
        (xy 29 -8)
        (xy 30.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -22.5)
        (xy 17 -22.5)
        (xy 17 -24)
        (xy 18.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -46.5)
        (xy 25 -46.5)
        (xy 25 -48)
        (xy 26.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -30.5)
        (xy 17 -30.5)
        (xy 17 -32)
        (xy 18.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -14.5)
        (xy 11 -14.5)
        (xy 11 -16)
        (xy 12.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -20.5)
        (xy 47 -20.5)
        (xy 47 -22)
        (xy 48.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -38.5)
        (xy 19 -38.5)
        (xy 19 -40)
        (xy 20.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -6.5)
        (xy 39 -6.5)
        (xy 39 -8)
        (xy 40.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.5 -6.5)
        (xy 71 -6.5)
        (xy 71 -8)
        (xy 72.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -32.5)
        (xy 29 -32.5)
        (xy 29 -34)
        (xy 30.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -16.5)
        (xy 35 -16.5)
        (xy 35 -18)
        (xy 36.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -8.5)
        (xy 47 -8.5)
        (xy 47 -10)
        (xy 48.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -6.5)
        (xy 51 -6.5)
        (xy 51 -8)
        (xy 52.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -36.5)
        (xy 7 -36.5)
        (xy 7 -38)
        (xy 8.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -14.5)
        (xy 33 -14.5)
        (xy 33 -16)
        (xy 34.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -40.5)
        (xy 13 -40.5)
        (xy 13 -42)
        (xy 14.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -28.5)
        (xy 37 -28.5)
        (xy 37 -30)
        (xy 38.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -8.5)
        (xy 9 -8.5)
        (xy 9 -10)
        (xy 10.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -46.5)
        (xy 17 -46.5)
        (xy 17 -48)
        (xy 18.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -12.5)
        (xy 25 -12.5)
        (xy 25 -14)
        (xy 26.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -12.5)
        (xy 23 -12.5)
        (xy 23 -14)
        (xy 24.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -8.5)
        (xy 21 -8.5)
        (xy 21 -10)
        (xy 22.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -46.5)
        (xy 19 -46.5)
        (xy 19 -48)
        (xy 20.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -32.5)
        (xy 13 -32.5)
        (xy 13 -34)
        (xy 14.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -18.5)
        (xy 17 -18.5)
        (xy 17 -20)
        (xy 18.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -22.5)
        (xy 45 -22.5)
        (xy 45 -24)
        (xy 46.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -6.5)
        (xy 37 -6.5)
        (xy 37 -8)
        (xy 38.5 -8)
      )
    )
  )
  (zone (net 115) (net_name "3VFPGA") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.2) (thermal_bridge_width 0.2))
    (polygon
      (pts
        (xy 57 -50.5)
        (xy 39 -50.5)
        (xy 39 -68.5)
        (xy 57 -68.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -22.5)
        (xy 15 -22.5)
        (xy 15 -24)
        (xy 16.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -2.5)
        (xy 27 -2.5)
        (xy 27 -4)
        (xy 28.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -12.5)
        (xy 9 -12.5)
        (xy 9 -14)
        (xy 10.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.5 -8.5)
        (xy 61 -8.5)
        (xy 61 -10)
        (xy 62.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -32.5)
        (xy 17 -32.5)
        (xy 17 -34)
        (xy 18.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -38.5)
        (xy 11 -38.5)
        (xy 11 -40)
        (xy 12.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -12.5)
        (xy 17 -12.5)
        (xy 17 -14)
        (xy 18.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.5 -10.5)
        (xy 67 -10.5)
        (xy 67 -12)
        (xy 68.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -22.5)
        (xy 49 -22.5)
        (xy 49 -24)
        (xy 50.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -12.5)
        (xy 39 -12.5)
        (xy 39 -14)
        (xy 40.5 -14)
      )
    )
  )
  (zone (net 69) (net_name "+8V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.1 -87.55)
        (xy 170.1 -87.55)
        (xy 170.1 -77.05)
        (xy 165.6 -77.05)
        (xy 165.6 -92.55)
        (xy 174.1 -92.55)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -12.5)
        (xy 43 -12.5)
        (xy 43 -14)
        (xy 44.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -34.5)
        (xy 19 -34.5)
        (xy 19 -36)
        (xy 20.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -14.5)
        (xy 47 -14.5)
        (xy 47 -16)
        (xy 48.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -10.5)
        (xy 53 -10.5)
        (xy 53 -12)
        (xy 54.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -28.5)
        (xy 7 -28.5)
        (xy 7 -30)
        (xy 8.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.5 -6.5)
        (xy 61 -6.5)
        (xy 61 -8)
        (xy 62.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -12.5)
        (xy 31 -12.5)
        (xy 31 -14)
        (xy 32.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -30.5)
        (xy 7 -30.5)
        (xy 7 -32)
        (xy 8.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -6.5)
        (xy 33 -6.5)
        (xy 33 -8)
        (xy 34.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -14.5)
        (xy 45 -14.5)
        (xy 45 -16)
        (xy 46.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -24.5)
        (xy 45 -24.5)
        (xy 45 -26)
        (xy 46.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -46.5)
        (xy 27 -46.5)
        (xy 27 -48)
        (xy 28.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -34.5)
        (xy 9 -34.5)
        (xy 9 -36)
        (xy 10.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -44.5)
        (xy 15 -44.5)
        (xy 15 -46)
        (xy 16.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -26.5)
        (xy 11 -26.5)
        (xy 11 -28)
        (xy 12.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -32.5)
        (xy 31 -32.5)
        (xy 31 -34)
        (xy 32.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -28.5)
        (xy 25 -28.5)
        (xy 25 -30)
        (xy 26.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -44.5)
        (xy 17 -44.5)
        (xy 17 -46)
        (xy 18.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -20.5)
        (xy 43 -20.5)
        (xy 43 -22)
        (xy 44.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -8.5)
        (xy 49 -8.5)
        (xy 49 -10)
        (xy 50.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -32.5)
        (xy 25 -32.5)
        (xy 25 -34)
        (xy 26.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -42.5)
        (xy 15 -42.5)
        (xy 15 -44)
        (xy 16.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -4.5)
        (xy 11 -4.5)
        (xy 11 -6)
        (xy 12.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -14.5)
        (xy 35 -14.5)
        (xy 35 -16)
        (xy 36.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.5 -10.5)
        (xy 59 -10.5)
        (xy 59 -12)
        (xy 60.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.5 -4.5)
        (xy 75 -4.5)
        (xy 75 -6)
        (xy 76.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -2.5)
        (xy 45 -2.5)
        (xy 45 -4)
        (xy 46.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -24.5)
        (xy 7 -24.5)
        (xy 7 -26)
        (xy 8.5 -26)
      )
    )
  )
  (zone (net 70) (net_name "-8V") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 164.1 -87.55)
        (xy 160.1 -87.55)
        (xy 160.1 -77.05)
        (xy 155.6 -77.05)
        (xy 155.6 -92.55)
        (xy 164.1 -92.55)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -20.5)
        (xy 39 -20.5)
        (xy 39 -22)
        (xy 40.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -28.5)
        (xy 15 -28.5)
        (xy 15 -30)
        (xy 16.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -42.5)
        (xy 19 -42.5)
        (xy 19 -44)
        (xy 20.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -34.5)
        (xy 15 -34.5)
        (xy 15 -36)
        (xy 16.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -38.5)
        (xy 15 -38.5)
        (xy 15 -40)
        (xy 16.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -8.5)
        (xy 45 -8.5)
        (xy 45 -10)
        (xy 46.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.5 -2.5)
        (xy 77 -2.5)
        (xy 77 -4)
        (xy 78.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -22.5)
        (xy 25 -22.5)
        (xy 25 -24)
        (xy 26.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -18.5)
        (xy 33 -18.5)
        (xy 33 -20)
        (xy 34.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -14.5)
        (xy 41 -14.5)
        (xy 41 -16)
        (xy 42.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -4.5)
        (xy 37 -4.5)
        (xy 37 -6)
        (xy 38.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -20.5)
        (xy 7 -20.5)
        (xy 7 -22)
        (xy 8.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -26.5)
        (xy 33 -26.5)
        (xy 33 -28)
        (xy 34.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.5 -8.5)
        (xy 71 -8.5)
        (xy 71 -10)
        (xy 72.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -30.5)
        (xy 23 -30.5)
        (xy 23 -32)
        (xy 24.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -34.5)
        (xy 13 -34.5)
        (xy 13 -36)
        (xy 14.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -14.5)
        (xy 17 -14.5)
        (xy 17 -16)
        (xy 18.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -28.5)
        (xy 23 -28.5)
        (xy 23 -30)
        (xy 24.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -28.5)
        (xy 39 -28.5)
        (xy 39 -30)
        (xy 40.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -93.5)
        (xy 42.5 -93.5)
        (xy 42.5 -99.5)
        (xy 48.5 -99.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -24.5)
        (xy 49 -24.5)
        (xy 49 -26)
        (xy 50.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -38.5)
        (xy 17 -38.5)
        (xy 17 -40)
        (xy 18.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -4.5)
        (xy 51 -4.5)
        (xy 51 -6)
        (xy 52.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.5 -6.5)
        (xy 65 -6.5)
        (xy 65 -8)
        (xy 66.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.5 -8.5)
        (xy 77 -8.5)
        (xy 77 -10)
        (xy 78.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -6.5)
        (xy 45 -6.5)
        (xy 45 -8)
        (xy 46.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.5 -4.5)
        (xy 77 -4.5)
        (xy 77 -6)
        (xy 78.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -4.5)
        (xy 15 -4.5)
        (xy 15 -6)
        (xy 16.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -34.5)
        (xy 17 -34.5)
        (xy 17 -36)
        (xy 18.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -40.5)
        (xy 27 -40.5)
        (xy 27 -42)
        (xy 28.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -8.5)
        (xy 41 -8.5)
        (xy 41 -10)
        (xy 42.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -18.5)
        (xy 9 -18.5)
        (xy 9 -20)
        (xy 10.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -44.5)
        (xy 29 -44.5)
        (xy 29 -46)
        (xy 30.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -4.5)
        (xy 25 -4.5)
        (xy 25 -6)
        (xy 26.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.5 -10.5)
        (xy 61 -10.5)
        (xy 61 -12)
        (xy 62.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -10.5)
        (xy 17 -10.5)
        (xy 17 -12)
        (xy 18.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 78.5 -10.5)
        (xy 77 -10.5)
        (xy 77 -12)
        (xy 78.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -30.5)
        (xy 25 -30.5)
        (xy 25 -32)
        (xy 26.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -16.5)
        (xy 45 -16.5)
        (xy 45 -18)
        (xy 46.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -2.5)
        (xy 49 -2.5)
        (xy 49 -4)
        (xy 50.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -14.5)
        (xy 29 -14.5)
        (xy 29 -16)
        (xy 30.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -22.5)
        (xy 31 -22.5)
        (xy 31 -24)
        (xy 32.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -22.5)
        (xy 7 -22.5)
        (xy 7 -24)
        (xy 8.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -40.5)
        (xy 11 -40.5)
        (xy 11 -42)
        (xy 12.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -8.5)
        (xy 15 -8.5)
        (xy 15 -10)
        (xy 16.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -10.5)
        (xy 51 -10.5)
        (xy 51 -12)
        (xy 52.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -48.5)
        (xy 21 -48.5)
        (xy 21 -50)
        (xy 22.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -34.5)
        (xy 27 -34.5)
        (xy 27 -36)
        (xy 28.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -24.5)
        (xy 23 -24.5)
        (xy 23 -26)
        (xy 24.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -4.5)
        (xy 43 -4.5)
        (xy 43 -6)
        (xy 44.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -46.5)
        (xy 15 -46.5)
        (xy 15 -48)
        (xy 16.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -32.5)
        (xy 11 -32.5)
        (xy 11 -34)
        (xy 12.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 56.5 -4.5)
        (xy 55 -4.5)
        (xy 55 -6)
        (xy 56.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -4.5)
        (xy 19 -4.5)
        (xy 19 -6)
        (xy 20.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -2.5)
        (xy 41 -2.5)
        (xy 41 -4)
        (xy 42.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -30.5)
        (xy 37 -30.5)
        (xy 37 -32)
        (xy 38.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -10.5)
        (xy 23 -10.5)
        (xy 23 -12)
        (xy 24.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -40.5)
        (xy 15 -40.5)
        (xy 15 -42)
        (xy 16.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -14.5)
        (xy 53 -14.5)
        (xy 53 -16)
        (xy 54.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.5 -4.5)
        (xy 59 -4.5)
        (xy 59 -6)
        (xy 60.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.5 -12.5)
        (xy 73 -12.5)
        (xy 73 -14)
        (xy 74.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -22.5)
        (xy 47 -22.5)
        (xy 47 -24)
        (xy 48.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -30.5)
        (xy 29 -30.5)
        (xy 29 -32)
        (xy 30.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -42.5)
        (xy 25 -42.5)
        (xy 25 -44)
        (xy 26.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -16.5)
        (xy 37 -16.5)
        (xy 37 -18)
        (xy 38.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -12.5)
        (xy 13 -12.5)
        (xy 13 -14)
        (xy 14.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -28.5)
        (xy 27 -28.5)
        (xy 27 -30)
        (xy 28.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -26.5)
        (xy 7 -26.5)
        (xy 7 -28)
        (xy 8.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -22.5)
        (xy 11 -22.5)
        (xy 11 -24)
        (xy 12.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -36.5)
        (xy 33 -36.5)
        (xy 33 -38)
        (xy 34.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -16.5)
        (xy 19 -16.5)
        (xy 19 -18)
        (xy 20.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -16.5)
        (xy 41 -16.5)
        (xy 41 -18)
        (xy 42.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -22.5)
        (xy 51 -22.5)
        (xy 51 -24)
        (xy 52.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 6 -97)
        (xy 0 -97)
        (xy 0 -103)
        (xy 6 -103)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -48.5)
        (xy 11 -48.5)
        (xy 11 -50)
        (xy 12.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 52.5 -20.5)
        (xy 51 -20.5)
        (xy 51 -22)
        (xy 52.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -4.5)
        (xy 31 -4.5)
        (xy 31 -6)
        (xy 32.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -36.5)
        (xy 41 -36.5)
        (xy 41 -38)
        (xy 42.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -22.5)
        (xy 41 -22.5)
        (xy 41 -24)
        (xy 42.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -16.5)
        (xy 13 -16.5)
        (xy 13 -18)
        (xy 14.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -24.5)
        (xy 47 -24.5)
        (xy 47 -26)
        (xy 48.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -22.5)
        (xy 43 -22.5)
        (xy 43 -24)
        (xy 44.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -4.5)
        (xy 35 -4.5)
        (xy 35 -6)
        (xy 36.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -32.5)
        (xy 27 -32.5)
        (xy 27 -34)
        (xy 28.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175 -97)
        (xy 169 -97)
        (xy 169 -103)
        (xy 175 -103)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -8.5)
        (xy 11 -8.5)
        (xy 11 -10)
        (xy 12.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -42.5)
        (xy 7 -42.5)
        (xy 7 -44)
        (xy 8.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -18.5)
        (xy 19 -18.5)
        (xy 19 -20)
        (xy 20.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -38.5)
        (xy 25 -38.5)
        (xy 25 -40)
        (xy 26.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.5 -2.5)
        (xy 57 -2.5)
        (xy 57 -4)
        (xy 58.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -42.5)
        (xy 17 -42.5)
        (xy 17 -44)
        (xy 18.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.5 -4.5)
        (xy 57 -4.5)
        (xy 57 -6)
        (xy 58.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.5 -8.5)
        (xy 59 -8.5)
        (xy 59 -10)
        (xy 60.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -10.5)
        (xy 19 -10.5)
        (xy 19 -12)
        (xy 20.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -30.5)
        (xy 31 -30.5)
        (xy 31 -32)
        (xy 32.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -36.5)
        (xy 23 -36.5)
        (xy 23 -38)
        (xy 24.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -26.5)
        (xy 29 -26.5)
        (xy 29 -28)
        (xy 30.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.5 -4.5)
        (xy 67 -4.5)
        (xy 67 -6)
        (xy 68.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -20.5)
        (xy 23 -20.5)
        (xy 23 -22)
        (xy 24.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -22.5)
        (xy 37 -22.5)
        (xy 37 -24)
        (xy 38.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -18.5)
        (xy 25 -18.5)
        (xy 25 -20)
        (xy 26.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 32.5 -16.5)
        (xy 31 -16.5)
        (xy 31 -18)
        (xy 32.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -24.5)
        (xy 11 -24.5)
        (xy 11 -26)
        (xy 12.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -24.5)
        (xy 13 -24.5)
        (xy 13 -26)
        (xy 14.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.5 -10.5)
        (xy 69 -10.5)
        (xy 69 -12)
        (xy 70.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -6.5)
        (xy 21 -6.5)
        (xy 21 -8)
        (xy 22.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -42.5)
        (xy 13 -42.5)
        (xy 13 -44)
        (xy 14.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 72.5 -4.5)
        (xy 71 -4.5)
        (xy 71 -6)
        (xy 72.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -46.5)
        (xy 9 -46.5)
        (xy 9 -48)
        (xy 10.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -18.5)
        (xy 15 -18.5)
        (xy 15 -20)
        (xy 16.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -16.5)
        (xy 17 -16.5)
        (xy 17 -18)
        (xy 18.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -6.5)
        (xy 25 -6.5)
        (xy 25 -8)
        (xy 26.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -2.5)
        (xy 37 -2.5)
        (xy 37 -4)
        (xy 38.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -20.5)
        (xy 33 -20.5)
        (xy 33 -22)
        (xy 34.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -6.5)
        (xy 13 -6.5)
        (xy 13 -8)
        (xy 14.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -2.5)
        (xy 39 -2.5)
        (xy 39 -4)
        (xy 40.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101 -97)
        (xy 88 -97)
        (xy 88 -103)
        (xy 101 -103)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -36.5)
        (xy 17 -36.5)
        (xy 17 -38)
        (xy 18.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -22.5)
        (xy 13 -22.5)
        (xy 13 -24)
        (xy 14.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -36.5)
        (xy 39 -36.5)
        (xy 39 -38)
        (xy 40.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -24.5)
        (xy 39 -24.5)
        (xy 39 -26)
        (xy 40.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 58.5 -12.5)
        (xy 57 -12.5)
        (xy 57 -14)
        (xy 58.5 -14)
      )
    )
  )
  (zone (net 35) (net_name "/nvm_pcb_analog_ada/VADC") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 140.7 -38.9)
        (xy 140.9 -38.9)
        (xy 140.9 -35.9)
        (xy 143.3 -35.9)
        (xy 143.3 -35.3)
        (xy 141.3 -35.3)
        (xy 141.3 -32.5)
        (xy 140.1 -32.5)
        (xy 140.1 -29.3)
        (xy 137.9 -29.3)
        (xy 137.9 -30.7)
        (xy 136.7 -30.7)
        (xy 136.7 -32.7)
        (xy 139.1 -32.7)
        (xy 139.1 -33.9)
        (xy 140.3 -34.9)
        (xy 140.3 -35.5)
        (xy 139.9 -35.9)
        (xy 138.9 -35.9)
        (xy 138.5 -36.3)
        (xy 138.5 -38.1)
        (xy 136.1 -38.1)
        (xy 136.1 -39.1)
        (xy 138.5 -39.1)
        (xy 138.5 -40.9)
        (xy 140.7 -40.9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -30.5)
        (xy 13 -30.5)
        (xy 13 -32)
        (xy 14.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -44.5)
        (xy 19 -44.5)
        (xy 19 -46)
        (xy 20.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -2.5)
        (xy 7 -2.5)
        (xy 7 -4)
        (xy 8.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 76.5 -12.5)
        (xy 75 -12.5)
        (xy 75 -14)
        (xy 76.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -28.5)
        (xy 11 -28.5)
        (xy 11 -30)
        (xy 12.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -14.5)
        (xy 43 -14.5)
        (xy 43 -16)
        (xy 44.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -22.5)
        (xy 23 -22.5)
        (xy 23 -24)
        (xy 24.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 16.5 -24.5)
        (xy 15 -24.5)
        (xy 15 -26)
        (xy 16.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -30.5)
        (xy 27 -30.5)
        (xy 27 -32)
        (xy 28.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 60.5 -6.5)
        (xy 59 -6.5)
        (xy 59 -8)
        (xy 60.5 -8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -28.5)
        (xy 13 -28.5)
        (xy 13 -30)
        (xy 14.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -40.5)
        (xy 29 -40.5)
        (xy 29 -42)
        (xy 30.5 -42)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -2.5)
        (xy 23 -2.5)
        (xy 23 -4)
        (xy 24.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -38.5)
        (xy 27 -38.5)
        (xy 27 -40)
        (xy 28.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -32.5)
        (xy 9 -32.5)
        (xy 9 -34)
        (xy 10.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -14.5)
        (xy 39 -14.5)
        (xy 39 -16)
        (xy 40.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 28.5 -10.5)
        (xy 27 -10.5)
        (xy 27 -12)
        (xy 28.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -28.5)
        (xy 19 -28.5)
        (xy 19 -30)
        (xy 20.5 -30)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -44.5)
        (xy 13 -44.5)
        (xy 13 -46)
        (xy 14.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -18.5)
        (xy 11 -18.5)
        (xy 11 -20)
        (xy 12.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 68.5 -8.5)
        (xy 67 -8.5)
        (xy 67 -10)
        (xy 68.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -36.5)
        (xy 11 -36.5)
        (xy 11 -38)
        (xy 12.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -12.5)
        (xy 53 -12.5)
        (xy 53 -14)
        (xy 54.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -4.5)
        (xy 13 -4.5)
        (xy 13 -6)
        (xy 14.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -32.5)
        (xy 33 -32.5)
        (xy 33 -34)
        (xy 34.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -22.5)
        (xy 39 -22.5)
        (xy 39 -24)
        (xy 40.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -46.5)
        (xy 29 -46.5)
        (xy 29 -48)
        (xy 30.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -48.5)
        (xy 13 -48.5)
        (xy 13 -50)
        (xy 14.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -36.5)
        (xy 13 -36.5)
        (xy 13 -38)
        (xy 14.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -48.5)
        (xy 25 -48.5)
        (xy 25 -50)
        (xy 26.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.5 -8.5)
        (xy 63 -8.5)
        (xy 63 -10)
        (xy 64.5 -10)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -48.5)
        (xy 23 -48.5)
        (xy 23 -50)
        (xy 24.5 -50)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 48.5 -18.5)
        (xy 47 -18.5)
        (xy 47 -20)
        (xy 48.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 12.5 -44.5)
        (xy 11 -44.5)
        (xy 11 -46)
        (xy 12.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -34.5)
        (xy 29 -34.5)
        (xy 29 -36)
        (xy 30.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -32.5)
        (xy 19 -32.5)
        (xy 19 -34)
        (xy 20.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -16.5)
        (xy 25 -16.5)
        (xy 25 -18)
        (xy 26.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -22.5)
        (xy 19 -22.5)
        (xy 19 -24)
        (xy 20.5 -24)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -36.5)
        (xy 25 -36.5)
        (xy 25 -38)
        (xy 26.5 -38)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 26.5 -10.5)
        (xy 25 -10.5)
        (xy 25 -12)
        (xy 26.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -26.5)
        (xy 19 -26.5)
        (xy 19 -28)
        (xy 20.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -4.5)
        (xy 49 -4.5)
        (xy 49 -6)
        (xy 50.5 -6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 46.5 -10.5)
        (xy 45 -10.5)
        (xy 45 -12)
        (xy 46.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -14.5)
        (xy 9 -14.5)
        (xy 9 -16)
        (xy 10.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 14.5 -20.5)
        (xy 13 -20.5)
        (xy 13 -22)
        (xy 14.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -26.5)
        (xy 23 -26.5)
        (xy 23 -28)
        (xy 24.5 -28)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 50.5 -18.5)
        (xy 49 -18.5)
        (xy 49 -20)
        (xy 50.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -38.5)
        (xy 21 -38.5)
        (xy 21 -40)
        (xy 22.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 70.5 -2.5)
        (xy 69 -2.5)
        (xy 69 -4)
        (xy 70.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -42.5)
        (xy 29 -42.5)
        (xy 29 -44)
        (xy 30.5 -44)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -38.5)
        (xy 9 -38.5)
        (xy 9 -40)
        (xy 10.5 -40)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -12.5)
        (xy 21 -12.5)
        (xy 21 -14)
        (xy 22.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -44.5)
        (xy 21 -44.5)
        (xy 21 -46)
        (xy 22.5 -46)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 62.5 -12.5)
        (xy 61 -12.5)
        (xy 61 -14)
        (xy 62.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 42.5 -18.5)
        (xy 41 -18.5)
        (xy 41 -20)
        (xy 42.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 18.5 -20.5)
        (xy 17 -20.5)
        (xy 17 -22)
        (xy 18.5 -22)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.5 -12.5)
        (xy 65 -12.5)
        (xy 65 -14)
        (xy 66.5 -14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 38.5 -14.5)
        (xy 37 -14.5)
        (xy 37 -16)
        (xy 38.5 -16)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 34.5 -34.5)
        (xy 33 -34.5)
        (xy 33 -36)
        (xy 34.5 -36)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 10.5 -24.5)
        (xy 9 -24.5)
        (xy 9 -26)
        (xy 10.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 24.5 -46.5)
        (xy 23 -46.5)
        (xy 23 -48)
        (xy 24.5 -48)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 74.5 -2.5)
        (xy 73 -2.5)
        (xy 73 -4)
        (xy 74.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 30.5 -2.5)
        (xy 29 -2.5)
        (xy 29 -4)
        (xy 30.5 -4)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 20.5 -24.5)
        (xy 19 -24.5)
        (xy 19 -26)
        (xy 20.5 -26)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 40.5 -18.5)
        (xy 39 -18.5)
        (xy 39 -20)
        (xy 40.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 54.5 -18.5)
        (xy 53 -18.5)
        (xy 53 -20)
        (xy 54.5 -20)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 22.5 -10.5)
        (xy 21 -10.5)
        (xy 21 -12)
        (xy 22.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 36.5 -30.5)
        (xy 35 -30.5)
        (xy 35 -32)
        (xy 36.5 -32)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 8.5 -32.5)
        (xy 7 -32.5)
        (xy 7 -34)
        (xy 8.5 -34)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -16.5)
        (xy 43 -16.5)
        (xy 43 -18)
        (xy 44.5 -18)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 44.5 -10.5)
        (xy 43 -10.5)
        (xy 43 -12)
        (xy 44.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 64.5 -10.5)
        (xy 63 -10.5)
        (xy 63 -12)
        (xy 64.5 -12)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -5.5)
        (xy 32.5 -5.5)
        (xy 32.5 -7)
        (xy 31 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -13.5)
        (xy 38.5 -13.5)
        (xy 38.5 -15)
        (xy 37 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -23.5)
        (xy 46.5 -23.5)
        (xy 46.5 -25)
        (xy 45 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -11.5)
        (xy 20.5 -11.5)
        (xy 20.5 -13)
        (xy 19 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -15.5)
        (xy 66.5 -15.5)
        (xy 66.5 -17)
        (xy 65 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -31.5)
        (xy 36.5 -31.5)
        (xy 36.5 -33)
        (xy 35 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -17.5)
        (xy 72.5 -17.5)
        (xy 72.5 -19)
        (xy 71 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -33.5)
        (xy 10.5 -33.5)
        (xy 10.5 -35)
        (xy 9 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -17.5)
        (xy 60.5 -17.5)
        (xy 60.5 -19)
        (xy 59 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -3.5)
        (xy 40.5 -3.5)
        (xy 40.5 -5)
        (xy 39 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -19.5)
        (xy 22.5 -19.5)
        (xy 22.5 -21)
        (xy 21 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -15.5)
        (xy 36.5 -15.5)
        (xy 36.5 -17)
        (xy 35 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -19.5)
        (xy 60.5 -19.5)
        (xy 60.5 -21)
        (xy 59 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -9.5)
        (xy 56.5 -9.5)
        (xy 56.5 -11)
        (xy 55 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -17.5)
        (xy 68.5 -17.5)
        (xy 68.5 -19)
        (xy 67 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -19.5)
        (xy 24.5 -19.5)
        (xy 24.5 -21)
        (xy 23 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -9.5)
        (xy 40.5 -9.5)
        (xy 40.5 -11)
        (xy 39 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -5.5)
        (xy 54.5 -5.5)
        (xy 54.5 -7)
        (xy 53 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -13.5)
        (xy 54.5 -13.5)
        (xy 54.5 -15)
        (xy 53 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -5.5)
        (xy 72.5 -5.5)
        (xy 72.5 -7)
        (xy 71 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -21.5)
        (xy 24.5 -21.5)
        (xy 24.5 -23)
        (xy 23 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -21.5)
        (xy 76.5 -21.5)
        (xy 76.5 -23)
        (xy 75 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -7.5)
        (xy 52.5 -7.5)
        (xy 52.5 -9)
        (xy 51 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -31.5)
        (xy 52.5 -31.5)
        (xy 52.5 -33)
        (xy 51 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -1.5)
        (xy 70.5 -1.5)
        (xy 70.5 -3)
        (xy 69 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -9.5)
        (xy 26.5 -9.5)
        (xy 26.5 -11)
        (xy 25 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -9.5)
        (xy 64.5 -9.5)
        (xy 64.5 -11)
        (xy 63 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -25.5)
        (xy 34.5 -25.5)
        (xy 34.5 -27)
        (xy 33 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -25.5)
        (xy 36.5 -25.5)
        (xy 36.5 -27)
        (xy 35 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -15.5)
        (xy 20.5 -15.5)
        (xy 20.5 -17)
        (xy 19 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -3.5)
        (xy 72.5 -3.5)
        (xy 72.5 -5)
        (xy 71 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -21.5)
        (xy 40.5 -21.5)
        (xy 40.5 -23)
        (xy 39 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -29.5)
        (xy 22.5 -29.5)
        (xy 22.5 -31)
        (xy 21 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -15.5)
        (xy 50.5 -15.5)
        (xy 50.5 -17)
        (xy 49 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -11.5)
        (xy 12.5 -11.5)
        (xy 12.5 -13)
        (xy 11 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -11.5)
        (xy 66.5 -11.5)
        (xy 66.5 -13)
        (xy 65 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -7.5)
        (xy 26.5 -7.5)
        (xy 26.5 -9)
        (xy 25 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -5.5)
        (xy 64.5 -5.5)
        (xy 64.5 -7)
        (xy 63 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -9.5)
        (xy 36.5 -9.5)
        (xy 36.5 -11)
        (xy 35 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -19.5)
        (xy 36.5 -19.5)
        (xy 36.5 -21)
        (xy 35 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -9.5)
        (xy 14.5 -9.5)
        (xy 14.5 -11)
        (xy 13 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -9.5)
        (xy 10.5 -9.5)
        (xy 10.5 -11)
        (xy 9 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -17.5)
        (xy 46.5 -17.5)
        (xy 46.5 -19)
        (xy 45 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -23.5)
        (xy 56.5 -23.5)
        (xy 56.5 -25)
        (xy 55 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -23.5)
        (xy 68.5 -23.5)
        (xy 68.5 -25)
        (xy 67 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -17.5)
        (xy 42.5 -17.5)
        (xy 42.5 -19)
        (xy 41 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -25.5)
        (xy 22.5 -25.5)
        (xy 22.5 -27)
        (xy 21 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -25.5)
        (xy 50.5 -25.5)
        (xy 50.5 -27)
        (xy 49 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -15.5)
        (xy 16.5 -15.5)
        (xy 16.5 -17)
        (xy 15 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -21.5)
        (xy 18.5 -21.5)
        (xy 18.5 -23)
        (xy 17 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -13.5)
        (xy 52.5 -13.5)
        (xy 52.5 -15)
        (xy 51 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -25.5)
        (xy 32.5 -25.5)
        (xy 32.5 -27)
        (xy 31 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -7.5)
        (xy 58.5 -7.5)
        (xy 58.5 -9)
        (xy 57 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -1.5)
        (xy 12.5 -1.5)
        (xy 12.5 -3)
        (xy 11 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -13.5)
        (xy 62.5 -13.5)
        (xy 62.5 -15)
        (xy 61 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -5.5)
        (xy 10.5 -5.5)
        (xy 10.5 -7)
        (xy 9 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -17.5)
        (xy 38.5 -17.5)
        (xy 38.5 -19)
        (xy 37 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -23.5)
        (xy 52.5 -23.5)
        (xy 52.5 -25)
        (xy 51 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -7.5)
        (xy 10.5 -7.5)
        (xy 10.5 -9)
        (xy 9 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -27.5)
        (xy 18.5 -27.5)
        (xy 18.5 -29)
        (xy 17 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -11.5)
        (xy 68.5 -11.5)
        (xy 68.5 -13)
        (xy 67 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -31.5)
        (xy 20.5 -31.5)
        (xy 20.5 -33)
        (xy 19 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -35.5)
        (xy 40.5 -35.5)
        (xy 40.5 -37)
        (xy 39 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -35.5)
        (xy 14.5 -35.5)
        (xy 14.5 -37)
        (xy 13 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -7.5)
        (xy 24.5 -7.5)
        (xy 24.5 -9)
        (xy 23 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -31.5)
        (xy 30.5 -31.5)
        (xy 30.5 -33)
        (xy 29 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -29.5)
        (xy 18.5 -29.5)
        (xy 18.5 -31)
        (xy 17 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -27.5)
        (xy 32.5 -27.5)
        (xy 32.5 -29)
        (xy 31 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -11.5)
        (xy 42.5 -11.5)
        (xy 42.5 -13)
        (xy 41 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -11.5)
        (xy 76.5 -11.5)
        (xy 76.5 -13)
        (xy 75 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -1.5)
        (xy 10.5 -1.5)
        (xy 10.5 -3)
        (xy 9 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -19.5)
        (xy 40.5 -19.5)
        (xy 40.5 -21)
        (xy 39 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -11.5)
        (xy 26.5 -11.5)
        (xy 26.5 -13)
        (xy 25 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -23.5)
        (xy 26.5 -23.5)
        (xy 26.5 -25)
        (xy 25 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -1.5)
        (xy 46.5 -1.5)
        (xy 46.5 -3)
        (xy 45 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -17.5)
        (xy 40.5 -17.5)
        (xy 40.5 -19)
        (xy 39 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -31.5)
        (xy 40.5 -31.5)
        (xy 40.5 -33)
        (xy 39 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -25.5)
        (xy 48.5 -25.5)
        (xy 48.5 -27)
        (xy 47 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -19.5)
        (xy 20.5 -19.5)
        (xy 20.5 -21)
        (xy 19 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -1.5)
        (xy 72.5 -1.5)
        (xy 72.5 -3)
        (xy 71 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -11.5)
        (xy 24.5 -11.5)
        (xy 24.5 -13)
        (xy 23 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -1.5)
        (xy 30.5 -1.5)
        (xy 30.5 -3)
        (xy 29 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -33.5)
        (xy 22.5 -33.5)
        (xy 22.5 -35)
        (xy 21 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -21.5)
        (xy 22.5 -21.5)
        (xy 22.5 -23)
        (xy 21 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -35.5)
        (xy 10.5 -35.5)
        (xy 10.5 -37)
        (xy 9 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -19.5)
        (xy 54.5 -19.5)
        (xy 54.5 -21)
        (xy 53 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -27.5)
        (xy 48.5 -27.5)
        (xy 48.5 -29)
        (xy 47 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -5.5)
        (xy 18.5 -5.5)
        (xy 18.5 -7)
        (xy 17 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -15.5)
        (xy 12.5 -15.5)
        (xy 12.5 -17)
        (xy 11 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -23.5)
        (xy 66.5 -23.5)
        (xy 66.5 -25)
        (xy 65 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -1.5)
        (xy 32.5 -1.5)
        (xy 32.5 -3)
        (xy 31 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -23.5)
        (xy 10.5 -23.5)
        (xy 10.5 -25)
        (xy 9 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -19.5)
        (xy 44.5 -19.5)
        (xy 44.5 -21)
        (xy 43 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -7.5)
        (xy 30.5 -7.5)
        (xy 30.5 -9)
        (xy 29 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -25.5)
        (xy 8.5 -25.5)
        (xy 8.5 -27)
        (xy 7 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -1.5)
        (xy 54.5 -1.5)
        (xy 54.5 -3)
        (xy 53 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -19.5)
        (xy 74.5 -19.5)
        (xy 74.5 -21)
        (xy 73 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -19.5)
        (xy 68.5 -19.5)
        (xy 68.5 -21)
        (xy 67 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -17.5)
        (xy 26.5 -17.5)
        (xy 26.5 -19)
        (xy 25 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -21.5)
        (xy 42.5 -21.5)
        (xy 42.5 -23)
        (xy 41 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -23.5)
        (xy 24.5 -23.5)
        (xy 24.5 -25)
        (xy 23 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -21.5)
        (xy 50.5 -21.5)
        (xy 50.5 -23)
        (xy 49 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -33.5)
        (xy 46.5 -33.5)
        (xy 46.5 -35)
        (xy 45 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -17.5)
        (xy 50.5 -17.5)
        (xy 50.5 -19)
        (xy 49 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -9.5)
        (xy 16.5 -9.5)
        (xy 16.5 -11)
        (xy 15 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -29.5)
        (xy 16.5 -29.5)
        (xy 16.5 -31)
        (xy 15 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -15.5)
        (xy 56.5 -15.5)
        (xy 56.5 -17)
        (xy 55 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -25.5)
        (xy 42.5 -25.5)
        (xy 42.5 -27)
        (xy 41 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -5.5)
        (xy 30.5 -5.5)
        (xy 30.5 -7)
        (xy 29 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -9.5)
        (xy 18.5 -9.5)
        (xy 18.5 -11)
        (xy 17 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -5.5)
        (xy 24.5 -5.5)
        (xy 24.5 -7)
        (xy 23 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -1.5)
        (xy 40.5 -1.5)
        (xy 40.5 -3)
        (xy 39 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -9.5)
        (xy 78.5 -9.5)
        (xy 78.5 -11)
        (xy 77 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -1.5)
        (xy 58.5 -1.5)
        (xy 58.5 -3)
        (xy 57 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -15.5)
        (xy 8.5 -15.5)
        (xy 8.5 -17)
        (xy 7 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -23.5)
        (xy 16.5 -23.5)
        (xy 16.5 -25)
        (xy 15 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -17.5)
        (xy 32.5 -17.5)
        (xy 32.5 -19)
        (xy 31 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -7.5)
        (xy 22.5 -7.5)
        (xy 22.5 -9)
        (xy 21 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -9.5)
        (xy 42.5 -9.5)
        (xy 42.5 -11)
        (xy 41 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -5.5)
        (xy 36.5 -5.5)
        (xy 36.5 -7)
        (xy 35 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -29.5)
        (xy 50.5 -29.5)
        (xy 50.5 -31)
        (xy 49 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -31.5)
        (xy 34.5 -31.5)
        (xy 34.5 -33)
        (xy 33 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -7.5)
        (xy 20.5 -7.5)
        (xy 20.5 -9)
        (xy 19 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -21.5)
        (xy 36.5 -21.5)
        (xy 36.5 -23)
        (xy 35 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -21.5)
        (xy 38.5 -21.5)
        (xy 38.5 -23)
        (xy 37 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -7.5)
        (xy 72.5 -7.5)
        (xy 72.5 -9)
        (xy 71 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -35.5)
        (xy 50.5 -35.5)
        (xy 50.5 -37)
        (xy 49 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -9.5)
        (xy 22.5 -9.5)
        (xy 22.5 -11)
        (xy 21 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -23.5)
        (xy 48.5 -23.5)
        (xy 48.5 -25)
        (xy 47 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -11.5)
        (xy 34.5 -11.5)
        (xy 34.5 -13)
        (xy 33 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -21.5)
        (xy 52.5 -21.5)
        (xy 52.5 -23)
        (xy 51 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -9.5)
        (xy 28.5 -9.5)
        (xy 28.5 -11)
        (xy 27 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -27.5)
        (xy 30.5 -27.5)
        (xy 30.5 -29)
        (xy 29 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -17.5)
        (xy 12.5 -17.5)
        (xy 12.5 -19)
        (xy 11 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -21.5)
        (xy 72.5 -21.5)
        (xy 72.5 -23)
        (xy 71 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -21.5)
        (xy 32.5 -21.5)
        (xy 32.5 -23)
        (xy 31 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -7.5)
        (xy 42.5 -7.5)
        (xy 42.5 -9)
        (xy 41 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -23.5)
        (xy 36.5 -23.5)
        (xy 36.5 -25)
        (xy 35 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -29.5)
        (xy 40.5 -29.5)
        (xy 40.5 -31)
        (xy 39 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -31.5)
        (xy 32.5 -31.5)
        (xy 32.5 -33)
        (xy 31 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -1.5)
        (xy 18.5 -1.5)
        (xy 18.5 -3)
        (xy 17 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -33.5)
        (xy 32.5 -33.5)
        (xy 32.5 -35)
        (xy 31 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -27.5)
        (xy 12.5 -27.5)
        (xy 12.5 -29)
        (xy 11 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -35.5)
        (xy 22.5 -35.5)
        (xy 22.5 -37)
        (xy 21 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -15.5)
        (xy 14.5 -15.5)
        (xy 14.5 -17)
        (xy 13 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -17.5)
        (xy 16.5 -17.5)
        (xy 16.5 -19)
        (xy 15 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -9.5)
        (xy 54.5 -9.5)
        (xy 54.5 -11)
        (xy 53 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -7.5)
        (xy 68.5 -7.5)
        (xy 68.5 -9)
        (xy 67 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -19.5)
        (xy 18.5 -19.5)
        (xy 18.5 -21)
        (xy 17 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -31.5)
        (xy 42.5 -31.5)
        (xy 42.5 -33)
        (xy 41 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -11.5)
        (xy 62.5 -11.5)
        (xy 62.5 -13)
        (xy 61 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -13.5)
        (xy 58.5 -13.5)
        (xy 58.5 -15)
        (xy 57 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -11.5)
        (xy 40.5 -11.5)
        (xy 40.5 -13)
        (xy 39 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -19.5)
        (xy 48.5 -19.5)
        (xy 48.5 -21)
        (xy 47 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -27.5)
        (xy 50.5 -27.5)
        (xy 50.5 -29)
        (xy 49 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -21.5)
        (xy 74.5 -21.5)
        (xy 74.5 -23)
        (xy 73 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -1.5)
        (xy 76.5 -1.5)
        (xy 76.5 -3)
        (xy 75 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -35.5)
        (xy 28.5 -35.5)
        (xy 28.5 -37)
        (xy 27 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -5.5)
        (xy 60.5 -5.5)
        (xy 60.5 -7)
        (xy 59 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -9.5)
        (xy 38.5 -9.5)
        (xy 38.5 -11)
        (xy 37 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -15.5)
        (xy 54.5 -15.5)
        (xy 54.5 -17)
        (xy 53 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -13.5)
        (xy 18.5 -13.5)
        (xy 18.5 -15)
        (xy 17 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -5.5)
        (xy 12.5 -5.5)
        (xy 12.5 -7)
        (xy 11 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -33.5)
        (xy 12.5 -33.5)
        (xy 12.5 -35)
        (xy 11 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -29.5)
        (xy 32.5 -29.5)
        (xy 32.5 -31)
        (xy 31 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -13.5)
        (xy 12.5 -13.5)
        (xy 12.5 -15)
        (xy 11 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -3.5)
        (xy 34.5 -3.5)
        (xy 34.5 -5)
        (xy 33 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -33.5)
        (xy 18.5 -33.5)
        (xy 18.5 -35)
        (xy 17 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -35.5)
        (xy 52.5 -35.5)
        (xy 52.5 -37)
        (xy 51 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -29.5)
        (xy 8.5 -29.5)
        (xy 8.5 -31)
        (xy 7 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -7.5)
        (xy 76.5 -7.5)
        (xy 76.5 -9)
        (xy 75 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -15.5)
        (xy 78.5 -15.5)
        (xy 78.5 -17)
        (xy 77 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -11.5)
        (xy 36.5 -11.5)
        (xy 36.5 -13)
        (xy 35 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -21.5)
        (xy 20.5 -21.5)
        (xy 20.5 -23)
        (xy 19 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -13.5)
        (xy 78.5 -13.5)
        (xy 78.5 -15)
        (xy 77 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -17.5)
        (xy 34.5 -17.5)
        (xy 34.5 -19)
        (xy 33 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -7.5)
        (xy 28.5 -7.5)
        (xy 28.5 -9)
        (xy 27 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -21.5)
        (xy 44.5 -21.5)
        (xy 44.5 -23)
        (xy 43 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -5.5)
        (xy 34.5 -5.5)
        (xy 34.5 -7)
        (xy 33 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -3.5)
        (xy 26.5 -3.5)
        (xy 26.5 -5)
        (xy 25 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -33.5)
        (xy 8.5 -33.5)
        (xy 8.5 -35)
        (xy 7 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -5.5)
        (xy 38.5 -5.5)
        (xy 38.5 -7)
        (xy 37 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -9.5)
        (xy 30.5 -9.5)
        (xy 30.5 -11)
        (xy 29 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -11.5)
        (xy 50.5 -11.5)
        (xy 50.5 -13)
        (xy 49 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -1.5)
        (xy 48.5 -1.5)
        (xy 48.5 -3)
        (xy 47 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -17.5)
        (xy 36.5 -17.5)
        (xy 36.5 -19)
        (xy 35 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -19.5)
        (xy 58.5 -19.5)
        (xy 58.5 -21)
        (xy 57 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -29.5)
        (xy 10.5 -29.5)
        (xy 10.5 -31)
        (xy 9 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -17.5)
        (xy 44.5 -17.5)
        (xy 44.5 -19)
        (xy 43 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -19.5)
        (xy 50.5 -19.5)
        (xy 50.5 -21)
        (xy 49 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -35.5)
        (xy 30.5 -35.5)
        (xy 30.5 -37)
        (xy 29 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -27.5)
        (xy 22.5 -27.5)
        (xy 22.5 -29)
        (xy 21 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -15.5)
        (xy 74.5 -15.5)
        (xy 74.5 -17)
        (xy 73 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -31.5)
        (xy 18.5 -31.5)
        (xy 18.5 -33)
        (xy 17 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -15.5)
        (xy 18.5 -15.5)
        (xy 18.5 -17)
        (xy 17 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -19.5)
        (xy 28.5 -19.5)
        (xy 28.5 -21)
        (xy 27 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -21.5)
        (xy 56.5 -21.5)
        (xy 56.5 -23)
        (xy 55 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -13.5)
        (xy 10.5 -13.5)
        (xy 10.5 -15)
        (xy 9 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -11.5)
        (xy 58.5 -11.5)
        (xy 58.5 -13)
        (xy 57 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -1.5)
        (xy 52.5 -1.5)
        (xy 52.5 -3)
        (xy 51 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -3.5)
        (xy 54.5 -3.5)
        (xy 54.5 -5)
        (xy 53 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -29.5)
        (xy 48.5 -29.5)
        (xy 48.5 -31)
        (xy 47 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -35.5)
        (xy 18.5 -35.5)
        (xy 18.5 -37)
        (xy 17 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -33.5)
        (xy 50.5 -33.5)
        (xy 50.5 -35)
        (xy 49 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -19.5)
        (xy 52.5 -19.5)
        (xy 52.5 -21)
        (xy 51 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -17.5)
        (xy 58.5 -17.5)
        (xy 58.5 -19)
        (xy 57 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -5.5)
        (xy 40.5 -5.5)
        (xy 40.5 -7)
        (xy 39 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -27.5)
        (xy 38.5 -27.5)
        (xy 38.5 -29)
        (xy 37 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -35.5)
        (xy 16.5 -35.5)
        (xy 16.5 -37)
        (xy 15 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -21.5)
        (xy 30.5 -21.5)
        (xy 30.5 -23)
        (xy 29 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -9.5)
        (xy 46.5 -9.5)
        (xy 46.5 -11)
        (xy 45 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -3.5)
        (xy 46.5 -3.5)
        (xy 46.5 -5)
        (xy 45 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -3.5)
        (xy 44.5 -3.5)
        (xy 44.5 -5)
        (xy 43 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -3.5)
        (xy 58.5 -3.5)
        (xy 58.5 -5)
        (xy 57 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -11.5)
        (xy 30.5 -11.5)
        (xy 30.5 -13)
        (xy 29 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -35.5)
        (xy 20.5 -35.5)
        (xy 20.5 -37)
        (xy 19 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -21.5)
        (xy 60.5 -21.5)
        (xy 60.5 -23)
        (xy 59 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -17.5)
        (xy 70.5 -17.5)
        (xy 70.5 -19)
        (xy 69 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -19.5)
        (xy 26.5 -19.5)
        (xy 26.5 -21)
        (xy 25 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -17.5)
        (xy 30.5 -17.5)
        (xy 30.5 -19)
        (xy 29 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -15.5)
        (xy 32.5 -15.5)
        (xy 32.5 -17)
        (xy 31 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -15.5)
        (xy 10.5 -15.5)
        (xy 10.5 -17)
        (xy 9 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -25.5)
        (xy 44.5 -25.5)
        (xy 44.5 -27)
        (xy 43 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -5.5)
        (xy 74.5 -5.5)
        (xy 74.5 -7)
        (xy 73 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -5.5)
        (xy 8.5 -5.5)
        (xy 8.5 -7)
        (xy 7 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -13.5)
        (xy 26.5 -13.5)
        (xy 26.5 -15)
        (xy 25 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -25.5)
        (xy 30.5 -25.5)
        (xy 30.5 -27)
        (xy 29 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -11.5)
        (xy 38.5 -11.5)
        (xy 38.5 -13)
        (xy 37 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -9.5)
        (xy 70.5 -9.5)
        (xy 70.5 -11)
        (xy 69 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -13.5)
        (xy 66.5 -13.5)
        (xy 66.5 -15)
        (xy 65 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -11.5)
        (xy 70.5 -11.5)
        (xy 70.5 -13)
        (xy 69 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -9.5)
        (xy 76.5 -9.5)
        (xy 76.5 -11)
        (xy 75 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -5.5)
        (xy 20.5 -5.5)
        (xy 20.5 -7)
        (xy 19 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -17.5)
        (xy 76.5 -17.5)
        (xy 76.5 -19)
        (xy 75 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -11.5)
        (xy 10.5 -11.5)
        (xy 10.5 -13)
        (xy 9 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -11.5)
        (xy 14.5 -11.5)
        (xy 14.5 -13)
        (xy 13 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -15.5)
        (xy 42.5 -15.5)
        (xy 42.5 -17)
        (xy 41 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -13.5)
        (xy 34.5 -13.5)
        (xy 34.5 -15)
        (xy 33 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -29.5)
        (xy 20.5 -29.5)
        (xy 20.5 -31)
        (xy 19 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -9.5)
        (xy 62.5 -9.5)
        (xy 62.5 -11)
        (xy 61 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -23.5)
        (xy 70.5 -23.5)
        (xy 70.5 -25)
        (xy 69 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -23.5)
        (xy 78.5 -23.5)
        (xy 78.5 -25)
        (xy 77 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -1.5)
        (xy 38.5 -1.5)
        (xy 38.5 -3)
        (xy 37 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -1.5)
        (xy 56.5 -1.5)
        (xy 56.5 -3)
        (xy 55 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -7.5)
        (xy 18.5 -7.5)
        (xy 18.5 -9)
        (xy 17 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -9.5)
        (xy 8.5 -9.5)
        (xy 8.5 -11)
        (xy 7 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -9.5)
        (xy 24.5 -9.5)
        (xy 24.5 -11)
        (xy 23 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -15.5)
        (xy 72.5 -15.5)
        (xy 72.5 -17)
        (xy 71 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -17.5)
        (xy 10.5 -17.5)
        (xy 10.5 -19)
        (xy 9 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -11.5)
        (xy 16.5 -11.5)
        (xy 16.5 -13)
        (xy 15 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -27.5)
        (xy 8.5 -27.5)
        (xy 8.5 -29)
        (xy 7 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -19.5)
        (xy 32.5 -19.5)
        (xy 32.5 -21)
        (xy 31 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -27.5)
        (xy 24.5 -27.5)
        (xy 24.5 -29)
        (xy 23 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -29.5)
        (xy 12.5 -29.5)
        (xy 12.5 -31)
        (xy 11 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -33.5)
        (xy 48.5 -33.5)
        (xy 48.5 -35)
        (xy 47 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -1.5)
        (xy 68.5 -1.5)
        (xy 68.5 -3)
        (xy 67 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -7.5)
        (xy 44.5 -7.5)
        (xy 44.5 -9)
        (xy 43 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -3.5)
        (xy 50.5 -3.5)
        (xy 50.5 -5)
        (xy 49 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -7.5)
        (xy 36.5 -7.5)
        (xy 36.5 -9)
        (xy 35 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -7.5)
        (xy 66.5 -7.5)
        (xy 66.5 -9)
        (xy 65 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -13.5)
        (xy 20.5 -13.5)
        (xy 20.5 -15)
        (xy 19 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -29.5)
        (xy 42.5 -29.5)
        (xy 42.5 -31)
        (xy 41 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -15.5)
        (xy 26.5 -15.5)
        (xy 26.5 -17)
        (xy 25 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -3.5)
        (xy 68.5 -3.5)
        (xy 68.5 -5)
        (xy 67 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -21.5)
        (xy 70.5 -21.5)
        (xy 70.5 -23)
        (xy 69 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -9.5)
        (xy 60.5 -9.5)
        (xy 60.5 -11)
        (xy 59 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -3.5)
        (xy 14.5 -3.5)
        (xy 14.5 -5)
        (xy 13 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -29.5)
        (xy 26.5 -29.5)
        (xy 26.5 -31)
        (xy 25 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -19.5)
        (xy 78.5 -19.5)
        (xy 78.5 -21)
        (xy 77 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -7.5)
        (xy 60.5 -7.5)
        (xy 60.5 -9)
        (xy 59 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -27.5)
        (xy 10.5 -27.5)
        (xy 10.5 -29)
        (xy 9 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -5.5)
        (xy 56.5 -5.5)
        (xy 56.5 -7)
        (xy 55 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -31.5)
        (xy 14.5 -31.5)
        (xy 14.5 -33)
        (xy 13 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -35.5)
        (xy 24.5 -35.5)
        (xy 24.5 -37)
        (xy 23 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -3.5)
        (xy 52.5 -3.5)
        (xy 52.5 -5)
        (xy 51 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -29.5)
        (xy 44.5 -29.5)
        (xy 44.5 -31)
        (xy 43 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -27.5)
        (xy 28.5 -27.5)
        (xy 28.5 -29)
        (xy 27 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -1.5)
        (xy 50.5 -1.5)
        (xy 50.5 -3)
        (xy 49 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -25.5)
        (xy 10.5 -25.5)
        (xy 10.5 -27)
        (xy 9 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -33.5)
        (xy 44.5 -33.5)
        (xy 44.5 -35)
        (xy 43 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -15.5)
        (xy 62.5 -15.5)
        (xy 62.5 -17)
        (xy 61 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -33.5)
        (xy 40.5 -33.5)
        (xy 40.5 -35)
        (xy 39 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -17.5)
        (xy 62.5 -17.5)
        (xy 62.5 -19)
        (xy 61 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -3.5)
        (xy 76.5 -3.5)
        (xy 76.5 -5)
        (xy 75 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -1.5)
        (xy 8.5 -1.5)
        (xy 8.5 -3)
        (xy 7 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -5.5)
        (xy 22.5 -5.5)
        (xy 22.5 -7)
        (xy 21 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -15.5)
        (xy 24.5 -15.5)
        (xy 24.5 -17)
        (xy 23 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -33.5)
        (xy 42.5 -33.5)
        (xy 42.5 -35)
        (xy 41 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -1.5)
        (xy 36.5 -1.5)
        (xy 36.5 -3)
        (xy 35 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -35.5)
        (xy 36.5 -35.5)
        (xy 36.5 -37)
        (xy 35 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -15.5)
        (xy 64.5 -15.5)
        (xy 64.5 -17)
        (xy 63 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -9.5)
        (xy 74.5 -9.5)
        (xy 74.5 -11)
        (xy 73 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -21.5)
        (xy 34.5 -21.5)
        (xy 34.5 -23)
        (xy 33 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -5.5)
        (xy 66.5 -5.5)
        (xy 66.5 -7)
        (xy 65 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -19.5)
        (xy 62.5 -19.5)
        (xy 62.5 -21)
        (xy 61 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -29.5)
        (xy 54.5 -29.5)
        (xy 54.5 -31)
        (xy 53 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -3.5)
        (xy 42.5 -3.5)
        (xy 42.5 -5)
        (xy 41 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -19.5)
        (xy 72.5 -19.5)
        (xy 72.5 -21)
        (xy 71 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -13.5)
        (xy 42.5 -13.5)
        (xy 42.5 -15)
        (xy 41 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -13.5)
        (xy 44.5 -13.5)
        (xy 44.5 -15)
        (xy 43 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -23.5)
        (xy 8.5 -23.5)
        (xy 8.5 -25)
        (xy 7 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -17.5)
        (xy 48.5 -17.5)
        (xy 48.5 -19)
        (xy 47 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -1.5)
        (xy 20.5 -1.5)
        (xy 20.5 -3)
        (xy 19 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -3.5)
        (xy 30.5 -3.5)
        (xy 30.5 -5)
        (xy 29 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -11.5)
        (xy 74.5 -11.5)
        (xy 74.5 -13)
        (xy 73 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -23.5)
        (xy 12.5 -23.5)
        (xy 12.5 -25)
        (xy 11 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -33.5)
        (xy 24.5 -33.5)
        (xy 24.5 -35)
        (xy 23 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -13.5)
        (xy 22.5 -13.5)
        (xy 22.5 -15)
        (xy 21 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -13.5)
        (xy 32.5 -13.5)
        (xy 32.5 -15)
        (xy 31 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -13.5)
        (xy 8.5 -13.5)
        (xy 8.5 -15)
        (xy 7 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -29.5)
        (xy 38.5 -29.5)
        (xy 38.5 -31)
        (xy 37 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -3.5)
        (xy 38.5 -3.5)
        (xy 38.5 -5)
        (xy 37 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -5.5)
        (xy 26.5 -5.5)
        (xy 26.5 -7)
        (xy 25 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -35.5)
        (xy 12.5 -35.5)
        (xy 12.5 -37)
        (xy 11 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -15.5)
        (xy 76.5 -15.5)
        (xy 76.5 -17)
        (xy 75 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -17.5)
        (xy 24.5 -17.5)
        (xy 24.5 -19)
        (xy 23 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -13.5)
        (xy 24.5 -13.5)
        (xy 24.5 -15)
        (xy 23 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -11.5)
        (xy 46.5 -11.5)
        (xy 46.5 -13)
        (xy 45 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -13.5)
        (xy 48.5 -13.5)
        (xy 48.5 -15)
        (xy 47 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -23.5)
        (xy 40.5 -23.5)
        (xy 40.5 -25)
        (xy 39 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -21.5)
        (xy 28.5 -21.5)
        (xy 28.5 -23)
        (xy 27 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -35.5)
        (xy 38.5 -35.5)
        (xy 38.5 -37)
        (xy 37 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -13.5)
        (xy 72.5 -13.5)
        (xy 72.5 -15)
        (xy 71 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -27.5)
        (xy 16.5 -27.5)
        (xy 16.5 -29)
        (xy 15 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -25.5)
        (xy 38.5 -25.5)
        (xy 38.5 -27)
        (xy 37 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -21.5)
        (xy 12.5 -21.5)
        (xy 12.5 -23)
        (xy 11 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -17.5)
        (xy 18.5 -17.5)
        (xy 18.5 -19)
        (xy 17 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -7.5)
        (xy 46.5 -7.5)
        (xy 46.5 -9)
        (xy 45 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -31.5)
        (xy 26.5 -31.5)
        (xy 26.5 -33)
        (xy 25 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -11.5)
        (xy 56.5 -11.5)
        (xy 56.5 -13)
        (xy 55 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -23.5)
        (xy 38.5 -23.5)
        (xy 38.5 -25)
        (xy 37 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -27.5)
        (xy 20.5 -27.5)
        (xy 20.5 -29)
        (xy 19 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -25.5)
        (xy 24.5 -25.5)
        (xy 24.5 -27)
        (xy 23 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -31.5)
        (xy 38.5 -31.5)
        (xy 38.5 -33)
        (xy 37 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -15.5)
        (xy 22.5 -15.5)
        (xy 22.5 -17)
        (xy 21 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -29.5)
        (xy 34.5 -29.5)
        (xy 34.5 -31)
        (xy 33 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -1.5)
        (xy 22.5 -1.5)
        (xy 22.5 -3)
        (xy 21 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -17.5)
        (xy 78.5 -17.5)
        (xy 78.5 -19)
        (xy 77 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -17.5)
        (xy 20.5 -17.5)
        (xy 20.5 -19)
        (xy 19 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -23.5)
        (xy 50.5 -23.5)
        (xy 50.5 -25)
        (xy 49 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -7.5)
        (xy 64.5 -7.5)
        (xy 64.5 -9)
        (xy 63 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -13.5)
        (xy 60.5 -13.5)
        (xy 60.5 -15)
        (xy 59 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -27.5)
        (xy 44.5 -27.5)
        (xy 44.5 -29)
        (xy 43 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -7.5)
        (xy 32.5 -7.5)
        (xy 32.5 -9)
        (xy 31 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -33.5)
        (xy 20.5 -33.5)
        (xy 20.5 -35)
        (xy 19 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -5.5)
        (xy 70.5 -5.5)
        (xy 70.5 -7)
        (xy 69 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -23.5)
        (xy 22.5 -23.5)
        (xy 22.5 -25)
        (xy 21 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -13.5)
        (xy 76.5 -13.5)
        (xy 76.5 -15)
        (xy 75 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -1.5)
        (xy 24.5 -1.5)
        (xy 24.5 -3)
        (xy 23 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -29.5)
        (xy 52.5 -29.5)
        (xy 52.5 -31)
        (xy 51 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -3.5)
        (xy 66.5 -3.5)
        (xy 66.5 -5)
        (xy 65 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -15.5)
        (xy 38.5 -15.5)
        (xy 38.5 -17)
        (xy 37 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -23.5)
        (xy 54.5 -23.5)
        (xy 54.5 -25)
        (xy 53 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -9.5)
        (xy 52.5 -9.5)
        (xy 52.5 -11)
        (xy 51 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -31.5)
        (xy 46.5 -31.5)
        (xy 46.5 -33)
        (xy 45 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -9.5)
        (xy 12.5 -9.5)
        (xy 12.5 -11)
        (xy 11 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -13.5)
        (xy 74.5 -13.5)
        (xy 74.5 -15)
        (xy 73 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -3.5)
        (xy 28.5 -3.5)
        (xy 28.5 -5)
        (xy 27 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -1.5)
        (xy 60.5 -1.5)
        (xy 60.5 -3)
        (xy 59 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -29.5)
        (xy 14.5 -29.5)
        (xy 14.5 -31)
        (xy 13 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -33.5)
        (xy 34.5 -33.5)
        (xy 34.5 -35)
        (xy 33 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -15.5)
        (xy 40.5 -15.5)
        (xy 40.5 -17)
        (xy 39 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -3.5)
        (xy 8.5 -3.5)
        (xy 8.5 -5)
        (xy 7 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -25.5)
        (xy 26.5 -25.5)
        (xy 26.5 -27)
        (xy 25 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -1.5)
        (xy 28.5 -1.5)
        (xy 28.5 -3)
        (xy 27 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -1.5)
        (xy 78.5 -1.5)
        (xy 78.5 -3)
        (xy 77 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -5.5)
        (xy 62.5 -5.5)
        (xy 62.5 -7)
        (xy 61 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -13.5)
        (xy 14.5 -13.5)
        (xy 14.5 -15)
        (xy 13 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -9.5)
        (xy 44.5 -9.5)
        (xy 44.5 -11)
        (xy 43 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -21.5)
        (xy 62.5 -21.5)
        (xy 62.5 -23)
        (xy 61 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -23.5)
        (xy 32.5 -23.5)
        (xy 32.5 -25)
        (xy 31 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -7.5)
        (xy 78.5 -7.5)
        (xy 78.5 -9)
        (xy 77 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -31.5)
        (xy 24.5 -31.5)
        (xy 24.5 -33)
        (xy 23 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -25.5)
        (xy 40.5 -25.5)
        (xy 40.5 -27)
        (xy 39 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -23.5)
        (xy 30.5 -23.5)
        (xy 30.5 -25)
        (xy 29 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -33.5)
        (xy 16.5 -33.5)
        (xy 16.5 -35)
        (xy 15 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -19.5)
        (xy 64.5 -19.5)
        (xy 64.5 -21)
        (xy 63 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -31.5)
        (xy 22.5 -31.5)
        (xy 22.5 -33)
        (xy 21 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -1.5)
        (xy 44.5 -1.5)
        (xy 44.5 -3)
        (xy 43 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -25.5)
        (xy 52.5 -25.5)
        (xy 52.5 -27)
        (xy 51 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -21.5)
        (xy 48.5 -21.5)
        (xy 48.5 -23)
        (xy 47 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -19.5)
        (xy 42.5 -19.5)
        (xy 42.5 -21)
        (xy 41 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -5.5)
        (xy 78.5 -5.5)
        (xy 78.5 -7)
        (xy 77 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -3.5)
        (xy 20.5 -3.5)
        (xy 20.5 -5)
        (xy 19 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -13.5)
        (xy 50.5 -13.5)
        (xy 50.5 -15)
        (xy 49 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -5.5)
        (xy 76.5 -5.5)
        (xy 76.5 -7)
        (xy 75 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -15.5)
        (xy 48.5 -15.5)
        (xy 48.5 -17)
        (xy 47 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -5.5)
        (xy 42.5 -5.5)
        (xy 42.5 -7)
        (xy 41 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -33.5)
        (xy 38.5 -33.5)
        (xy 38.5 -35)
        (xy 37 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -27.5)
        (xy 26.5 -27.5)
        (xy 26.5 -29)
        (xy 25 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -19.5)
        (xy 10.5 -19.5)
        (xy 10.5 -21)
        (xy 9 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -27.5)
        (xy 40.5 -27.5)
        (xy 40.5 -29)
        (xy 39 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -15.5)
        (xy 46.5 -15.5)
        (xy 46.5 -17)
        (xy 45 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -3.5)
        (xy 56.5 -3.5)
        (xy 56.5 -5)
        (xy 55 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -33.5)
        (xy 30.5 -33.5)
        (xy 30.5 -35)
        (xy 29 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -3.5)
        (xy 32.5 -3.5)
        (xy 32.5 -5)
        (xy 31 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -7.5)
        (xy 12.5 -7.5)
        (xy 12.5 -9)
        (xy 11 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -27.5)
        (xy 46.5 -27.5)
        (xy 46.5 -29)
        (xy 45 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -27.5)
        (xy 14.5 -27.5)
        (xy 14.5 -29)
        (xy 13 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -11.5)
        (xy 8.5 -11.5)
        (xy 8.5 -13)
        (xy 7 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -5.5)
        (xy 16.5 -5.5)
        (xy 16.5 -7)
        (xy 15 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -13.5)
        (xy 68.5 -13.5)
        (xy 68.5 -15)
        (xy 67 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -27.5)
        (xy 42.5 -27.5)
        (xy 42.5 -29)
        (xy 41 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -5.5)
        (xy 28.5 -5.5)
        (xy 28.5 -7)
        (xy 27 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -3.5)
        (xy 16.5 -3.5)
        (xy 16.5 -5)
        (xy 15 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -35.5)
        (xy 48.5 -35.5)
        (xy 48.5 -37)
        (xy 47 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -15.5)
        (xy 34.5 -15.5)
        (xy 34.5 -17)
        (xy 33 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -13.5)
        (xy 36.5 -13.5)
        (xy 36.5 -15)
        (xy 35 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -1.5)
        (xy 34.5 -1.5)
        (xy 34.5 -3)
        (xy 33 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -11.5)
        (xy 48.5 -11.5)
        (xy 48.5 -13)
        (xy 47 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -11.5)
        (xy 64.5 -11.5)
        (xy 64.5 -13)
        (xy 63 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -17.5)
        (xy 64.5 -17.5)
        (xy 64.5 -19)
        (xy 63 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -9.5)
        (xy 32.5 -9.5)
        (xy 32.5 -11)
        (xy 31 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -17.5)
        (xy 66.5 -17.5)
        (xy 66.5 -19)
        (xy 65 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -11.5)
        (xy 72.5 -11.5)
        (xy 72.5 -13)
        (xy 71 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -5.5)
        (xy 58.5 -5.5)
        (xy 58.5 -7)
        (xy 57 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -35.5)
        (xy 32.5 -35.5)
        (xy 32.5 -37)
        (xy 31 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -13.5)
        (xy 40.5 -13.5)
        (xy 40.5 -15)
        (xy 39 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -3.5)
        (xy 48.5 -3.5)
        (xy 48.5 -5)
        (xy 47 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -11.5)
        (xy 28.5 -11.5)
        (xy 28.5 -13)
        (xy 27 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -15.5)
        (xy 44.5 -15.5)
        (xy 44.5 -17)
        (xy 43 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -3.5)
        (xy 60.5 -3.5)
        (xy 60.5 -5)
        (xy 59 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -15.5)
        (xy 68.5 -15.5)
        (xy 68.5 -17)
        (xy 67 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -7.5)
        (xy 70.5 -7.5)
        (xy 70.5 -9)
        (xy 69 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -1.5)
        (xy 26.5 -1.5)
        (xy 26.5 -3)
        (xy 25 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -9.5)
        (xy 48.5 -9.5)
        (xy 48.5 -11)
        (xy 47 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -3.5)
        (xy 24.5 -3.5)
        (xy 24.5 -5)
        (xy 23 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -29.5)
        (xy 36.5 -29.5)
        (xy 36.5 -31)
        (xy 35 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -23.5)
        (xy 28.5 -23.5)
        (xy 28.5 -25)
        (xy 27 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -21.5)
        (xy 8.5 -21.5)
        (xy 8.5 -23)
        (xy 7 -23)
      )
    )
  )
  (zone (net 23) (net_name "GNDA") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.25))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.25) (thermal_bridge_width 0.25))
    (polygon
      (pts
        (xy 175 -48.5)
        (xy 156.5 -48.5)
        (xy 156.5 0)
        (xy 0 0)
        (xy 0 -103)
        (xy 175 -103)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -1.5)
        (xy 64.5 -1.5)
        (xy 64.5 -3)
        (xy 63 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -9.5)
        (xy 50.5 -9.5)
        (xy 50.5 -11)
        (xy 49 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -7.5)
        (xy 8.5 -7.5)
        (xy 8.5 -9)
        (xy 7 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -3.5)
        (xy 62.5 -3.5)
        (xy 62.5 -5)
        (xy 61 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -19.5)
        (xy 12.5 -19.5)
        (xy 12.5 -21)
        (xy 11 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -21.5)
        (xy 26.5 -21.5)
        (xy 26.5 -23)
        (xy 25 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -13.5)
        (xy 28.5 -13.5)
        (xy 28.5 -15)
        (xy 27 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -3.5)
        (xy 36.5 -3.5)
        (xy 36.5 -5)
        (xy 35 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -21.5)
        (xy 58.5 -21.5)
        (xy 58.5 -23)
        (xy 57 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -31.5)
        (xy 16.5 -31.5)
        (xy 16.5 -33)
        (xy 15 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -19.5)
        (xy 14.5 -19.5)
        (xy 14.5 -21)
        (xy 13 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -3.5)
        (xy 10.5 -3.5)
        (xy 10.5 -5)
        (xy 9 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -11.5)
        (xy 78.5 -11.5)
        (xy 78.5 -13)
        (xy 77 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -25.5)
        (xy 18.5 -25.5)
        (xy 18.5 -27)
        (xy 17 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -23.5)
        (xy 64.5 -23.5)
        (xy 64.5 -25)
        (xy 63 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -17.5)
        (xy 54.5 -17.5)
        (xy 54.5 -19)
        (xy 53 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -23.5)
        (xy 74.5 -23.5)
        (xy 74.5 -25)
        (xy 73 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -13.5)
        (xy 56.5 -13.5)
        (xy 56.5 -15)
        (xy 55 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -23.5)
        (xy 42.5 -23.5)
        (xy 42.5 -25)
        (xy 41 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -25.5)
        (xy 14.5 -25.5)
        (xy 14.5 -27)
        (xy 13 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -17.5)
        (xy 52.5 -17.5)
        (xy 52.5 -19)
        (xy 51 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -5.5)
        (xy 50.5 -5.5)
        (xy 50.5 -7)
        (xy 49 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 39 -7.5)
        (xy 40.5 -7.5)
        (xy 40.5 -9)
        (xy 39 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -33.5)
        (xy 14.5 -33.5)
        (xy 14.5 -35)
        (xy 13 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -7.5)
        (xy 16.5 -7.5)
        (xy 16.5 -9)
        (xy 15 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -17.5)
        (xy 8.5 -17.5)
        (xy 8.5 -19)
        (xy 7 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -35.5)
        (xy 44.5 -35.5)
        (xy 44.5 -37)
        (xy 43 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -5.5)
        (xy 48.5 -5.5)
        (xy 48.5 -7)
        (xy 47 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -25.5)
        (xy 20.5 -25.5)
        (xy 20.5 -27)
        (xy 19 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -3.5)
        (xy 64.5 -3.5)
        (xy 64.5 -5)
        (xy 63 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -25.5)
        (xy 12.5 -25.5)
        (xy 12.5 -27)
        (xy 11 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -7.5)
        (xy 54.5 -7.5)
        (xy 54.5 -9)
        (xy 53 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -19.5)
        (xy 16.5 -19.5)
        (xy 16.5 -21)
        (xy 15 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31 -11.5)
        (xy 32.5 -11.5)
        (xy 32.5 -13)
        (xy 31 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -3.5)
        (xy 70.5 -3.5)
        (xy 70.5 -5)
        (xy 69 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -9.5)
        (xy 72.5 -9.5)
        (xy 72.5 -11)
        (xy 71 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -19.5)
        (xy 70.5 -19.5)
        (xy 70.5 -21)
        (xy 69 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -29.5)
        (xy 30.5 -29.5)
        (xy 30.5 -31)
        (xy 29 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -23.5)
        (xy 44.5 -23.5)
        (xy 44.5 -25)
        (xy 43 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -7.5)
        (xy 56.5 -7.5)
        (xy 56.5 -9)
        (xy 55 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -19.5)
        (xy 66.5 -19.5)
        (xy 66.5 -21)
        (xy 65 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -3.5)
        (xy 74.5 -3.5)
        (xy 74.5 -5)
        (xy 73 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -1.5)
        (xy 74.5 -1.5)
        (xy 74.5 -3)
        (xy 73 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -33.5)
        (xy 26.5 -33.5)
        (xy 26.5 -35)
        (xy 25 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 25 -35.5)
        (xy 26.5 -35.5)
        (xy 26.5 -37)
        (xy 25 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -5.5)
        (xy 68.5 -5.5)
        (xy 68.5 -7)
        (xy 67 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -7.5)
        (xy 14.5 -7.5)
        (xy 14.5 -9)
        (xy 13 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -9.5)
        (xy 34.5 -9.5)
        (xy 34.5 -11)
        (xy 33 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -21.5)
        (xy 68.5 -21.5)
        (xy 68.5 -23)
        (xy 67 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -33.5)
        (xy 52.5 -33.5)
        (xy 52.5 -35)
        (xy 51 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -23.5)
        (xy 18.5 -23.5)
        (xy 18.5 -25)
        (xy 17 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -25.5)
        (xy 54.5 -25.5)
        (xy 54.5 -27)
        (xy 53 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -15.5)
        (xy 70.5 -15.5)
        (xy 70.5 -17)
        (xy 69 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -25.5)
        (xy 28.5 -25.5)
        (xy 28.5 -27)
        (xy 27 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -15.5)
        (xy 60.5 -15.5)
        (xy 60.5 -17)
        (xy 59 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -21.5)
        (xy 14.5 -21.5)
        (xy 14.5 -23)
        (xy 13 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -17.5)
        (xy 22.5 -17.5)
        (xy 22.5 -19)
        (xy 21 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -21.5)
        (xy 10.5 -21.5)
        (xy 10.5 -23)
        (xy 9 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -19.5)
        (xy 56.5 -19.5)
        (xy 56.5 -21)
        (xy 55 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -15.5)
        (xy 30.5 -15.5)
        (xy 30.5 -17)
        (xy 29 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -27.5)
        (xy 34.5 -27.5)
        (xy 34.5 -29)
        (xy 33 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -19.5)
        (xy 8.5 -19.5)
        (xy 8.5 -21)
        (xy 7 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -9.5)
        (xy 58.5 -9.5)
        (xy 58.5 -11)
        (xy 57 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -11.5)
        (xy 52.5 -11.5)
        (xy 52.5 -13)
        (xy 51 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -23.5)
        (xy 20.5 -23.5)
        (xy 20.5 -25)
        (xy 19 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -31.5)
        (xy 28.5 -31.5)
        (xy 28.5 -33)
        (xy 27 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -11.5)
        (xy 54.5 -11.5)
        (xy 54.5 -13)
        (xy 53 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -13.5)
        (xy 64.5 -13.5)
        (xy 64.5 -15)
        (xy 63 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -5.5)
        (xy 46.5 -5.5)
        (xy 46.5 -7)
        (xy 45 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -33.5)
        (xy 28.5 -33.5)
        (xy 28.5 -35)
        (xy 27 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -17.5)
        (xy 14.5 -17.5)
        (xy 14.5 -19)
        (xy 13 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -21.5)
        (xy 54.5 -21.5)
        (xy 54.5 -23)
        (xy 53 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -25.5)
        (xy 16.5 -25.5)
        (xy 16.5 -27)
        (xy 15 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -19.5)
        (xy 38.5 -19.5)
        (xy 38.5 -21)
        (xy 37 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 19 -9.5)
        (xy 20.5 -9.5)
        (xy 20.5 -11)
        (xy 19 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -7.5)
        (xy 50.5 -7.5)
        (xy 50.5 -9)
        (xy 49 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -35.5)
        (xy 8.5 -35.5)
        (xy 8.5 -37)
        (xy 7 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -35.5)
        (xy 34.5 -35.5)
        (xy 34.5 -37)
        (xy 33 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -15.5)
        (xy 52.5 -15.5)
        (xy 52.5 -17)
        (xy 51 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -35.5)
        (xy 46.5 -35.5)
        (xy 46.5 -37)
        (xy 45 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -33.5)
        (xy 36.5 -33.5)
        (xy 36.5 -35)
        (xy 35 -35)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7 -31.5)
        (xy 8.5 -31.5)
        (xy 8.5 -33)
        (xy 7 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -17.5)
        (xy 28.5 -17.5)
        (xy 28.5 -19)
        (xy 27 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -7.5)
        (xy 34.5 -7.5)
        (xy 34.5 -9)
        (xy 33 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 9 -31.5)
        (xy 10.5 -31.5)
        (xy 10.5 -33)
        (xy 9 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -1.5)
        (xy 14.5 -1.5)
        (xy 14.5 -3)
        (xy 13 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -1.5)
        (xy 16.5 -1.5)
        (xy 16.5 -3)
        (xy 15 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -5.5)
        (xy 44.5 -5.5)
        (xy 44.5 -7)
        (xy 43 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -7.5)
        (xy 74.5 -7.5)
        (xy 74.5 -9)
        (xy 73 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -1.5)
        (xy 62.5 -1.5)
        (xy 62.5 -3)
        (xy 61 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 71 -23.5)
        (xy 72.5 -23.5)
        (xy 72.5 -25)
        (xy 71 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -3.5)
        (xy 12.5 -3.5)
        (xy 12.5 -5)
        (xy 11 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -9.5)
        (xy 66.5 -9.5)
        (xy 66.5 -11)
        (xy 65 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 67 -9.5)
        (xy 68.5 -9.5)
        (xy 68.5 -11)
        (xy 67 -11)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -29.5)
        (xy 46.5 -29.5)
        (xy 46.5 -31)
        (xy 45 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 23 -29.5)
        (xy 24.5 -29.5)
        (xy 24.5 -31)
        (xy 23 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -11.5)
        (xy 60.5 -11.5)
        (xy 60.5 -13)
        (xy 59 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -13.5)
        (xy 30.5 -13.5)
        (xy 30.5 -15)
        (xy 29 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -27.5)
        (xy 54.5 -27.5)
        (xy 54.5 -29)
        (xy 53 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -3.5)
        (xy 78.5 -3.5)
        (xy 78.5 -5)
        (xy 77 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -1.5)
        (xy 66.5 -1.5)
        (xy 66.5 -3)
        (xy 65 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -19.5)
        (xy 76.5 -19.5)
        (xy 76.5 -21)
        (xy 75 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -13.5)
        (xy 46.5 -13.5)
        (xy 46.5 -15)
        (xy 45 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -15.5)
        (xy 58.5 -15.5)
        (xy 58.5 -17)
        (xy 57 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -31.5)
        (xy 44.5 -31.5)
        (xy 44.5 -33)
        (xy 43 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -31.5)
        (xy 48.5 -31.5)
        (xy 48.5 -33)
        (xy 47 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 57 -23.5)
        (xy 58.5 -23.5)
        (xy 58.5 -25)
        (xy 57 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -5.5)
        (xy 52.5 -5.5)
        (xy 52.5 -7)
        (xy 51 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -35.5)
        (xy 42.5 -35.5)
        (xy 42.5 -37)
        (xy 41 -37)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 69 -13.5)
        (xy 70.5 -13.5)
        (xy 70.5 -15)
        (xy 69 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -11.5)
        (xy 18.5 -11.5)
        (xy 18.5 -13)
        (xy 17 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77 -21.5)
        (xy 78.5 -21.5)
        (xy 78.5 -23)
        (xy 77 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 75 -23.5)
        (xy 76.5 -23.5)
        (xy 76.5 -25)
        (xy 75 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 29 -19.5)
        (xy 30.5 -19.5)
        (xy 30.5 -21)
        (xy 29 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 17 -3.5)
        (xy 18.5 -3.5)
        (xy 18.5 -5)
        (xy 17 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 55 -17.5)
        (xy 56.5 -17.5)
        (xy 56.5 -19)
        (xy 55 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -23.5)
        (xy 14.5 -23.5)
        (xy 14.5 -25)
        (xy 13 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 41 -1.5)
        (xy 42.5 -1.5)
        (xy 42.5 -3)
        (xy 41 -3)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -19.5)
        (xy 34.5 -19.5)
        (xy 34.5 -21)
        (xy 33 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -15.5)
        (xy 28.5 -15.5)
        (xy 28.5 -17)
        (xy 27 -17)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -25.5)
        (xy 46.5 -25.5)
        (xy 46.5 -27)
        (xy 45 -27)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -23.5)
        (xy 62.5 -23.5)
        (xy 62.5 -25)
        (xy 61 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -11.5)
        (xy 22.5 -11.5)
        (xy 22.5 -13)
        (xy 21 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 61 -7.5)
        (xy 62.5 -7.5)
        (xy 62.5 -9)
        (xy 61 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -19.5)
        (xy 46.5 -19.5)
        (xy 46.5 -21)
        (xy 45 -21)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 73 -17.5)
        (xy 74.5 -17.5)
        (xy 74.5 -19)
        (xy 73 -19)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 35 -27.5)
        (xy 36.5 -27.5)
        (xy 36.5 -29)
        (xy 35 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 33 -23.5)
        (xy 34.5 -23.5)
        (xy 34.5 -25)
        (xy 33 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 11 -31.5)
        (xy 12.5 -31.5)
        (xy 12.5 -33)
        (xy 11 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 63 -21.5)
        (xy 64.5 -21.5)
        (xy 64.5 -23)
        (xy 63 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 45 -21.5)
        (xy 46.5 -21.5)
        (xy 46.5 -23)
        (xy 45 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 21 -3.5)
        (xy 22.5 -3.5)
        (xy 22.5 -5)
        (xy 21 -5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 37 -7.5)
        (xy 38.5 -7.5)
        (xy 38.5 -9)
        (xy 37 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 59 -23.5)
        (xy 60.5 -23.5)
        (xy 60.5 -25)
        (xy 59 -25)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 13 -5.5)
        (xy 14.5 -5.5)
        (xy 14.5 -7)
        (xy 13 -7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 51 -27.5)
        (xy 52.5 -27.5)
        (xy 52.5 -29)
        (xy 51 -29)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -13.5)
        (xy 16.5 -13.5)
        (xy 16.5 -15)
        (xy 15 -15)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 27 -29.5)
        (xy 28.5 -29.5)
        (xy 28.5 -31)
        (xy 27 -31)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 49 -31.5)
        (xy 50.5 -31.5)
        (xy 50.5 -33)
        (xy 49 -33)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65 -21.5)
        (xy 66.5 -21.5)
        (xy 66.5 -23)
        (xy 65 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 43 -11.5)
        (xy 44.5 -11.5)
        (xy 44.5 -13)
        (xy 43 -13)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 47 -7.5)
        (xy 48.5 -7.5)
        (xy 48.5 -9)
        (xy 47 -9)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Cu") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 15 -21.5)
        (xy 16.5 -21.5)
        (xy 16.5 -23)
        (xy 15 -23)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "B.Mask") (hatch edge 0.508)
    (priority 1)
    (connect_pads yes (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 53 -31.5)
        (xy 55 -31.5)
        (xy 55 -25.5)
        (xy 79 -25.5)
        (xy 79 -2)
        (xy 6.5 -2)
        (xy 6.5 -37.5)
        (xy 53 -37.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Mask") (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.2))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 31.5 -39)
        (xy 43.5 -39)
        (xy 43.5 -27)
        (xy 55.5 -27)
        (xy 55.5 -15)
        (xy 79.5 -15)
        (xy 79.5 -2.5)
        (xy 6.5 -2.5)
        (xy 6.5 -51)
        (xy 31 -51)
      )
    )
  )
)
