(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (title_block
    (title "Nanovoltmeter - LISA")
    (date "2022-05-15")
    (rev "2")
  )
  (lib_symbols
    (symbol "74xx:74LS08" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 1.27 0))
      (property "Value" "74LS08" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS08" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL and2" (id 5) (at 0 0 0))
      (property "ki_description" "Quad And2" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0))
      (symbol "74LS08_1_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "2")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS08_1_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1855 -2.584) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1928 2.5925) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "1")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "2")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "3")
        )
      )
      (symbol "74LS08_2_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS08_2_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1855 -2.584) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1928 2.5925) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "4")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74LS08_3_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS08_3_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1855 -2.584) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1928 2.5925) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "10")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "9")
        )
      )
      (symbol "74LS08_4_1"
        (arc (start 0 -3.81) (mid 3.81 0) (end 0 3.81)
          (fill (type background))
        )
        (polyline
          (pts
            (xy 0 3.81)
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 0 -3.81)
          )
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input line (at -7.62 2.54 0) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 -2.54 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS08_4_2"
        (arc (start -3.81 -3.81) (mid -2.589 0) (end -3.81 3.81)
          (fill (type none))
        )
        (arc (start -0.6096 -3.81) (mid 2.1855 -2.584) (end 3.81 0)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -0.635 3.81)
          )
          (fill (type background))
        )
        (polyline
          (pts
            (xy -0.635 3.81)
            (xy -3.81 3.81)
            (xy -3.81 3.81)
            (xy -3.556 3.4036)
            (xy -3.0226 2.2606)
            (xy -2.6924 1.0414)
            (xy -2.6162 -0.254)
            (xy -2.7686 -1.4986)
            (xy -3.175 -2.7178)
            (xy -3.81 -3.81)
            (xy -3.81 -3.81)
            (xy -0.635 -3.81)
          )
          (fill (type background))
        )
        (arc (start 3.81 0) (mid 2.1928 2.5925) (end -0.6096 3.81)
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "11")
        )
        (pin input inverted (at -7.62 2.54 0) (length 4.318)
          (name "~")
          (number "12")
        )
        (pin input inverted (at -7.62 -2.54 0) (length 4.318)
          (name "~")
          (number "13")
        )
      )
      (symbol "74LS08_5_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74LS08_5_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "Connector:Conn_01x02_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 2.54 0))
      (property "Value" "Conn_01x02_Male" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x02_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
      )
    )
    (symbol "Connector:USB_B" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at -5.08 11.43 0))
      (property "Value" "USB_B" (id 1) (at -5.08 8.89 0))
      (property "Footprint" "" (id 2) (at 3.81 -1.27 0))
      (property "Datasheet" " ~" (id 3) (at 3.81 -1.27 0))
      (property "ki_keywords" "connector USB" (id 4) (at 0 0 0))
      (property "ki_description" "USB Type B connector" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "USB*" (id 6) (at 0 0 0))
      (symbol "USB_B_0_1"
        (rectangle (start -5.08 -7.62) (end 5.08 7.62)
          (fill (type background))
        )
        (circle (center -3.81 2.159) (radius 0.635)
          (fill (type outline))
        )
        (rectangle (start -3.81 5.588) (end -2.54 4.572)
          (fill (type outline))
        )
        (circle (center -0.635 3.429) (radius 0.381)
          (fill (type outline))
        )
        (rectangle (start -0.127 -7.62) (end 0.127 -6.858)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 2.159)
            (xy 0.635 2.159)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.175 2.159)
            (xy -2.54 2.159)
            (xy -1.27 3.429)
            (xy -0.635 3.429)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 2.159)
            (xy -1.905 2.159)
            (xy -1.27 0.889)
            (xy 0 0.889)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 2.794)
            (xy 0.635 1.524)
            (xy 1.905 2.159)
            (xy 0.635 2.794)
          )
          (fill (type outline))
        )
        (polyline
          (pts
            (xy -4.064 4.318)
            (xy -2.286 4.318)
            (xy -2.286 5.715)
            (xy -2.667 6.096)
            (xy -3.683 6.096)
            (xy -4.064 5.715)
            (xy -4.064 4.318)
          )
          (fill (type none))
        )
        (rectangle (start 0.254 1.27) (end -0.508 0.508)
          (fill (type outline))
        )
        (rectangle (start 5.08 -2.667) (end 4.318 -2.413)
          (fill (type none))
        )
        (rectangle (start 5.08 -0.127) (end 4.318 0.127)
          (fill (type none))
        )
        (rectangle (start 5.08 4.953) (end 4.318 5.207)
          (fill (type none))
        )
      )
      (symbol "USB_B_1_1"
        (pin power_out line (at 7.62 5.08 180) (length 2.54)
          (name "VBUS")
          (number "1")
        )
        (pin bidirectional line (at 7.62 -2.54 180) (length 2.54)
          (name "D-")
          (number "2")
        )
        (pin bidirectional line (at 7.62 0 180) (length 2.54)
          (name "D+")
          (number "3")
        )
        (pin power_out line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin passive line (at -2.54 -10.16 90) (length 2.54)
          (name "Shield")
          (number "5")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x03_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 5.08 0))
      (property "Value" "Conn_02x03_Odd_Even" (id 1) (at 1.27 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x03_Odd_Even_1_1"
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 3.81) (end 3.81 -3.81)
          (fill (type background))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x08_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 10.16 0))
      (property "Value" "Conn_02x08_Odd_Even" (id 1) (at 1.27 -12.7 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x08_Odd_Even_1_1"
        (rectangle (start -1.27 -10.033) (end 0 -10.287)
          (fill (type none))
        )
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (fill (type none))
        )
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 8.89) (end 3.81 -11.43)
          (fill (type background))
        )
        (rectangle (start 3.81 -10.033) (end 2.54 -10.287)
          (fill (type none))
        )
        (rectangle (start 3.81 -7.493) (end 2.54 -7.747)
          (fill (type none))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (rectangle (start 3.81 7.747) (end 2.54 7.493)
          (fill (type none))
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_12")
          (number "12")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_13")
          (number "13")
        )
        (pin passive line (at 7.62 -7.62 180) (length 3.81)
          (name "Pin_14")
          (number "14")
        )
        (pin passive line (at -5.08 -10.16 0) (length 3.81)
          (name "Pin_15")
          (number "15")
        )
        (pin passive line (at 7.62 -10.16 180) (length 3.81)
          (name "Pin_16")
          (number "16")
        )
        (pin passive line (at 7.62 7.62 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x12_Top_Bottom" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 15.24 0))
      (property "Value" "Conn_02x12_Top_Bottom" (id 1) (at 1.27 -17.78 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x12, top/bottom pin numbering scheme (row 1: 1...pins_per_row, row2: pins_per_row+1 ... num_pins), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x12_Top_Bottom_1_1"
        (rectangle (start -1.27 -15.113) (end 0 -15.367)
          (fill (type none))
        )
        (rectangle (start -1.27 -12.573) (end 0 -12.827)
          (fill (type none))
        )
        (rectangle (start -1.27 -10.033) (end 0 -10.287)
          (fill (type none))
        )
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (fill (type none))
        )
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 10.287) (end 0 10.033)
          (fill (type none))
        )
        (rectangle (start -1.27 12.827) (end 0 12.573)
          (fill (type none))
        )
        (rectangle (start -1.27 13.97) (end 3.81 -16.51)
          (fill (type background))
        )
        (rectangle (start 3.81 -15.113) (end 2.54 -15.367)
          (fill (type none))
        )
        (rectangle (start 3.81 -12.573) (end 2.54 -12.827)
          (fill (type none))
        )
        (rectangle (start 3.81 -10.033) (end 2.54 -10.287)
          (fill (type none))
        )
        (rectangle (start 3.81 -7.493) (end 2.54 -7.747)
          (fill (type none))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (rectangle (start 3.81 7.747) (end 2.54 7.493)
          (fill (type none))
        )
        (rectangle (start 3.81 10.287) (end 2.54 10.033)
          (fill (type none))
        )
        (rectangle (start 3.81 12.827) (end 2.54 12.573)
          (fill (type none))
        )
        (pin passive line (at -5.08 12.7 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at -5.08 -10.16 0) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 -12.7 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at -5.08 -15.24 0) (length 3.81)
          (name "Pin_12")
          (number "12")
        )
        (pin passive line (at 7.62 12.7 180) (length 3.81)
          (name "Pin_13")
          (number "13")
        )
        (pin passive line (at 7.62 10.16 180) (length 3.81)
          (name "Pin_14")
          (number "14")
        )
        (pin passive line (at 7.62 7.62 180) (length 3.81)
          (name "Pin_15")
          (number "15")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_16")
          (number "16")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_17")
          (number "17")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_18")
          (number "18")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_19")
          (number "19")
        )
        (pin passive line (at -5.08 10.16 0) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_20")
          (number "20")
        )
        (pin passive line (at 7.62 -7.62 180) (length 3.81)
          (name "Pin_21")
          (number "21")
        )
        (pin passive line (at 7.62 -10.16 180) (length 3.81)
          (name "Pin_22")
          (number "22")
        )
        (pin passive line (at 7.62 -12.7 180) (length 3.81)
          (name "Pin_23")
          (number "23")
        )
        (pin passive line (at 7.62 -15.24 180) (length 3.81)
          (name "Pin_24")
          (number "24")
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:C_Polarized" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C_Polarized" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Polarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
      (symbol "C_Polarized_0_1"
        (rectangle (start -2.286 0.508) (end 2.286 1.016)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 2.794)
            (xy -1.27 1.778)
          )
          (fill (type none))
        )
        (rectangle (start 2.286 -0.508) (end -2.286 -1.016)
          (fill (type outline))
        )
      )
      (symbol "C_Polarized_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Crystal" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 0 3.81 0))
      (property "Value" "Crystal" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "Two pin crystal" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0))
      (symbol "Crystal_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -1.905 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 -1.27)
            (xy 1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.905 0)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Diode:BAV99" (pin_names hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 5.08 0))
      (property "Value" "BAV99" (id 1) (at 0 2.54 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 0 -12.7 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV99_SER.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "diode" (id 4) (at 0 0 0))
      (property "ki_description" "BAV99 High-speed switching diodes, SOT-23" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0))
      (symbol "BAV99_0_1"
        (polyline
          (pts
            (xy -5.08 0)
            (xy 5.08 0)
          )
          (fill (type none))
        )
      )
      (symbol "BAV99_1_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 1.27)
            (xy 3.81 -1.27)
            (xy 3.81 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 1.27)
            (xy -1.27 0)
            (xy -3.81 -1.27)
            (xy -3.81 1.27)
            (xy -3.81 1.27)
            (xy -3.81 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 3.81 0)
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy 1.27 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (circle (center 0 0) (radius 0.254)
          (fill (type outline))
        )
        (pin passive line (at -7.62 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 7.62 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
        (pin passive line (at 0 -5.08 90) (length 2.54)
          (name "K")
          (number "3")
        )
      )
    )
    (symbol "Diode:SM6T6V8A" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "SM6T6V8A" (id 1) (at 0 -2.54 0))
      (property "Footprint" "Diode_SMD:D_SMB" (id 2) (at 0 -5.08 0))
      (property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf" (id 3) (at -1.27 0 0))
      (property "ki_keywords" "diode TVS voltage suppressor" (id 4) (at 0 0 0))
      (property "ki_description" "600W unidirectional Transil Transient Voltage Suppressor, 6.8Vrwm, DO-214AA" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "D*SMB*" (id 6) (at 0 0 0))
      (symbol "SM6T6V8A_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 1.27)
            (xy 1.27 -1.27)
            (xy -1.27 0)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "SM6T6V8A_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "A1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A2")
          (number "2")
        )
      )
    )
    (symbol "Interface_USB:CH340G" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -5.08 13.97 0))
      (property "Value" "CH340G" (id 1) (at 1.27 13.97 0))
      (property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (id 2) (at 1.27 -13.97 0))
      (property "Datasheet" "http://www.datasheet5.com/pdf-local-2195953" (id 3) (at -8.89 20.32 0))
      (property "ki_keywords" "USB UART Serial Converter Interface" (id 4) (at 0 0 0))
      (property "ki_description" "USB serial converter, UART, SOIC-16" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*" (id 6) (at 0 0 0))
      (symbol "CH340G_0_1"
        (rectangle (start -7.62 12.7) (end 7.62 -12.7)
          (fill (type background))
        )
      )
      (symbol "CH340G_1_1"
        (pin power_in line (at 0 -15.24 90) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin input line (at 10.16 0 180) (length 2.54)
          (name "~{DSR}")
          (number "10")
        )
        (pin input line (at 10.16 -2.54 180) (length 2.54)
          (name "~{RI}")
          (number "11")
        )
        (pin input line (at 10.16 -5.08 180) (length 2.54)
          (name "~{DCD}")
          (number "12")
        )
        (pin output line (at 10.16 -7.62 180) (length 2.54)
          (name "~{DTR}")
          (number "13")
        )
        (pin output line (at 10.16 -10.16 180) (length 2.54)
          (name "~{RTS}")
          (number "14")
        )
        (pin input line (at -10.16 7.62 0) (length 2.54)
          (name "R232")
          (number "15")
        )
        (pin power_in line (at 0 15.24 270) (length 2.54)
          (name "VCC")
          (number "16")
        )
        (pin output line (at 10.16 10.16 180) (length 2.54)
          (name "TXD")
          (number "2")
        )
        (pin input line (at 10.16 7.62 180) (length 2.54)
          (name "RXD")
          (number "3")
        )
        (pin passive line (at -2.54 15.24 270) (length 2.54)
          (name "V3")
          (number "4")
        )
        (pin bidirectional line (at -10.16 2.54 0) (length 2.54)
          (name "UD+")
          (number "5")
        )
        (pin bidirectional line (at -10.16 0 0) (length 2.54)
          (name "UD-")
          (number "6")
        )
        (pin input line (at -10.16 -5.08 0) (length 2.54)
          (name "XI")
          (number "7")
        )
        (pin output line (at -10.16 -10.16 0) (length 2.54)
          (name "XO")
          (number "8")
        )
        (pin input line (at 10.16 2.54 180) (length 2.54)
          (name "~{CTS}")
          (number "9")
        )
      )
    )
    (symbol "MCU_Microchip_ATmega:ATmega8A-A" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -12.7 34.29 0))
      (property "Value" "ATmega8A-A" (id 1) (at 5.08 -34.29 0))
      (property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm" (id 2) (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "AVR 8bit Microcontroller MegaAVR" (id 4) (at 0 0 0))
      (property "ki_description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*" (id 6) (at 0 0 0))
      (symbol "ATmega8A-A_0_1"
        (rectangle (start -12.7 -33.02) (end 12.7 33.02)
          (fill (type background))
        )
      )
      (symbol "ATmega8A-A_1_1"
        (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
          (name "PD3")
          (number "1")
        )
        (pin bidirectional line (at 15.24 -22.86 180) (length 2.54)
          (name "PD6")
          (number "10")
        )
        (pin bidirectional line (at 15.24 -25.4 180) (length 2.54)
          (name "PD7")
          (number "11")
        )
        (pin bidirectional line (at 15.24 27.94 180) (length 2.54)
          (name "PB0")
          (number "12")
        )
        (pin bidirectional line (at 15.24 25.4 180) (length 2.54)
          (name "PB1")
          (number "13")
        )
        (pin bidirectional line (at 15.24 22.86 180) (length 2.54)
          (name "PB2")
          (number "14")
        )
        (pin bidirectional line (at 15.24 20.32 180) (length 2.54)
          (name "PB3")
          (number "15")
        )
        (pin bidirectional line (at 15.24 17.78 180) (length 2.54)
          (name "PB4")
          (number "16")
        )
        (pin bidirectional line (at 15.24 15.24 180) (length 2.54)
          (name "PB5")
          (number "17")
        )
        (pin power_in line (at 2.54 35.56 270) (length 2.54)
          (name "AVCC")
          (number "18")
        )
        (pin input line (at -15.24 7.62 0) (length 2.54)
          (name "ADC6")
          (number "19")
        )
        (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
          (name "PD4")
          (number "2")
        )
        (pin passive line (at -15.24 12.7 0) (length 2.54)
          (name "AREF")
          (number "20")
        )
        (pin power_in line (at 2.54 -35.56 90) (length 2.54)
          (name "AGND")
          (number "21")
        )
        (pin input line (at -15.24 5.08 0) (length 2.54)
          (name "ADC7")
          (number "22")
        )
        (pin bidirectional line (at 15.24 10.16 180) (length 2.54)
          (name "PC0")
          (number "23")
        )
        (pin bidirectional line (at 15.24 7.62 180) (length 2.54)
          (name "PC1")
          (number "24")
        )
        (pin bidirectional line (at 15.24 5.08 180) (length 2.54)
          (name "PC2")
          (number "25")
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
          (name "PC3")
          (number "26")
        )
        (pin bidirectional line (at 15.24 0 180) (length 2.54)
          (name "PC4")
          (number "27")
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
          (name "PC5")
          (number "28")
        )
        (pin bidirectional line (at -15.24 27.94 0) (length 2.54)
          (name "PC6/~{RESET}")
          (number "29")
        )
        (pin power_in line (at 0 -35.56 90) (length 2.54)
          (name "GND")
          (number "3")
        )
        (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
          (name "PD0")
          (number "30")
        )
        (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
          (name "PD1")
          (number "31")
        )
        (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
          (name "PD2")
          (number "32")
        )
        (pin power_in line (at 0 35.56 270) (length 2.54)
          (name "VCC")
          (number "4")
        )
        (pin passive line (at 0 -35.56 90) (length 2.54) hide
          (name "GND")
          (number "5")
        )
        (pin passive line (at 0 35.56 270) (length 2.54) hide
          (name "VCC")
          (number "6")
        )
        (pin bidirectional line (at -15.24 22.86 0) (length 2.54)
          (name "PB6/XTAL1")
          (number "7")
        )
        (pin bidirectional line (at -15.24 17.78 0) (length 2.54)
          (name "PB7/XTAL2")
          (number "8")
        )
        (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
          (name "PD5")
          (number "9")
        )
      )
    )
    (symbol "Mechanical:MountingHole" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "H" (id 0) (at 0 5.08 0))
      (property "Value" "MountingHole" (id 1) (at 0 3.175 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "mounting hole" (id 4) (at 0 0 0))
      (property "ki_description" "Mounting Hole without connection" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "MountingHole*" (id 6) (at 0 0 0))
      (symbol "MountingHole_0_1"
        (circle (center 0 0) (radius 1.27)
          (fill (type none))
        )
      )
    )
    (symbol "j_lib:75160" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 -15.24 0))
      (property "Value" "75160" (id 1) (at -1.27 16.51 0))
      (property "Footprint" "" (id 2) (at 6.35 -21.59 0))
      (property "Datasheet" "" (id 3) (at 6.35 -21.59 0))
      (symbol "75160_0_0"
        (pin input line (at -11.43 -2.54 0) (length 2.54)
          (name "D7")
          (number "13")
        )
        (pin input line (at -11.43 0 0) (length 2.54)
          (name "D6")
          (number "14")
        )
        (pin input line (at -11.43 2.54 0) (length 2.54)
          (name "D5")
          (number "15")
        )
        (pin input line (at -11.43 5.08 0) (length 2.54)
          (name "D4")
          (number "16")
        )
        (pin input line (at -11.43 7.62 0) (length 2.54)
          (name "D3")
          (number "17")
        )
        (pin input line (at -11.43 10.16 0) (length 2.54)
          (name "D2")
          (number "18")
        )
        (pin input line (at -11.43 12.7 0) (length 2.54)
          (name "D1")
          (number "19")
        )
        (pin input line (at 10.16 -7.62 180) (length 2.54)
          (name "VCC")
          (number "20")
        )
      )
      (symbol "75160_0_1"
        (rectangle (start -8.89 15.24) (end 7.62 -12.7)
          (fill (type background))
        )
      )
      (symbol "75160_1_1"
        (pin input line (at -11.43 -7.62 0) (length 2.54)
          (name "TE")
          (number "1")
        )
        (pin input line (at 10.16 -10.16 180) (length 2.54)
          (name "GND")
          (number "10")
        )
        (pin input line (at -11.43 -10.16 0) (length 2.54)
          (name "PE")
          (number "11")
        )
        (pin input line (at -11.43 -5.08 0) (length 2.54)
          (name "D8")
          (number "12")
        )
        (pin input line (at 10.16 12.7 180) (length 2.54)
          (name "B1")
          (number "2")
        )
        (pin input line (at 10.16 10.16 180) (length 2.54)
          (name "B2")
          (number "3")
        )
        (pin input line (at 10.16 7.62 180) (length 2.54)
          (name "B3")
          (number "4")
        )
        (pin input line (at 10.16 5.08 180) (length 2.54)
          (name "B4")
          (number "5")
        )
        (pin input line (at 10.16 2.54 180) (length 2.54)
          (name "B5")
          (number "6")
        )
        (pin input line (at 10.16 0 180) (length 2.54)
          (name "B6")
          (number "7")
        )
        (pin input line (at 10.16 -2.54 180) (length 2.54)
          (name "B7")
          (number "8")
        )
        (pin input line (at 10.16 -5.08 180) (length 2.54)
          (name "B8")
          (number "9")
        )
      )
    )
    (symbol "j_lib:75161" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 -15.24 0))
      (property "Value" "75161" (id 1) (at 1.27 15.24 0))
      (property "Footprint" "" (id 2) (at -20.32 -24.13 0))
      (property "Datasheet" "" (id 3) (at -20.32 -24.13 0))
      (symbol "75161_0_0"
        (pin bidirectional line (at -10.16 -11.43 0) (length 2.54)
          (name "TE")
          (number "1")
        )
        (pin bidirectional line (at 11.43 -11.43 180) (length 2.54)
          (name "GND")
          (number "10")
        )
        (pin bidirectional line (at -10.16 -8.89 0) (length 2.54)
          (name "DC")
          (number "11")
        )
        (pin bidirectional line (at -10.16 -6.35 0) (length 2.54)
          (name "SRQ_D")
          (number "12")
        )
        (pin bidirectional line (at -10.16 -3.81 0) (length 2.54)
          (name "ATN_D")
          (number "13")
        )
        (pin bidirectional line (at -10.16 -1.27 0) (length 2.54)
          (name "EOI_D")
          (number "14")
        )
        (pin bidirectional line (at -10.16 1.27 0) (length 2.54)
          (name "DAV_D")
          (number "15")
        )
        (pin bidirectional line (at -10.16 3.81 0) (length 2.54)
          (name "NRFD_D")
          (number "16")
        )
        (pin bidirectional line (at -10.16 6.35 0) (length 2.54)
          (name "NDAC_D")
          (number "17")
        )
        (pin bidirectional line (at -10.16 8.89 0) (length 2.54)
          (name "IFC_D")
          (number "18")
        )
        (pin bidirectional line (at -10.16 11.43 0) (length 2.54)
          (name "REN_D")
          (number "19")
        )
        (pin bidirectional line (at 11.43 11.43 180) (length 2.54)
          (name "REN_G")
          (number "2")
        )
        (pin bidirectional line (at 11.43 -8.89 180) (length 2.54)
          (name "VCC")
          (number "20")
        )
        (pin bidirectional line (at 11.43 8.89 180) (length 2.54)
          (name "IFC_G")
          (number "3")
        )
        (pin bidirectional line (at 11.43 6.35 180) (length 2.54)
          (name "NDAC_G")
          (number "4")
        )
        (pin bidirectional line (at 11.43 3.81 180) (length 2.54)
          (name "NRFD_G")
          (number "5")
        )
        (pin bidirectional line (at 11.43 1.27 180) (length 2.54)
          (name "DAV_G")
          (number "6")
        )
        (pin bidirectional line (at 11.43 -1.27 180) (length 2.54)
          (name "EOI_G")
          (number "7")
        )
        (pin bidirectional line (at 11.43 -3.81 180) (length 2.54)
          (name "ATN_G")
          (number "8")
        )
        (pin bidirectional line (at 11.43 -6.35 180) (length 2.54)
          (name "SRQ_G")
          (number "9")
        )
      )
      (symbol "75161_0_1"
        (rectangle (start -7.62 13.97) (end 8.89 -13.97)
          (fill (type background))
        )
      )
    )
    (symbol "j_lib:W5500_bo" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 -9.525 0))
      (property "Value" "W5500_bo" (id 1) (at 0 10.16 0))
      (property "Footprint" "" (id 2) (at -4.445 0.635 0))
      (property "Datasheet" "" (id 3) (at -4.445 0.635 0))
      (symbol "W5500_bo_0_1"
        (rectangle (start 6.985 -8.255) (end -6.985 8.89)
          (fill (type none))
        )
      )
      (symbol "W5500_bo_1_1"
        (pin input line (at 9.525 -6.35 180) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin input line (at 9.525 3.81 180) (length 2.54)
          (name "3V")
          (number "10")
        )
        (pin input line (at 9.525 6.35 180) (length 2.54)
          (name "3V")
          (number "11")
        )
        (pin input line (at 9.525 -1.27 180) (length 2.54)
          (name "GND")
          (number "12")
        )
        (pin input line (at 9.525 -3.81 180) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin input line (at -9.525 1.27 0) (length 2.54)
          (name "MOSI")
          (number "3")
        )
        (pin input line (at -9.525 -1.27 0) (length 2.54)
          (name "SCLK")
          (number "4")
        )
        (pin input line (at -9.525 -3.81 0) (length 2.54)
          (name "CS")
          (number "5")
        )
        (pin input line (at -9.525 -6.35 0) (length 2.54)
          (name "INT")
          (number "6")
        )
        (pin input line (at -9.525 3.81 0) (length 2.54)
          (name "MISO")
          (number "7")
        )
        (pin input line (at -9.525 6.35 0) (length 2.54)
          (name "RST")
          (number "8")
        )
      )
    )
    (symbol "j_lib:logo_generic" (in_bom yes) (on_board yes)
      (property "Reference" "LOGO" (id 0) (at 0 3.81 0))
      (property "Value" "logo_generic" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "logo_generic_0_1"
        (rectangle (start -3.81 2.54) (end 3.81 -2.54)
          (fill (type none))
        )
      )
    )
    (symbol "power:+3V3" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3V3" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3V3\"" (id 5) (at 0 0 0))
      (symbol "+3V3_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3V3_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 43.18 96.52) (diameter 0) (color 0 0 0 0))
  (junction (at 266.7 90.17) (diameter 0) (color 0 0 0 0))
  (junction (at 266.7 85.09) (diameter 0) (color 0 0 0 0))
  (junction (at 268.605 34.925) (diameter 0) (color 0 0 0 0))
  (junction (at 55.88 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 97.155 42.545) (diameter 0) (color 0 0 0 0))
  (junction (at 240.665 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 248.92 147.32) (diameter 0) (color 0 0 0 0))
  (junction (at 262.255 146.685) (diameter 0) (color 0 0 0 0))
  (junction (at 187.96 129.54) (diameter 0) (color 0 0 0 0))
  (junction (at 36.195 41.275) (diameter 0) (color 0 0 0 0))
  (junction (at 131.445 142.24) (diameter 0) (color 0 0 0 0))
  (junction (at 262.255 32.385) (diameter 0) (color 0 0 0 0))
  (junction (at 198.755 88.265) (diameter 0) (color 0 0 0 0))
  (junction (at 88.9 42.545) (diameter 0) (color 0 0 0 0))
  (junction (at 266.7 77.47) (diameter 0) (color 0 0 0 0))
  (junction (at 160.02 67.945) (diameter 0) (color 0 0 0 0))
  (junction (at 262.255 34.925) (diameter 0) (color 0 0 0 0))
  (junction (at 40.005 41.275) (diameter 0) (color 0 0 0 0))
  (junction (at 266.7 82.55) (diameter 0) (color 0 0 0 0))
  (junction (at 40.005 43.815) (diameter 0) (color 0 0 0 0))
  (junction (at 100.965 32.385) (diameter 0) (color 0 0 0 0))
  (junction (at 266.7 87.63) (diameter 0) (color 0 0 0 0))
  (junction (at 147.32 83.185) (diameter 0) (color 0 0 0 0))
  (junction (at 118.11 95.885) (diameter 0) (color 0 0 0 0))
  (junction (at 118.11 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 262.255 22.225) (diameter 0) (color 0 0 0 0))
  (junction (at 266.7 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 22.225 73.025) (diameter 0) (color 0 0 0 0))
  (junction (at 40.005 38.735) (diameter 0) (color 0 0 0 0))
  (junction (at 52.07 29.21) (diameter 0) (color 0 0 0 0))
  (junction (at 204.47 146.685) (diameter 0) (color 0 0 0 0))
  (junction (at 268.605 22.225) (diameter 0) (color 0 0 0 0))
  (junction (at 248.92 118.745) (diameter 0) (color 0 0 0 0))
  (junction (at 43.18 104.14) (diameter 0) (color 0 0 0 0))
  (no_connect (at 214.63 134.62))
  (no_connect (at 214.63 137.16))
  (no_connect (at 214.63 139.7))
  (no_connect (at 214.63 142.24))
  (no_connect (at 214.63 144.78))
  (no_connect (at 214.63 147.32))
  (no_connect (at 243.205 34.925))
  (no_connect (at 234.95 129.54))
  (no_connect (at 146.685 139.7))
  (no_connect (at 102.87 55.245))
  (no_connect (at 102.87 52.705))
  (wire (pts (xy 43.18 101.6) (xy 43.18 104.14)))
  (wire (pts (xy 240.665 147.32) (xy 234.95 147.32)))
  (wire (pts (xy 100.33 47.625) (xy 102.87 47.625)))
  (wire (pts (xy 266.7 77.47) (xy 266.7 80.01)))
  (wire (pts (xy 264.795 144.78) (xy 264.795 146.685)))
  (wire (pts (xy 96.52 42.545) (xy 97.155 42.545)))
  (wire (pts (xy 266.7 87.63) (xy 266.7 90.17)))
  (polyline (pts (xy 275.59 115.57) (xy 275.59 161.925)))
  (wire (pts (xy 245.745 85.09) (xy 254 85.09)))
  (wire (pts (xy 273.05 97.155) (xy 273.05 72.39)))
  (wire (pts (xy 227.965 103.505) (xy 245.745 103.505)))
  (wire (pts (xy 160.02 67.945) (xy 160.02 70.485)))
  (wire (pts (xy 102.87 32.385) (xy 100.965 32.385)))
  (wire (pts (xy 142.875 45.085) (xy 142.875 53.975)))
  (wire (pts (xy 187.96 129.54) (xy 187.96 132.08)))
  (polyline (pts (xy 67.31 61.595) (xy 16.51 61.595)))
  (wire (pts (xy 241.935 85.725) (xy 241.935 97.155)))
  (wire (pts (xy 32.385 29.21) (xy 29.845 29.21)))
  (wire (pts (xy 187.96 127) (xy 187.96 129.54)))
  (wire (pts (xy 88.9 42.545) (xy 88.9 45.72)))
  (wire (pts (xy 262.255 32.385) (xy 262.255 34.925)))
  (wire (pts (xy 245.11 60.325) (xy 245.11 67.31)))
  (polyline (pts (xy 175.895 45.085) (xy 275.59 45.085)))
  (wire (pts (xy 43.18 96.52) (xy 43.18 99.06)))
  (wire (pts (xy 243.84 100.965) (xy 243.84 87.63)))
  (wire (pts (xy 234.95 70.485) (xy 234.95 51.435)))
  (wire (pts (xy 133.35 70.485) (xy 147.32 70.485)))
  (polyline (pts (xy 173.99 15.875) (xy 173.99 113.665)))
  (wire (pts (xy 28.575 73.025) (xy 28.575 86.36)))
  (wire (pts (xy 262.255 22.225) (xy 262.255 24.765)))
  (wire (pts (xy 43.18 86.36) (xy 55.88 86.36)))
  (polyline (pts (xy 175.895 115.57) (xy 275.59 115.57)))
  (wire (pts (xy 47.625 29.21) (xy 52.07 29.21)))
  (wire (pts (xy 248.285 62.23) (xy 254 62.23)))
  (wire (pts (xy 236.22 77.47) (xy 254 77.47)))
  (wire (pts (xy 273.05 72.39) (xy 266.7 72.39)))
  (wire (pts (xy 248.92 142.24) (xy 248.92 147.32)))
  (wire (pts (xy 197.485 78.105) (xy 206.375 78.105)))
  (wire (pts (xy 266.7 47.625) (xy 266.7 62.23)))
  (wire (pts (xy 198.755 75.565) (xy 206.375 75.565)))
  (polyline (pts (xy 228.6 13.97) (xy 275.59 13.97)))
  (wire (pts (xy 266.7 82.55) (xy 266.7 85.09)))
  (wire (pts (xy 234.315 90.805) (xy 234.315 80.01)))
  (wire (pts (xy 227.965 55.245) (xy 248.285 55.245)))
  (wire (pts (xy 142.875 53.975) (xy 144.78 53.975)))
  (wire (pts (xy 268.605 64.77) (xy 268.605 49.53)))
  (wire (pts (xy 243.84 121.92) (xy 243.84 123.825)))
  (wire (pts (xy 254 72.39) (xy 240.03 72.39)))
  (polyline (pts (xy 228.6 43.18) (xy 228.6 13.97)))
  (wire (pts (xy 133.35 40.005) (xy 144.78 40.005)))
  (wire (pts (xy 247.015 64.77) (xy 247.015 57.785)))
  (wire (pts (xy 238.125 74.93) (xy 254 74.93)))
  (wire (pts (xy 227.965 65.405) (xy 231.14 65.405)))
  (wire (pts (xy 262.255 146.685) (xy 264.795 146.685)))
  (polyline (pts (xy 65.405 58.42) (xy 16.51 58.42)))
  (wire (pts (xy 266.7 69.85) (xy 272.415 69.85)))
  (polyline (pts (xy 175.895 161.925) (xy 175.895 115.57)))
  (wire (pts (xy 272.415 53.34) (xy 236.855 53.34)))
  (polyline (pts (xy 173.99 115.57) (xy 173.99 161.925)))
  (wire (pts (xy 240.665 147.32) (xy 240.665 150.495)))
  (wire (pts (xy 243.84 87.63) (xy 254 87.63)))
  (wire (pts (xy 224.79 118.745) (xy 248.92 118.745)))
  (wire (pts (xy 234.95 137.16) (xy 254.635 137.16)))
  (wire (pts (xy 212.09 132.715) (xy 212.09 127)))
  (wire (pts (xy 241.3 147.32) (xy 240.665 147.32)))
  (wire (pts (xy 97.155 42.545) (xy 102.87 42.545)))
  (wire (pts (xy 254 64.77) (xy 247.015 64.77)))
  (wire (pts (xy 262.255 29.845) (xy 262.255 32.385)))
  (wire (pts (xy 131.445 137.16) (xy 131.445 142.24)))
  (wire (pts (xy 22.225 73.025) (xy 28.575 73.025)))
  (wire (pts (xy 31.75 41.275) (xy 36.195 41.275)))
  (wire (pts (xy 227.965 62.865) (xy 243.205 62.865)))
  (wire (pts (xy 204.47 139.065) (xy 204.47 132.715)))
  (wire (pts (xy 204.47 132.715) (xy 212.09 132.715)))
  (wire (pts (xy 236.855 73.025) (xy 227.965 73.025)))
  (polyline (pts (xy 67.31 20.32) (xy 67.31 58.42)))
  (polyline (pts (xy 175.895 113.665) (xy 175.895 45.085)))
  (wire (pts (xy 88.9 37.465) (xy 88.9 42.545)))
  (wire (pts (xy 198.755 108.585) (xy 198.755 88.265)))
  (polyline (pts (xy 173.99 161.925) (xy 121.285 161.925)))
  (wire (pts (xy 247.015 57.785) (xy 227.965 57.785)))
  (wire (pts (xy 40.005 38.735) (xy 40.005 41.275)))
  (wire (pts (xy 160.02 65.405) (xy 160.02 67.945)))
  (wire (pts (xy 198.755 88.265) (xy 198.755 75.565)))
  (wire (pts (xy 245.11 67.31) (xy 254 67.31)))
  (wire (pts (xy 232.41 82.55) (xy 254 82.55)))
  (wire (pts (xy 236.22 93.345) (xy 236.22 77.47)))
  (wire (pts (xy 227.33 121.92) (xy 236.22 121.92)))
  (wire (pts (xy 40.005 48.895) (xy 40.005 43.815)))
  (wire (pts (xy 232.41 88.265) (xy 232.41 82.55)))
  (polyline (pts (xy 16.51 113.03) (xy 67.31 113.03)))
  (wire (pts (xy 231.14 47.625) (xy 266.7 47.625)))
  (wire (pts (xy 240.03 72.39) (xy 240.03 98.425)))
  (wire (pts (xy 36.195 41.275) (xy 40.005 41.275)))
  (wire (pts (xy 262.255 22.225) (xy 268.605 22.225)))
  (wire (pts (xy 233.045 67.945) (xy 227.965 67.945)))
  (wire (pts (xy 266.7 85.09) (xy 266.7 87.63)))
  (wire (pts (xy 191.77 146.685) (xy 204.47 146.685)))
  (wire (pts (xy 240.03 98.425) (xy 227.965 98.425)))
  (wire (pts (xy 248.92 147.32) (xy 248.92 150.495)))
  (polyline (pts (xy 275.59 45.085) (xy 275.59 113.665)))
  (wire (pts (xy 133.35 67.945) (xy 144.78 67.945)))
  (polyline (pts (xy 274.955 161.925) (xy 175.895 161.925)))
  (wire (pts (xy 248.92 129.54) (xy 254.635 129.54)))
  (wire (pts (xy 236.855 53.34) (xy 236.855 73.025)))
  (wire (pts (xy 262.255 34.925) (xy 268.605 34.925)))
  (wire (pts (xy 224.79 121.92) (xy 224.79 118.745)))
  (wire (pts (xy 40.005 38.735) (xy 43.18 38.735)))
  (wire (pts (xy 160.02 67.945) (xy 162.56 67.945)))
  (wire (pts (xy 227.965 60.325) (xy 245.11 60.325)))
  (polyline (pts (xy 16.51 58.42) (xy 16.51 20.32)))
  (wire (pts (xy 238.125 95.885) (xy 238.125 74.93)))
  (wire (pts (xy 40.005 41.275) (xy 40.005 43.815)))
  (wire (pts (xy 198.12 106.045) (xy 206.375 106.045)))
  (polyline (pts (xy 69.85 113.665) (xy 69.85 15.875)))
  (polyline (pts (xy 16.51 61.595) (xy 16.51 113.03)))
  (wire (pts (xy 270.51 67.31) (xy 266.7 67.31)))
  (wire (pts (xy 144.78 42.545) (xy 144.78 46.99)))
  (wire (pts (xy 234.95 142.24) (xy 248.92 142.24)))
  (wire (pts (xy 234.315 80.01) (xy 254 80.01)))
  (polyline (pts (xy 275.59 43.18) (xy 228.6 43.18)))
  (wire (pts (xy 24.13 43.815) (xy 24.13 49.53)))
  (wire (pts (xy 40.005 34.29) (xy 40.005 38.735)))
  (wire (pts (xy 118.11 95.885) (xy 120.65 95.885)))
  (wire (pts (xy 52.07 38.735) (xy 52.07 29.21)))
  (wire (pts (xy 248.285 55.245) (xy 248.285 62.23)))
  (wire (pts (xy 270.51 51.435) (xy 270.51 67.31)))
  (wire (pts (xy 227.965 95.885) (xy 238.125 95.885)))
  (wire (pts (xy 241.935 97.155) (xy 273.05 97.155)))
  (wire (pts (xy 262.255 144.78) (xy 262.255 146.685)))
  (wire (pts (xy 245.745 103.505) (xy 245.745 85.09)))
  (wire (pts (xy 97.155 42.545) (xy 97.155 45.72)))
  (wire (pts (xy 231.14 65.405) (xy 231.14 47.625)))
  (polyline (pts (xy 275.59 13.97) (xy 275.59 42.545)))
  (wire (pts (xy 212.09 127) (xy 214.63 127)))
  (wire (pts (xy 233.045 49.53) (xy 233.045 67.945)))
  (polyline (pts (xy 67.31 61.595) (xy 67.31 113.03)))
  (wire (pts (xy 227.965 93.345) (xy 236.22 93.345)))
  (wire (pts (xy 227.965 88.265) (xy 232.41 88.265)))
  (wire (pts (xy 133.35 42.545) (xy 144.78 42.545)))
  (wire (pts (xy 227.965 100.965) (xy 243.84 100.965)))
  (polyline (pts (xy 173.99 113.665) (xy 69.85 113.665)))
  (wire (pts (xy 210.82 129.54) (xy 214.63 129.54)))
  (wire (pts (xy 50.8 38.735) (xy 52.07 38.735)))
  (wire (pts (xy 102.87 37.465) (xy 88.9 37.465)))
  (wire (pts (xy 118.11 24.765) (xy 120.65 24.765)))
  (wire (pts (xy 100.965 32.385) (xy 100.965 29.21)))
  (wire (pts (xy 266.7 64.77) (xy 268.605 64.77)))
  (wire (pts (xy 28.575 86.36) (xy 30.48 86.36)))
  (wire (pts (xy 92.71 32.385) (xy 100.965 32.385)))
  (wire (pts (xy 227.965 90.805) (xy 234.315 90.805)))
  (polyline (pts (xy 275.59 113.665) (xy 175.895 113.665)))
  (wire (pts (xy 268.605 49.53) (xy 233.045 49.53)))
  (wire (pts (xy 227.965 70.485) (xy 234.95 70.485)))
  (wire (pts (xy 243.205 69.85) (xy 254 69.85)))
  (wire (pts (xy 234.95 134.62) (xy 254.635 134.62)))
  (polyline (pts (xy 69.85 15.875) (xy 173.99 15.875)))
  (wire (pts (xy 266.7 80.01) (xy 266.7 82.55)))
  (wire (pts (xy 147.32 83.185) (xy 152.4 83.185)))
  (wire (pts (xy 268.605 29.845) (xy 268.605 34.925)))
  (wire (pts (xy 266.7 74.93) (xy 266.7 77.47)))
  (wire (pts (xy 133.35 45.085) (xy 142.875 45.085)))
  (wire (pts (xy 243.205 62.865) (xy 243.205 69.85)))
  (polyline (pts (xy 121.285 115.57) (xy 173.99 115.57)))
  (wire (pts (xy 272.415 69.85) (xy 272.415 53.34)))
  (wire (pts (xy 197.485 88.265) (xy 198.755 88.265)))
  (polyline (pts (xy 16.51 20.32) (xy 67.31 20.32)))
  (polyline (pts (xy 121.285 161.925) (xy 121.285 115.57)))
  (wire (pts (xy 262.255 146.685) (xy 262.255 147.955)))
  (wire (pts (xy 198.755 108.585) (xy 206.375 108.585)))
  (wire (pts (xy 234.95 51.435) (xy 270.51 51.435)))
  (wire (pts (xy 248.92 118.745) (xy 248.92 129.54)))
  (polyline (pts (xy 65.405 58.42) (xy 67.31 58.42)))
  (wire (pts (xy 147.32 70.485) (xy 147.32 75.565)))
  (wire (pts (xy 186.055 129.54) (xy 187.96 129.54)))
  (wire (pts (xy 227.965 85.725) (xy 241.935 85.725)))
  (text "MCU and supporting circuitry" (at 71.12 19.05 0))
  (text "Connector to Marge board" (at 38.1 64.77 0))
  (text "Misc stuff" (at 122.555 118.745 0))
  (text "USB interface" (at 177.165 118.745 0))
  (text "TRIG input" (at 17.78 23.495 0))
  (text "Ethernet breakout" (at 229.87 17.145 0))
  (text "GPIB interface" (at 177.165 48.26 0))
  (label "ETH_CS" (at 243.205 32.385 180))
  (label "D1" (at 206.375 55.245 180))
  (label "ISP_MISO" (at 81.915 74.93 180))
  (label "ISP_MOSI" (at 133.35 40.005 0))
  (label "ISP_MOSI" (at 94.615 77.47 0))
  (label "GPIB_TRIG" (at 133.35 50.165 0))
  (label "D8" (at 133.35 80.645 0))
  (label "TXD_USB" (at 30.48 88.9 180))
  (label "RXD_USB" (at 43.18 88.9 0))
  (label "TE" (at 133.35 62.865 0))
  (label "D6" (at 133.35 75.565 0))
  (label "DAV" (at 133.35 37.465 0))
  (label "TXD_USB" (at 191.77 146.685 180))
  (label "ISP_SCK" (at 133.35 45.085 0))
  (label "D6" (at 206.375 67.945 180))
  (label "SRQ" (at 206.375 103.505 180))
  (label "RXD_GPIB" (at 162.56 67.945 0))
  (label "D4" (at 133.35 60.325 0))
  (label "ATN" (at 133.35 85.725 0))
  (label "NRFD" (at 206.375 93.345 180))
  (label "ETH_SCLK" (at 243.205 29.845 180))
  (label "ETH_CS" (at 30.48 96.52 180))
  (label "SRQ" (at 152.4 40.005 0))
  (label "D7" (at 133.35 78.105 0))
  (label "GPIB_TRIG" (at 55.88 78.74 0))
  (label "IFC" (at 206.375 88.265 180))
  (label "D2" (at 133.35 55.245 0))
  (label "ETH_MISO" (at 30.48 99.06 180))
  (label "D2" (at 206.375 57.785 180))
  (label "RXD_USB" (at 186.055 129.54 180))
  (label "NRFD" (at 133.35 34.925 0))
  (label "ETH_RST" (at 243.205 22.225 180))
  (label "EOI" (at 133.35 83.185 0))
  (label "ETH_SCLK" (at 30.48 104.14 180))
  (label "REN" (at 152.4 53.975 0))
  (label "TXD_GPIB" (at 152.4 83.185 0))
  (label "D7" (at 206.375 70.485 180))
  (label "D5" (at 133.35 73.025 0))
  (label "RESET" (at 81.915 80.01 180))
  (label "RESET" (at 92.71 32.385 0))
  (label "D5" (at 206.375 65.405 180))
  (label "IFC" (at 152.4 46.99 0))
  (label "ATN" (at 206.375 100.965 180))
  (label "ISP_SCK" (at 81.915 77.47 180))
  (label "REN" (at 206.375 85.725 180))
  (label "D8" (at 206.375 73.025 180))
  (label "EXT_TRIG" (at 22.225 65.405 0))
  (label "EXT_TRIG" (at 55.245 46.355 0))
  (label "ISP_MISO" (at 133.35 42.545 0))
  (label "DAV" (at 206.375 95.885 180))
  (label "RXD_GPIB" (at 43.18 91.44 0))
  (label "ETH_MOSI" (at 243.205 27.305 180))
  (label "D3" (at 206.375 60.325 180))
  (label "ETH_MISO" (at 243.205 24.765 180))
  (label "D4" (at 206.375 62.865 180))
  (label "D1" (at 133.35 52.705 0))
  (label "NDAC" (at 206.375 90.805 180))
  (label "ETH_MOSI" (at 30.48 101.6 180))
  (label "D3" (at 133.35 57.785 0))
  (label "EOI" (at 206.375 98.425 180))
  (label "NDAC" (at 133.35 32.385 0))
  (label "ETH_RST" (at 30.48 93.98 180))
  (label "TXD_GPIB" (at 30.48 91.44 180))
  (label "TE" (at 198.755 75.565 180))
  (symbol (lib_id "Connector_Generic:Conn_02x03_Odd_Even") (at 86.995 77.47 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J2" (id 0) (at 88.265 69.6935 0))
    (property "Value" "IDC_6pin" (id 1) (at 88.265 72.4686 0))
    (property "Footprint" "Connector_IDC:IDC-Header_2x03_P2.54mm_Vertical" (id 2) (at 86.995 77.47 0))
    (property "Datasheet" "~" (id 3) (at 86.995 77.47 0))
    (property "comment" "" (id 4) (at 86.995 77.47 0))
    (property "supplier" "TME" (id 5) (at 86.995 77.47 0))
    (property "PN" "75869-331LF" (id 6) (at 86.995 77.47 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "Interface_USB:CH340G") (at 224.79 137.16 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U6" (id 0) (at 231.14 152.4 0))
    (property "Value" "CH340G" (id 1) (at 228.6 154.305 0))
    (property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (id 2) (at 223.52 151.13 0))
    (property "Datasheet" "http://www.datasheet5.com/pdf-local-2195953" (id 3) (at 233.68 116.84 0))
    (property "comment" "" (id 4) (at 224.79 137.16 0))
    (property "supplier" "LCSC" (id 5) (at 224.79 137.16 0))
    (property "PN" "CH340G" (id 6) (at 224.79 137.16 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R") (at 148.59 53.975 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R4" (id 0) (at 148.59 56.515 90))
    (property "Value" "120R" (id 1) (at 148.59 58.42 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 148.59 55.753 90))
    (property "Datasheet" "~" (id 3) (at 148.59 53.975 0))
    (property "comment" "" (id 4) (at 148.59 53.975 0))
    (property "supplier" "TME" (id 5) (at 148.59 53.975 0))
    (property "PN" "MMA02040C1200" (id 6) (at 148.59 53.975 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 22.225 80.645 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR034" (id 0) (at 22.225 86.995 0))
    (property "Value" "GND" (id 1) (at 22.225 85.2075 0))
    (property "Footprint" "" (id 2) (at 22.225 80.645 0))
    (property "Datasheet" "" (id 3) (at 22.225 80.645 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 43.18 96.52 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR041" (id 0) (at 39.37 96.52 0))
    (property "Value" "+3V3" (id 1) (at 46.355 96.999 90))
    (property "Footprint" "" (id 2) (at 43.18 96.52 0))
    (property "Datasheet" "" (id 3) (at 43.18 96.52 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 80.01 97.155 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR026" (id 0) (at 80.01 103.505 0))
    (property "Value" "GND" (id 1) (at 80.01 101.6 0))
    (property "Footprint" "" (id 2) (at 80.01 97.155 0))
    (property "Datasheet" "" (id 3) (at 80.01 97.155 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:USB_B") (at 262.255 134.62 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J4" (id 0) (at 268.097 133.7115 0))
    (property "Value" "USB_B" (id 1) (at 268.097 136.4866 0))
    (property "Footprint" "Connector_USB:USB_B_Lumberg_2411_02_Horizontal" (id 2) (at 258.445 135.89 0))
    (property "Datasheet" " ~" (id 3) (at 258.445 135.89 0))
    (property "comment" "" (id 4) (at 262.255 134.62 0))
    (property "supplier" "TME" (id 5) (at 262.255 134.62 0))
    (property "PN" "TUEB4F2D0B" (id 6) (at 262.255 134.62 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R") (at 147.32 86.995 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R8" (id 0) (at 144.145 86.36 0))
    (property "Value" "3k9" (id 1) (at 144.145 88.265 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 145.542 86.995 90))
    (property "Datasheet" "~" (id 3) (at 147.32 86.995 0))
    (property "comment" "" (id 4) (at 147.32 86.995 0))
    (property "supplier" "TME" (id 5) (at 147.32 86.995 0))
    (property "PN" "MMA02040C3902" (id 6) (at 147.32 86.995 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "MCU_Microchip_ATmega:ATmega8A-A") (at 118.11 60.325 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U3" (id 0) (at 122.6694 23.3385 0))
    (property "Value" "AT90S4433" (id 1) (at 122.6694 26.1136 0))
    (property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm" (id 2) (at 118.11 60.325 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf" (id 3) (at 118.11 60.325 0))
    (property "comment" "possible to use Atmega8" (id 4) (at 118.11 60.325 0))
    (property "link" "" (id 5) (at 118.11 60.325 0))
    (property "supplier" "NA" (id 6) (at 118.11 60.325 0))
    (property "PN" "AT90S4433" (id 7) (at 118.11 60.325 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:GND") (at 240.665 158.115 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR042" (id 0) (at 240.665 164.465 0))
    (property "Value" "GND" (id 1) (at 237.49 160.655 0))
    (property "Footprint" "" (id 2) (at 240.665 158.115 0))
    (property "Datasheet" "" (id 3) (at 240.665 158.115 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 148.59 40.005 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 148.59 42.545 90))
    (property "Value" "120R" (id 1) (at 148.59 44.45 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 148.59 41.783 90))
    (property "Datasheet" "~" (id 3) (at 148.59 40.005 0))
    (property "comment" "" (id 4) (at 148.59 40.005 0))
    (property "supplier" "TME" (id 5) (at 148.59 40.005 0))
    (property "PN" "MMA02040C1200" (id 6) (at 148.59 40.005 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 207.01 129.54 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R12" (id 0) (at 207.01 125.095 90))
    (property "Value" "12k" (id 1) (at 207.01 127 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 207.01 127.762 90))
    (property "Datasheet" "~" (id 3) (at 207.01 129.54 0))
    (property "comment" "" (id 4) (at 207.01 129.54 0))
    (property "supplier" "TME" (id 5) (at 207.01 129.54 0))
    (property "PN" "MMA02040C1203" (id 6) (at 207.01 129.54 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 190.5 106.045 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR024" (id 0) (at 190.5 109.855 0))
    (property "Value" "+5V" (id 1) (at 190.5 102.4405 0))
    (property "Footprint" "" (id 2) (at 190.5 106.045 0))
    (property "Datasheet" "" (id 3) (at 190.5 106.045 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 147.32 79.375 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R7" (id 0) (at 144.145 78.74 0))
    (property "Value" "2k4" (id 1) (at 144.145 80.645 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 145.542 79.375 90))
    (property "Datasheet" "~" (id 3) (at 147.32 79.375 0))
    (property "comment" "" (id 4) (at 147.32 79.375 0))
    (property "supplier" "TME" (id 5) (at 147.32 79.375 0))
    (property "PN" "MMA02040C2402" (id 6) (at 147.32 79.375 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 94.615 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR015" (id 0) (at 94.615 78.74 0))
    (property "Value" "+5V" (id 1) (at 94.615 71.3255 0))
    (property "Footprint" "" (id 2) (at 94.615 74.93 0))
    (property "Datasheet" "" (id 3) (at 94.615 74.93 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 131.445 142.24 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR046" (id 0) (at 131.445 148.59 0))
    (property "Value" "GND" (id 1) (at 131.445 146.8025 0))
    (property "Footprint" "" (id 2) (at 131.445 142.24 0))
    (property "Datasheet" "" (id 3) (at 131.445 142.24 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:Conn_01x02_Male") (at 19.05 41.275 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J3" (id 0) (at 19.685 37.2323 0))
    (property "Value" "Conn_01x02_Male" (id 1) (at 19.685 40.0074 0))
    (property "Footprint" "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical" (id 2) (at 19.05 41.275 0))
    (property "Datasheet" "~" (id 3) (at 19.05 41.275 0))
    (property "comment" "" (id 4) (at 19.05 41.275 0))
    (property "supplier" "TME" (id 5) (at 19.05 41.275 0))
    (property "PN" "NS25-W2P" (id 6) (at 19.05 41.275 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 159.385 151.765 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR047" (id 0) (at 159.385 158.115 0))
    (property "Value" "GND" (id 1) (at 159.385 156.3275 0))
    (property "Footprint" "" (id 2) (at 159.385 151.765 0))
    (property "Datasheet" "" (id 3) (at 159.385 151.765 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 59.69 29.21 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0101" (id 0) (at 59.69 35.56 0))
    (property "Value" "GND" (id 1) (at 62.23 32.385 0))
    (property "Footprint" "" (id 2) (at 59.69 29.21 0))
    (property "Datasheet" "" (id 3) (at 59.69 29.21 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 90.17 97.155 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR027" (id 0) (at 90.17 103.505 0))
    (property "Value" "GND" (id 1) (at 90.17 101.6 0))
    (property "Footprint" "" (id 2) (at 90.17 97.155 0))
    (property "Datasheet" "" (id 3) (at 90.17 97.155 0))
    (pin "1")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 142.24 123.19 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H2" (id 0) (at 144.78 122.2815 0))
    (property "Value" "MountingHole" (id 1) (at 144.78 125.0566 0))
    (property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (id 2) (at 142.24 123.19 0))
    (property "Datasheet" "~" (id 3) (at 142.24 123.19 0))
    (property "comment" "" (id 4) (at 142.24 123.19 0))
    (property "link" "DNP" (id 5) (at 142.24 123.19 0))
  )
  (symbol (lib_id "power:+5V") (at 189.865 88.265 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR016" (id 0) (at 189.865 92.075 0))
    (property "Value" "+5V" (id 1) (at 189.865 84.6605 0))
    (property "Footprint" "" (id 2) (at 189.865 88.265 0))
    (property "Datasheet" "" (id 3) (at 189.865 88.265 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74LS08") (at 139.065 139.7 0) (unit 4)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U4" (id 0) (at 139.065 131.9235 0))
    (property "Value" "74HCT08" (id 1) (at 139.065 134.6986 0))
    (property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (id 2) (at 139.065 139.7 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS08" (id 3) (at 139.065 139.7 0))
    (property "comment" "" (id 4) (at 139.065 139.7 0))
    (property "supplier" "TME" (id 5) (at 139.065 139.7 0))
    (property "PN" "74HCT08PW.112" (id 6) (at 139.065 139.7 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "power:GND") (at 204.47 154.305 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR038" (id 0) (at 204.47 160.655 0))
    (property "Value" "GND" (id 1) (at 204.47 158.8675 0))
    (property "Footprint" "" (id 2) (at 204.47 154.305 0))
    (property "Datasheet" "" (id 3) (at 204.47 154.305 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 262.255 147.955 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR036" (id 0) (at 262.255 154.305 0))
    (property "Value" "GND" (id 1) (at 264.16 149.704 0))
    (property "Footprint" "" (id 2) (at 262.255 147.955 0))
    (property "Datasheet" "" (id 3) (at 262.255 147.955 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Crystal") (at 92.71 42.545 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Y1" (id 0) (at 81.915 40.005 0))
    (property "Value" "7.3728MHz" (id 1) (at 82.55 42.545 0))
    (property "Footprint" "Crystal:Crystal_SMD_HC49-SD" (id 2) (at 92.71 42.545 0))
    (property "Datasheet" "~" (id 3) (at 92.71 42.545 0))
    (property "PN" "7.372M-SMDHC49S " (id 4) (at 92.71 42.545 0))
    (property "supplier" "TME" (id 5) (at 92.71 42.545 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 55.88 93.98 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR040" (id 0) (at 55.88 100.33 0))
    (property "Value" "GND" (id 1) (at 55.88 98.5425 0))
    (property "Footprint" "" (id 2) (at 55.88 93.98 0))
    (property "Datasheet" "" (id 3) (at 55.88 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 100.33 47.625 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR07" (id 0) (at 100.33 51.435 0))
    (property "Value" "+5V" (id 1) (at 100.33 44.0205 0))
    (property "Footprint" "" (id 2) (at 100.33 47.625 0))
    (property "Datasheet" "" (id 3) (at 100.33 47.625 0))
    (pin "1")
  )
  (symbol (lib_id "j_lib:75161") (at 216.535 97.155 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U5" (id 0) (at 217.17 79.2693 0))
    (property "Value" "75ALS161" (id 1) (at 217.17 82.0444 0))
    (property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (id 2) (at 196.215 121.285 0))
    (property "Datasheet" "" (id 3) (at 196.215 121.285 0))
    (property "link" "" (id 4) (at 216.535 97.155 0))
    (property "supplier" "MOUSER" (id 5) (at 216.535 97.155 0))
    (property "comment" "" (id 6) (at 216.535 97.155 0))
    (property "PN" "SN75ALS161DW " (id 7) (at 216.535 97.155 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R") (at 204.47 142.875 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R15" (id 0) (at 201.295 142.24 0))
    (property "Value" "2k4" (id 1) (at 201.295 144.145 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 202.692 142.875 90))
    (property "Datasheet" "~" (id 3) (at 204.47 142.875 0))
    (property "comment" "" (id 4) (at 204.47 142.875 0))
    (property "supplier" "TME" (id 5) (at 204.47 142.875 0))
    (property "PN" "MMA02040C2402" (id 6) (at 204.47 142.875 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x12_Top_Bottom") (at 259.08 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J1" (id 0) (at 260.35 56.9935 0))
    (property "Value" "Centronics 24, socket" (id 1) (at 260.35 59.7686 0))
    (property "Footprint" "j_lib:CENTR_24P_F" (id 2) (at 259.08 74.93 0))
    (property "Datasheet" "~" (id 3) (at 259.08 74.93 0))
    (property "comment" "" (id 4) (at 259.08 74.93 0))
    (property "link" "https://www.aliexpress.com/item/32795413098.html" (id 5) (at 259.08 74.93 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "74xx:74LS08") (at 47.625 46.355 0) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 51.435 51.435 0))
    (property "Value" "74HCT08" (id 1) (at 50.165 53.34 0))
    (property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (id 2) (at 47.625 46.355 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS08" (id 3) (at 47.625 46.355 0))
    (property "comment" "" (id 4) (at 47.625 46.355 0))
    (property "supplier" "TME" (id 5) (at 47.625 46.355 0))
    (property "PN" "74HCT08PW.112" (id 6) (at 47.625 46.355 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "power:+5V") (at 100.965 21.59 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR02" (id 0) (at 100.965 25.4 0))
    (property "Value" "+5V" (id 1) (at 103.505 18.415 0))
    (property "Footprint" "" (id 2) (at 100.965 21.59 0))
    (property "Datasheet" "" (id 3) (at 100.965 21.59 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 195.58 57.15 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C3" (id 0) (at 189.865 57.15 0))
    (property "Value" "1u" (id 1) (at 189.23 59.055 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 196.5452 53.34 0))
    (property "Datasheet" "~" (id 3) (at 195.58 57.15 0))
    (property "comment" "" (id 4) (at 195.58 57.15 0))
    (property "supplier" "TME" (id 5) (at 195.58 57.15 0))
    (property "PN" "CL21B105KAFNNNG" (id 6) (at 195.58 57.15 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 195.58 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR09" (id 0) (at 195.58 67.31 0))
    (property "Value" "GND" (id 1) (at 195.58 65.5225 0))
    (property "Footprint" "" (id 2) (at 195.58 60.96 0))
    (property "Datasheet" "" (id 3) (at 195.58 60.96 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 195.58 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR06" (id 0) (at 195.58 57.15 0))
    (property "Value" "+5V" (id 1) (at 195.58 49.7355 0))
    (property "Footprint" "" (id 2) (at 195.58 53.34 0))
    (property "Datasheet" "" (id 3) (at 195.58 53.34 0))
    (pin "1")
  )
  (symbol (lib_id "j_lib:W5500_bo") (at 252.73 28.575 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 240.665 38.1 0))
    (property "Value" "W5500_breakout" (id 1) (at 252.73 38.1 0))
    (property "Footprint" "j_lib:W5500_bo" (id 2) (at 248.285 27.94 0))
    (property "Datasheet" "" (id 3) (at 248.285 27.94 0))
    (property "comment" "" (id 4) (at 252.73 28.575 0))
    (property "link" "W5500 breakout" (id 5) (at 252.73 28.575 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "power:GND") (at 97.155 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR011" (id 0) (at 97.155 59.69 0))
    (property "Value" "GND" (id 1) (at 97.155 57.9025 0))
    (property "Footprint" "" (id 2) (at 97.155 53.34 0))
    (property "Datasheet" "" (id 3) (at 97.155 53.34 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 254 90.17 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR018" (id 0) (at 254 96.52 0))
    (property "Value" "GND" (id 1) (at 254 94.7325 0))
    (property "Footprint" "" (id 2) (at 254 90.17 0))
    (property "Datasheet" "" (id 3) (at 254 90.17 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 248.92 158.115 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR043" (id 0) (at 248.92 164.465 0))
    (property "Value" "GND" (id 1) (at 252.73 160.02 0))
    (property "Footprint" "" (id 2) (at 248.92 158.115 0))
    (property "Datasheet" "" (id 3) (at 248.92 158.115 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 193.675 78.105 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R5" (id 0) (at 193.675 80.645 90))
    (property "Value" "12k" (id 1) (at 193.675 82.55 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 193.675 79.883 90))
    (property "Datasheet" "~" (id 3) (at 193.675 78.105 0))
    (property "comment" "" (id 4) (at 193.675 78.105 0))
    (property "supplier" "TME" (id 5) (at 193.675 78.105 0))
    (property "PN" "MMA02040C1203" (id 6) (at 193.675 78.105 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 193.675 88.265 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R6" (id 0) (at 193.675 90.805 90))
    (property "Value" "12k" (id 1) (at 193.675 92.71 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 193.675 90.043 90))
    (property "Datasheet" "~" (id 3) (at 193.675 88.265 0))
    (property "comment" "" (id 4) (at 193.675 88.265 0))
    (property "supplier" "TME" (id 5) (at 193.675 88.265 0))
    (property "PN" "MMA02040C1203" (id 6) (at 193.675 88.265 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 97.155 49.53 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C5" (id 0) (at 91.44 48.895 0))
    (property "Value" "22p" (id 1) (at 90.805 51.435 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 98.1202 53.34 0))
    (property "Datasheet" "~" (id 3) (at 97.155 49.53 0))
    (property "comment" "" (id 4) (at 97.155 49.53 0))
    (property "supplier" "TME" (id 5) (at 97.155 49.53 0))
    (property "PN" "VJ0805A220JXACW1BC" (id 6) (at 97.155 49.53 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Diode:BAV99") (at 40.005 29.21 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D1" (id 0) (at 40.005 23.9989 0))
    (property "Value" "BAV99" (id 1) (at 40.005 26.774 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 40.005 41.91 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/BAV99_SER.pdf" (id 3) (at 40.005 29.21 0))
    (property "comment" "" (id 4) (at 40.005 29.21 0))
    (property "supplier" "TME" (id 5) (at 40.005 29.21 0))
    (property "PN" "BAV99" (id 6) (at 40.005 29.21 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:+5V") (at 189.865 78.105 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR013" (id 0) (at 189.865 81.915 0))
    (property "Value" "+5V" (id 1) (at 189.865 74.5005 0))
    (property "Footprint" "" (id 2) (at 189.865 78.105 0))
    (property "Datasheet" "" (id 3) (at 189.865 78.105 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3V3") (at 268.605 22.225 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR01" (id 0) (at 268.605 26.035 0))
    (property "Value" "+3V3" (id 1) (at 268.605 18.6205 0))
    (property "Footprint" "" (id 2) (at 268.605 22.225 0))
    (property "Datasheet" "" (id 3) (at 268.605 22.225 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 240.03 121.92 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C9" (id 0) (at 240.665 126.365 90))
    (property "Value" "1u" (id 1) (at 240.665 128.905 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 243.84 122.8852 0))
    (property "Datasheet" "~" (id 3) (at 240.03 121.92 0))
    (property "comment" "" (id 4) (at 240.03 121.92 0))
    (property "supplier" "TME" (id 5) (at 240.03 121.92 0))
    (property "PN" "CL21B105KAFNNNG" (id 6) (at 240.03 121.92 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 266.7 90.17 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR019" (id 0) (at 266.7 96.52 0))
    (property "Value" "GND" (id 1) (at 266.7 94.7325 0))
    (property "Footprint" "" (id 2) (at 266.7 90.17 0))
    (property "Datasheet" "" (id 3) (at 266.7 90.17 0))
    (pin "1")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 133.985 127.635 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H3" (id 0) (at 136.525 126.7265 0))
    (property "Value" "MountingHole" (id 1) (at 136.525 129.5016 0))
    (property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (id 2) (at 133.985 127.635 0))
    (property "Datasheet" "~" (id 3) (at 133.985 127.635 0))
    (property "comment" "" (id 4) (at 133.985 127.635 0))
    (property "link" "DNP" (id 5) (at 133.985 127.635 0))
  )
  (symbol (lib_id "power:GND") (at 88.9 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR010" (id 0) (at 88.9 59.69 0))
    (property "Value" "GND" (id 1) (at 88.9 57.9025 0))
    (property "Footprint" "" (id 2) (at 88.9 53.34 0))
    (property "Datasheet" "" (id 3) (at 88.9 53.34 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 24.13 49.53 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR033" (id 0) (at 24.13 55.88 0))
    (property "Value" "GND" (id 1) (at 24.13 54.0925 0))
    (property "Footprint" "" (id 2) (at 24.13 49.53 0))
    (property "Datasheet" "" (id 3) (at 24.13 49.53 0))
    (pin "1")
  )
  (symbol (lib_id "Diode:SM6T6V8A") (at 55.88 29.21 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D2" (id 0) (at 56.515 33.655 0))
    (property "Value" "SM6T6V8A" (id 1) (at 57.15 35.56 0))
    (property "Footprint" "Diode_SMD:D_SMB" (id 2) (at 55.88 34.29 0))
    (property "Datasheet" "https://www.st.com/resource/en/datasheet/sm6t.pdf" (id 3) (at 54.61 29.21 0))
    (property "comment" "" (id 4) (at 55.88 29.21 0))
    (property "supplier" "TME" (id 5) (at 55.88 29.21 0))
    (property "PN" "SM6T6V8A" (id 6) (at 55.88 29.21 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 22.225 76.835 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R14" (id 0) (at 25.4 76.2 0))
    (property "Value" "3k9" (id 1) (at 25.4 78.105 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 24.003 76.835 90))
    (property "Datasheet" "~" (id 3) (at 22.225 76.835 0))
    (property "comment" "" (id 4) (at 22.225 76.835 0))
    (property "supplier" "TME" (id 5) (at 22.225 76.835 0))
    (property "PN" "MMA02040C3902" (id 6) (at 22.225 76.835 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 88.9 49.53 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C4" (id 0) (at 83.185 48.895 0))
    (property "Value" "22p" (id 1) (at 82.55 51.435 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 89.8652 53.34 0))
    (property "Datasheet" "~" (id 3) (at 88.9 49.53 0))
    (property "comment" "" (id 4) (at 88.9 49.53 0))
    (property "supplier" "TME" (id 5) (at 88.9 49.53 0))
    (property "PN" "VJ0805A220JXACW1BC" (id 6) (at 88.9 49.53 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 36.195 48.895 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR035" (id 0) (at 36.195 55.245 0))
    (property "Value" "GND" (id 1) (at 36.195 53.4575 0))
    (property "Footprint" "" (id 2) (at 36.195 48.895 0))
    (property "Datasheet" "" (id 3) (at 36.195 48.895 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74LS08") (at 195.58 129.54 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U4" (id 0) (at 195.58 121.7635 0))
    (property "Value" "74HCT08" (id 1) (at 195.58 124.5386 0))
    (property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (id 2) (at 195.58 129.54 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS08" (id 3) (at 195.58 129.54 0))
    (property "comment" "" (id 4) (at 195.58 129.54 0))
    (property "supplier" "TME" (id 5) (at 195.58 129.54 0))
    (property "PN" "74HCT08PW.112" (id 6) (at 195.58 129.54 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "power:+5V") (at 186.055 53.34 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR05" (id 0) (at 186.055 57.15 0))
    (property "Value" "+5V" (id 1) (at 186.055 49.7355 0))
    (property "Footprint" "" (id 2) (at 186.055 53.34 0))
    (property "Datasheet" "" (id 3) (at 186.055 53.34 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 186.055 57.15 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C2" (id 0) (at 180.34 57.15 0))
    (property "Value" "1u" (id 1) (at 179.705 59.055 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 187.0202 53.34 0))
    (property "Datasheet" "~" (id 3) (at 186.055 57.15 0))
    (property "comment" "" (id 4) (at 186.055 57.15 0))
    (property "supplier" "TME" (id 5) (at 186.055 57.15 0))
    (property "PN" "CL21B105KAFNNNG" (id 6) (at 186.055 57.15 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 36.195 45.085 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C10" (id 0) (at 32.385 45.085 0))
    (property "Value" "470p" (id 1) (at 32.385 47.625 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 35.2298 48.895 0))
    (property "Datasheet" "~" (id 3) (at 36.195 45.085 0))
    (property "comment" "" (id 4) (at 36.195 45.085 0))
    (property "supplier" "TME" (id 5) (at 36.195 45.085 0))
    (property "PN" "VJ0805Y471KXACW1BC" (id 6) (at 36.195 45.085 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 29.845 29.21 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR029" (id 0) (at 29.845 35.56 0))
    (property "Value" "GND" (id 1) (at 29.845 33.7725 0))
    (property "Footprint" "" (id 2) (at 29.845 29.21 0))
    (property "Datasheet" "" (id 3) (at 29.845 29.21 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74LS08") (at 159.385 139.065 0) (unit 5)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U4" (id 0) (at 165.227 138.1565 0))
    (property "Value" "74HCT08" (id 1) (at 165.227 140.9316 0))
    (property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (id 2) (at 159.385 139.065 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS08" (id 3) (at 159.385 139.065 0))
    (property "comment" "" (id 4) (at 159.385 139.065 0))
    (property "supplier" "TME" (id 5) (at 159.385 139.065 0))
    (property "PN" "74HCT08PW.112" (id 6) (at 159.385 139.065 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "power:GND") (at 268.605 34.925 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR04" (id 0) (at 268.605 41.275 0))
    (property "Value" "GND" (id 1) (at 268.605 39.4875 0))
    (property "Footprint" "" (id 2) (at 268.605 34.925 0))
    (property "Datasheet" "" (id 3) (at 268.605 34.925 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 204.47 150.495 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R17" (id 0) (at 201.295 149.86 0))
    (property "Value" "3k9" (id 1) (at 201.295 151.765 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 202.692 150.495 90))
    (property "Datasheet" "~" (id 3) (at 204.47 150.495 0))
    (property "comment" "" (id 4) (at 204.47 150.495 0))
    (property "supplier" "TME" (id 5) (at 204.47 150.495 0))
    (property "PN" "MMA02040C3902" (id 6) (at 204.47 150.495 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "j_lib:logo_generic") (at 137.795 153.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "LOGO1" (id 0) (at 134.62 149.86 0))
    (property "Value" "PCB logo" (id 1) (at 137.795 157.48 0))
    (property "Footprint" "j_lib:logo_rpg7x9" (id 2) (at 137.795 153.67 0))
    (property "Datasheet" "" (id 3) (at 137.795 153.67 0))
    (property "link" "DNP" (id 4) (at 137.795 153.67 0))
  )
  (symbol (lib_id "Device:C") (at 80.01 93.345 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C6" (id 0) (at 74.295 93.345 0))
    (property "Value" "1u" (id 1) (at 73.66 95.25 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 80.9752 89.535 0))
    (property "Datasheet" "~" (id 3) (at 80.01 93.345 0))
    (property "comment" "" (id 4) (at 80.01 93.345 0))
    (property "supplier" "TME" (id 5) (at 80.01 93.345 0))
    (property "PN" "CL21B105KAFNNNG" (id 6) (at 80.01 93.345 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 43.18 104.14 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR045" (id 0) (at 43.18 110.49 0))
    (property "Value" "GND" (id 1) (at 43.18 108.7025 0))
    (property "Footprint" "" (id 2) (at 43.18 104.14 0))
    (property "Datasheet" "" (id 3) (at 43.18 104.14 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 224.79 152.4 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR037" (id 0) (at 224.79 158.75 0))
    (property "Value" "GND" (id 1) (at 224.79 156.9625 0))
    (property "Footprint" "" (id 2) (at 224.79 152.4 0))
    (property "Datasheet" "" (id 3) (at 224.79 152.4 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74LS08") (at 152.4 67.945 180) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "U4" (id 0) (at 153.035 77.47 0))
    (property "Value" "74HCT08" (id 1) (at 152.4 72.9464 0))
    (property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (id 2) (at 152.4 67.945 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS08" (id 3) (at 152.4 67.945 0))
    (property "comment" "" (id 4) (at 152.4 67.945 0))
    (property "supplier" "TME" (id 5) (at 152.4 67.945 0))
    (property "PN" "74HCT08PW.112" (id 6) (at 152.4 67.945 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "10")
    (pin "8")
    (pin "9")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "Device:R") (at 194.31 106.045 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R9" (id 0) (at 194.31 108.585 90))
    (property "Value" "12k" (id 1) (at 194.31 110.49 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 194.31 107.823 90))
    (property "Datasheet" "~" (id 3) (at 194.31 106.045 0))
    (property "comment" "" (id 4) (at 194.31 106.045 0))
    (property "supplier" "TME" (id 5) (at 194.31 106.045 0))
    (property "PN" "MMA02040C1203" (id 6) (at 194.31 106.045 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x08_Odd_Even") (at 35.56 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J5" (id 0) (at 36.83 81.1235 0))
    (property "Value" "IDC_16" (id 1) (at 36.83 83.8986 0))
    (property "Footprint" "Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical" (id 2) (at 35.56 93.98 0))
    (property "Datasheet" "~" (id 3) (at 35.56 93.98 0))
    (property "comment" "" (id 4) (at 35.56 93.98 0))
    (property "supplier" "TME" (id 5) (at 35.56 93.98 0))
    (property "PN" "T821-1-16-S1" (id 6) (at 35.56 93.98 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:GND") (at 227.965 78.105 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR014" (id 0) (at 227.965 84.455 0))
    (property "Value" "GND" (id 1) (at 227.965 82.6675 0))
    (property "Footprint" "" (id 2) (at 227.965 78.105 0))
    (property "Datasheet" "" (id 3) (at 227.965 78.105 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 118.11 24.765 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR03" (id 0) (at 118.11 28.575 0))
    (property "Value" "+5V" (id 1) (at 118.11 21.1605 0))
    (property "Footprint" "" (id 2) (at 118.11 24.765 0))
    (property "Datasheet" "" (id 3) (at 118.11 24.765 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C_Polarized") (at 268.605 26.035 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C1" (id 0) (at 271.526 24.2375 0))
    (property "Value" "100u" (id 1) (at 271.526 27.0126 0))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-7132-28_AVX-C_Pad2.72x3.50mm_HandSolder" (id 2) (at 269.5702 29.845 0))
    (property "Datasheet" "~" (id 3) (at 268.605 26.035 0))
    (property "comment" "" (id 4) (at 268.605 26.035 0))
    (property "supplier" "TME" (id 5) (at 268.605 26.035 0))
    (property "PN" "T491C107K010AT" (id 6) (at 268.605 26.035 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 248.92 154.305 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C12" (id 0) (at 254.635 153.67 0))
    (property "Value" "22p" (id 1) (at 255.27 156.21 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 247.9548 158.115 0))
    (property "Datasheet" "~" (id 3) (at 248.92 154.305 0))
    (property "comment" "" (id 4) (at 248.92 154.305 0))
    (property "supplier" "TME" (id 5) (at 248.92 154.305 0))
    (property "PN" "VJ0805A220JXACW1BC" (id 6) (at 248.92 154.305 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 90.17 93.345 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C7" (id 0) (at 84.455 93.345 0))
    (property "Value" "1u" (id 1) (at 83.82 95.25 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 91.1352 89.535 0))
    (property "Datasheet" "~" (id 3) (at 90.17 93.345 0))
    (property "comment" "" (id 4) (at 90.17 93.345 0))
    (property "supplier" "TME" (id 5) (at 90.17 93.345 0))
    (property "PN" "CL21B105KAFNNNG" (id 6) (at 90.17 93.345 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 227.965 108.585 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR028" (id 0) (at 227.965 114.935 0))
    (property "Value" "GND" (id 1) (at 231.775 110.49 0))
    (property "Footprint" "" (id 2) (at 227.965 108.585 0))
    (property "Datasheet" "" (id 3) (at 227.965 108.585 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 55.88 90.17 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R18" (id 0) (at 59.055 89.535 0))
    (property "Value" "3k9" (id 1) (at 59.055 91.44 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.658 90.17 90))
    (property "Datasheet" "~" (id 3) (at 55.88 90.17 0))
    (property "comment" "" (id 4) (at 55.88 90.17 0))
    (property "supplier" "TME" (id 5) (at 55.88 90.17 0))
    (property "PN" "MMA02040C3902" (id 6) (at 55.88 90.17 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Crystal") (at 245.11 147.32 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Y2" (id 0) (at 252.095 144.78 0))
    (property "Value" "12MHz" (id 1) (at 252.73 146.685 0))
    (property "Footprint" "Crystal:Crystal_SMD_HC49-SD" (id 2) (at 245.11 147.32 0))
    (property "Datasheet" "~" (id 3) (at 245.11 147.32 0))
    (property "PN" "12.00M-SMDHC49S" (id 4) (at 245.11 147.32 0))
    (property "supplier" "TME" (id 5) (at 245.11 147.32 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 90.17 89.535 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR021" (id 0) (at 90.17 93.345 0))
    (property "Value" "+5V" (id 1) (at 90.17 85.9305 0))
    (property "Footprint" "" (id 2) (at 90.17 89.535 0))
    (property "Datasheet" "" (id 3) (at 90.17 89.535 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 227.965 106.045 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR025" (id 0) (at 224.155 106.045 0))
    (property "Value" "+5V" (id 1) (at 231.14 106.524 90))
    (property "Footprint" "" (id 2) (at 227.965 106.045 0))
    (property "Datasheet" "" (id 3) (at 227.965 106.045 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 22.225 69.215 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R13" (id 0) (at 25.4 68.58 0))
    (property "Value" "2k4" (id 1) (at 25.4 70.485 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 24.003 69.215 90))
    (property "Datasheet" "~" (id 3) (at 22.225 69.215 0))
    (property "comment" "" (id 4) (at 22.225 69.215 0))
    (property "supplier" "TME" (id 5) (at 22.225 69.215 0))
    (property "PN" "MMA02040C2402" (id 6) (at 22.225 69.215 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 186.055 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR08" (id 0) (at 186.055 67.31 0))
    (property "Value" "GND" (id 1) (at 186.055 65.5225 0))
    (property "Footprint" "" (id 2) (at 186.055 60.96 0))
    (property "Datasheet" "" (id 3) (at 186.055 60.96 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 243.84 123.825 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR032" (id 0) (at 243.84 130.175 0))
    (property "Value" "GND" (id 1) (at 243.84 128.3875 0))
    (property "Footprint" "" (id 2) (at 243.84 123.825 0))
    (property "Datasheet" "" (id 3) (at 243.84 123.825 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 240.665 154.305 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C11" (id 0) (at 246.38 153.67 0))
    (property "Value" "22p" (id 1) (at 247.015 156.21 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 239.6998 158.115 0))
    (property "Datasheet" "~" (id 3) (at 240.665 154.305 0))
    (property "comment" "" (id 4) (at 240.665 154.305 0))
    (property "supplier" "TME" (id 5) (at 240.665 154.305 0))
    (property "PN" "VJ0805A220JXACW1BC" (id 6) (at 240.665 154.305 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 46.99 38.735 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R10" (id 0) (at 48.26 33.02 90))
    (property "Value" "39k" (id 1) (at 48.26 35.56 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 46.99 36.957 90))
    (property "Datasheet" "~" (id 3) (at 46.99 38.735 0))
    (property "comment" "" (id 4) (at 46.99 38.735 0))
    (property "supplier" "TME" (id 5) (at 46.99 38.735 0))
    (property "PN" "MMA02040C3903" (id 6) (at 46.99 38.735 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 252.73 118.745 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C8" (id 0) (at 254 123.19 90))
    (property "Value" "1u" (id 1) (at 254 125.73 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 256.54 119.7102 0))
    (property "Datasheet" "~" (id 3) (at 252.73 118.745 0))
    (property "comment" "" (id 4) (at 252.73 118.745 0))
    (property "supplier" "TME" (id 5) (at 252.73 118.745 0))
    (property "PN" "CL21B105KAFNNNG" (id 6) (at 252.73 118.745 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 133.985 123.19 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H1" (id 0) (at 136.525 122.2815 0))
    (property "Value" "MountingHole" (id 1) (at 136.525 125.0566 0))
    (property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (id 2) (at 133.985 123.19 0))
    (property "Datasheet" "~" (id 3) (at 133.985 123.19 0))
    (property "comment" "" (id 4) (at 133.985 123.19 0))
    (property "link" "DNP" (id 5) (at 133.985 123.19 0))
  )
  (symbol (lib_id "Device:R") (at 148.59 46.99 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R3" (id 0) (at 148.59 49.53 90))
    (property "Value" "120R" (id 1) (at 148.59 51.435 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 148.59 48.768 90))
    (property "Datasheet" "~" (id 3) (at 148.59 46.99 0))
    (property "comment" "" (id 4) (at 148.59 46.99 0))
    (property "supplier" "TME" (id 5) (at 148.59 46.99 0))
    (property "PN" "MMA02040C1200" (id 6) (at 148.59 46.99 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 256.54 118.745 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR031" (id 0) (at 256.54 125.095 0))
    (property "Value" "GND" (id 1) (at 256.54 123.3075 0))
    (property "Footprint" "" (id 2) (at 256.54 118.745 0))
    (property "Datasheet" "" (id 3) (at 256.54 118.745 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 27.94 41.275 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R11" (id 0) (at 29.21 35.56 90))
    (property "Value" "3k9" (id 1) (at 29.21 38.1 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 27.94 39.497 90))
    (property "Datasheet" "~" (id 3) (at 27.94 41.275 0))
    (property "comment" "" (id 4) (at 27.94 41.275 0))
    (property "supplier" "TME" (id 5) (at 27.94 41.275 0))
    (property "PN" "MMA02040C3902" (id 6) (at 27.94 41.275 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Mechanical:MountingHole") (at 142.24 127.635 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "H4" (id 0) (at 144.78 126.7265 0))
    (property "Value" "MountingHole" (id 1) (at 144.78 129.5016 0))
    (property "Footprint" "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (id 2) (at 142.24 127.635 0))
    (property "Datasheet" "~" (id 3) (at 142.24 127.635 0))
    (property "comment" "" (id 4) (at 142.24 127.635 0))
    (property "link" "DNP" (id 5) (at 142.24 127.635 0))
  )
  (symbol (lib_id "power:GND") (at 147.32 90.805 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR022" (id 0) (at 147.32 97.155 0))
    (property "Value" "GND" (id 1) (at 147.32 95.3675 0))
    (property "Footprint" "" (id 2) (at 147.32 90.805 0))
    (property "Datasheet" "" (id 3) (at 147.32 90.805 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 52.07 29.21 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR030" (id 0) (at 52.07 33.02 0))
    (property "Value" "+5V" (id 1) (at 52.07 25.6055 0))
    (property "Footprint" "" (id 2) (at 52.07 29.21 0))
    (property "Datasheet" "" (id 3) (at 52.07 29.21 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 118.11 95.885 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR023" (id 0) (at 118.11 102.235 0))
    (property "Value" "GND" (id 1) (at 118.11 100.4475 0))
    (property "Footprint" "" (id 2) (at 118.11 95.885 0))
    (property "Datasheet" "" (id 3) (at 118.11 95.885 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 100.965 25.4 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 104.775 22.86 0))
    (property "Value" "12k" (id 1) (at 104.775 25.4 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 102.743 25.4 90))
    (property "Datasheet" "~" (id 3) (at 100.965 25.4 0))
    (property "comment" "" (id 4) (at 100.965 25.4 0))
    (property "supplier" "TME" (id 5) (at 100.965 25.4 0))
    (property "PN" "MMA02040C1203" (id 6) (at 100.965 25.4 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 80.01 89.535 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR020" (id 0) (at 80.01 93.345 0))
    (property "Value" "+5V" (id 1) (at 80.01 85.9305 0))
    (property "Footprint" "" (id 2) (at 80.01 89.535 0))
    (property "Datasheet" "" (id 3) (at 80.01 89.535 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 227.965 75.565 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR012" (id 0) (at 224.155 75.565 0))
    (property "Value" "+5V" (id 1) (at 231.14 76.044 90))
    (property "Footprint" "" (id 2) (at 227.965 75.565 0))
    (property "Datasheet" "" (id 3) (at 227.965 75.565 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 43.18 93.98 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR039" (id 0) (at 39.37 93.98 0))
    (property "Value" "+5V" (id 1) (at 46.355 94.459 90))
    (property "Footprint" "" (id 2) (at 43.18 93.98 0))
    (property "Datasheet" "" (id 3) (at 43.18 93.98 0))
    (pin "1")
  )
  (symbol (lib_id "j_lib:75160") (at 217.805 67.945 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U2" (id 0) (at 217.17 48.7893 0))
    (property "Value" "75ALS160" (id 1) (at 217.17 51.5644 0))
    (property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (id 2) (at 224.155 89.535 0))
    (property "Datasheet" "" (id 3) (at 224.155 89.535 0))
    (property "link" "" (id 4) (at 217.805 67.945 0))
    (property "supplier" "MOUSER" (id 5) (at 217.805 67.945 0))
    (property "comment" "" (id 6) (at 217.805 67.945 0))
    (property "PN" "SN75ALS160DW" (id 7) (at 217.805 67.945 0))
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "20")
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R") (at 55.88 82.55 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R16" (id 0) (at 59.055 81.915 0))
    (property "Value" "2k4" (id 1) (at 59.055 83.82 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.658 82.55 90))
    (property "Datasheet" "~" (id 3) (at 55.88 82.55 0))
    (property "comment" "" (id 4) (at 55.88 82.55 0))
    (property "supplier" "TME" (id 5) (at 55.88 82.55 0))
    (property "PN" "MMA02040C2402" (id 6) (at 55.88 82.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 94.615 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR017" (id 0) (at 94.615 86.36 0))
    (property "Value" "GND" (id 1) (at 94.615 84.5725 0))
    (property "Footprint" "" (id 2) (at 94.615 80.01 0))
    (property "Datasheet" "" (id 3) (at 94.615 80.01 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5V") (at 159.385 126.365 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR044" (id 0) (at 159.385 130.175 0))
    (property "Value" "+5V" (id 1) (at 159.385 122.7605 0))
    (property "Footprint" "" (id 2) (at 159.385 126.365 0))
    (property "Datasheet" "" (id 3) (at 159.385 126.365 0))
    (pin "1")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "+3V3") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR03") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR05") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR06") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR07") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR08") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR09") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR010") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR011") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR012") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR013") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR014") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR015") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR016") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR017") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR018") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR019") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR020") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR021") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR022") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR023") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR024") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR025") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR026") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR027") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR028") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR029") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR030") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR031") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR032") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR033") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR034") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR035") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR036") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR037") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR038") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR039") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR040") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR041") (unit 1) (value "+3V3") (footprint "")
    )
    (path
      (reference "#PWR042") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR043") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR044") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "#PWR045") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR046") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR047") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0101") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "100u") (footprint "Capacitor_Tantalum_SMD:CP_EIA-7132-28_AVX-C_Pad2.72x3.50mm_HandSolder")
    )
    (path
      (reference "C2") (unit 1) (value "1u") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C3") (unit 1) (value "1u") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C4") (unit 1) (value "22p") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C5") (unit 1) (value "22p") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C6") (unit 1) (value "1u") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C7") (unit 1) (value "1u") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C8") (unit 1) (value "1u") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C9") (unit 1) (value "1u") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C10") (unit 1) (value "470p") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C11") (unit 1) (value "22p") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "C12") (unit 1) (value "22p") (footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder")
    )
    (path
      (reference "D1") (unit 1) (value "BAV99") (footprint "Package_TO_SOT_SMD:SOT-23")
    )
    (path
      (reference "D2") (unit 1) (value "SM6T6V8A") (footprint "Diode_SMD:D_SMB")
    )
    (path
      (reference "H1") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad")
    )
    (path
      (reference "H2") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad")
    )
    (path
      (reference "H3") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad")
    )
    (path
      (reference "H4") (unit 1) (value "MountingHole") (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad")
    )
    (path
      (reference "J1") (unit 1) (value "Centronics 24, socket") (footprint "j_lib:CENTR_24P_F")
    )
    (path
      (reference "J2") (unit 1) (value "IDC_6pin") (footprint "Connector_IDC:IDC-Header_2x03_P2.54mm_Vertical")
    )
    (path
      (reference "J3") (unit 1) (value "Conn_01x02_Male") (footprint "Connector_Molex:Molex_KK-254_AE-6410-02A_1x02_P2.54mm_Vertical")
    )
    (path
      (reference "J4") (unit 1) (value "USB_B") (footprint "Connector_USB:USB_B_Lumberg_2411_02_Horizontal")
    )
    (path
      (reference "J5") (unit 1) (value "IDC_16") (footprint "Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical")
    )
    (path
      (reference "LOGO1") (unit 1) (value "PCB logo") (footprint "j_lib:logo_rpg7x9")
    )
    (path
      (reference "R1") (unit 1) (value "12k") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R2") (unit 1) (value "120R") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R3") (unit 1) (value "120R") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R4") (unit 1) (value "120R") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R5") (unit 1) (value "12k") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R6") (unit 1) (value "12k") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R7") (unit 1) (value "2k4") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R8") (unit 1) (value "3k9") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R9") (unit 1) (value "12k") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R10") (unit 1) (value "39k") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R11") (unit 1) (value "3k9") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R12") (unit 1) (value "12k") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R13") (unit 1) (value "2k4") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R14") (unit 1) (value "3k9") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R15") (unit 1) (value "2k4") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R16") (unit 1) (value "2k4") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R17") (unit 1) (value "3k9") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "R18") (unit 1) (value "3k9") (footprint "Resistor_SMD:R_MiniMELF_MMA-0204")
    )
    (path
      (reference "U1") (unit 1) (value "W5500_breakout") (footprint "j_lib:W5500_bo")
    )
    (path
      (reference "U2") (unit 1) (value "75ALS160") (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm")
    )
    (path
      (reference "U3") (unit 1) (value "AT90S4433") (footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm")
    )
    (path
      (reference "U4") (unit 1) (value "74HCT08") (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm")
    )
    (path
      (reference "U4") (unit 2) (value "74HCT08") (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm")
    )
    (path
      (reference "U4") (unit 3) (value "74HCT08") (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm")
    )
    (path
      (reference "U4") (unit 4) (value "74HCT08") (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm")
    )
    (path
      (reference "U4") (unit 5) (value "74HCT08") (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm")
    )
    (path
      (reference "U5") (unit 1) (value "75ALS161") (footprint "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm")
    )
    (path
      (reference "U6") (unit 1) (value "CH340G") (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm")
    )
    (path
      (reference "Y1") (unit 1) (value "7.3728MHz") (footprint "Crystal:Crystal_SMD_HC49-SD")
    )
    (path
      (reference "Y2") (unit 1) (value "12MHz") (footprint "Crystal:Crystal_SMD_HC49-SD")
    )
  )
)
