(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "74xGxx:74LVC1G14" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -2.54 3.81 0))
      (property "Value" "74LVC1G14" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "Single Gate NOT Schmitt LVC CMOS" (id 4) (at 0 0 0))
      (property "ki_description" "Single Schmitt NOT Gate, Low-Voltage CMOS" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT* SG-*" (id 6) (at 0 0 0))
      (symbol "74LVC1G14_0_1"
        (polyline
          (pts
            (xy -1.905 -0.635)
            (xy -1.27 -0.635)
            (xy -1.27 0.635)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.81 2.54)
            (xy -3.81 -2.54)
            (xy 2.54 0)
            (xy -3.81 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -0.635)
            (xy -1.905 -0.635)
            (xy -1.905 0.635)
            (xy -0.635 0.635)
          )
          (fill (type none))
        )
      )
      (symbol "74LVC1G14_1_1"
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "2")
        )
        (pin power_in line (at 0 -2.54 270) (length 0) hide
          (name "GND")
          (number "3")
        )
        (pin output inverted (at 6.35 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
        (pin power_in line (at 0 2.54 90) (length 0) hide
          (name "VCC")
          (number "5")
        )
      )
    )
    (symbol "74xx:74HC244" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 16.51 0))
      (property "Value" "74HC244" (id 1) (at -7.62 -16.51 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT244.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "HCMOS BUFFER 3State" (id 4) (at 0 0 0))
      (property "ki_description" "8-bit Buffer/Line Driver 3-state" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm* SSOP*4.4x6.5mm*P0.65mm*" (id 6) (at 0 0 0))
      (symbol "74HC244_1_0"
        (polyline
          (pts
            (xy 1.27 0)
            (xy -1.27 1.27)
            (xy -1.27 -1.27)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (pin input inverted (at -12.7 -10.16 0) (length 5.08)
          (name "1OE")
          (number "1")
        )
        (pin power_in line (at 0 -20.32 90) (length 5.08)
          (name "GND")
          (number "10")
        )
        (pin input line (at -12.7 -5.08 0) (length 5.08)
          (name "2A3")
          (number "11")
        )
        (pin tri_state line (at 12.7 5.08 180) (length 5.08)
          (name "1Y3")
          (number "12")
        )
        (pin input line (at -12.7 -2.54 0) (length 5.08)
          (name "2A2")
          (number "13")
        )
        (pin tri_state line (at 12.7 7.62 180) (length 5.08)
          (name "1Y2")
          (number "14")
        )
        (pin input line (at -12.7 0 0) (length 5.08)
          (name "2A1")
          (number "15")
        )
        (pin tri_state line (at 12.7 10.16 180) (length 5.08)
          (name "1Y1")
          (number "16")
        )
        (pin input line (at -12.7 2.54 0) (length 5.08)
          (name "2A0")
          (number "17")
        )
        (pin tri_state line (at 12.7 12.7 180) (length 5.08)
          (name "1Y0")
          (number "18")
        )
        (pin input inverted (at -12.7 -12.7 0) (length 5.08)
          (name "2OE")
          (number "19")
        )
        (pin input line (at -12.7 12.7 0) (length 5.08)
          (name "1A0")
          (number "2")
        )
        (pin power_in line (at 0 20.32 270) (length 5.08)
          (name "VCC")
          (number "20")
        )
        (pin tri_state line (at 12.7 2.54 180) (length 5.08)
          (name "2Y0")
          (number "3")
        )
        (pin input line (at -12.7 10.16 0) (length 5.08)
          (name "1A1")
          (number "4")
        )
        (pin tri_state line (at 12.7 0 180) (length 5.08)
          (name "2Y1")
          (number "5")
        )
        (pin input line (at -12.7 7.62 0) (length 5.08)
          (name "1A2")
          (number "6")
        )
        (pin tri_state line (at 12.7 -2.54 180) (length 5.08)
          (name "2Y2")
          (number "7")
        )
        (pin input line (at -12.7 5.08 0) (length 5.08)
          (name "1A3")
          (number "8")
        )
        (pin tri_state line (at 12.7 -5.08 180) (length 5.08)
          (name "2Y3")
          (number "9")
        )
      )
      (symbol "74HC244_1_1"
        (rectangle (start -7.62 15.24) (end 7.62 -15.24)
          (fill (type background))
        )
      )
    )
    (symbol "Connector:Conn_01x05_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 7.62 0))
      (property "Value" "Conn_01x05_Male" (id 1) (at 0 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x05, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x05_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 0.8636 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 5.08)
            (xy 0.8636 5.08)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -4.953) (end 0 -5.207)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (rectangle (start 0.8636 5.207) (end 0 4.953)
          (fill (type outline))
        )
        (pin passive line (at 5.08 5.08 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
      )
    )
    (symbol "Connector:Conn_01x06_Male" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 7.62 0))
      (property "Value" "Conn_01x06_Male" (id 1) (at 0 -10.16 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, single row, 01x06, script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_1x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_01x06_Male_1_1"
        (polyline
          (pts
            (xy 1.27 -7.62)
            (xy 0.8636 -7.62)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -5.08)
            (xy 0.8636 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -2.54)
            (xy 0.8636 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 0)
            (xy 0.8636 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 2.54)
            (xy 0.8636 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 5.08)
            (xy 0.8636 5.08)
          )
          (fill (type none))
        )
        (rectangle (start 0.8636 -7.493) (end 0 -7.747)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -4.953) (end 0 -5.207)
          (fill (type outline))
        )
        (rectangle (start 0.8636 -2.413) (end 0 -2.667)
          (fill (type outline))
        )
        (rectangle (start 0.8636 0.127) (end 0 -0.127)
          (fill (type outline))
        )
        (rectangle (start 0.8636 2.667) (end 0 2.413)
          (fill (type outline))
        )
        (rectangle (start 0.8636 5.207) (end 0 4.953)
          (fill (type outline))
        )
        (pin passive line (at 5.08 5.08 180) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 5.08 2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at 5.08 0 180) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 5.08 -2.54 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at 5.08 -5.08 180) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 5.08 -7.62 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
      )
    )
    (symbol "Connector:TestPoint" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 6.858 0))
      (property "Value" "TestPoint" (id 1) (at 0 5.08 0))
      (property "Footprint" "" (id 2) (at 5.08 0 0))
      (property "Datasheet" "~" (id 3) (at 5.08 0 0))
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0))
      (property "ki_description" "test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_0_1"
        (circle (center 0 3.302) (radius 0.762)
          (fill (type none))
        )
      )
      (symbol "TestPoint_1_1"
        (pin passive line (at 0 0 90) (length 2.54)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x05_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 7.62 0))
      (property "Value" "Conn_02x05_Odd_Even" (id 1) (at 1.27 -7.62 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x05_Odd_Even_1_1"
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 6.35) (end 3.81 -6.35)
          (fill (type background))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x07_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 10.16 0))
      (property "Value" "Conn_02x07_Odd_Even" (id 1) (at 1.27 -10.16 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x07, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x07_Odd_Even_1_1"
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (fill (type none))
        )
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 8.89) (end 3.81 -8.89)
          (fill (type background))
        )
        (rectangle (start 3.81 -7.493) (end 2.54 -7.747)
          (fill (type none))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (rectangle (start 3.81 7.747) (end 2.54 7.493)
          (fill (type none))
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_12")
          (number "12")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_13")
          (number "13")
        )
        (pin passive line (at 7.62 -7.62 180) (length 3.81)
          (name "Pin_14")
          (number "14")
        )
        (pin passive line (at 7.62 7.62 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x08_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 10.16 0))
      (property "Value" "Conn_02x08_Odd_Even" (id 1) (at 1.27 -12.7 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x08_Odd_Even_1_1"
        (rectangle (start -1.27 -10.033) (end 0 -10.287)
          (fill (type none))
        )
        (rectangle (start -1.27 -7.493) (end 0 -7.747)
          (fill (type none))
        )
        (rectangle (start -1.27 -4.953) (end 0 -5.207)
          (fill (type none))
        )
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 5.207) (end 0 4.953)
          (fill (type none))
        )
        (rectangle (start -1.27 7.747) (end 0 7.493)
          (fill (type none))
        )
        (rectangle (start -1.27 8.89) (end 3.81 -11.43)
          (fill (type background))
        )
        (rectangle (start 3.81 -10.033) (end 2.54 -10.287)
          (fill (type none))
        )
        (rectangle (start 3.81 -7.493) (end 2.54 -7.747)
          (fill (type none))
        )
        (rectangle (start 3.81 -4.953) (end 2.54 -5.207)
          (fill (type none))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (rectangle (start 3.81 5.207) (end 2.54 4.953)
          (fill (type none))
        )
        (rectangle (start 3.81 7.747) (end 2.54 7.493)
          (fill (type none))
        )
        (pin passive line (at -5.08 7.62 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_10")
          (number "10")
        )
        (pin passive line (at -5.08 -5.08 0) (length 3.81)
          (name "Pin_11")
          (number "11")
        )
        (pin passive line (at 7.62 -5.08 180) (length 3.81)
          (name "Pin_12")
          (number "12")
        )
        (pin passive line (at -5.08 -7.62 0) (length 3.81)
          (name "Pin_13")
          (number "13")
        )
        (pin passive line (at 7.62 -7.62 180) (length 3.81)
          (name "Pin_14")
          (number "14")
        )
        (pin passive line (at -5.08 -10.16 0) (length 3.81)
          (name "Pin_15")
          (number "15")
        )
        (pin passive line (at 7.62 -10.16 180) (length 3.81)
          (name "Pin_16")
          (number "16")
        )
        (pin passive line (at 7.62 7.62 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 5.08 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 5.08 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_7")
          (number "7")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_8")
          (number "8")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_9")
          (number "9")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Crystal" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Y" (id 0) (at 0 3.81 0))
      (property "Value" "Crystal" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "quartz ceramic resonator oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "Two pin crystal" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Crystal*" (id 6) (at 0 0 0))
      (symbol "Crystal_0_1"
        (rectangle (start -1.143 2.54) (end 1.143 -2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 0)
            (xy -1.905 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.905 -1.27)
            (xy 1.905 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.905 0)
          )
          (fill (type none))
        )
      )
      (symbol "Crystal_1_1"
        (pin passive line (at -3.81 0 0) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:Ferrite_Bead_Small" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "FB" (id 0) (at 1.905 1.27 0))
      (property "Value" "Ferrite_Bead_Small" (id 1) (at 1.905 -1.27 0))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "L ferrite bead inductor filter" (id 4) (at 0 0 0))
      (property "ki_description" "Ferrite bead, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Inductor_* L_* *Ferrite*" (id 6) (at 0 0 0))
      (symbol "Ferrite_Bead_Small_0_1"
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 -0.7874)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.889)
            (xy 0 1.2954)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.8288 0.2794)
            (xy -1.1176 1.4986)
            (xy 1.8288 -0.2032)
            (xy 1.1176 -1.4224)
            (xy -1.8288 0.2794)
          )
          (fill (type none))
        )
      )
      (symbol "Ferrite_Bead_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Pack04_Split" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RN" (id 0) (at 2.032 0 90))
      (property "Value" "R_Pack04_Split" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -2.032 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R network parallel topology isolated" (id 4) (at 0 0 0))
      (property "ki_description" "4 resistor network, parallel topology, split" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP* SOIC* R*Array*Concave* R*Array*Convex*" (id 6) (at 0 0 0))
      (symbol "R_Pack04_Split_0_1"
        (rectangle (start 1.016 2.54) (end -1.016 -2.54)
          (fill (type none))
        )
      )
      (symbol "R_Pack04_Split_1_1"
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "R1.1")
          (number "1")
        )
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "R1.2")
          (number "8")
        )
      )
      (symbol "R_Pack04_Split_2_1"
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "R2.1")
          (number "2")
        )
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "R2.2")
          (number "7")
        )
      )
      (symbol "R_Pack04_Split_3_1"
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "R3.1")
          (number "3")
        )
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "R3.2")
          (number "6")
        )
      )
      (symbol "R_Pack04_Split_4_1"
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "R4.1")
          (number "4")
        )
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "R4.2")
          (number "5")
        )
      )
    )
    (symbol "Device:Speaker" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "LS" (id 0) (at 1.27 5.715 0))
      (property "Value" "Speaker" (id 1) (at 1.27 3.81 0))
      (property "Footprint" "" (id 2) (at 0 -5.08 0))
      (property "Datasheet" "~" (id 3) (at -0.254 -1.27 0))
      (property "ki_keywords" "speaker sound" (id 4) (at 0 0 0))
      (property "ki_description" "Speaker" (id 5) (at 0 0 0))
      (symbol "Speaker_0_0"
        (rectangle (start -2.54 1.27) (end 1.016 -3.81)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.27)
            (xy 3.556 3.81)
            (xy 3.556 -6.35)
            (xy 1.016 -3.81)
          )
          (fill (type none))
        )
      )
      (symbol "Speaker_1_1"
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin input line (at -5.08 -2.54 0) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Memory_EEPROM:25LCxxx" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 6.35 0))
      (property "Value" "25LCxxx" (id 1) (at 2.54 -6.35 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21832H.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "EEPROM memory SPI serial" (id 4) (at 0 0 0))
      (property "ki_description" "SPI Serial EEPROM, DIP-8/SOIC-8/TSSOP-8" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm* TSSOP*4.4x3mm*P0.65mm*" (id 6) (at 0 0 0))
      (symbol "25LCxxx_1_1"
        (rectangle (start -7.62 5.08) (end 7.62 -5.08)
          (fill (type background))
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "~{CS}")
          (number "1")
        )
        (pin tri_state line (at 10.16 -2.54 180) (length 2.54)
          (name "MISO")
          (number "2")
        )
        (pin input line (at -10.16 2.54 0) (length 2.54)
          (name "~{WP}")
          (number "3")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin input line (at 10.16 0 180) (length 2.54)
          (name "MOSI")
          (number "5")
        )
        (pin input line (at 10.16 2.54 180) (length 2.54)
          (name "SCK")
          (number "6")
        )
        (pin input line (at -10.16 0 0) (length 2.54)
          (name "~{HOLD}")
          (number "7")
        )
        (pin power_in line (at 0 7.62 270) (length 2.54)
          (name "VCC")
          (number "8")
        )
      )
    )
    (symbol "Reference_Voltage:MCP1525-TT" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 1.27 8.255 0))
      (property "Value" "MCP1525-TT" (id 1) (at 1.27 6.35 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 0.635 -6.35 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21653b.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "Voltage Reference 2.5V" (id 4) (at 0 0 0))
      (property "ki_description" "2.5V Voltage Reference, SOT-23" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0))
      (symbol "MCP1525-TT_0_1"
        (rectangle (start -2.54 5.08) (end 7.62 -5.08)
          (fill (type background))
        )
      )
      (symbol "MCP1525-TT_1_1"
        (pin power_in line (at 0 7.62 270) (length 2.54)
          (name "Vin")
          (number "1")
        )
        (pin power_out line (at 10.16 0 180) (length 2.54)
          (name "Vout")
          (number "2")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "Vss")
          (number "3")
        )
      )
    )
    (symbol "Transistor_BJT:BC847" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "Q" (id 0) (at 5.08 1.905 0))
      (property "Value" "BC847" (id 1) (at 5.08 0 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 5.08 -1.905 0))
      (property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657" (id 3) (at 0 0 0))
      (property "ki_keywords" "NPN Small Signal Transistor" (id 4) (at 0 0 0))
      (property "ki_description" "0.1A Ic, 45V Vce, NPN Transistor, SOT-23" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0))
      (symbol "BC847_0_1"
        (polyline
          (pts
            (xy 0.635 0.635)
            (xy 2.54 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 -0.635)
            (xy 2.54 -2.54)
            (xy 2.54 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0.635 1.905)
            (xy 0.635 -1.905)
            (xy 0.635 -1.905)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.778)
            (xy 1.778 -1.27)
            (xy 2.286 -2.286)
            (xy 1.27 -1.778)
            (xy 1.27 -1.778)
          )
          (fill (type outline))
        )
        (circle (center 1.27 0) (radius 2.8194)
          (fill (type none))
        )
      )
      (symbol "BC847_1_1"
        (pin input line (at -5.08 0 0) (length 5.715)
          (name "B")
          (number "1")
        )
        (pin passive line (at 2.54 -5.08 90) (length 2.54)
          (name "E")
          (number "2")
        )
        (pin passive line (at 2.54 5.08 270) (length 2.54)
          (name "C")
          (number "3")
        )
      )
    )
    (symbol "jlib_1:STM32F373VB" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -2.54 -74.295 0))
      (property "Value" "jlib_1_STM32F373VB" (id 1) (at 5.08 67.31 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "STM32F373VB_0_0"
        (rectangle (start -15.24 66.04) (end 15.24 -73.025)
          (fill (type none))
        )
      )
      (symbol "STM32F373VB_1_1"
        (pin input line (at 20.32 16.51 180) (length 5.08)
          (name "PE2")
          (number "1")
        )
        (pin input line (at -20.32 -67.31 0) (length 5.08)
          (name "PF9")
          (number "10")
        )
        (pin input line (at 20.32 -35.56 180) (length 5.08)
          (name "VDD")
          (number "100")
        )
        (pin input line (at -20.32 -69.85 0) (length 5.08)
          (name "PF10")
          (number "11")
        )
        (pin input line (at -20.32 -54.61 0) (length 5.08)
          (name "PF0/OSC_IN")
          (number "12")
        )
        (pin input line (at -20.32 -57.15 0) (length 5.08)
          (name "PF1/OSC_OUT")
          (number "13")
        )
        (pin input line (at 20.32 -25.4 180) (length 5.08)
          (name "NRST")
          (number "14")
        )
        (pin input line (at -20.32 -12.7 0) (length 5.08)
          (name "PC0")
          (number "15")
        )
        (pin input line (at -20.32 -15.24 0) (length 5.08)
          (name "PC1")
          (number "16")
        )
        (pin input line (at -20.32 -17.78 0) (length 5.08)
          (name "PC2")
          (number "17")
        )
        (pin input line (at -20.32 -20.32 0) (length 5.08)
          (name "PC3")
          (number "18")
        )
        (pin input line (at -20.32 -59.69 0) (length 5.08)
          (name "PF2")
          (number "19")
        )
        (pin input line (at 20.32 13.97 180) (length 5.08)
          (name "PE3")
          (number "2")
        )
        (pin input line (at 20.32 -64.77 180) (length 5.08)
          (name "VSSA/VREF-")
          (number "20")
        )
        (pin input line (at 20.32 -43.18 180) (length 5.08)
          (name "VDDA")
          (number "21")
        )
        (pin input line (at 20.32 -54.61 180) (length 5.08)
          (name "VREF+")
          (number "22")
        )
        (pin input line (at -20.32 63.5 0) (length 5.08)
          (name "PA0")
          (number "23")
        )
        (pin input line (at -20.32 60.96 0) (length 5.08)
          (name "PA1")
          (number "24")
        )
        (pin input line (at -20.32 58.42 0) (length 5.08)
          (name "PA2")
          (number "25")
        )
        (pin input line (at -20.32 55.88 0) (length 5.08)
          (name "PA3")
          (number "26")
        )
        (pin input line (at -20.32 -62.23 0) (length 5.08)
          (name "PF4")
          (number "27")
        )
        (pin input line (at 20.32 -38.1 180) (length 5.08)
          (name "VDD")
          (number "28")
        )
        (pin input line (at -20.32 53.34 0) (length 5.08)
          (name "PA4")
          (number "29")
        )
        (pin input line (at 20.32 11.43 180) (length 5.08)
          (name "PE4")
          (number "3")
        )
        (pin input line (at -20.32 50.8 0) (length 5.08)
          (name "PA5")
          (number "30")
        )
        (pin input line (at -20.32 48.26 0) (length 5.08)
          (name "PA6")
          (number "31")
        )
        (pin input line (at -20.32 45.72 0) (length 5.08)
          (name "PA7")
          (number "32")
        )
        (pin input line (at -20.32 -22.86 0) (length 5.08)
          (name "PC4")
          (number "33")
        )
        (pin input line (at -20.32 -25.4 0) (length 5.08)
          (name "PC5")
          (number "34")
        )
        (pin input line (at -20.32 21.59 0) (length 5.08)
          (name "PB0")
          (number "35")
        )
        (pin input line (at -20.32 19.05 0) (length 5.08)
          (name "PB1")
          (number "36")
        )
        (pin input line (at -20.32 16.51 0) (length 5.08)
          (name "PB2")
          (number "37")
        )
        (pin input line (at 20.32 3.81 180) (length 5.08)
          (name "PE7")
          (number "38")
        )
        (pin input line (at 20.32 1.27 180) (length 5.08)
          (name "PE8")
          (number "39")
        )
        (pin input line (at 20.32 8.89 180) (length 5.08)
          (name "PE5")
          (number "4")
        )
        (pin input line (at 20.32 -1.27 180) (length 5.08)
          (name "PE9")
          (number "40")
        )
        (pin input line (at 20.32 -3.81 180) (length 5.08)
          (name "PE10")
          (number "41")
        )
        (pin input line (at 20.32 -6.35 180) (length 5.08)
          (name "PE11")
          (number "42")
        )
        (pin input line (at 20.32 -8.89 180) (length 5.08)
          (name "PE12")
          (number "43")
        )
        (pin input line (at 20.32 -11.43 180) (length 5.08)
          (name "PE13")
          (number "44")
        )
        (pin input line (at 20.32 -13.97 180) (length 5.08)
          (name "PE14")
          (number "45")
        )
        (pin input line (at 20.32 -16.51 180) (length 5.08)
          (name "PE15")
          (number "46")
        )
        (pin input line (at -20.32 -3.81 0) (length 5.08)
          (name "PB10")
          (number "47")
        )
        (pin input line (at 20.32 -62.23 180) (length 5.08)
          (name "VREFSD-")
          (number "48")
        )
        (pin input line (at 20.32 -59.69 180) (length 5.08)
          (name "VSSSD")
          (number "49")
        )
        (pin input line (at 20.32 6.35 180) (length 5.08)
          (name "PE6")
          (number "5")
        )
        (pin input line (at 20.32 -48.26 180) (length 5.08)
          (name "VDDSD12")
          (number "50")
        )
        (pin input line (at 20.32 -45.72 180) (length 5.08)
          (name "VDDSD3")
          (number "51")
        )
        (pin input line (at 20.32 -52.07 180) (length 5.08)
          (name "VREFSD+")
          (number "52")
        )
        (pin input line (at -20.32 -6.35 0) (length 5.08)
          (name "PB14")
          (number "53")
        )
        (pin input line (at -20.32 -8.89 0) (length 5.08)
          (name "PB15")
          (number "54")
        )
        (pin input line (at 20.32 43.18 180) (length 5.08)
          (name "PD8")
          (number "55")
        )
        (pin input line (at 20.32 40.64 180) (length 5.08)
          (name "PD9")
          (number "56")
        )
        (pin input line (at 20.32 38.1 180) (length 5.08)
          (name "PD10")
          (number "57")
        )
        (pin input line (at 20.32 35.56 180) (length 5.08)
          (name "PD11")
          (number "58")
        )
        (pin input line (at 20.32 33.02 180) (length 5.08)
          (name "PD12")
          (number "59")
        )
        (pin input line (at 20.32 -30.48 180) (length 5.08)
          (name "VBAT")
          (number "6")
        )
        (pin input line (at 20.32 30.48 180) (length 5.08)
          (name "PD13")
          (number "60")
        )
        (pin input line (at 20.32 27.94 180) (length 5.08)
          (name "PD14")
          (number "61")
        )
        (pin input line (at 20.32 25.4 180) (length 5.08)
          (name "PD15")
          (number "62")
        )
        (pin input line (at -20.32 -27.94 0) (length 5.08)
          (name "PC6")
          (number "63")
        )
        (pin input line (at -20.32 -30.48 0) (length 5.08)
          (name "PC7")
          (number "64")
        )
        (pin input line (at -20.32 -33.02 0) (length 5.08)
          (name "PC8")
          (number "65")
        )
        (pin input line (at -20.32 -35.56 0) (length 5.08)
          (name "PC9")
          (number "66")
        )
        (pin input line (at -20.32 43.18 0) (length 5.08)
          (name "PA8")
          (number "67")
        )
        (pin input line (at -20.32 40.64 0) (length 5.08)
          (name "PA9")
          (number "68")
        )
        (pin input line (at -20.32 38.1 0) (length 5.08)
          (name "PA10")
          (number "69")
        )
        (pin input line (at -20.32 -45.72 0) (length 5.08)
          (name "PC13")
          (number "7")
        )
        (pin input line (at -20.32 35.56 0) (length 5.08)
          (name "PA11")
          (number "70")
        )
        (pin input line (at -20.32 33.02 0) (length 5.08)
          (name "PA12")
          (number "71")
        )
        (pin input line (at -20.32 30.48 0) (length 5.08)
          (name "PA13")
          (number "72")
        )
        (pin input line (at -20.32 -64.77 0) (length 5.08)
          (name "PF6")
          (number "73")
        )
        (pin input line (at 20.32 -69.85 180) (length 5.08)
          (name "VSS")
          (number "74")
        )
        (pin input line (at 20.32 -33.02 180) (length 5.08)
          (name "VDD")
          (number "75")
        )
        (pin input line (at -20.32 27.94 0) (length 5.08)
          (name "PA14")
          (number "76")
        )
        (pin input line (at -20.32 25.4 0) (length 5.08)
          (name "PA15")
          (number "77")
        )
        (pin input line (at -20.32 -38.1 0) (length 5.08)
          (name "PC10")
          (number "78")
        )
        (pin input line (at -20.32 -40.64 0) (length 5.08)
          (name "PC11")
          (number "79")
        )
        (pin input line (at -20.32 -48.26 0) (length 5.08)
          (name "PC14/OSC32_IN")
          (number "8")
        )
        (pin input line (at -20.32 -43.18 0) (length 5.08)
          (name "PC12")
          (number "80")
        )
        (pin input line (at 20.32 63.5 180) (length 5.08)
          (name "PD0")
          (number "81")
        )
        (pin input line (at 20.32 60.96 180) (length 5.08)
          (name "PD1")
          (number "82")
        )
        (pin input line (at 20.32 58.42 180) (length 5.08)
          (name "PD2")
          (number "83")
        )
        (pin input line (at 20.32 55.88 180) (length 5.08)
          (name "PD3")
          (number "84")
        )
        (pin input line (at 20.32 53.34 180) (length 5.08)
          (name "PD4")
          (number "85")
        )
        (pin input line (at 20.32 50.8 180) (length 5.08)
          (name "PD5")
          (number "86")
        )
        (pin input line (at 20.32 48.26 180) (length 5.08)
          (name "PD6")
          (number "87")
        )
        (pin input line (at 20.32 45.72 180) (length 5.08)
          (name "PD7")
          (number "88")
        )
        (pin input line (at -20.32 13.97 0) (length 5.08)
          (name "PB3")
          (number "89")
        )
        (pin input line (at -20.32 -50.8 0) (length 5.08)
          (name "PC15/OSC32_OUT")
          (number "9")
        )
        (pin input line (at -20.32 11.43 0) (length 5.08)
          (name "PB4")
          (number "90")
        )
        (pin input line (at -20.32 8.89 0) (length 5.08)
          (name "PB5")
          (number "91")
        )
        (pin input line (at -20.32 6.35 0) (length 5.08)
          (name "PB6")
          (number "92")
        )
        (pin input line (at -20.32 3.81 0) (length 5.08)
          (name "PB7")
          (number "93")
        )
        (pin input line (at 20.32 -22.86 180) (length 5.08)
          (name "BOOT0")
          (number "94")
        )
        (pin input line (at -20.32 1.27 0) (length 5.08)
          (name "PB8")
          (number "95")
        )
        (pin input line (at -20.32 -1.27 0) (length 5.08)
          (name "PB9")
          (number "96")
        )
        (pin input line (at 20.32 21.59 180) (length 5.08)
          (name "PE0")
          (number "97")
        )
        (pin input line (at 20.32 19.05 180) (length 5.08)
          (name "PE1")
          (number "98")
        )
        (pin input line (at 20.32 -67.31 180) (length 5.08)
          (name "VSS")
          (number "99")
        )
      )
    )
    (symbol "power:+3.3V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3.3V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3.3V\"" (id 5) (at 0 0 0))
      (symbol "+3.3V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3.3V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3V3")
          (number "1")
        )
      )
    )
    (symbol "power:+3.3VADC" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 3.81 -1.27 0))
      (property "Value" "+3.3VADC" (id 1) (at 0 2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3.3VADC\"" (id 5) (at 0 0 0))
      (symbol "+3.3VADC_0_0"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3.3VADC")
          (number "1")
        )
      )
      (symbol "+3.3VADC_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 73.025 165.1) (diameter 0) (color 0 0 0 0))
  (junction (at 158.115 151.765) (diameter 0) (color 0 0 0 0))
  (junction (at 40.64 40.64) (diameter 0) (color 0 0 0 0))
  (junction (at 59.055 76.2) (diameter 0) (color 0 0 0 0))
  (junction (at 84.455 180.975) (diameter 0) (color 0 0 0 0))
  (junction (at 61.595 40.64) (diameter 0) (color 0 0 0 0))
  (junction (at 158.115 114.935) (diameter 0) (color 0 0 0 0))
  (junction (at 40.64 157.48) (diameter 0) (color 0 0 0 0))
  (junction (at 158.115 149.225) (diameter 0) (color 0 0 0 0))
  (junction (at 223.52 135.255) (diameter 0) (color 0 0 0 0))
  (junction (at 205.105 67.945) (diameter 0) (color 0 0 0 0))
  (junction (at 245.11 109.22) (diameter 0) (color 0 0 0 0))
  (junction (at 28.575 157.48) (diameter 0) (color 0 0 0 0))
  (junction (at 158.115 117.475) (diameter 0) (color 0 0 0 0))
  (junction (at 158.115 127.635) (diameter 0) (color 0 0 0 0))
  (junction (at 74.295 115.57) (diameter 0) (color 0 0 0 0))
  (junction (at 84.455 186.055) (diameter 0) (color 0 0 0 0))
  (junction (at 158.115 144.145) (diameter 0) (color 0 0 0 0))
  (junction (at 158.115 146.685) (diameter 0) (color 0 0 0 0))
  (junction (at 257.175 81.28) (diameter 0) (color 0 0 0 0))
  (junction (at 192.405 60.325) (diameter 0) (color 0 0 0 0))
  (junction (at 41.275 120.015) (diameter 0) (color 0 0 0 0))
  (junction (at 229.87 135.255) (diameter 0) (color 0 0 0 0))
  (junction (at 257.175 83.82) (diameter 0) (color 0 0 0 0))
  (junction (at 206.375 135.255) (diameter 0) (color 0 0 0 0))
  (junction (at 194.945 135.255) (diameter 0) (color 0 0 0 0))
  (junction (at 206.375 149.225) (diameter 0) (color 0 0 0 0))
  (junction (at 59.055 71.12) (diameter 0) (color 0 0 0 0))
  (junction (at 205.105 27.305) (diameter 0) (color 0 0 0 0))
  (junction (at 233.045 114.3) (diameter 0) (color 0 0 0 0))
  (junction (at 192.405 57.785) (diameter 0) (color 0 0 0 0))
  (junction (at 257.175 86.36) (diameter 0) (color 0 0 0 0))
  (junction (at 217.17 135.255) (diameter 0) (color 0 0 0 0))
  (polyline (pts (xy 62.23 104.775) (xy 62.23 124.46)))
  (wire (pts (xy 209.55 88.9) (xy 213.36 88.9)))
  (wire (pts (xy 41.275 125.095) (xy 41.275 127)))
  (wire (pts (xy 59.055 73.66) (xy 55.245 73.66)))
  (polyline (pts (xy 186.69 100.33) (xy 186.69 161.925)))
  (polyline (pts (xy 186.69 74.93) (xy 251.46 74.93)))
  (wire (pts (xy 233.045 116.84) (xy 233.045 114.3)))
  (wire (pts (xy 198.12 149.225) (xy 194.945 149.225)))
  (wire (pts (xy 257.175 86.36) (xy 257.175 88.9)))
  (wire (pts (xy 40.64 38.1) (xy 40.64 40.64)))
  (wire (pts (xy 161.29 104.775) (xy 156.845 104.775)))
  (wire (pts (xy 156.845 141.605) (xy 158.115 141.605)))
  (wire (pts (xy 85.725 186.055) (xy 84.455 186.055)))
  (wire (pts (xy 229.235 86.36) (xy 226.06 86.36)))
  (polyline (pts (xy 83.185 124.46) (xy 83.185 104.775)))
  (wire (pts (xy 228.6 34.29) (xy 228.6 38.1)))
  (polyline (pts (xy 279.4 97.79) (xy 279.4 74.93)))
  (wire (pts (xy 233.045 109.22) (xy 233.045 114.3)))
  (polyline (pts (xy 59.69 140.97) (xy 16.51 140.97)))
  (wire (pts (xy 217.17 135.255) (xy 223.52 135.255)))
  (wire (pts (xy 156.845 151.765) (xy 158.115 151.765)))
  (wire (pts (xy 156.845 112.395) (xy 158.115 112.395)))
  (polyline (pts (xy 102.87 159.385) (xy 102.87 189.23)))
  (wire (pts (xy 84.455 175.895) (xy 84.455 180.975)))
  (wire (pts (xy 158.115 149.225) (xy 158.115 151.765)))
  (wire (pts (xy 271.78 34.29) (xy 271.78 38.735)))
  (polyline (pts (xy 16.51 142.875) (xy 59.69 142.875)))
  (wire (pts (xy 192.405 52.705) (xy 192.405 57.785)))
  (wire (pts (xy 36.195 183.515) (xy 43.815 183.515)))
  (wire (pts (xy 158.115 112.395) (xy 158.115 114.935)))
  (wire (pts (xy 85.725 183.515) (xy 66.04 183.515)))
  (wire (pts (xy 55.245 66.04) (xy 62.23 66.04)))
  (polyline (pts (xy 102.87 189.23) (xy 160.655 189.23)))
  (wire (pts (xy 158.115 146.685) (xy 158.115 149.225)))
  (polyline (pts (xy 16.51 15.875) (xy 83.185 15.875)))
  (wire (pts (xy 156.845 144.145) (xy 158.115 144.145)))
  (wire (pts (xy 129.54 174.625) (xy 121.92 174.625)))
  (wire (pts (xy 237.49 135.255) (xy 229.87 135.255)))
  (polyline (pts (xy 98.425 189.23) (xy 62.23 189.23)))
  (wire (pts (xy 245.11 109.22) (xy 233.045 109.22)))
  (wire (pts (xy 257.175 83.82) (xy 257.175 86.36)))
  (wire (pts (xy 73.025 165.1) (xy 80.01 165.1)))
  (wire (pts (xy 55.245 71.12) (xy 59.055 71.12)))
  (wire (pts (xy 192.405 57.785) (xy 192.405 60.325)))
  (wire (pts (xy 156.845 146.685) (xy 158.115 146.685)))
  (wire (pts (xy 156.845 130.175) (xy 158.115 130.175)))
  (wire (pts (xy 61.595 40.64) (xy 65.405 40.64)))
  (wire (pts (xy 156.845 125.095) (xy 158.115 125.095)))
  (wire (pts (xy 53.34 40.64) (xy 61.595 40.64)))
  (wire (pts (xy 85.725 175.895) (xy 84.455 175.895)))
  (polyline (pts (xy 59.69 189.23) (xy 16.51 189.23)))
  (wire (pts (xy 158.115 125.095) (xy 158.115 127.635)))
  (polyline (pts (xy 16.51 83.82) (xy 16.51 102.87)))
  (polyline (pts (xy 62.23 159.385) (xy 100.33 159.385)))
  (wire (pts (xy 158.115 144.145) (xy 158.115 146.685)))
  (wire (pts (xy 205.105 67.945) (xy 192.405 67.945)))
  (wire (pts (xy 156.845 114.935) (xy 158.115 114.935)))
  (wire (pts (xy 85.725 173.355) (xy 80.01 173.355)))
  (polyline (pts (xy 62.23 124.46) (xy 83.185 124.46)))
  (polyline (pts (xy 16.51 44.45) (xy 16.51 15.875)))
  (polyline (pts (xy 16.51 104.775) (xy 59.69 104.775)))
  (polyline (pts (xy 102.87 159.385) (xy 160.655 159.385)))
  (wire (pts (xy 59.055 71.12) (xy 59.055 68.58)))
  (wire (pts (xy 264.795 36.83) (xy 264.795 38.735)))
  (wire (pts (xy 59.055 76.2) (xy 55.245 76.2)))
  (polyline (pts (xy 83.185 46.355) (xy 16.51 46.355)))
  (wire (pts (xy 194.945 135.255) (xy 206.375 135.255)))
  (wire (pts (xy 235.585 36.83) (xy 235.585 38.1)))
  (polyline (pts (xy 279.4 74.93) (xy 251.46 74.93)))
  (wire (pts (xy 28.575 157.48) (xy 33.02 157.48)))
  (polyline (pts (xy 279.4 72.39) (xy 279.4 16.51)))
  (polyline (pts (xy 59.69 104.775) (xy 59.69 140.97)))
  (polyline (pts (xy 186.69 72.39) (xy 279.4 72.39)))
  (wire (pts (xy 25.4 157.48) (xy 28.575 157.48)))
  (wire (pts (xy 229.235 83.82) (xy 226.06 83.82)))
  (wire (pts (xy 158.115 120.015) (xy 158.115 117.475)))
  (wire (pts (xy 41.275 120.015) (xy 41.275 122.555)))
  (wire (pts (xy 158.115 114.935) (xy 158.115 117.475)))
  (polyline (pts (xy 83.185 102.87) (xy 83.185 83.185)))
  (polyline (pts (xy 62.23 104.775) (xy 83.185 104.775)))
  (wire (pts (xy 255.905 34.29) (xy 271.78 34.29)))
  (wire (pts (xy 160.655 127.635) (xy 158.115 127.635)))
  (wire (pts (xy 85.725 178.435) (xy 73.025 178.435)))
  (polyline (pts (xy 83.185 44.45) (xy 16.51 44.45)))
  (wire (pts (xy 255.905 36.83) (xy 264.795 36.83)))
  (polyline (pts (xy 186.69 100.33) (xy 278.765 100.33)))
  (wire (pts (xy 243.205 34.29) (xy 228.6 34.29)))
  (wire (pts (xy 229.235 81.28) (xy 226.06 81.28)))
  (polyline (pts (xy 83.185 83.185) (xy 16.51 83.185)))
  (polyline (pts (xy 278.765 161.925) (xy 186.69 161.925)))
  (wire (pts (xy 194.945 149.225) (xy 194.945 135.255)))
  (polyline (pts (xy 278.765 100.33) (xy 278.765 161.925)))
  (polyline (pts (xy 186.69 16.51) (xy 279.4 16.51)))
  (polyline (pts (xy 186.69 74.93) (xy 186.69 97.79)))
  (polyline (pts (xy 160.655 189.23) (xy 160.655 159.385)))
  (polyline (pts (xy 16.51 83.185) (xy 16.51 83.82)))
  (wire (pts (xy 158.115 114.935) (xy 161.29 114.935)))
  (wire (pts (xy 223.52 135.255) (xy 229.87 135.255)))
  (wire (pts (xy 80.01 173.355) (xy 80.01 172.72)))
  (polyline (pts (xy 186.69 16.51) (xy 186.69 72.39)))
  (wire (pts (xy 206.375 135.255) (xy 217.17 135.255)))
  (polyline (pts (xy 83.185 81.28) (xy 83.185 46.355)))
  (wire (pts (xy 257.175 81.28) (xy 259.715 81.28)))
  (wire (pts (xy 55.245 68.58) (xy 59.055 68.58)))
  (wire (pts (xy 229.235 88.9) (xy 226.06 88.9)))
  (wire (pts (xy 158.115 141.605) (xy 158.115 144.145)))
  (polyline (pts (xy 83.185 15.875) (xy 83.185 44.45)))
  (wire (pts (xy 156.845 120.015) (xy 158.115 120.015)))
  (polyline (pts (xy 16.51 50.8) (xy 16.51 81.28)))
  (wire (pts (xy 59.055 71.12) (xy 63.5 71.12)))
  (wire (pts (xy 234.95 119.38) (xy 229.616 119.38)))
  (wire (pts (xy 234.95 116.84) (xy 233.045 116.84)))
  (wire (pts (xy 156.845 117.475) (xy 158.115 117.475)))
  (wire (pts (xy 257.175 86.36) (xy 259.715 86.36)))
  (wire (pts (xy 265.43 147.32) (xy 267.335 147.32)))
  (polyline (pts (xy 16.51 46.355) (xy 16.51 50.8)))
  (wire (pts (xy 221.996 119.38) (xy 221.488 119.38)))
  (wire (pts (xy 74.295 111.76) (xy 74.295 115.57)))
  (polyline (pts (xy 98.425 189.23) (xy 100.33 189.23)))
  (wire (pts (xy 158.115 130.175) (xy 158.115 127.635)))
  (polyline (pts (xy 16.51 140.97) (xy 16.51 104.775)))
  (wire (pts (xy 192.405 67.945) (xy 192.405 60.325)))
  (wire (pts (xy 156.845 149.225) (xy 158.115 149.225)))
  (wire (pts (xy 61.595 40.64) (xy 61.595 38.1)))
  (wire (pts (xy 158.115 127.635) (xy 156.845 127.635)))
  (wire (pts (xy 85.725 180.975) (xy 84.455 180.975)))
  (wire (pts (xy 243.205 36.83) (xy 235.585 36.83)))
  (wire (pts (xy 168.91 104.775) (xy 168.91 106.045)))
  (wire (pts (xy 84.455 180.975) (xy 84.455 186.055)))
  (polyline (pts (xy 16.51 102.87) (xy 83.185 102.87)))
  (wire (pts (xy 209.55 86.36) (xy 213.36 86.36)))
  (wire (pts (xy 257.175 83.82) (xy 257.175 81.28)))
  (polyline (pts (xy 100.33 159.385) (xy 100.33 189.23)))
  (wire (pts (xy 59.055 73.66) (xy 59.055 76.2)))
  (wire (pts (xy 73.025 178.435) (xy 73.025 172.72)))
  (wire (pts (xy 259.715 83.82) (xy 257.175 83.82)))
  (polyline (pts (xy 62.23 189.23) (xy 62.23 159.385)))
  (wire (pts (xy 203.2 149.225) (xy 206.375 149.225)))
  (wire (pts (xy 206.375 149.225) (xy 214.63 149.225)))
  (polyline (pts (xy 186.69 97.79) (xy 279.4 97.79)))
  (wire (pts (xy 209.55 81.28) (xy 213.36 81.28)))
  (wire (pts (xy 257.175 88.9) (xy 259.715 88.9)))
  (polyline (pts (xy 16.51 81.28) (xy 83.185 81.28)))
  (polyline (pts (xy 59.69 142.875) (xy 59.69 189.23)))
  (wire (pts (xy 209.55 83.82) (xy 213.36 83.82)))
  (wire (pts (xy 66.04 165.1) (xy 73.025 165.1)))
  (wire (pts (xy 234.95 114.3) (xy 233.045 114.3)))
  (wire (pts (xy 66.04 183.515) (xy 66.04 172.72)))
  (polyline (pts (xy 16.51 142.875) (xy 16.51 189.23)))
  (wire (pts (xy 53.34 38.1) (xy 61.595 38.1)))
  (text "Beeper" (at 18.415 108.585 0))
  (text "Expansion connector" (at 17.78 19.05 0))
  (text "Temperature probes connector" (at 62.865 161.925 0))
  (text "SWDIO connector, crystal" (at 103.505 162.56 0))
  (text "Communication connector (to Lisa PCB)" (at 17.145 49.53 0))
  (text "Ground test points" (at 62.865 107.315 0))
  (text "ADC connector\n(to Homer PCB)" (at 18.415 88.9 0))
  (text "Keyboard connector (to Meggie PCB)" (at 187.96 78.105 0))
  (text "spi1/3" (at 102.235 70.485 0))
  (text "usart3" (at 102.235 81.28 0))
  (text "Display IO buffer" (at 187.96 19.685 0))
  (text "usart1" (at 102.235 76.2 0))
  (text "EEPROM, indication, local reference" (at 187.96 103.505 0))
  (text "Misc stuff" (at 17.145 146.05 0))
  (label "DO6" (at 192.405 45.085 180))
  (label "EX4" (at 60.96 25.4 0))
  (label "EE_CS" (at 234.95 119.38 180))
  (label "NRST" (at 129.54 174.625 180))
  (label "EX1" (at 156.845 28.575 0))
  (label "K4" (at 236.855 86.36 0))
  (label "S_MUTE" (at 43.815 176.53 0))
  (label "EIO2" (at 62.865 58.42 0))
  (label "DO8" (at 156.845 46.355 0))
  (label "EU2TX" (at 116.205 80.645 180))
  (label "EE_CS" (at 116.205 90.805 180))
  (label "KC8" (at 267.335 88.9 0))
  (label "K6" (at 116.205 38.735 180))
  (label "DOT2" (at 217.805 37.465 0))
  (label "AB_CTRL" (at 59.055 94.615 180))
  (label "K2" (at 236.855 88.9 0))
  (label "EE_MISO" (at 156.845 43.815 0))
  (label "K8" (at 236.855 81.28 0))
  (label "BEEP" (at 116.205 99.695 180))
  (label "K5" (at 201.93 83.82 180))
  (label "DOT6" (at 255.905 31.75 0))
  (label "K3" (at 116.205 46.355 180))
  (label "EIO1" (at 34.925 58.42 180))
  (label "DO5" (at 192.405 42.545 180))
  (label "K3" (at 201.93 86.36 180))
  (label "KC6" (at 226.06 83.82 0))
  (label "EX10" (at 60.96 33.02 0))
  (label "AN1" (at 81.915 173.355 0))
  (label "X1" (at 116.205 136.525 180))
  (label "VREF_M" (at 73.025 165.1 0))
  (label "S_MUTE" (at 116.205 151.765 180))
  (label "EX3" (at 156.845 33.655 0))
  (label "LED1" (at 197.358 107.188 0))
  (label "EX6" (at 116.205 70.485 180))
  (label "EX11" (at 33.02 35.56 180))
  (label "EX2" (at 60.96 22.86 0))
  (label "DOT3" (at 255.905 39.37 0))
  (label "DO1" (at 192.405 34.925 180))
  (label "K1" (at 116.205 146.685 180))
  (label "EX5" (at 116.205 67.945 180))
  (label "EX8" (at 60.96 30.48 0))
  (label "E_RST" (at 34.925 66.04 180))
  (label "SWDIO" (at 129.54 172.085 180))
  (label "DO8" (at 192.405 50.165 180))
  (label "EX6" (at 60.96 27.94 0))
  (label "AN1" (at 116.205 62.865 180))
  (label "KC5" (at 210.185 83.82 0))
  (label "K2" (at 116.205 48.895 180))
  (label "X2" (at 116.205 139.065 180))
  (label "AN2" (at 116.205 60.325 180))
  (label "ZCD" (at 116.205 56.515 180))
  (label "DOT1" (at 255.905 41.91 0))
  (label "K7" (at 201.93 81.28 180))
  (label "KC6" (at 267.335 83.82 0))
  (label "DOT6" (at 217.805 45.085 0))
  (label "AN3" (at 116.205 107.315 180))
  (label "AN3" (at 77.47 183.515 0))
  (label "AN2" (at 77.47 178.435 0))
  (label "E_MISO" (at 116.205 122.555 180))
  (label "EX9" (at 33.02 33.02 180))
  (label "VREF_M" (at 267.335 147.32 0))
  (label "K4" (at 116.205 43.815 180))
  (label "E_CS" (at 34.925 68.58 180))
  (label "EU2TX" (at 62.865 60.96 0))
  (label "AB_RX" (at 59.055 86.995 180))
  (label "DO3" (at 156.845 56.515 0))
  (label "EIO2" (at 156.845 23.495 0))
  (label "EX10" (at 156.845 65.405 0))
  (label "E_MISO" (at 34.925 71.12 180))
  (label "DOT7" (at 217.805 47.625 0))
  (label "DOT7" (at 243.205 29.21 180))
  (label "DOT5" (at 217.805 42.545 0))
  (label "DO5" (at 156.845 53.975 0))
  (label "EU1RX" (at 116.205 78.105 180))
  (label "DOT8" (at 217.805 50.165 0))
  (label "EX11" (at 156.845 67.945 0))
  (label "LED1" (at 156.845 73.025 0))
  (label "ZCD" (at 54.61 157.48 0))
  (label "EE_MOSI" (at 156.845 41.275 0))
  (label "KC7" (at 267.335 86.36 0))
  (label "E_MOSI" (at 116.205 125.095 180))
  (label "X1" (at 145.415 173.99 180))
  (label "E_SCK" (at 34.925 76.2 180))
  (label "BEEP" (at 26.035 132.08 180))
  (label "K7" (at 116.205 117.475 180))
  (label "LED2" (at 207.518 107.188 0))
  (label "K8" (at 116.205 114.935 180))
  (label "EX7" (at 33.02 30.48 180))
  (label "LED2" (at 156.845 75.565 0))
  (label "DO1" (at 116.205 112.395 180))
  (label "EX3" (at 33.02 25.4 180))
  (label "EU2RX" (at 116.205 83.185 180))
  (label "DOT5" (at 243.205 31.75 180))
  (label "E_SCK" (at 116.205 120.015 180))
  (label "AB_TX" (at 116.205 23.495 180))
  (label "E_CS" (at 156.845 20.955 0))
  (label "K5" (at 116.205 41.275 180))
  (label "KC7" (at 210.185 81.28 0))
  (label "EE_SCK" (at 255.27 114.3 0))
  (label "SWCLK" (at 116.205 53.975 180))
  (label "DOT8" (at 255.905 29.21 0))
  (label "EX12" (at 60.96 35.56 0))
  (label "DO2" (at 192.405 37.465 180))
  (label "DOT1" (at 217.805 34.925 0))
  (label "DO7" (at 192.405 47.625 180))
  (label "EX12" (at 156.845 70.485 0))
  (label "VREF_M" (at 156.845 133.985 0))
  (label "E_RST" (at 156.845 18.415 0))
  (label "EX5" (at 33.02 27.94 180))
  (label "KC8" (at 226.06 81.28 0))
  (label "EIO1" (at 156.845 26.035 0))
  (label "NRST" (at 156.845 107.315 0))
  (label "KC5" (at 267.335 81.28 0))
  (label "DO2" (at 116.205 109.855 180))
  (label "EE_MOSI" (at 255.27 116.84 0))
  (label "AB_RST" (at 116.205 20.955 180))
  (label "EU2RX" (at 34.925 60.96 180))
  (label "EX1" (at 33.02 22.86 180))
  (label "EX9" (at 156.845 62.865 0))
  (label "DO3" (at 192.405 40.005 180))
  (label "DO6" (at 156.845 51.435 0))
  (label "EU1RX" (at 34.925 63.5 180))
  (label "SWDIO" (at 116.205 51.435 180))
  (label "AB_TX" (at 59.055 89.535 180))
  (label "K6" (at 236.855 83.82 0))
  (label "DOT2" (at 243.205 39.37 180))
  (label "EX2" (at 156.845 31.115 0))
  (label "AB_CTRL" (at 116.205 18.415 180))
  (label "EE_MISO" (at 255.27 119.38 0))
  (label "E_MOSI" (at 34.925 73.66 180))
  (label "AB_RST" (at 59.055 92.075 180))
  (label "EU1TX" (at 116.205 75.565 180))
  (label "K1" (at 201.93 88.9 180))
  (label "EU1TX" (at 62.865 63.5 0))
  (label "SWCLK" (at 129.54 177.165 180))
  (label "S_DRIV" (at 116.205 149.225 180))
  (label "DOT3" (at 217.805 40.005 0))
  (label "EE_SCK" (at 156.845 38.735 0))
  (label "S_DRIV" (at 43.815 183.515 0))
  (label "EX8" (at 156.845 60.325 0))
  (label "DO7" (at 156.845 48.895 0))
  (label "EX4" (at 156.845 36.195 0))
  (label "X2" (at 153.035 173.99 0))
  (label "VREF_M" (at 156.845 136.525 0))
  (label "AB_RX" (at 116.205 26.035 180))
  (label "EX7" (at 116.205 73.025 180))
  (hierarchical_label "MUTE" (shape input) (at 36.195 176.53 180))
  (hierarchical_label "ZCD_C" (shape input) (at 25.4 157.48 180))
  (hierarchical_label "CLK" (shape input) (at 36.195 183.515 180))
  (symbol (lib_id "power:GND") (at 158.115 151.765 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0106" (id 0) (at 158.115 158.115 0))
    (property "Value" "GND" (id 1) (at 161.925 153.67 0))
    (property "Footprint" "" (id 2) (at 158.115 151.765 0))
    (property "Datasheet" "" (id 3) (at 158.115 151.765 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 66.675 99.695 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR076" (id 0) (at 66.675 106.045 0))
    (property "Value" "GND" (id 1) (at 70.485 101.6 0))
    (property "Footprint" "" (id 2) (at 66.675 99.695 0))
    (property "Datasheet" "" (id 3) (at 66.675 99.695 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 36.83 157.48 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R45" (id 0) (at 36.83 153.035 90))
    (property "Value" "18k7" (id 1) (at 36.83 154.94 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 36.83 159.258 90))
    (property "Datasheet" "~" (id 3) (at 36.83 157.48 0))
    (property "comment" "" (id 4) (at 36.83 157.48 0))
    (property "PN" "SMDMM0204-18K7" (id 5) (at 36.83 157.48 0))
    (property "supplier" "TME" (id 6) (at 36.83 157.48 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x08_Odd_Even") (at 45.72 30.48 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J10" (id 0) (at 36.195 40.64 0))
    (property "Value" "Conn_02x08_Odd_Even" (id 1) (at 46.99 20.3986 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x08_P2.54mm_Vertical" (id 2) (at 45.72 30.48 0))
    (property "Datasheet" "~" (id 3) (at 45.72 30.48 0))
    (property "comment" "" (id 4) (at 45.72 30.48 0))
    (property "PN" "ZL201-10G" (id 5) (at 45.72 30.48 0))
    (property "supplier" "TME" (id 6) (at 45.72 30.48 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:GND") (at 153.035 181.61 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0110" (id 0) (at 153.035 187.96 0))
    (property "Value" "GND" (id 1) (at 156.845 183.515 0))
    (property "Footprint" "" (id 2) (at 153.035 181.61 0))
    (property "Datasheet" "" (id 3) (at 153.035 181.61 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 80.01 168.91 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R55" (id 0) (at 81.788 167.7416 0))
    (property "Value" "2K4" (id 1) (at 81.788 170.053 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 81.788 168.91 90))
    (property "Datasheet" "~" (id 3) (at 80.01 168.91 0))
    (property "comment" "" (id 4) (at 80.01 168.91 0))
    (property "PN" "MMA02040C2401" (id 5) (at 80.01 168.91 0))
    (property "supplier" "TME" (id 6) (at 80.01 168.91 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3.3V") (at 257.175 81.28 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR074" (id 0) (at 257.175 85.09 0))
    (property "Value" "+3.3V" (id 1) (at 257.556 76.8858 0))
    (property "Footprint" "" (id 2) (at 257.175 81.28 0))
    (property "Datasheet" "" (id 3) (at 257.175 81.28 0))
    (pin "1")
  )
  (symbol (lib_id "Memory_EEPROM:25LCxxx") (at 245.11 116.84 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U11" (id 0) (at 250.825 107.95 0))
    (property "Value" "25LC640" (id 1) (at 251.46 109.855 0))
    (property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (id 2) (at 245.11 116.84 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21832H.pdf" (id 3) (at 245.11 116.84 0))
    (property "comment" "" (id 4) (at 245.11 116.84 0))
    (property "PN" "25LC640A-I/SN" (id 5) (at 245.11 116.84 0))
    (property "supplier" "TME" (id 6) (at 245.11 116.84 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Device:R") (at 264.795 42.545 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R42" (id 0) (at 267.97 41.275 0))
    (property "Value" "620R" (id 1) (at 267.97 43.815 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 266.573 42.545 90))
    (property "Datasheet" "~" (id 3) (at 264.795 42.545 0))
    (property "comment" "" (id 4) (at 264.795 42.545 0))
    (property "PN" "MMA02040C6200" (id 5) (at 264.795 42.545 0))
    (property "supplier" "TME" (id 6) (at 264.795 42.545 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 38.735 63.5 90) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN3" (id 0) (at 22.86 63.5 90))
    (property "Value" "51R" (id 1) (at 40.6016 61.722 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 38.735 65.532 90))
    (property "Datasheet" "~" (id 3) (at 38.735 63.5 0))
    (property "link" "" (id 4) (at 38.735 63.5 0))
    (property "supplier" "MOUSER" (id 5) (at 38.735 63.5 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 38.735 63.5 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 62.865 86.995 90) (mirror x) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN7" (id 0) (at 46.99 86.995 90))
    (property "Value" "51R" (id 1) (at 64.7316 88.773 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 62.865 84.963 90))
    (property "Datasheet" "~" (id 3) (at 62.865 86.995 0))
    (property "link" "" (id 4) (at 62.865 86.995 0))
    (property "supplier" "MOUSER" (id 5) (at 62.865 86.995 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 62.865 86.995 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 57.15 25.4 270) (mirror x) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN8" (id 0) (at 73.025 25.4 90))
    (property "Value" "51R" (id 1) (at 55.2834 23.622 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 57.15 27.432 90))
    (property "Datasheet" "~" (id 3) (at 57.15 25.4 0))
    (property "link" "" (id 4) (at 57.15 25.4 0))
    (property "supplier" "MOUSER" (id 5) (at 57.15 25.4 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 57.15 25.4 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 38.735 66.04 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN3" (id 0) (at 22.86 66.04 90))
    (property "Value" "51R" (id 1) (at 40.6016 64.262 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 38.735 68.072 90))
    (property "Datasheet" "~" (id 3) (at 38.735 66.04 0))
    (property "link" "" (id 4) (at 38.735 66.04 0))
    (property "supplier" "MOUSER" (id 5) (at 38.735 66.04 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 38.735 66.04 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 263.525 81.28 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN6" (id 0) (at 252.095 81.28 90))
    (property "Value" "20k" (id 1) (at 265.3916 79.502 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 263.525 83.312 90))
    (property "Datasheet" "~" (id 3) (at 263.525 81.28 0))
    (property "link" "" (id 4) (at 263.525 81.28 0))
    (property "supplier" "MOUSER" (id 5) (at 263.525 81.28 0))
    (property "PN" "EXB-S8V203J" (id 6) (at 263.525 81.28 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 266.065 120.65 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR088" (id 0) (at 266.065 127 0))
    (property "Value" "GND" (id 1) (at 269.875 122.555 0))
    (property "Footprint" "" (id 2) (at 266.065 120.65 0))
    (property "Datasheet" "" (id 3) (at 266.065 120.65 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 266.065 116.84 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C44" (id 0) (at 266.7 114.3 0))
    (property "Value" "220n" (id 1) (at 266.7 119.38 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 267.0302 120.65 0))
    (property "Datasheet" "~" (id 3) (at 266.065 116.84 0))
    (property "comment" "" (id 4) (at 266.065 116.84 0))
    (property "PN" "VJ0805Y224KXATW1BC" (id 5) (at 266.065 116.84 0))
    (property "supplier" "TME" (id 6) (at 266.065 116.84 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 225.806 119.38 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R50" (id 0) (at 225.806 114.1222 90))
    (property "Value" "18k7" (id 1) (at 225.806 116.4336 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 225.806 117.602 90))
    (property "Datasheet" "~" (id 3) (at 225.806 119.38 0))
    (property "comment" "" (id 4) (at 225.806 119.38 0))
    (property "PN" "SMDMM0204-18K7" (id 5) (at 225.806 119.38 0))
    (property "supplier" "TME" (id 6) (at 225.806 119.38 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 66.04 168.91 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R53" (id 0) (at 67.818 167.7416 0))
    (property "Value" "2K4" (id 1) (at 67.818 170.053 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 67.818 168.91 90))
    (property "Datasheet" "~" (id 3) (at 66.04 168.91 0))
    (property "comment" "" (id 4) (at 66.04 168.91 0))
    (property "PN" "MMA02040C2401" (id 5) (at 66.04 168.91 0))
    (property "supplier" "TME" (id 6) (at 66.04 168.91 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 267.335 151.13 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C51" (id 0) (at 267.97 148.59 0))
    (property "Value" "2u2" (id 1) (at 267.97 153.67 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 268.3002 154.94 0))
    (property "Datasheet" "~" (id 3) (at 267.335 151.13 0))
    (property "comment" "" (id 4) (at 267.335 151.13 0))
    (property "PN" "CL21B225KPFNNNE" (id 5) (at 267.335 151.13 0))
    (property "supplier" "TME" (id 6) (at 267.335 151.13 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5V") (at 62.23 66.04 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR068" (id 0) (at 58.42 66.04 0))
    (property "Value" "+5V" (id 1) (at 65.4812 66.421 90))
    (property "Footprint" "" (id 2) (at 62.23 66.04 0))
    (property "Datasheet" "" (id 3) (at 62.23 66.04 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 207.518 122.428 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR090" (id 0) (at 207.518 128.778 0))
    (property "Value" "GND" (id 1) (at 211.328 124.333 0))
    (property "Footprint" "" (id 2) (at 207.518 122.428 0))
    (property "Datasheet" "" (id 3) (at 207.518 122.428 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 229.87 139.065 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C49" (id 0) (at 230.505 136.525 0))
    (property "Value" "100n" (id 1) (at 230.505 141.605 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 230.8352 142.875 0))
    (property "Datasheet" "~" (id 3) (at 229.87 139.065 0))
    (property "comment" "" (id 4) (at 229.87 139.065 0))
    (property "PN" "CL10B104KB8NNND" (id 5) (at 229.87 139.065 0))
    (property "supplier" "TME" (id 6) (at 229.87 139.065 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 38.735 76.2 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN5" (id 0) (at 22.86 76.2 90))
    (property "Value" "51R" (id 1) (at 40.6016 77.978 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 38.735 74.168 90))
    (property "Datasheet" "~" (id 3) (at 38.735 76.2 0))
    (property "link" "" (id 4) (at 38.735 76.2 0))
    (property "supplier" "MOUSER" (id 5) (at 38.735 76.2 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 38.735 76.2 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R") (at 41.275 116.205 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R47" (id 0) (at 44.45 114.3 0))
    (property "Value" "24R" (id 1) (at 44.45 116.205 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 39.497 116.205 90))
    (property "Datasheet" "~" (id 3) (at 41.275 116.205 0))
    (property "comment" "" (id 4) (at 41.275 116.205 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 41.275 116.205 0))
    (property "supplier" "TME" (id 6) (at 41.275 116.205 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 62.865 92.075 90) (mirror x) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN7" (id 0) (at 46.99 92.075 90))
    (property "Value" "51R" (id 1) (at 64.7316 93.853 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 62.865 90.043 90))
    (property "Datasheet" "~" (id 3) (at 62.865 92.075 0))
    (property "link" "" (id 4) (at 62.865 92.075 0))
    (property "supplier" "MOUSER" (id 5) (at 62.865 92.075 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 62.865 92.075 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 129.54 182.245 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0111" (id 0) (at 129.54 188.595 0))
    (property "Value" "GND" (id 1) (at 133.35 184.15 0))
    (property "Footprint" "" (id 2) (at 129.54 182.245 0))
    (property "Datasheet" "" (id 3) (at 129.54 182.245 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 57.15 33.02 270) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN10" (id 0) (at 73.025 33.02 90))
    (property "Value" "51R" (id 1) (at 55.2834 34.798 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 57.15 30.988 90))
    (property "Datasheet" "~" (id 3) (at 57.15 33.02 0))
    (property "link" "" (id 4) (at 57.15 33.02 0))
    (property "supplier" "MOUSER" (id 5) (at 57.15 33.02 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 57.15 33.02 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:+3.3V") (at 161.29 114.935 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR087" (id 0) (at 161.29 118.745 0))
    (property "Value" "+3.3V" (id 1) (at 161.671 110.5408 0))
    (property "Footprint" "" (id 2) (at 161.29 114.935 0))
    (property "Datasheet" "" (id 3) (at 161.29 114.935 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 38.735 58.42 90) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN1" (id 0) (at 22.86 58.42 90))
    (property "Value" "51R" (id 1) (at 40.6016 56.642 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 38.735 60.452 90))
    (property "Datasheet" "~" (id 3) (at 38.735 58.42 0))
    (property "link" "" (id 4) (at 38.735 58.42 0))
    (property "supplier" "MOUSER" (id 5) (at 38.735 58.42 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 38.735 58.42 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 36.83 35.56 90) (mirror x) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN10" (id 0) (at 20.955 35.56 90))
    (property "Value" "51R" (id 1) (at 38.6966 37.338 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 36.83 33.528 90))
    (property "Datasheet" "~" (id 3) (at 36.83 35.56 0))
    (property "link" "" (id 4) (at 36.83 35.56 0))
    (property "supplier" "MOUSER" (id 5) (at 36.83 35.56 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 36.83 35.56 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:C") (at 237.49 139.065 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C50" (id 0) (at 238.125 136.525 0))
    (property "Value" "100n" (id 1) (at 238.125 141.605 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 238.4552 142.875 0))
    (property "Datasheet" "~" (id 3) (at 237.49 139.065 0))
    (property "comment" "" (id 4) (at 237.49 139.065 0))
    (property "PN" "CL10B104KB8NNND" (id 5) (at 237.49 139.065 0))
    (property "supplier" "TME" (id 6) (at 237.49 139.065 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 84.455 186.055 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0114" (id 0) (at 84.455 192.405 0))
    (property "Value" "GND" (id 1) (at 88.265 187.96 0))
    (property "Footprint" "" (id 2) (at 84.455 186.055 0))
    (property "Datasheet" "" (id 3) (at 84.455 186.055 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 233.045 83.82 270) (mirror x) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN2" (id 0) (at 244.475 83.82 90))
    (property "Value" "51R" (id 1) (at 231.1784 82.042 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 233.045 85.852 90))
    (property "Datasheet" "~" (id 3) (at 233.045 83.82 0))
    (property "link" "" (id 4) (at 233.045 83.82 0))
    (property "supplier" "MOUSER" (id 5) (at 233.045 83.82 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 233.045 83.82 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:+3.3V") (at 194.945 135.255 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR093" (id 0) (at 194.945 139.065 0))
    (property "Value" "+3.3V" (id 1) (at 195.326 130.8608 0))
    (property "Footprint" "" (id 2) (at 194.945 135.255 0))
    (property "Datasheet" "" (id 3) (at 194.945 135.255 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 38.735 73.66 90) (mirror x) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN5" (id 0) (at 22.86 73.66 90))
    (property "Value" "51R" (id 1) (at 40.6016 75.438 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 38.735 71.628 90))
    (property "Datasheet" "~" (id 3) (at 38.735 73.66 0))
    (property "link" "" (id 4) (at 38.735 73.66 0))
    (property "supplier" "MOUSER" (id 5) (at 38.735 73.66 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 38.735 73.66 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:+3.3V") (at 63.5 71.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR071" (id 0) (at 63.5 74.93 0))
    (property "Value" "+3.3V" (id 1) (at 64.135 69.215 0))
    (property "Footprint" "" (id 2) (at 63.5 71.12 0))
    (property "Datasheet" "" (id 3) (at 63.5 71.12 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 74.295 115.57 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP2" (id 0) (at 67.945 115.57 90))
    (property "Value" "TestPoint" (id 1) (at 72.4662 112.9284 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D3.50mm_Drill1.4mm_Beaded" (id 2) (at 74.295 110.49 0))
    (property "Datasheet" "~" (id 3) (at 74.295 110.49 0))
    (property "comment" "optional" (id 4) (at 74.295 115.57 0))
    (property "supplier" "aliexpress" (id 5) (at 74.295 115.57 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 205.105 67.945 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR072" (id 0) (at 205.105 74.295 0))
    (property "Value" "GND" (id 1) (at 208.915 69.85 0))
    (property "Footprint" "" (id 2) (at 205.105 67.945 0))
    (property "Datasheet" "" (id 3) (at 205.105 67.945 0))
    (pin "1")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x07_Odd_Even") (at 248.285 36.83 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J6" (id 0) (at 249.555 26.035 0))
    (property "Value" "Conn_02x07_Odd_Even" (id 1) (at 249.555 26.0096 0))
    (property "Footprint" "Connector_IDC:IDC-Header_2x07_P2.54mm_Vertical" (id 2) (at 248.285 36.83 0))
    (property "Datasheet" "~" (id 3) (at 248.285 36.83 0))
    (property "comment" "" (id 4) (at 248.285 36.83 0))
    (property "PN" " T821-1-14-S1" (id 5) (at 248.285 36.83 0))
    (property "supplier" "TME" (id 6) (at 248.285 36.83 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "jlib_1:STM32F373VB") (at 136.525 81.915 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U9" (id 0) (at 135.255 43.18 0))
    (property "Value" "STM32F373VB" (id 1) (at 134.62 46.99 0))
    (property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm" (id 2) (at 136.525 81.915 0))
    (property "Datasheet" "" (id 3) (at 136.525 81.915 0))
    (property "comment" "" (id 4) (at 136.525 81.915 0))
    (property "PN" "STM32F373VBT6" (id 5) (at 136.525 81.915 0))
    (property "supplier" "MOUSER" (id 6) (at 136.525 81.915 0))
    (pin "1")
    (pin "10")
    (pin "100")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "50")
    (pin "51")
    (pin "52")
    (pin "53")
    (pin "54")
    (pin "55")
    (pin "56")
    (pin "57")
    (pin "58")
    (pin "59")
    (pin "6")
    (pin "60")
    (pin "61")
    (pin "62")
    (pin "63")
    (pin "64")
    (pin "65")
    (pin "66")
    (pin "67")
    (pin "68")
    (pin "69")
    (pin "7")
    (pin "70")
    (pin "71")
    (pin "72")
    (pin "73")
    (pin "74")
    (pin "75")
    (pin "76")
    (pin "77")
    (pin "78")
    (pin "79")
    (pin "8")
    (pin "80")
    (pin "81")
    (pin "82")
    (pin "83")
    (pin "84")
    (pin "85")
    (pin "86")
    (pin "87")
    (pin "88")
    (pin "89")
    (pin "9")
    (pin "90")
    (pin "91")
    (pin "92")
    (pin "93")
    (pin "94")
    (pin "95")
    (pin "96")
    (pin "97")
    (pin "98")
    (pin "99")
  )
  (symbol (lib_id "power:GND") (at 145.415 181.61 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0109" (id 0) (at 145.415 187.96 0))
    (property "Value" "GND" (id 1) (at 149.225 183.515 0))
    (property "Footprint" "" (id 2) (at 145.415 181.61 0))
    (property "Datasheet" "" (id 3) (at 145.415 181.61 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 41.275 137.16 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR094" (id 0) (at 41.275 143.51 0))
    (property "Value" "GND" (id 1) (at 45.085 139.065 0))
    (property "Footprint" "" (id 2) (at 41.275 137.16 0))
    (property "Datasheet" "" (id 3) (at 41.275 137.16 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3V") (at 245.11 109.22 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR080" (id 0) (at 245.11 113.03 0))
    (property "Value" "+3.3V" (id 1) (at 245.491 104.8258 0))
    (property "Footprint" "" (id 2) (at 245.11 109.22 0))
    (property "Datasheet" "" (id 3) (at 245.11 109.22 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Speaker") (at 46.355 122.555 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "LS1" (id 0) (at 50.673 122.9165 0))
    (property "Value" "Speaker" (id 1) (at 50.673 125.6916 0))
    (property "Footprint" "jlib2:beeper12" (id 2) (at 46.355 127.635 0))
    (property "Datasheet" "~" (id 3) (at 46.101 123.825 0))
    (property "comment" "" (id 4) (at 46.355 122.555 0))
    (property "PN" "LD-BZEN-1205" (id 5) (at 46.355 122.555 0))
    (property "supplier" "TME" (id 6) (at 46.355 122.555 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 205.74 81.28 90) (mirror x) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN2" (id 0) (at 195.58 81.28 90))
    (property "Value" "51R" (id 1) (at 207.6066 83.058 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 205.74 79.248 90))
    (property "Datasheet" "~" (id 3) (at 205.74 81.28 0))
    (property "link" "" (id 4) (at 205.74 81.28 0))
    (property "supplier" "MOUSER" (id 5) (at 205.74 81.28 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 205.74 81.28 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 205.74 83.82 90) (mirror x) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN2" (id 0) (at 195.58 83.82 90))
    (property "Value" "51R" (id 1) (at 207.6066 85.598 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 205.74 81.788 90))
    (property "Datasheet" "~" (id 3) (at 205.74 83.82 0))
    (property "link" "" (id 4) (at 205.74 83.82 0))
    (property "supplier" "MOUSER" (id 5) (at 205.74 83.82 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 205.74 83.82 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:+3.3V") (at 221.488 119.38 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR085" (id 0) (at 221.488 123.19 0))
    (property "Value" "+3.3V" (id 1) (at 220.726 115.062 0))
    (property "Footprint" "" (id 2) (at 221.488 119.38 0))
    (property "Datasheet" "" (id 3) (at 221.488 119.38 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 263.525 88.9 90) (mirror x) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN6" (id 0) (at 252.095 88.9 90))
    (property "Value" "20k" (id 1) (at 265.3916 90.678 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 263.525 86.868 90))
    (property "Datasheet" "~" (id 3) (at 263.525 88.9 0))
    (property "link" "" (id 4) (at 263.525 88.9 0))
    (property "supplier" "MOUSER" (id 5) (at 263.525 88.9 0))
    (property "PN" "EXB-S8V203J" (id 6) (at 263.525 88.9 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 229.87 142.875 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR099" (id 0) (at 229.87 149.225 0))
    (property "Value" "GND" (id 1) (at 233.68 144.78 0))
    (property "Footprint" "" (id 2) (at 229.87 142.875 0))
    (property "Datasheet" "" (id 3) (at 229.87 142.875 0))
    (pin "1")
  )
  (symbol (lib_id "Device:LED") (at 197.358 110.998 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D8" (id 0) (at 200.3552 110.0074 90))
    (property "Value" "LED" (id 1) (at 200.3552 112.3188 90))
    (property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (id 2) (at 197.358 110.998 0))
    (property "Datasheet" "~" (id 3) (at 197.358 110.998 0))
    (property "comment" "" (id 4) (at 197.358 110.998 0))
    (property "PN" "KP-2012YD" (id 5) (at 197.358 110.998 0))
    (property "supplier" "TME" (id 6) (at 197.358 110.998 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xGxx:74LVC1G14") (at 48.26 157.48 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U10" (id 0) (at 53.34 164.465 0))
    (property "Value" "74LVC1G14" (id 1) (at 52.705 167.005 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (id 2) (at 48.26 157.48 0))
    (property "Datasheet" "http://www.ti.com/lit/sg/scyt129e/scyt129e.pdf" (id 3) (at 48.26 157.48 0))
    (property "comment" "" (id 4) (at 48.26 157.48 0))
    (property "PN" "SN74LVC1G14DBVR" (id 5) (at 48.26 157.48 0))
    (property "supplier" "TME" (id 6) (at 48.26 157.48 0))
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R") (at 118.11 174.625 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R56" (id 0) (at 118.11 169.3672 90))
    (property "Value" "18k7" (id 1) (at 118.11 171.6786 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 118.11 172.847 90))
    (property "Datasheet" "~" (id 3) (at 118.11 174.625 0))
    (property "comment" "" (id 4) (at 118.11 174.625 0))
    (property "PN" "SMDMM0204-18K7" (id 5) (at 118.11 174.625 0))
    (property "supplier" "TME" (id 6) (at 118.11 174.625 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 36.83 30.48 90) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN9" (id 0) (at 20.955 30.48 90))
    (property "Value" "51R" (id 1) (at 38.6966 28.702 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 36.83 32.512 90))
    (property "Datasheet" "~" (id 3) (at 36.83 30.48 0))
    (property "link" "" (id 4) (at 36.83 30.48 0))
    (property "supplier" "MOUSER" (id 5) (at 36.83 30.48 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 36.83 30.48 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 263.525 83.82 90) (mirror x) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN6" (id 0) (at 252.095 83.82 90))
    (property "Value" "20k" (id 1) (at 265.3916 85.598 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 263.525 81.788 90))
    (property "Datasheet" "~" (id 3) (at 263.525 83.82 0))
    (property "link" "" (id 4) (at 263.525 83.82 0))
    (property "supplier" "MOUSER" (id 5) (at 263.525 83.82 0))
    (property "PN" "EXB-S8V203J" (id 6) (at 263.525 83.82 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:C") (at 223.52 139.065 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C48" (id 0) (at 224.155 136.525 0))
    (property "Value" "100n" (id 1) (at 224.155 141.605 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 224.4852 142.875 0))
    (property "Datasheet" "~" (id 3) (at 223.52 139.065 0))
    (property "comment" "" (id 4) (at 223.52 139.065 0))
    (property "PN" "CL10B104KB8NNND" (id 5) (at 223.52 139.065 0))
    (property "supplier" "TME" (id 6) (at 223.52 139.065 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3.3V") (at 65.405 40.64 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0113" (id 0) (at 65.405 44.45 0))
    (property "Value" "+3.3V" (id 1) (at 66.04 38.1 0))
    (property "Footprint" "" (id 2) (at 65.405 40.64 0))
    (property "Datasheet" "" (id 3) (at 65.405 40.64 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 217.17 139.065 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C47" (id 0) (at 217.805 136.525 0))
    (property "Value" "100n" (id 1) (at 217.805 141.605 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 218.1352 142.875 0))
    (property "Datasheet" "~" (id 3) (at 217.17 139.065 0))
    (property "comment" "" (id 4) (at 217.17 139.065 0))
    (property "PN" "CL10B104KB8NNND" (id 5) (at 217.17 139.065 0))
    (property "supplier" "TME" (id 6) (at 217.17 139.065 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 36.83 27.94 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN9" (id 0) (at 20.955 27.94 90))
    (property "Value" "51R" (id 1) (at 38.6966 26.162 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 36.83 29.972 90))
    (property "Datasheet" "~" (id 3) (at 36.83 27.94 0))
    (property "link" "" (id 4) (at 36.83 27.94 0))
    (property "supplier" "MOUSER" (id 5) (at 36.83 27.94 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 36.83 27.94 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Reference_Voltage:MCP1525-TT") (at 255.27 147.32 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U12" (id 0) (at 266.065 138.43 0))
    (property "Value" "MCP1525-TT" (id 1) (at 269.875 140.97 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 255.905 153.67 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21653b.pdf" (id 3) (at 255.27 147.32 0))
    (property "comment" "" (id 4) (at 255.27 147.32 0))
    (property "PN" "MCP1525T-I/TT" (id 5) (at 255.27 147.32 0))
    (property "supplier" "TME" (id 6) (at 255.27 147.32 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:+3.3V") (at 41.275 112.395 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR082" (id 0) (at 41.275 116.205 0))
    (property "Value" "+3.3V" (id 1) (at 38.735 107.95 0))
    (property "Footprint" "" (id 2) (at 41.275 112.395 0))
    (property "Datasheet" "" (id 3) (at 41.275 112.395 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3V") (at 66.675 97.155 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR075" (id 0) (at 70.485 97.155 0))
    (property "Value" "+3.3V" (id 1) (at 63.5 99.06 90))
    (property "Footprint" "" (id 2) (at 66.675 97.155 0))
    (property "Datasheet" "" (id 3) (at 66.675 97.155 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Ferrite_Bead_Small") (at 200.66 149.225 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "FB1" (id 0) (at 200.66 145.542 90))
    (property "Value" "Ferrite_Bead_Small" (id 1) (at 200.66 145.5166 90))
    (property "Footprint" "Inductor_SMD:L_0805_2012Metric_Pad1.05x1.20mm_HandSolder" (id 2) (at 200.66 147.447 90))
    (property "Datasheet" "~" (id 3) (at 200.66 149.225 0))
    (property "comment" "" (id 4) (at 200.66 149.225 0))
    (property "PN" "BLM21A102SPT" (id 5) (at 200.66 149.225 0))
    (property "supplier" "TME" (id 6) (at 200.66 149.225 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 271.78 42.545 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R43" (id 0) (at 274.955 41.275 0))
    (property "Value" "620R" (id 1) (at 274.955 43.815 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 273.558 42.545 90))
    (property "Datasheet" "~" (id 3) (at 271.78 42.545 0))
    (property "comment" "" (id 4) (at 271.78 42.545 0))
    (property "PN" "MMA02040C6200" (id 5) (at 271.78 42.545 0))
    (property "supplier" "TME" (id 6) (at 271.78 42.545 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 59.055 63.5 270) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN3" (id 0) (at 73.66 63.5 90))
    (property "Value" "51R" (id 1) (at 57.1884 65.278 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 59.055 61.468 90))
    (property "Datasheet" "~" (id 3) (at 59.055 63.5 0))
    (property "link" "" (id 4) (at 59.055 63.5 0))
    (property "supplier" "MOUSER" (id 5) (at 59.055 63.5 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 59.055 63.5 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x08_Odd_Even") (at 47.625 66.04 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "J8" (id 0) (at 48.895 53.1835 0))
    (property "Value" "Conn_02x08_Odd_Even" (id 1) (at 48.895 55.9586 0))
    (property "Footprint" "Connector_IDC:IDC-Header_2x08_P2.54mm_Vertical" (id 2) (at 47.625 66.04 0))
    (property "Datasheet" "~" (id 3) (at 47.625 66.04 0))
    (property "comment" "" (id 4) (at 47.625 66.04 0))
    (property "PN" "T821-1-16-S1" (id 5) (at 47.625 66.04 0))
    (property "supplier" "TME" (id 6) (at 47.625 66.04 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 59.055 58.42 270) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN1" (id 0) (at 73.66 58.42 90))
    (property "Value" "51R" (id 1) (at 57.1884 60.198 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 59.055 56.388 90))
    (property "Datasheet" "~" (id 3) (at 59.055 58.42 0))
    (property "link" "" (id 4) (at 59.055 58.42 0))
    (property "supplier" "MOUSER" (id 5) (at 59.055 58.42 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 59.055 58.42 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:+3.3V") (at 266.065 113.03 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR083" (id 0) (at 266.065 116.84 0))
    (property "Value" "+3.3V" (id 1) (at 266.446 108.6358 0))
    (property "Footprint" "" (id 2) (at 266.065 113.03 0))
    (property "Datasheet" "" (id 3) (at 266.065 113.03 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 62.865 94.615 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN7" (id 0) (at 46.99 94.615 90))
    (property "Value" "51R" (id 1) (at 64.7316 96.393 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 62.865 92.583 90))
    (property "Datasheet" "~" (id 3) (at 62.865 94.615 0))
    (property "link" "" (id 4) (at 62.865 94.615 0))
    (property "supplier" "MOUSER" (id 5) (at 62.865 94.615 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 62.865 94.615 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 59.055 60.96 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN1" (id 0) (at 73.66 60.96 90))
    (property "Value" "51R" (id 1) (at 57.1884 62.738 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 59.055 58.928 90))
    (property "Datasheet" "~" (id 3) (at 59.055 60.96 0))
    (property "link" "" (id 4) (at 59.055 60.96 0))
    (property "supplier" "MOUSER" (id 5) (at 59.055 60.96 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 59.055 60.96 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:C") (at 201.295 27.305 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C42" (id 0) (at 194.31 23.495 90))
    (property "Value" "220n" (id 1) (at 194.31 25.4 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 197.485 28.2702 0))
    (property "Datasheet" "~" (id 3) (at 201.295 27.305 0))
    (property "comment" "" (id 4) (at 201.295 27.305 0))
    (property "PN" "VJ0805Y224KXATW1BC" (id 5) (at 201.295 27.305 0))
    (property "supplier" "TME" (id 6) (at 201.295 27.305 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 217.17 142.875 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR097" (id 0) (at 217.17 149.225 0))
    (property "Value" "GND" (id 1) (at 220.98 144.78 0))
    (property "Footprint" "" (id 2) (at 217.17 142.875 0))
    (property "Datasheet" "" (id 3) (at 217.17 142.875 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 213.36 91.44 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR069" (id 0) (at 213.36 97.79 0))
    (property "Value" "GND" (id 1) (at 215.9 94.615 0))
    (property "Footprint" "" (id 2) (at 213.36 91.44 0))
    (property "Datasheet" "" (id 3) (at 213.36 91.44 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3V") (at 114.3 174.625 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0107" (id 0) (at 118.11 174.625 0))
    (property "Value" "+3.3V" (id 1) (at 111.0488 174.244 90))
    (property "Footprint" "" (id 2) (at 114.3 174.625 0))
    (property "Datasheet" "" (id 3) (at 114.3 174.625 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 243.205 44.45 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR062" (id 0) (at 243.205 50.8 0))
    (property "Value" "GND" (id 1) (at 247.015 46.355 0))
    (property "Footprint" "" (id 2) (at 243.205 44.45 0))
    (property "Datasheet" "" (id 3) (at 243.205 44.45 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 38.735 68.58 90) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN3" (id 0) (at 22.86 68.58 90))
    (property "Value" "51R" (id 1) (at 40.6016 66.802 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 38.735 70.612 90))
    (property "Datasheet" "~" (id 3) (at 38.735 68.58 0))
    (property "link" "" (id 4) (at 38.735 68.58 0))
    (property "supplier" "MOUSER" (id 5) (at 38.735 68.58 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 38.735 68.58 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector:Conn_01x06_Male") (at 71.755 94.615 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J9" (id 0) (at 72.4662 93.9546 0))
    (property "Value" "Conn_01x06_Male" (id 1) (at 72.4662 91.6432 0))
    (property "Footprint" "Connector_Molex:Molex_KK-254_AE-6410-06A_1x06_P2.54mm_Vertical" (id 2) (at 71.755 94.615 0))
    (property "Datasheet" "~" (id 3) (at 71.755 94.615 0))
    (property "comment" "" (id 4) (at 71.755 94.615 0))
    (property "PN" "NS25-W6P" (id 5) (at 71.755 94.615 0))
    (property "supplier" "TME" (id 6) (at 71.755 94.615 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "power:GND") (at 235.585 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR065" (id 0) (at 235.585 52.07 0))
    (property "Value" "GND" (id 1) (at 239.395 47.625 0))
    (property "Footprint" "" (id 2) (at 235.585 45.72 0))
    (property "Datasheet" "" (id 3) (at 235.585 45.72 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 38.735 71.12 90) (mirror x) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN5" (id 0) (at 22.86 71.12 90))
    (property "Value" "51R" (id 1) (at 40.6016 72.898 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 38.735 69.088 90))
    (property "Datasheet" "~" (id 3) (at 38.735 71.12 0))
    (property "link" "" (id 4) (at 38.735 71.12 0))
    (property "supplier" "MOUSER" (id 5) (at 38.735 71.12 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 38.735 71.12 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R") (at 197.358 118.618 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R48" (id 0) (at 199.136 117.4496 0))
    (property "Value" "620R" (id 1) (at 199.136 119.761 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 199.136 118.618 90))
    (property "Datasheet" "~" (id 3) (at 197.358 118.618 0))
    (property "comment" "" (id 4) (at 197.358 118.618 0))
    (property "PN" "MMA02040C6200" (id 5) (at 197.358 118.618 0))
    (property "supplier" "TME" (id 6) (at 197.358 118.618 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 57.15 30.48 270) (mirror x) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN9" (id 0) (at 73.025 30.48 90))
    (property "Value" "51R" (id 1) (at 55.2834 28.702 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 57.15 32.512 90))
    (property "Datasheet" "~" (id 3) (at 57.15 30.48 0))
    (property "link" "" (id 4) (at 57.15 30.48 0))
    (property "supplier" "MOUSER" (id 5) (at 57.15 30.48 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 57.15 30.48 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 57.15 22.86 270) (mirror x) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN8" (id 0) (at 73.025 22.86 90))
    (property "Value" "51R" (id 1) (at 55.2834 21.082 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 57.15 24.892 90))
    (property "Datasheet" "~" (id 3) (at 57.15 22.86 0))
    (property "link" "" (id 4) (at 57.15 22.86 0))
    (property "supplier" "MOUSER" (id 5) (at 57.15 22.86 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 57.15 22.86 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:+5V") (at 255.905 44.45 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR063" (id 0) (at 252.095 44.45 0))
    (property "Value" "+5V" (id 1) (at 259.1562 44.831 90))
    (property "Footprint" "" (id 2) (at 255.905 44.45 0))
    (property "Datasheet" "" (id 3) (at 255.905 44.45 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:Conn_01x05_Male") (at 134.62 177.165 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J11" (id 0) (at 135.3312 176.6062 0))
    (property "Value" "Conn_01x05_Male" (id 1) (at 135.3312 175.4632 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x05_P2.54mm_Vertical" (id 2) (at 134.62 177.165 0))
    (property "Datasheet" "~" (id 3) (at 134.62 177.165 0))
    (property "comment" "" (id 4) (at 134.62 177.165 0))
    (property "PN" "ZL201-10G" (id 5) (at 134.62 177.165 0))
    (property "supplier" "TME" (id 6) (at 134.62 177.165 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 264.795 46.355 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR066" (id 0) (at 264.795 52.705 0))
    (property "Value" "GND" (id 1) (at 268.605 48.26 0))
    (property "Footprint" "" (id 2) (at 264.795 46.355 0))
    (property "Datasheet" "" (id 3) (at 264.795 46.355 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 271.78 46.355 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR067" (id 0) (at 271.78 52.705 0))
    (property "Value" "GND" (id 1) (at 275.59 48.26 0))
    (property "Footprint" "" (id 2) (at 271.78 46.355 0))
    (property "Datasheet" "" (id 3) (at 271.78 46.355 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 255.27 154.94 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0102" (id 0) (at 255.27 161.29 0))
    (property "Value" "GND" (id 1) (at 259.08 156.845 0))
    (property "Footprint" "" (id 2) (at 255.27 154.94 0))
    (property "Datasheet" "" (id 3) (at 255.27 154.94 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 62.865 89.535 90) (mirror x) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN7" (id 0) (at 46.99 89.535 90))
    (property "Value" "51R" (id 1) (at 64.7316 91.313 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 62.865 87.503 90))
    (property "Datasheet" "~" (id 3) (at 62.865 89.535 0))
    (property "link" "" (id 4) (at 62.865 89.535 0))
    (property "supplier" "MOUSER" (id 5) (at 62.865 89.535 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 62.865 89.535 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 205.74 86.36 90) (mirror x) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN4" (id 0) (at 195.58 86.36 90))
    (property "Value" "51R" (id 1) (at 207.6066 88.138 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 205.74 84.328 90))
    (property "Datasheet" "~" (id 3) (at 205.74 86.36 0))
    (property "link" "" (id 4) (at 205.74 86.36 0))
    (property "supplier" "MOUSER" (id 5) (at 205.74 86.36 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 205.74 86.36 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 57.15 27.94 270) (mirror x) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN9" (id 0) (at 73.025 27.94 90))
    (property "Value" "51R" (id 1) (at 55.2834 26.162 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 57.15 29.972 90))
    (property "Datasheet" "~" (id 3) (at 57.15 27.94 0))
    (property "link" "" (id 4) (at 57.15 27.94 0))
    (property "supplier" "MOUSER" (id 5) (at 57.15 27.94 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 57.15 27.94 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:+5V") (at 205.105 27.305 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR060" (id 0) (at 205.105 31.115 0))
    (property "Value" "+5V" (id 1) (at 205.486 22.9108 0))
    (property "Footprint" "" (id 2) (at 205.105 27.305 0))
    (property "Datasheet" "" (id 3) (at 205.105 27.305 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3VADC") (at 160.655 127.635 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR092" (id 0) (at 164.465 128.905 0))
    (property "Value" "+3.3VADC" (id 1) (at 161.036 123.2408 0))
    (property "Footprint" "" (id 2) (at 160.655 127.635 0))
    (property "Datasheet" "" (id 3) (at 160.655 127.635 0))
    (pin "1")
  )
  (symbol (lib_id "Transistor_BJT:BC847") (at 38.735 132.08 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Q3" (id 0) (at 43.5864 131.1715 0))
    (property "Value" "BC847" (id 1) (at 32.385 137.795 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 43.815 133.985 0))
    (property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657" (id 3) (at 38.735 132.08 0))
    (property "comment" "" (id 4) (at 38.735 132.08 0))
    (property "PN" "BC847.215" (id 5) (at 38.735 132.08 0))
    (property "supplier" "TME" (id 6) (at 38.735 132.08 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 233.045 86.36 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN4" (id 0) (at 244.475 86.36 90))
    (property "Value" "51R" (id 1) (at 231.1784 88.138 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 233.045 84.328 90))
    (property "Datasheet" "~" (id 3) (at 233.045 86.36 0))
    (property "link" "" (id 4) (at 233.045 86.36 0))
    (property "supplier" "MOUSER" (id 5) (at 233.045 86.36 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 233.045 86.36 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 206.375 156.845 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0104" (id 0) (at 206.375 163.195 0))
    (property "Value" "GND" (id 1) (at 210.185 158.75 0))
    (property "Footprint" "" (id 2) (at 206.375 156.845 0))
    (property "Datasheet" "" (id 3) (at 206.375 156.845 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 165.1 104.775 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R46" (id 0) (at 165.1 99.5172 90))
    (property "Value" "18k7" (id 1) (at 165.1 101.8286 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 165.1 102.997 90))
    (property "Datasheet" "~" (id 3) (at 165.1 104.775 0))
    (property "comment" "" (id 4) (at 165.1 104.775 0))
    (property "PN" "SMDMM0204-18K7" (id 5) (at 165.1 104.775 0))
    (property "supplier" "TME" (id 6) (at 165.1 104.775 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 37.465 120.015 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C45" (id 0) (at 37.465 114.3 90))
    (property "Value" "2u2" (id 1) (at 38.1 116.205 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 41.275 119.0498 0))
    (property "Datasheet" "~" (id 3) (at 37.465 120.015 0))
    (property "comment" "" (id 4) (at 37.465 120.015 0))
    (property "PN" "CL21B225KPFNNNE" (id 5) (at 37.465 120.015 0))
    (property "supplier" "TME" (id 6) (at 37.465 120.015 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 205.74 88.9 90) (mirror x) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN4" (id 0) (at 195.58 88.9 90))
    (property "Value" "51R" (id 1) (at 207.6066 90.678 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 205.74 86.868 90))
    (property "Datasheet" "~" (id 3) (at 205.74 88.9 0))
    (property "link" "" (id 4) (at 205.74 88.9 0))
    (property "supplier" "MOUSER" (id 5) (at 205.74 88.9 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 205.74 88.9 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:LED") (at 207.518 110.998 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D9" (id 0) (at 210.5152 110.0074 90))
    (property "Value" "LED" (id 1) (at 210.5152 112.3188 90))
    (property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (id 2) (at 207.518 110.998 0))
    (property "Datasheet" "~" (id 3) (at 207.518 110.998 0))
    (property "comment" "" (id 4) (at 207.518 110.998 0))
    (property "PN" "KP-2012YD" (id 5) (at 207.518 110.998 0))
    (property "supplier" "TME" (id 6) (at 207.518 110.998 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 228.6 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR064" (id 0) (at 228.6 52.07 0))
    (property "Value" "GND" (id 1) (at 232.41 47.625 0))
    (property "Footprint" "" (id 2) (at 228.6 45.72 0))
    (property "Datasheet" "" (id 3) (at 228.6 45.72 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 228.6 41.91 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R40" (id 0) (at 231.775 40.64 0))
    (property "Value" "620R" (id 1) (at 231.775 43.18 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 230.378 41.91 90))
    (property "Datasheet" "~" (id 3) (at 228.6 41.91 0))
    (property "comment" "" (id 4) (at 228.6 41.91 0))
    (property "PN" "MMA02040C6200" (id 5) (at 228.6 41.91 0))
    (property "supplier" "TME" (id 6) (at 228.6 41.91 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 153.035 177.8 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C55" (id 0) (at 155.575 177.8 0))
    (property "Value" "33p" (id 1) (at 153.67 180.34 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 154.0002 181.61 0))
    (property "Datasheet" "~" (id 3) (at 153.035 177.8 0))
    (property "comment" "" (id 4) (at 153.035 177.8 0))
    (property "PN" "VJ0805A330FXAAC" (id 5) (at 153.035 177.8 0))
    (property "supplier" "TME" (id 6) (at 153.035 177.8 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 197.485 27.305 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR059" (id 0) (at 197.485 33.655 0))
    (property "Value" "GND" (id 1) (at 194.31 29.845 0))
    (property "Footprint" "" (id 2) (at 197.485 27.305 0))
    (property "Datasheet" "" (id 3) (at 197.485 27.305 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 235.585 41.91 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R41" (id 0) (at 238.76 40.64 0))
    (property "Value" "620R" (id 1) (at 238.76 43.18 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 237.363 41.91 90))
    (property "Datasheet" "~" (id 3) (at 235.585 41.91 0))
    (property "comment" "" (id 4) (at 235.585 41.91 0))
    (property "PN" "MMA02040C6200" (id 5) (at 235.585 41.91 0))
    (property "supplier" "TME" (id 6) (at 235.585 41.91 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 214.63 156.845 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0105" (id 0) (at 214.63 163.195 0))
    (property "Value" "GND" (id 1) (at 218.44 158.75 0))
    (property "Footprint" "" (id 2) (at 214.63 156.845 0))
    (property "Datasheet" "" (id 3) (at 214.63 156.845 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 57.15 35.56 270) (mirror x) (unit 4)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN10" (id 0) (at 73.025 35.56 90))
    (property "Value" "51R" (id 1) (at 55.2834 33.782 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 57.15 37.592 90))
    (property "Datasheet" "~" (id 3) (at 57.15 35.56 0))
    (property "link" "" (id 4) (at 57.15 35.56 0))
    (property "supplier" "MOUSER" (id 5) (at 57.15 35.56 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 57.15 35.56 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:+3.3V") (at 48.26 154.94 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR078" (id 0) (at 48.26 158.75 0))
    (property "Value" "+3.3V" (id 1) (at 45.72 150.495 0))
    (property "Footprint" "" (id 2) (at 48.26 154.94 0))
    (property "Datasheet" "" (id 3) (at 48.26 154.94 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 267.335 154.94 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0103" (id 0) (at 267.335 161.29 0))
    (property "Value" "GND" (id 1) (at 271.145 156.845 0))
    (property "Footprint" "" (id 2) (at 267.335 154.94 0))
    (property "Datasheet" "" (id 3) (at 267.335 154.94 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3VADC") (at 206.375 149.225 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0101" (id 0) (at 210.185 150.495 0))
    (property "Value" "+3.3VADC" (id 1) (at 212.09 147.32 0))
    (property "Footprint" "" (id 2) (at 206.375 149.225 0))
    (property "Datasheet" "" (id 3) (at 206.375 149.225 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 145.415 177.8 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C54" (id 0) (at 142.875 177.165 0))
    (property "Value" "33p" (id 1) (at 144.78 180.34 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 144.4498 181.61 0))
    (property "Datasheet" "~" (id 3) (at 145.415 177.8 0))
    (property "comment" "" (id 4) (at 145.415 177.8 0))
    (property "PN" "VJ0805A330FXAAC" (id 5) (at 145.415 177.8 0))
    (property "supplier" "TME" (id 6) (at 145.415 177.8 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 28.575 153.67 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R44" (id 0) (at 31.75 151.765 0))
    (property "Value" "18k7" (id 1) (at 31.75 153.67 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 26.797 153.67 90))
    (property "Datasheet" "~" (id 3) (at 28.575 153.67 0))
    (property "comment" "" (id 4) (at 28.575 153.67 0))
    (property "PN" "SMDMM0204-18K7" (id 5) (at 28.575 153.67 0))
    (property "supplier" "TME" (id 6) (at 28.575 153.67 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 73.025 168.91 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R54" (id 0) (at 74.803 167.7416 0))
    (property "Value" "2K4" (id 1) (at 74.803 170.053 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 74.803 168.91 90))
    (property "Datasheet" "~" (id 3) (at 73.025 168.91 0))
    (property "comment" "" (id 4) (at 73.025 168.91 0))
    (property "PN" "MMA02040C2401" (id 5) (at 73.025 168.91 0))
    (property "supplier" "TME" (id 6) (at 73.025 168.91 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3.3V") (at 226.06 91.44 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR070" (id 0) (at 222.25 91.44 0))
    (property "Value" "+3.3V" (id 1) (at 229.3112 91.821 90))
    (property "Footprint" "" (id 2) (at 226.06 91.44 0))
    (property "Datasheet" "" (id 3) (at 226.06 91.44 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 206.375 153.035 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C52" (id 0) (at 207.01 150.495 0))
    (property "Value" "100n" (id 1) (at 207.01 155.575 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 207.3402 156.845 0))
    (property "Datasheet" "~" (id 3) (at 206.375 153.035 0))
    (property "comment" "" (id 4) (at 206.375 153.035 0))
    (property "PN" "CL10B104KB8NNND" (id 5) (at 206.375 153.035 0))
    (property "supplier" "TME" (id 6) (at 206.375 153.035 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+3.3V") (at 129.54 179.705 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0108" (id 0) (at 133.35 179.705 0))
    (property "Value" "+3.3V" (id 1) (at 126.2888 179.324 90))
    (property "Footprint" "" (id 2) (at 129.54 179.705 0))
    (property "Datasheet" "" (id 3) (at 129.54 179.705 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 237.49 142.875 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0100" (id 0) (at 237.49 149.225 0))
    (property "Value" "GND" (id 1) (at 241.3 144.78 0))
    (property "Footprint" "" (id 2) (at 237.49 142.875 0))
    (property "Datasheet" "" (id 3) (at 237.49 142.875 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 40.005 176.53 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R51" (id 0) (at 40.005 172.085 90))
    (property "Value" "240R" (id 1) (at 40.005 173.99 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 40.005 178.308 90))
    (property "Datasheet" "~" (id 3) (at 40.005 176.53 0))
    (property "comment" "" (id 4) (at 40.005 176.53 0))
    (property "PN" "MMA02040C2400" (id 5) (at 40.005 176.53 0))
    (property "supplier" "TME" (id 6) (at 40.005 176.53 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 40.64 40.64 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0112" (id 0) (at 40.64 46.99 0))
    (property "Value" "GND" (id 1) (at 44.45 42.545 0))
    (property "Footprint" "" (id 2) (at 40.64 40.64 0))
    (property "Datasheet" "" (id 3) (at 40.64 40.64 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 207.518 118.618 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R49" (id 0) (at 209.296 117.4496 0))
    (property "Value" "620R" (id 1) (at 209.296 119.761 0))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 209.296 118.618 90))
    (property "Datasheet" "~" (id 3) (at 207.518 118.618 0))
    (property "comment" "" (id 4) (at 207.518 118.618 0))
    (property "PN" "MMA02040C6200" (id 5) (at 207.518 118.618 0))
    (property "supplier" "TME" (id 6) (at 207.518 118.618 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 168.91 106.045 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR081" (id 0) (at 168.91 112.395 0))
    (property "Value" "GND" (id 1) (at 168.275 110.49 0))
    (property "Footprint" "" (id 2) (at 168.91 106.045 0))
    (property "Datasheet" "" (id 3) (at 168.91 106.045 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 245.11 124.46 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR091" (id 0) (at 245.11 130.81 0))
    (property "Value" "GND" (id 1) (at 248.92 126.365 0))
    (property "Footprint" "" (id 2) (at 245.11 124.46 0))
    (property "Datasheet" "" (id 3) (at 245.11 124.46 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 38.735 60.96 90) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN1" (id 0) (at 22.86 60.96 90))
    (property "Value" "51R" (id 1) (at 40.6016 59.182 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 38.735 62.992 90))
    (property "Datasheet" "~" (id 3) (at 38.735 60.96 0))
    (property "link" "" (id 4) (at 38.735 60.96 0))
    (property "supplier" "MOUSER" (id 5) (at 38.735 60.96 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 38.735 60.96 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 223.52 142.875 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR098" (id 0) (at 223.52 149.225 0))
    (property "Value" "GND" (id 1) (at 227.33 144.78 0))
    (property "Footprint" "" (id 2) (at 223.52 142.875 0))
    (property "Datasheet" "" (id 3) (at 223.52 142.875 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3V") (at 28.575 149.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR077" (id 0) (at 28.575 153.67 0))
    (property "Value" "+3.3V" (id 1) (at 29.21 147.32 0))
    (property "Footprint" "" (id 2) (at 28.575 149.86 0))
    (property "Datasheet" "" (id 3) (at 28.575 149.86 0))
    (pin "1")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x05_Odd_Even") (at 218.44 86.36 0) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J7" (id 0) (at 221.615 95.25 0))
    (property "Value" "Conn_02x05_Odd_Even" (id 1) (at 219.71 94.6404 0))
    (property "Footprint" "Connector_IDC:IDC-Header_2x05_P2.54mm_Vertical" (id 2) (at 218.44 86.36 0))
    (property "Datasheet" "~" (id 3) (at 218.44 86.36 0))
    (property "comment" "" (id 4) (at 218.44 86.36 0))
    (property "PN" "T821-1-10-S1" (id 5) (at 218.44 86.36 0))
    (property "supplier" "TME" (id 6) (at 218.44 86.36 0))
    (pin "1")
    (pin "10")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 36.83 25.4 90) (mirror x) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN8" (id 0) (at 20.955 25.4 90))
    (property "Value" "51R" (id 1) (at 38.6966 27.178 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 36.83 23.368 90))
    (property "Datasheet" "~" (id 3) (at 36.83 25.4 0))
    (property "link" "" (id 4) (at 36.83 25.4 0))
    (property "supplier" "MOUSER" (id 5) (at 36.83 25.4 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 36.83 25.4 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:C") (at 206.375 139.065 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C46" (id 0) (at 207.01 136.525 0))
    (property "Value" "100n" (id 1) (at 207.01 141.605 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 207.3402 142.875 0))
    (property "Datasheet" "~" (id 3) (at 206.375 139.065 0))
    (property "comment" "" (id 4) (at 206.375 139.065 0))
    (property "PN" "CL10B104KB8NNND" (id 5) (at 206.375 139.065 0))
    (property "supplier" "TME" (id 6) (at 206.375 139.065 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 214.63 153.035 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C53" (id 0) (at 215.265 150.495 0))
    (property "Value" "100n" (id 1) (at 215.265 155.575 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder" (id 2) (at 215.5952 156.845 0))
    (property "Datasheet" "~" (id 3) (at 214.63 153.035 0))
    (property "comment" "" (id 4) (at 214.63 153.035 0))
    (property "PN" "CL10B104KB8NNND" (id 5) (at 214.63 153.035 0))
    (property "supplier" "TME" (id 6) (at 214.63 153.035 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 40.64 165.1 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR084" (id 0) (at 40.64 171.45 0))
    (property "Value" "GND" (id 1) (at 44.45 167.005 0))
    (property "Footprint" "" (id 2) (at 40.64 165.1 0))
    (property "Datasheet" "" (id 3) (at 40.64 165.1 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 36.83 33.02 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN10" (id 0) (at 20.955 33.02 90))
    (property "Value" "51R" (id 1) (at 38.6966 31.242 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 36.83 35.052 90))
    (property "Datasheet" "~" (id 3) (at 36.83 33.02 0))
    (property "link" "" (id 4) (at 36.83 33.02 0))
    (property "supplier" "MOUSER" (id 5) (at 36.83 33.02 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 36.83 33.02 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Connector:Conn_01x06_Male") (at 90.805 180.975 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J12" (id 0) (at 91.5162 179.1462 0))
    (property "Value" "Conn_01x06_Male" (id 1) (at 91.5162 180.2892 0))
    (property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (id 2) (at 90.805 180.975 0))
    (property "Datasheet" "~" (id 3) (at 90.805 180.975 0))
    (property "comment" "" (id 4) (at 90.805 180.975 0))
    (property "PN" "ZL201-10G" (id 5) (at 90.805 180.975 0))
    (property "supplier" "TME" (id 6) (at 90.805 180.975 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "power:GND") (at 197.358 122.428 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR089" (id 0) (at 197.358 128.778 0))
    (property "Value" "GND" (id 1) (at 201.168 124.333 0))
    (property "Footprint" "" (id 2) (at 197.358 122.428 0))
    (property "Datasheet" "" (id 3) (at 197.358 122.428 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 74.295 115.57 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR061" (id 0) (at 74.295 121.92 0))
    (property "Value" "GND" (id 1) (at 78.105 117.475 0))
    (property "Footprint" "" (id 2) (at 74.295 115.57 0))
    (property "Datasheet" "" (id 3) (at 74.295 115.57 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 40.64 161.29 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C43" (id 0) (at 33.02 163.83 0))
    (property "Value" "220n" (id 1) (at 33.02 165.735 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 41.6052 165.1 0))
    (property "Datasheet" "~" (id 3) (at 40.64 161.29 0))
    (property "comment" "" (id 4) (at 40.64 161.29 0))
    (property "PN" "VJ0805Y224KXATW1BC" (id 5) (at 40.64 161.29 0))
    (property "supplier" "TME" (id 6) (at 40.64 161.29 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint") (at 74.295 111.76 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP1" (id 0) (at 67.945 111.76 90))
    (property "Value" "TestPoint" (id 1) (at 72.4662 109.1184 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D3.50mm_Drill1.4mm_Beaded" (id 2) (at 74.295 106.68 0))
    (property "Datasheet" "~" (id 3) (at 74.295 106.68 0))
    (property "comment" "optional" (id 4) (at 74.295 111.76 0))
    (property "supplier" "aliexpress" (id 5) (at 74.295 111.76 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74HC244") (at 205.105 47.625 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U8" (id 0) (at 210.82 28.575 0))
    (property "Value" "74HCT244" (id 1) (at 210.82 31.115 0))
    (property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm" (id 2) (at 205.105 47.625 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT244.pdf" (id 3) (at 205.105 47.625 0))
    (property "comment" "" (id 4) (at 205.105 47.625 0))
    (property "PN" "74HCT244D.653" (id 5) (at 205.105 47.625 0))
    (property "supplier" "TME" (id 6) (at 205.105 47.625 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 36.83 22.86 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN8" (id 0) (at 20.955 22.86 90))
    (property "Value" "51R" (id 1) (at 38.6966 24.638 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 36.83 20.828 90))
    (property "Datasheet" "~" (id 3) (at 36.83 22.86 0))
    (property "link" "" (id 4) (at 36.83 22.86 0))
    (property "supplier" "MOUSER" (id 5) (at 36.83 22.86 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 36.83 22.86 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 59.055 76.2 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR073" (id 0) (at 59.055 82.55 0))
    (property "Value" "GND" (id 1) (at 62.865 78.105 0))
    (property "Footprint" "" (id 2) (at 59.055 76.2 0))
    (property "Datasheet" "" (id 3) (at 59.055 76.2 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 48.26 160.02 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR079" (id 0) (at 48.26 166.37 0))
    (property "Value" "GND" (id 1) (at 52.07 161.925 0))
    (property "Footprint" "" (id 2) (at 48.26 160.02 0))
    (property "Datasheet" "" (id 3) (at 48.26 160.02 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 33.655 120.015 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR086" (id 0) (at 33.655 126.365 0))
    (property "Value" "GND" (id 1) (at 30.48 123.19 0))
    (property "Footprint" "" (id 2) (at 33.655 120.015 0))
    (property "Datasheet" "" (id 3) (at 33.655 120.015 0))
    (pin "1")
  )
  (symbol (lib_id "power:+3.3VADC") (at 255.27 139.7 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR095" (id 0) (at 259.08 140.97 0))
    (property "Value" "+3.3VADC" (id 1) (at 255.651 135.3058 0))
    (property "Footprint" "" (id 2) (at 255.27 139.7 0))
    (property "Datasheet" "" (id 3) (at 255.27 139.7 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 233.045 88.9 270) (mirror x) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN4" (id 0) (at 244.475 88.9 90))
    (property "Value" "51R" (id 1) (at 231.1784 87.122 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 233.045 90.932 90))
    (property "Datasheet" "~" (id 3) (at 233.045 88.9 0))
    (property "link" "" (id 4) (at 233.045 88.9 0))
    (property "supplier" "MOUSER" (id 5) (at 233.045 88.9 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 233.045 88.9 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "power:GND") (at 206.375 142.875 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR096" (id 0) (at 206.375 149.225 0))
    (property "Value" "GND" (id 1) (at 210.185 144.78 0))
    (property "Footprint" "" (id 2) (at 206.375 142.875 0))
    (property "Datasheet" "" (id 3) (at 206.375 142.875 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 29.845 132.08 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R52" (id 0) (at 31.115 127.635 90))
    (property "Value" "6k2" (id 1) (at 31.115 129.54 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 29.845 133.858 90))
    (property "Datasheet" "~" (id 3) (at 29.845 132.08 0))
    (property "comment" "" (id 4) (at 29.845 132.08 0))
    (property "PN" "MMA02040C6202" (id 5) (at 29.845 132.08 0))
    (property "supplier" "TME" (id 6) (at 29.845 132.08 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Crystal") (at 149.225 173.99 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "Y1" (id 0) (at 149.225 167.1828 0))
    (property "Value" "8MHz" (id 1) (at 149.225 169.4942 0))
    (property "Footprint" "Crystal:Crystal_SMD_HC49-SD" (id 2) (at 149.225 173.99 0))
    (property "Datasheet" "~" (id 3) (at 149.225 173.99 0))
    (property "comment" "" (id 4) (at 149.225 173.99 0))
    (property "PN" "8.00M-SMDHC49R" (id 5) (at 149.225 173.99 0))
    (property "supplier" "TME" (id 6) (at 149.225 173.99 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 263.525 86.36 90) (mirror x) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN6" (id 0) (at 252.095 86.36 90))
    (property "Value" "20k" (id 1) (at 265.3916 88.138 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 263.525 84.328 90))
    (property "Datasheet" "~" (id 3) (at 263.525 86.36 0))
    (property "link" "" (id 4) (at 263.525 86.36 0))
    (property "supplier" "MOUSER" (id 5) (at 263.525 86.36 0))
    (property "PN" "EXB-S8V203J" (id 6) (at 263.525 86.36 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:R_Pack04_Split") (at 233.045 81.28 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RN2" (id 0) (at 244.475 81.28 90))
    (property "Value" "51R" (id 1) (at 231.1784 83.058 0))
    (property "Footprint" "Resistor_SMD:R_Array_Convex_4x1206" (id 2) (at 233.045 79.248 90))
    (property "Datasheet" "~" (id 3) (at 233.045 81.28 0))
    (property "link" "" (id 4) (at 233.045 81.28 0))
    (property "supplier" "MOUSER" (id 5) (at 233.045 81.28 0))
    (property "PN" "EXB-S8V510J " (id 6) (at 233.045 81.28 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "7")
    (pin "3")
    (pin "6")
    (pin "4")
    (pin "5")
  )
)
