(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer false)
      (plotframeref false)
      (viasonmask true)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerb/")
    )
  )
  (net 0 "")
  (net 1 "/KR1")
  (net 2 "/KR2")
  (net 3 "/KR3")
  (net 4 "/KR4")
  (net 5 "/KC1")
  (net 6 "/KC2")
  (net 7 "/KC3")
  (net 8 "/KC4")
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 71 -9)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW3" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "/KC3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "/KR1") (pinfunction "2") (pintype "passive"))
  )
  (footprint "j_lib:logo_rpg7x9" (layer "F.Cu")
    (tedit 61CE1C18)
    (at 158.2 -39.4)
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr board_only exclude_from_pos_files)
    (fp_text reference "LOGO1" (at 0.956014 12.7) (layer "F.SilkS") hide)
    (fp_text value "logo_generic" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 191 -9)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW9" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "/KC1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "/KR3") (pinfunction "2") (pintype "passive"))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 151 -9)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW7" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "/KC3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "/KR2") (pinfunction "2") (pintype "passive"))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 31 -9)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "/KC1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "/KR1") (pinfunction "2") (pintype "passive"))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 191 -49)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW13" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "/KC1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "/KR4") (pinfunction "2") (pintype "passive"))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 131 -9)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW6" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "/KC2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "/KR2") (pinfunction "2") (pintype "passive"))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 171 -9)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW8" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "/KC4") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "/KR2") (pinfunction "2") (pintype "passive"))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 171 -49)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW12" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "/KC4") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "/KR3") (pinfunction "2") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 3 -63)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 91 -9)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW4" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "/KC4") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "/KR1") (pinfunction "2") (pintype "passive"))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 51 -9)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "/KC2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "/KR1") (pinfunction "2") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 3 -3)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 191 -29)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW11" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "/KC3") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "/KR3") (pinfunction "2") (pintype "passive"))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 111 -9)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW5" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "/KC1") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "/KR2") (pinfunction "2") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 155 -23)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H6" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 16 -59)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H5" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "j_lib:MQ_6450" (layer "F.Cu")
    (tedit 5E6E9275)
    (at 171 -29)
    (property "PN" "6450")
    (property "SUPPLIER" "TME")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW10" (at 0 5) (layer "F.SilkS"))
    (fp_text value "SW_Push" (at 0 -0.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 5 5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -5 -5) (size 1.3 1.3) (drill 1.3) (layers *.Cu *.Mask))
    (pad "1" thru_hole circle locked (at 0 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "/KC2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle locked (at 5 0) (size 2 2) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "/KR3") (pinfunction "2") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 206 -63)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H7" (at 0.2 3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 155 -59)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_3.2mm_M3_DIN965_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 206 -3)
    (descr "Mounting Hole 3.2mm, M3, DIN965")
    (tags "mounting hole 3.2mm m3 din965")
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H8" (at 0 -3.8) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.8) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5.6 5.6) (drill 3.2) (layers *.Cu *.Mask))
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 16 -23)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 0 -3.5) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.3 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "Connector_Molex:Molex_KK-254_AE-6410-08A_1x08_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5EA53D3B)
    (at 187.96 -59 180)
    (descr "Molex KK-254 Interconnect System, old/engineering part number: AE-6410-08A example for new part number: 22-27-2081, 8 Pins (http://www.molex.com/pdm_docs/sd/022272021_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex KK-254 vertical")
    (property "Comment" "DNP")
    (property "Sheetfile" "rnvm_meggie.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at 8.89 4.12) (layer "B.SilkS"))
    (fp_text value "Conn_01x08_Male" (at 8.89 -4.08) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 8.89 2.22) (layer "B.Fab"))
    (pad "1" thru_hole roundrect locked (at 0 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask) (roundrect_rratio 0.1436781609)
      (net 1 "/KR1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 2.54 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 2 "/KR2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 5.08 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 3 "/KR3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 7.62 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 4 "/KR4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval locked (at 10.16 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 5 "/KC1") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 12.7 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 6 "/KC2") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval locked (at 15.24 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 7 "/KC3") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval locked (at 17.78 0 180) (size 1.74 2.19) (drill 1.19) (layers *.Cu *.Mask)
      (net 8 "/KC4") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_KK-254_AE-6410-08A_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_circle (center 11 -9) (end 16 -9) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_rect (start 19 -23) (end 152 -59) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_rect (start 0 0) (end 209 -66) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "NVM\nMEGGIE PCB REV 1" (at 4.8 -39.8 270) (layer "F.SilkS"))
)
