(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "Connector:TestPoint" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "TP" (id 0) (at 0 6.858 0))
      (property "Value" "TestPoint" (id 1) (at 0 5.08 0))
      (property "Footprint" "" (id 2) (at 5.08 0 0))
      (property "Datasheet" "~" (id 3) (at 5.08 0 0))
      (property "ki_keywords" "test point tp" (id 4) (at 0 0 0))
      (property "ki_description" "test point" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Pin* Test*" (id 6) (at 0 0 0))
      (symbol "TestPoint_0_1"
        (circle (center 0 3.302) (radius 0.762)
          (fill (type none))
        )
      )
      (symbol "TestPoint_1_1"
        (pin passive line (at 0 0 90) (length 2.54)
          (name "1")
          (number "1")
        )
      )
    )
    (symbol "Connector_Generic:Conn_02x03_Odd_Even" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 1.27 5.08 0))
      (property "Value" "Conn_02x03_Odd_Even" (id 1) (at 1.27 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "connector" (id 4) (at 0 0 0))
      (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Connector*:*_2x??_*" (id 6) (at 0 0 0))
      (symbol "Conn_02x03_Odd_Even_1_1"
        (rectangle (start -1.27 -2.413) (end 0 -2.667)
          (fill (type none))
        )
        (rectangle (start -1.27 0.127) (end 0 -0.127)
          (fill (type none))
        )
        (rectangle (start -1.27 2.667) (end 0 2.413)
          (fill (type none))
        )
        (rectangle (start -1.27 3.81) (end 3.81 -3.81)
          (fill (type background))
        )
        (rectangle (start 3.81 -2.413) (end 2.54 -2.667)
          (fill (type none))
        )
        (rectangle (start 3.81 0.127) (end 2.54 -0.127)
          (fill (type none))
        )
        (rectangle (start 3.81 2.667) (end 2.54 2.413)
          (fill (type none))
        )
        (pin passive line (at -5.08 2.54 0) (length 3.81)
          (name "Pin_1")
          (number "1")
        )
        (pin passive line (at 7.62 2.54 180) (length 3.81)
          (name "Pin_2")
          (number "2")
        )
        (pin passive line (at -5.08 0 0) (length 3.81)
          (name "Pin_3")
          (number "3")
        )
        (pin passive line (at 7.62 0 180) (length 3.81)
          (name "Pin_4")
          (number "4")
        )
        (pin passive line (at -5.08 -2.54 0) (length 3.81)
          (name "Pin_5")
          (number "5")
        )
        (pin passive line (at 7.62 -2.54 180) (length 3.81)
          (name "Pin_6")
          (number "6")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Ferrite_Bead_Small" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "FB" (id 0) (at 1.905 1.27 0))
      (property "Value" "Ferrite_Bead_Small" (id 1) (at 1.905 -1.27 0))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "L ferrite bead inductor filter" (id 4) (at 0 0 0))
      (property "ki_description" "Ferrite bead, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Inductor_* L_* *Ferrite*" (id 6) (at 0 0 0))
      (symbol "Ferrite_Bead_Small_0_1"
        (polyline
          (pts
            (xy 0 -1.27)
            (xy 0 -0.7874)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.889)
            (xy 0 1.2954)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.8288 0.2794)
            (xy -1.1176 1.4986)
            (xy 1.8288 -0.2032)
            (xy 1.1176 -1.4224)
            (xy -1.8288 0.2794)
          )
          (fill (type none))
        )
      )
      (symbol "Ferrite_Bead_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Gekkio_FPGA_Lattice:LCMXO2-1200xx-xTG100" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 10.16 31.75 0))
      (property "Value" "Gekkio_FPGA_Lattice_LCMXO2-1200xx-xTG100" (id 1) (at 15.24 27.94 0))
      (property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm" (id 2) (at 1.27 -30.48 0))
      (property "Datasheet" "" (id 3) (at -7.62 -2.54 90))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*" (id 5) (at 0 0 0))
      (symbol "LCMXO2-1200xx-xTG100_1_1"
        (rectangle (start -36.83 33.02) (end 31.75 -29.21)
          (fill (type background))
        )
        (pin bidirectional line (at 36.83 -26.67 180) (length 5.08)
          (name "PR10D/BANK1/C/DQ1")
          (number "51")
        )
        (pin bidirectional line (at 36.83 -24.13 180) (length 5.08)
          (name "PR10C/BANK1/T/DQ1")
          (number "52")
        )
        (pin bidirectional line (at 36.83 -21.59 180) (length 5.08)
          (name "PR9D/BANK1/C/DQ1")
          (number "53")
        )
        (pin bidirectional line (at 36.83 -19.05 180) (length 5.08)
          (name "PR9C/BANK1/T/DQ1")
          (number "54")
        )
        (pin power_in line (at -27.94 38.1 270) (length 5.08)
          (name "VCCIO1")
          (number "55")
        )
        (pin bidirectional line (at 36.83 -16.51 180) (length 5.08)
          (name "PR9B/BANK1/C/DQ1")
          (number "57")
        )
        (pin bidirectional line (at 36.83 -13.97 180) (length 5.08)
          (name "PR9A/BANK1/T/DQ1")
          (number "58")
        )
        (pin bidirectional line (at 36.83 -11.43 180) (length 5.08)
          (name "PR8D/BANK1/C/DQ1")
          (number "59")
        )
        (pin bidirectional line (at 36.83 -8.89 180) (length 5.08)
          (name "PR8C/BANK1/T/DQ1")
          (number "60")
        )
        (pin bidirectional line (at 36.83 -6.35 180) (length 5.08)
          (name "PR8A/BANK1/DQS1")
          (number "61")
        )
        (pin bidirectional line (at 36.83 -3.81 180) (length 5.08)
          (name "PR5D/BANK1/C/PCLKC1_0/DQ0")
          (number "62")
        )
        (pin bidirectional line (at 36.83 -1.27 180) (length 5.08)
          (name "PR5C/BANK1/T/PCLKT1_0/DQ0")
          (number "63")
        )
        (pin bidirectional line (at 36.83 1.27 180) (length 5.08)
          (name "PR5B/BANK1/C/DQS0N")
          (number "64")
        )
        (pin bidirectional line (at 36.83 3.81 180) (length 5.08)
          (name "PR5A/BANK1/T/DQS0")
          (number "65")
        )
        (pin bidirectional line (at 36.83 6.35 180) (length 5.08)
          (name "PR4D/BANK1/C/DQ0")
          (number "66")
        )
        (pin bidirectional line (at 36.83 8.89 180) (length 5.08)
          (name "PR4C/BANK1/T/DQ0")
          (number "67")
        )
        (pin bidirectional line (at 36.83 11.43 180) (length 5.08)
          (name "PR4B/BANK1/C/DQ0")
          (number "68")
        )
        (pin bidirectional line (at 36.83 13.97 180) (length 5.08)
          (name "PR4A/BANK1/T/DQ0")
          (number "69")
        )
        (pin bidirectional line (at 36.83 16.51 180) (length 5.08)
          (name "PR3B/BANK1/C/DQ0")
          (number "70")
        )
        (pin bidirectional line (at 36.83 19.05 180) (length 5.08)
          (name "PR3A/BANK1/T/DQ0")
          (number "71")
        )
        (pin power_in line (at -25.4 38.1 270) (length 5.08)
          (name "VCCIO1")
          (number "73")
        )
        (pin bidirectional line (at 36.83 21.59 180) (length 5.08)
          (name "PR2B/BANK1/C/DQ0")
          (number "74")
        )
        (pin bidirectional line (at 36.83 24.13 180) (length 5.08)
          (name "PR2A/BANK1/T/DQ0")
          (number "75")
        )
        (pin bidirectional line (at -41.91 -22.86 0) (length 5.08)
          (name "PT17D/BANK0/C/DONE")
          (number "76")
        )
        (pin bidirectional line (at -41.91 -20.32 0) (length 5.08)
          (name "PT17C/BANK0/T/INITN")
          (number "77")
        )
        (pin bidirectional line (at -41.91 -17.78 0) (length 5.08)
          (name "PT16C/BANK0")
          (number "78")
        )
        (pin power_in line (at -33.02 38.1 270) (length 5.08)
          (name "VCCIO0")
          (number "80")
        )
        (pin bidirectional line (at -41.91 -15.24 0) (length 5.08)
          (name "PT15D/BANK0/C/PROGRAMN")
          (number "81")
        )
        (pin bidirectional line (at -41.91 -12.7 0) (length 5.08)
          (name "PT15C/BANK0/T/JTAGENB")
          (number "82")
        )
        (pin bidirectional line (at -41.91 -10.16 0) (length 5.08)
          (name "PT15B/BANK0/C/LVDS")
          (number "83")
        )
        (pin bidirectional line (at -41.91 -7.62 0) (length 5.08)
          (name "PT15A/BANK0/T/LVDS")
          (number "84")
        )
        (pin bidirectional line (at -41.91 -5.08 0) (length 5.08)
          (name "PT12D/BANK0/C/SDA/PCLKC0_0")
          (number "85")
        )
        (pin bidirectional line (at -41.91 -2.54 0) (length 5.08)
          (name "PT12C/BANK0/T/SCL/PCLKT0_0")
          (number "86")
        )
        (pin bidirectional line (at -41.91 0 0) (length 5.08)
          (name "PT12B/BANK0/C/PCLKC0_1/LVDS")
          (number "87")
        )
        (pin bidirectional line (at -41.91 2.54 0) (length 5.08)
          (name "PT12A/BANK0/T/PCLKT0_1/LVDS")
          (number "88")
        )
        (pin no_connect line (at -41.91 -25.4 0) (length 5.08) hide
          (name "NC")
          (number "89")
        )
        (pin bidirectional line (at -41.91 5.08 0) (length 5.08)
          (name "PT11D/BANK0/C/TMS")
          (number "90")
        )
        (pin bidirectional line (at -41.91 7.62 0) (length 5.08)
          (name "PT11C/BANK0/T/TCK")
          (number "91")
        )
        (pin power_in line (at -30.48 38.1 270) (length 5.08)
          (name "VCCIO0")
          (number "93")
        )
        (pin bidirectional line (at -41.91 10.16 0) (length 5.08)
          (name "PT10D/BANK0/C/TDI")
          (number "94")
        )
        (pin bidirectional line (at -41.91 12.7 0) (length 5.08)
          (name "PT10C/BANK0/T/TDO")
          (number "95")
        )
        (pin bidirectional line (at -41.91 15.24 0) (length 5.08)
          (name "PT10B/BANK0/C/LVDS")
          (number "96")
        )
        (pin bidirectional line (at -41.91 17.78 0) (length 5.08)
          (name "PT10A/BANK0/T/LVDS")
          (number "97")
        )
        (pin bidirectional line (at -41.91 20.32 0) (length 5.08)
          (name "PT9B/BANK0/C/LVDS")
          (number "98")
        )
        (pin bidirectional line (at -41.91 22.86 0) (length 5.08)
          (name "PT9A/BANK0/T/LVDS")
          (number "99")
        )
      )
      (symbol "LCMXO2-1200xx-xTG100_2_1"
        (rectangle (start -29.21 33.02) (end 30.48 -27.94)
          (fill (type background))
        )
        (pin bidirectional line (at 35.56 22.86 180) (length 5.08)
          (name "PL2C/BANK3/T/L_GPLLT_IN")
          (number "1")
        )
        (pin bidirectional line (at 35.56 5.08 180) (length 5.08)
          (name "PL4B/BANK3/C")
          (number "10")
        )
        (pin power_in line (at -16.51 38.1 270) (length 5.08)
          (name "VCCIO3")
          (number "11")
        )
        (pin bidirectional line (at 35.56 2.54 180) (length 5.08)
          (name "PL5A/BANK3/T/PCLKT3_1")
          (number "12")
        )
        (pin bidirectional line (at 35.56 0 180) (length 5.08)
          (name "PL5B/BANK3/C/PCLKC3_1")
          (number "13")
        )
        (pin bidirectional line (at 35.56 -2.54 180) (length 5.08)
          (name "PL5C/BANK3/T")
          (number "14")
        )
        (pin bidirectional line (at 35.56 -5.08 180) (length 5.08)
          (name "PL5D/BANK3/C")
          (number "15")
        )
        (pin bidirectional line (at 35.56 -7.62 180) (length 5.08)
          (name "PL8A/BANK3/T")
          (number "16")
        )
        (pin bidirectional line (at 35.56 -10.16 180) (length 5.08)
          (name "PL8B/BANK3/C")
          (number "17")
        )
        (pin bidirectional line (at 35.56 -12.7 180) (length 5.08)
          (name "PL8C/BANK3/T")
          (number "18")
        )
        (pin bidirectional line (at 35.56 -15.24 180) (length 5.08)
          (name "PL8D/BANK3/C")
          (number "19")
        )
        (pin bidirectional line (at 35.56 20.32 180) (length 5.08)
          (name "PL2D/BANK3/C/L_GPLLC_IN")
          (number "2")
        )
        (pin bidirectional line (at 35.56 -17.78 180) (length 5.08)
          (name "PL9A/BANK3/T/PCLKT3_0")
          (number "20")
        )
        (pin bidirectional line (at 35.56 -20.32 180) (length 5.08)
          (name "PL9B/BANK3/C/PCLKC3_0")
          (number "21")
        )
        (pin power_in line (at -19.05 38.1 270) (length 5.08)
          (name "VCCIO3")
          (number "23")
        )
        (pin bidirectional line (at 35.56 -22.86 180) (length 5.08)
          (name "PL10C/BANK3/T")
          (number "24")
        )
        (pin bidirectional line (at 35.56 -25.4 180) (length 5.08)
          (name "PL10D/BANK3/C")
          (number "25")
        )
        (pin power_in line (at -24.13 38.1 270) (length 5.08)
          (name "VCCIO2")
          (number "26")
        )
        (pin bidirectional line (at -34.29 22.86 0) (length 5.08)
          (name "PB4C/BANK2/T/CSSPIN")
          (number "27")
        )
        (pin bidirectional line (at -34.29 20.32 0) (length 5.08)
          (name "PB4D/BANK2/C")
          (number "28")
        )
        (pin bidirectional line (at -34.29 17.78 0) (length 5.08)
          (name "PB6A/BANK2/T")
          (number "29")
        )
        (pin bidirectional line (at 35.56 17.78 180) (length 5.08)
          (name "PL3A/BANK3/T/PCLKT3_2")
          (number "3")
        )
        (pin bidirectional line (at -34.29 15.24 0) (length 5.08)
          (name "PB6B/BANK2/C")
          (number "30")
        )
        (pin bidirectional line (at -34.29 12.7 0) (length 5.08)
          (name "PB6C/BANK2/T/MCLK/CCLK")
          (number "31")
        )
        (pin bidirectional line (at -34.29 10.16 0) (length 5.08)
          (name "PB6D/BANK2/C/SO/SPISO")
          (number "32")
        )
        (pin bidirectional line (at -34.29 7.62 0) (length 5.08)
          (name "PB9A/BANK2/T/PCLKT2_0")
          (number "34")
        )
        (pin bidirectional line (at -34.29 5.08 0) (length 5.08)
          (name "PB9B/BANK2/C/PCLKC2_0")
          (number "35")
        )
        (pin bidirectional line (at -34.29 2.54 0) (length 5.08)
          (name "PB11C/BANK2/T")
          (number "36")
        )
        (pin bidirectional line (at -34.29 0 0) (length 5.08)
          (name "PB11D/BANK2/C")
          (number "37")
        )
        (pin bidirectional line (at -34.29 -2.54 0) (length 5.08)
          (name "PB11A/BANK2/T/PCLKT2_1")
          (number "38")
        )
        (pin bidirectional line (at -34.29 -5.08 0) (length 5.08)
          (name "PB11B/BANK2/C/PCLKC2_1")
          (number "39")
        )
        (pin bidirectional line (at 35.56 15.24 180) (length 5.08)
          (name "PL3B/BANK3/C/PCLKC3_2")
          (number "4")
        )
        (pin bidirectional line (at -34.29 -7.62 0) (length 5.08)
          (name "PB15A/BANK2/T")
          (number "40")
        )
        (pin bidirectional line (at -34.29 -10.16 0) (length 5.08)
          (name "PB15B/BANK2/C")
          (number "41")
        )
        (pin bidirectional line (at -34.29 -12.7 0) (length 5.08)
          (name "PB18A/BANK2/T")
          (number "42")
        )
        (pin bidirectional line (at -34.29 -15.24 0) (length 5.08)
          (name "PB18B/BANK2/C")
          (number "43")
        )
        (pin bidirectional line (at -34.29 -17.78 0) (length 5.08)
          (name "PB18C/BANK2/T")
          (number "45")
        )
        (pin power_in line (at -21.59 38.1 270) (length 5.08)
          (name "VCCIO2")
          (number "46")
        )
        (pin bidirectional line (at -34.29 -20.32 0) (length 5.08)
          (name "PB18D/BANK2/C")
          (number "47")
        )
        (pin bidirectional line (at -34.29 -22.86 0) (length 5.08)
          (name "PB20C/BANK2/T/SN")
          (number "48")
        )
        (pin bidirectional line (at -34.29 -25.4 0) (length 5.08)
          (name "PB20D/BANK2/C/SI/SISPI")
          (number "49")
        )
        (pin power_in line (at -13.97 38.1 270) (length 5.08)
          (name "VCCIO3")
          (number "5")
        )
        (pin bidirectional line (at 35.56 12.7 180) (length 5.08)
          (name "PL3C/BANK3/T")
          (number "7")
        )
        (pin bidirectional line (at 35.56 10.16 180) (length 5.08)
          (name "PL3D/BANK3/C")
          (number "8")
        )
        (pin bidirectional line (at 35.56 7.62 180) (length 5.08)
          (name "PL4A/BANK3/T")
          (number "9")
        )
      )
      (symbol "LCMXO2-1200xx-xTG100_3_1"
        (rectangle (start -10.16 -7.62) (end 10.16 10.16)
          (fill (type background))
        )
        (pin power_in line (at 15.24 6.35 180) (length 5.08)
          (name "VCC")
          (number "100")
        )
        (pin power_in line (at -15.24 -2.54 0) (length 5.08)
          (name "GND")
          (number "22")
        )
        (pin power_in line (at -15.24 0 0) (length 5.08)
          (name "GND")
          (number "33")
        )
        (pin power_in line (at -15.24 2.54 0) (length 5.08)
          (name "GND")
          (number "44")
        )
        (pin power_in line (at -15.24 6.35 0) (length 5.08)
          (name "VCC")
          (number "50")
        )
        (pin power_in line (at 15.24 -5.08 180) (length 5.08)
          (name "GND")
          (number "56")
        )
        (pin power_in line (at -15.24 -5.08 0) (length 5.08)
          (name "GND")
          (number "6")
        )
        (pin power_in line (at 15.24 -2.54 180) (length 5.08)
          (name "GND")
          (number "72")
        )
        (pin power_in line (at 15.24 0 180) (length 5.08)
          (name "GND")
          (number "79")
        )
        (pin power_in line (at 15.24 2.54 180) (length 5.08)
          (name "GND")
          (number "92")
        )
      )
    )
    (symbol "Oscillator:SG-5032CAN" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "X" (id 0) (at -5.08 6.35 0))
      (property "Value" "SG-5032CAN" (id 1) (at 1.27 -6.35 0))
      (property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm" (id 2) (at 17.78 -8.89 0))
      (property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG5032CAN&lang=en" (id 3) (at -2.54 0 0))
      (property "ki_keywords" "Crystal Clock Oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "CMOS Clock Oscillator 1 to 75 MHz" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002LB*5.0x3.2mm*" (id 6) (at 0 0 0))
      (symbol "SG-5032CAN_0_1"
        (rectangle (start -5.08 5.08) (end 5.08 -5.08)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -1.27 -0.762)
            (xy -1.016 -0.762)
            (xy -1.016 0.762)
            (xy -0.508 0.762)
            (xy -0.508 -0.762)
            (xy 0 -0.762)
            (xy 0 0.762)
            (xy 0.508 0.762)
            (xy 0.508 -0.762)
            (xy 0.762 -0.762)
          )
          (fill (type none))
        )
      )
      (symbol "SG-5032CAN_1_1"
        (pin input line (at -7.62 0 0) (length 2.54)
          (name "~{ST}")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "OUT")
          (number "3")
        )
        (pin power_in line (at 0 7.62 270) (length 2.54)
          (name "VCC")
          (number "4")
        )
      )
    )
    (symbol "Regulator_Linear:MCP1700-1202E_SOT23" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 3.175 0))
      (property "Value" "MCP1700-1202E_SOT23" (id 1) (at 0 3.175 0))
      (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 0 5.715 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "regulator linear ldo" (id 4) (at 0 0 0))
      (property "ki_description" "250mA Low Quiscent Current LDO, 1.2V output, SOT-23" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOT?23*" (id 6) (at 0 0 0))
      (symbol "MCP1700-1202E_SOT23_0_1"
        (rectangle (start -5.08 1.905) (end 5.08 -5.08)
          (fill (type background))
        )
      )
      (symbol "MCP1700-1202E_SOT23_1_1"
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "2")
        )
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "3")
        )
      )
    )
    (symbol "jlib_1:tc77-SOT23-5" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -1.27 6.35 0))
      (property "Value" "jlib_1_tc77-SOT23-5" (id 1) (at 0 -6.35 0))
      (property "Footprint" "" (id 2) (at -6.35 -2.54 0))
      (property "Datasheet" "" (id 3) (at -6.35 -2.54 0))
      (symbol "tc77-SOT23-5_0_1"
        (rectangle (start -6.35 5.08) (end 6.35 -5.08)
          (fill (type background))
        )
      )
      (symbol "tc77-SOT23-5_1_1"
        (pin input line (at -8.89 2.54 0) (length 2.54)
          (name "CS")
          (number "1")
        )
        (pin power_in line (at 8.89 0 180) (length 2.54)
          (name "VSS")
          (number "2")
        )
        (pin input line (at -8.89 0 0) (length 2.54)
          (name "SCK")
          (number "3")
        )
        (pin bidirectional line (at -8.89 -2.54 0) (length 2.54)
          (name "SIO")
          (number "4")
        )
        (pin power_in line (at 8.89 2.54 180) (length 2.54)
          (name "VDD")
          (number "5")
        )
      )
    )
    (symbol "power:+3.3VA" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+3.3VA" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+3.3VA\"" (id 5) (at 0 0 0))
      (symbol "+3.3VA_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+3.3VA_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+3.3VA")
          (number "1")
        )
      )
    )
    (symbol "power:+5VD" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5VD" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5VD\"" (id 5) (at 0 0 0))
      (symbol "+5VD_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5VD_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5VD")
          (number "1")
        )
      )
    )
    (symbol "power:GNDD" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GNDD" (id 1) (at 0 -3.175 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GNDD\" , digital ground" (id 5) (at 0 0 0))
      (symbol "GNDD_0_1"
        (rectangle (start -1.27 -1.524) (end 1.27 -2.032)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "GNDD_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GNDD")
          (number "1")
        )
      )
    )
  )
  (junction (at 208.28 34.925) (diameter 0) (color 0 0 0 0))
  (junction (at 245.11 61.595) (diameter 0) (color 0 0 0 0))
  (junction (at 245.11 46.99) (diameter 0) (color 0 0 0 0))
  (junction (at 81.915 125.095) (diameter 0) (color 0 0 0 0))
  (junction (at 173.99 25.4) (diameter 0) (color 0 0 0 0))
  (junction (at 208.28 24.765) (diameter 0) (color 0 0 0 0))
  (junction (at 245.11 64.135) (diameter 0) (color 0 0 0 0))
  (junction (at 66.04 43.815) (diameter 0) (color 0 0 0 0))
  (junction (at 71.755 125.095) (diameter 0) (color 0 0 0 0))
  (junction (at 245.11 59.055) (diameter 0) (color 0 0 0 0))
  (junction (at 71.12 43.815) (diameter 0) (color 0 0 0 0))
  (junction (at 68.58 43.815) (diameter 0) (color 0 0 0 0))
  (junction (at 214.63 64.135) (diameter 0) (color 0 0 0 0))
  (junction (at 239.395 34.925) (diameter 0) (color 0 0 0 0))
  (junction (at 214.63 61.595) (diameter 0) (color 0 0 0 0))
  (junction (at 58.42 125.095) (diameter 0) (color 0 0 0 0))
  (junction (at 245.11 34.925) (diameter 0) (color 0 0 0 0))
  (junction (at 74.295 125.095) (diameter 0) (color 0 0 0 0))
  (junction (at 214.63 52.705) (diameter 0) (color 0 0 0 0))
  (junction (at 195.58 25.4) (diameter 0) (color 0 0 0 0))
  (junction (at 63.5 43.815) (diameter 0) (color 0 0 0 0))
  (junction (at 79.375 125.095) (diameter 0) (color 0 0 0 0))
  (junction (at 214.63 59.055) (diameter 0) (color 0 0 0 0))
  (junction (at 76.835 125.095) (diameter 0) (color 0 0 0 0))
  (wire (pts (xy 66.04 43.815) (xy 68.58 43.815)))
  (wire (pts (xy 245.11 59.055) (xy 245.11 56.515)))
  (wire (pts (xy 208.28 24.765) (xy 208.28 34.925)))
  (wire (pts (xy 66.04 125.095) (xy 71.755 125.095)))
  (wire (pts (xy 148.59 163.195) (xy 148.59 168.275)))
  (wire (pts (xy 265.43 121.285) (xy 266.065 121.285)))
  (wire (pts (xy 245.11 52.705) (xy 245.11 46.99)))
  (wire (pts (xy 79.375 125.095) (xy 81.915 125.095)))
  (wire (pts (xy 74.295 125.095) (xy 71.755 125.095)))
  (wire (pts (xy 76.835 125.095) (xy 74.295 125.095)))
  (wire (pts (xy 214.63 61.595) (xy 214.63 64.135)))
  (wire (pts (xy 173.99 25.4) (xy 175.26 25.4)))
  (wire (pts (xy 214.63 52.705) (xy 214.63 46.99)))
  (wire (pts (xy 155.575 160.655) (xy 155.575 168.275)))
  (wire (pts (xy 66.04 120.015) (xy 71.755 120.015)))
  (wire (pts (xy 214.63 56.515) (xy 214.63 59.055)))
  (wire (pts (xy 58.42 120.015) (xy 58.42 125.095)))
  (wire (pts (xy 208.915 22.225) (xy 208.28 22.225)))
  (wire (pts (xy 195.58 25.4) (xy 201.295 25.4)))
  (wire (pts (xy 76.835 125.095) (xy 79.375 125.095)))
  (wire (pts (xy 63.5 43.815) (xy 66.04 43.815)))
  (wire (pts (xy 230.505 24.765) (xy 245.11 24.765)))
  (wire (pts (xy 71.755 120.015) (xy 71.755 125.095)))
  (wire (pts (xy 131.445 163.195) (xy 148.59 163.195)))
  (wire (pts (xy 245.11 61.595) (xy 245.11 59.055)))
  (wire (pts (xy 190.5 25.4) (xy 195.58 25.4)))
  (wire (pts (xy 214.63 64.135) (xy 214.63 68.58)))
  (wire (pts (xy 245.11 61.595) (xy 245.11 64.135)))
  (wire (pts (xy 222.885 24.765) (xy 208.28 24.765)))
  (wire (pts (xy 245.11 69.215) (xy 245.11 64.135)))
  (wire (pts (xy 58.42 127.635) (xy 58.42 125.095)))
  (wire (pts (xy 201.295 25.4) (xy 201.295 34.925)))
  (wire (pts (xy 214.63 59.055) (xy 214.63 61.595)))
  (wire (pts (xy 71.12 43.815) (xy 75.565 43.815)))
  (wire (pts (xy 131.445 160.655) (xy 155.575 160.655)))
  (wire (pts (xy 245.11 34.925) (xy 245.11 46.99)))
  (wire (pts (xy 219.075 34.925) (xy 208.28 34.925)))
  (wire (pts (xy 234.315 34.925) (xy 239.395 34.925)))
  (wire (pts (xy 172.085 25.4) (xy 173.99 25.4)))
  (wire (pts (xy 201.295 34.925) (xy 203.2 34.925)))
  (wire (pts (xy 239.395 34.925) (xy 245.11 34.925)))
  (wire (pts (xy 245.11 46.99) (xy 214.63 46.99)))
  (wire (pts (xy 245.11 24.765) (xy 245.11 34.925)))
  (wire (pts (xy 59.055 43.815) (xy 63.5 43.815)))
  (wire (pts (xy 81.915 125.095) (xy 85.09 125.095)))
  (wire (pts (xy 167.005 25.4) (xy 164.465 25.4)))
  (wire (pts (xy 68.58 43.815) (xy 71.12 43.815)))
  (wire (pts (xy 208.28 22.225) (xy 208.28 24.765)))
  (text "Temperature sensor" (at 200.66 96.52 0))
  (text "JTAG header" (at 241.3 96.52 0))
  (text "R52/U19 depend on FPGA flavour:\nFor XC version:\n* mount U19\n* do not mount R52\n\nFor ZC version\n* do not mount U19\n* mount R52"
    (at 248.285 55.88 0)
  )
  (text "32MHz oscillator" (at 260.985 138.43 0))
  (label "3V_FPGA" (at 208.28 34.925 0))
  (label "TCS" (at 200.66 85.725 180))
  (label "TCK" (at 245.11 92.075 180))
  (label "FPGA_CLK" (at 54.61 79.375 180))
  (label "TCS" (at 54.61 61.595 180))
  (label "3V_FPGA" (at 222.25 109.855 0))
  (label "TDO" (at 245.11 86.995 180))
  (label "TDI" (at 245.11 89.535 180))
  (label "FPGA_CLK" (at 265.43 128.905 0))
  (label "TDI" (at 54.61 71.755 180))
  (label "TMS" (at 54.61 76.835 180))
  (label "3V_FPGA" (at 200.66 109.855 0))
  (label "3V_FPGA" (at 211.455 109.855 0))
  (label "TDAT" (at 54.61 66.675 180))
  (label "TCK" (at 54.61 74.295 180))
  (label "TMS" (at 257.81 86.995 0))
  (label "3V_FPGA" (at 257.81 121.285 180))
  (label "TDAT" (at 200.66 90.805 180))
  (label "TDO" (at 54.61 69.215 180))
  (label "3V_FPGA" (at 257.81 89.535 0))
  (label "3V_FPGA" (at 75.565 43.815 0))
  (label "3V_FPGA" (at 85.09 125.095 0))
  (label "3V_FPGA" (at 232.41 109.855 0))
  (label "TSCK" (at 200.66 88.265 180))
  (label "TSCK" (at 54.61 64.135 180))
  (label "3V_FPGA" (at 163.83 168.275 0))
  (label "3V_FPGA" (at 218.44 85.725 0))
  (global_label "3VFPGA" (shape input) (at 208.915 22.225 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 218.3433 22.1456 0))
  )
  (hierarchical_label "FC6" (shape input) (at 53.975 175.895 180))
  (hierarchical_label "FPGA_CTRL" (shape input) (at 53.975 163.195 180))
  (hierarchical_label "FC18" (shape input) (at 140.97 67.945 0))
  (hierarchical_label "FC32" (shape input) (at 140.97 95.885 0))
  (hierarchical_label "FC5" (shape input) (at 53.975 173.355 180))
  (hierarchical_label "FC9" (shape input) (at 53.975 168.275 180))
  (hierarchical_label "FC12" (shape input) (at 139.065 145.415 0))
  (hierarchical_label "FC29" (shape input) (at 140.97 90.805 0))
  (hierarchical_label "FC20" (shape input) (at 140.97 65.405 0))
  (hierarchical_label "FC14" (shape input) (at 139.065 155.575 0))
  (hierarchical_label "FC10" (shape input) (at 139.065 140.335 0))
  (hierarchical_label "FC3" (shape input) (at 140.97 100.965 0))
  (hierarchical_label "FC17" (shape input) (at 140.97 62.865 0))
  (hierarchical_label "FC19" (shape input) (at 140.97 60.325 0))
  (hierarchical_label "FC22" (shape input) (at 140.97 75.565 0))
  (hierarchical_label "FC1" (shape input) (at 140.97 106.045 0))
  (hierarchical_label "FC16" (shape input) (at 140.97 57.785 0))
  (hierarchical_label "FC2" (shape input) (at 140.97 103.505 0))
  (hierarchical_label "FC27" (shape input) (at 140.97 83.185 0))
  (hierarchical_label "FC21" (shape input) (at 140.97 70.485 0))
  (hierarchical_label "FC23" (shape input) (at 140.97 80.645 0))
  (hierarchical_label "FC25" (shape input) (at 140.97 73.025 0))
  (hierarchical_label "FC28" (shape input) (at 140.97 88.265 0))
  (hierarchical_label "FC15" (shape input) (at 139.065 158.115 0))
  (hierarchical_label "FC24" (shape input) (at 140.97 85.725 0))
  (hierarchical_label "FPGA_STB" (shape input) (at 53.975 160.655 180))
  (hierarchical_label "FPGA_TX" (shape input) (at 53.975 165.735 180))
  (hierarchical_label "FC26" (shape input) (at 140.97 78.105 0))
  (hierarchical_label "FC13" (shape input) (at 139.065 153.035 0))
  (hierarchical_label "FPGA_RX" (shape input) (at 53.975 158.115 180))
  (hierarchical_label "FC30" (shape input) (at 140.97 93.345 0))
  (hierarchical_label "FC11" (shape input) (at 139.065 142.875 0))
  (hierarchical_label "FC4" (shape input) (at 140.97 108.585 0))
  (hierarchical_label "FC31" (shape input) (at 140.97 98.425 0))
  (hierarchical_label "FC0" (shape input) (at 53.975 170.815 180))
  (symbol (lib_id "Gekkio_FPGA_Lattice:LCMXO2-1200xx-xTG100") (at 96.52 81.915 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U20" (id 0) (at 93.345 107.95 0))
    (property "Value" "LCMXO2-1200xx-xTG100" (id 1) (at 95.25 109.855 0))
    (property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm" (id 2) (at 96.52 117.475 0))
    (property "Datasheet" "https://www.latticesemi.com/view_document?document_id=38834" (id 3) (at 87.63 74.295 0))
    (property "comment" "" (id 4) (at 96.52 81.915 0))
    (property "PN" "XO21200HC4TG100C" (id 5) (at 96.52 81.915 0))
    (property "supplier" "MOUSER" (id 6) (at 96.52 81.915 0))
    (pin "51")
    (pin "52")
    (pin "53")
    (pin "54")
    (pin "55")
    (pin "57")
    (pin "58")
    (pin "59")
    (pin "60")
    (pin "61")
    (pin "62")
    (pin "63")
    (pin "64")
    (pin "65")
    (pin "66")
    (pin "67")
    (pin "68")
    (pin "69")
    (pin "70")
    (pin "71")
    (pin "73")
    (pin "74")
    (pin "75")
    (pin "76")
    (pin "77")
    (pin "78")
    (pin "80")
    (pin "81")
    (pin "82")
    (pin "83")
    (pin "84")
    (pin "85")
    (pin "86")
    (pin "87")
    (pin "88")
    (pin "89")
    (pin "90")
    (pin "91")
    (pin "93")
    (pin "94")
    (pin "95")
    (pin "96")
    (pin "97")
    (pin "98")
    (pin "99")
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "100")
    (pin "22")
    (pin "33")
    (pin "44")
    (pin "50")
    (pin "56")
    (pin "6")
    (pin "72")
    (pin "79")
    (pin "92")
  )
  (symbol (lib_id "Gekkio_FPGA_Lattice:LCMXO2-1200xx-xTG100") (at 95.885 163.195 0) (unit 2)
    (in_bom yes) (on_board yes)
    (property "Reference" "U20" (id 0) (at 101.6 132.715 0))
    (property "Value" "LCMXO2-1200xx-xTG100" (id 1) (at 111.125 134.62 0))
    (property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm" (id 2) (at 95.885 198.755 0))
    (property "Datasheet" "https://www.latticesemi.com/view_document?document_id=38834" (id 3) (at 86.995 155.575 0))
    (property "comment" "" (id 4) (at 95.885 163.195 0))
    (property "PN" "XO21200HC4TG100C" (id 5) (at 95.885 163.195 0))
    (property "supplier" "MOUSER" (id 6) (at 95.885 163.195 0))
    (pin "51")
    (pin "52")
    (pin "53")
    (pin "54")
    (pin "55")
    (pin "57")
    (pin "58")
    (pin "59")
    (pin "60")
    (pin "61")
    (pin "62")
    (pin "63")
    (pin "64")
    (pin "65")
    (pin "66")
    (pin "67")
    (pin "68")
    (pin "69")
    (pin "70")
    (pin "71")
    (pin "73")
    (pin "74")
    (pin "75")
    (pin "76")
    (pin "77")
    (pin "78")
    (pin "80")
    (pin "81")
    (pin "82")
    (pin "83")
    (pin "84")
    (pin "85")
    (pin "86")
    (pin "87")
    (pin "88")
    (pin "89")
    (pin "90")
    (pin "91")
    (pin "93")
    (pin "94")
    (pin "95")
    (pin "96")
    (pin "97")
    (pin "98")
    (pin "99")
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "100")
    (pin "22")
    (pin "33")
    (pin "44")
    (pin "50")
    (pin "56")
    (pin "6")
    (pin "72")
    (pin "79")
    (pin "92")
  )
  (symbol (lib_id "Gekkio_FPGA_Lattice:LCMXO2-1200xx-xTG100") (at 229.87 59.055 0) (unit 3)
    (in_bom yes) (on_board yes)
    (property "Reference" "U20" (id 0) (at 228.6 64.135 0))
    (property "Value" "LCMXO2-1200xx-xTG100" (id 1) (at 219.71 67.945 0))
    (property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm" (id 2) (at 229.87 94.615 0))
    (property "Datasheet" "https://www.latticesemi.com/view_document?document_id=38834" (id 3) (at 220.98 51.435 0))
    (property "comment" "" (id 4) (at 229.87 59.055 0))
    (property "PN" "XO21200HC4TG100C" (id 5) (at 229.87 59.055 0))
    (property "supplier" "MOUSER" (id 6) (at 229.87 59.055 0))
    (pin "51")
    (pin "52")
    (pin "53")
    (pin "54")
    (pin "55")
    (pin "57")
    (pin "58")
    (pin "59")
    (pin "60")
    (pin "61")
    (pin "62")
    (pin "63")
    (pin "64")
    (pin "65")
    (pin "66")
    (pin "67")
    (pin "68")
    (pin "69")
    (pin "70")
    (pin "71")
    (pin "73")
    (pin "74")
    (pin "75")
    (pin "76")
    (pin "77")
    (pin "78")
    (pin "80")
    (pin "81")
    (pin "82")
    (pin "83")
    (pin "84")
    (pin "85")
    (pin "86")
    (pin "87")
    (pin "88")
    (pin "89")
    (pin "90")
    (pin "91")
    (pin "93")
    (pin "94")
    (pin "95")
    (pin "96")
    (pin "97")
    (pin "98")
    (pin "99")
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "7")
    (pin "8")
    (pin "9")
    (pin "100")
    (pin "22")
    (pin "33")
    (pin "44")
    (pin "50")
    (pin "56")
    (pin "6")
    (pin "72")
    (pin "79")
    (pin "92")
  )
  (symbol (lib_id "power:+3.3VA") (at 267.335 19.685 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0150" (id 0) (at 267.335 23.495 0))
    (property "Value" "+3.3VA" (id 1) (at 267.716 15.2908 0))
    (property "Footprint" "" (id 2) (at 267.335 19.685 0))
    (property "Datasheet" "" (id 3) (at 267.335 19.685 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Ferrite_Bead_Small") (at 205.74 34.925 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "FB7" (id 0) (at 205.74 31.75 0))
    (property "Value" "Ferrite_Bead_Small" (id 1) (at 206.883 32.385 0))
    (property "Footprint" "Inductor_SMD:L_1206_3216Metric_Pad1.22x1.90mm_HandSolder" (id 2) (at 205.74 36.703 90))
    (property "Datasheet" "~" (id 3) (at 205.74 34.925 0))
    (property "comment" "" (id 4) (at 205.74 34.925 0))
    (property "PN" "BLM31A260SPT" (id 5) (at 205.74 34.925 0))
    (property "supplier" "TME" (id 6) (at 205.74 34.925 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 210.82 52.705 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C49" (id 0) (at 209.55 58.42 90))
    (property "Value" "100n" (id 1) (at 209.55 60.96 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 207.01 53.6702 0))
    (property "Datasheet" "~" (id 3) (at 210.82 52.705 0))
    (property "comment" "" (id 4) (at 210.82 52.705 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 210.82 52.705 0))
    (property "supplier" "TME" (id 6) (at 210.82 52.705 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 62.23 125.095 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C52" (id 0) (at 55.88 122.555 90))
    (property "Value" "100n" (id 1) (at 55.245 124.46 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 58.42 126.0602 0))
    (property "Datasheet" "~" (id 3) (at 62.23 125.095 0))
    (property "comment" "" (id 4) (at 62.23 125.095 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 62.23 125.095 0))
    (property "supplier" "TME" (id 6) (at 62.23 125.095 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 62.23 120.015 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C50" (id 0) (at 56.515 116.84 90))
    (property "Value" "100n" (id 1) (at 56.515 118.745 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 58.42 120.9802 0))
    (property "Datasheet" "~" (id 3) (at 62.23 120.015 0))
    (property "comment" "" (id 4) (at 62.23 120.015 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 62.23 120.015 0))
    (property "supplier" "TME" (id 6) (at 62.23 120.015 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector_Generic:Conn_02x03_Odd_Even") (at 250.19 89.535 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J7" (id 0) (at 251.46 83.82 0))
    (property "Value" "Conn_02x03_Odd_Even" (id 1) (at 251.46 83.7946 0))
    (property "Footprint" "Connector_IDC:IDC-Header_2x03_P2.54mm_Vertical" (id 2) (at 250.19 89.535 0))
    (property "Datasheet" "~" (id 3) (at 250.19 89.535 0))
    (property "comment" "" (id 4) (at 250.19 89.535 0))
    (property "PN" "75869-331LF" (id 5) (at 250.19 89.535 0))
    (property "supplier" "TME" (id 6) (at 250.19 89.535 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
  )
  (symbol (lib_id "jlib_1:tc77-SOT23-5") (at 209.55 88.265 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U21" (id 0) (at 209.55 78.994 0))
    (property "Value" "tc77-SOT23-5" (id 1) (at 209.55 81.3054 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23-5_HandSoldering" (id 2) (at 203.2 90.805 0))
    (property "Datasheet" "" (id 3) (at 203.2 90.805 0))
    (property "comment" "" (id 4) (at 209.55 88.265 0))
    (property "PN" "TC77-3.3MCTTR" (id 5) (at 209.55 88.265 0))
    (property "supplier" "MOUSER" (id 6) (at 209.55 88.265 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
  )
  (symbol (lib_id "Device:C") (at 55.245 43.815 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C48" (id 0) (at 55.245 38.1 90))
    (property "Value" "100n" (id 1) (at 55.245 40.005 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 59.055 42.8498 0))
    (property "Datasheet" "~" (id 3) (at 55.245 43.815 0))
    (property "comment" "" (id 4) (at 55.245 43.815 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 55.245 43.815 0))
    (property "supplier" "TME" (id 6) (at 55.245 43.815 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 155.575 179.705 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R89" (id 0) (at 153.035 178.435 90))
    (property "Value" "620R" (id 1) (at 150.495 177.165 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 157.353 179.705 90))
    (property "Datasheet" "~" (id 3) (at 155.575 179.705 0))
    (property "comment" "" (id 4) (at 155.575 179.705 0))
    (property "PN" "MMA02040C6200" (id 5) (at 155.575 179.705 0))
    (property "supplier" "TME" (id 6) (at 155.575 179.705 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 155.575 172.085 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D9" (id 0) (at 158.5722 171.0944 90))
    (property "Value" "LED" (id 1) (at 158.5722 173.4058 90))
    (property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (id 2) (at 155.575 172.085 0))
    (property "Datasheet" "~" (id 3) (at 155.575 172.085 0))
    (property "comment" "" (id 4) (at 155.575 172.085 0))
    (property "PN" "KP-2012YD" (id 5) (at 155.575 172.085 0))
    (property "supplier" "TME" (id 6) (at 155.575 172.085 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Oscillator:SG-5032CAN") (at 257.81 128.905 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "X1" (id 0) (at 252.095 135.255 0))
    (property "Value" "SG-5032CAN" (id 1) (at 256.54 137.16 0))
    (property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002LB-4Pin_5.0x3.2mm" (id 2) (at 275.59 137.795 0))
    (property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?dl=brief_SG5032CAN&lang=en" (id 3) (at 255.27 128.905 0))
    (property "comment" "" (id 4) (at 257.81 128.905 0))
    (property "PN" "5032CAN320M" (id 5) (at 257.81 128.905 0))
    (property "supplier" "MOUSER" (id 6) (at 257.81 128.905 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Device:C") (at 261.62 121.285 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C51" (id 0) (at 259.08 115.57 90))
    (property "Value" "100n" (id 1) (at 258.445 117.475 90))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 265.43 122.2502 0))
    (property "Datasheet" "~" (id 3) (at 261.62 121.285 0))
    (property "comment" "" (id 4) (at 261.62 121.285 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 261.62 121.285 0))
    (property "supplier" "TME" (id 6) (at 261.62 121.285 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 106.045 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R72" (id 0) (at 153.67 106.045 90))
    (property "Value" "24R" (id 1) (at 161.29 106.045 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 107.823 90))
    (property "Datasheet" "~" (id 3) (at 137.16 106.045 0))
    (property "comment" "" (id 4) (at 137.16 106.045 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 106.045 0))
    (property "supplier" "TME" (id 6) (at 137.16 106.045 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 103.505 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R71" (id 0) (at 153.67 103.505 90))
    (property "Value" "24R" (id 1) (at 161.29 103.505 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 105.283 90))
    (property "Datasheet" "~" (id 3) (at 137.16 103.505 0))
    (property "comment" "" (id 4) (at 137.16 103.505 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 103.505 0))
    (property "supplier" "TME" (id 6) (at 137.16 103.505 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 100.965 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R70" (id 0) (at 153.67 100.965 90))
    (property "Value" "24R" (id 1) (at 161.29 100.965 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 102.743 90))
    (property "Datasheet" "~" (id 3) (at 137.16 100.965 0))
    (property "comment" "" (id 4) (at 137.16 100.965 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 100.965 0))
    (property "supplier" "TME" (id 6) (at 137.16 100.965 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 108.585 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R73" (id 0) (at 153.67 108.585 90))
    (property "Value" "24R" (id 1) (at 161.29 108.585 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 106.807 90))
    (property "Datasheet" "~" (id 3) (at 137.16 108.585 0))
    (property "comment" "" (id 4) (at 137.16 108.585 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 108.585 0))
    (property "supplier" "TME" (id 6) (at 137.16 108.585 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 57.785 170.815 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R85" (id 0) (at 38.735 170.815 90))
    (property "Value" "24R" (id 1) (at 31.115 170.815 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.785 169.037 90))
    (property "Datasheet" "~" (id 3) (at 57.785 170.815 0))
    (property "comment" "" (id 4) (at 57.785 170.815 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 57.785 170.815 0))
    (property "supplier" "TME" (id 6) (at 57.785 170.815 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 57.785 173.355 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R86" (id 0) (at 38.735 173.355 90))
    (property "Value" "24R" (id 1) (at 31.115 173.355 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.785 171.577 90))
    (property "Datasheet" "~" (id 3) (at 57.785 173.355 0))
    (property "comment" "" (id 4) (at 57.785 173.355 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 57.785 173.355 0))
    (property "supplier" "TME" (id 6) (at 57.785 173.355 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 57.785 175.895 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R87" (id 0) (at 38.735 175.895 90))
    (property "Value" "24R" (id 1) (at 31.115 175.895 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.785 174.117 90))
    (property "Datasheet" "~" (id 3) (at 57.785 175.895 0))
    (property "comment" "" (id 4) (at 57.785 175.895 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 57.785 175.895 0))
    (property "supplier" "TME" (id 6) (at 57.785 175.895 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 57.785 168.275 270) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R84" (id 0) (at 38.735 168.275 90))
    (property "Value" "24R" (id 1) (at 31.115 168.275 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.785 170.053 90))
    (property "Datasheet" "~" (id 3) (at 57.785 168.275 0))
    (property "comment" "" (id 4) (at 57.785 168.275 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 57.785 168.275 0))
    (property "supplier" "TME" (id 6) (at 57.785 168.275 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 135.255 140.335 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R74" (id 0) (at 151.765 140.335 90))
    (property "Value" "24R" (id 1) (at 159.385 140.335 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 135.255 138.557 90))
    (property "Datasheet" "~" (id 3) (at 135.255 140.335 0))
    (property "comment" "" (id 4) (at 135.255 140.335 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 135.255 140.335 0))
    (property "supplier" "TME" (id 6) (at 135.255 140.335 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 135.255 142.875 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R75" (id 0) (at 151.765 142.875 90))
    (property "Value" "24R" (id 1) (at 159.385 142.875 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 135.255 141.097 90))
    (property "Datasheet" "~" (id 3) (at 135.255 142.875 0))
    (property "comment" "" (id 4) (at 135.255 142.875 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 135.255 142.875 0))
    (property "supplier" "TME" (id 6) (at 135.255 142.875 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 135.255 145.415 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R76" (id 0) (at 151.765 145.415 90))
    (property "Value" "24R" (id 1) (at 159.385 145.415 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 135.255 143.637 90))
    (property "Datasheet" "~" (id 3) (at 135.255 145.415 0))
    (property "comment" "" (id 4) (at 135.255 145.415 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 135.255 145.415 0))
    (property "supplier" "TME" (id 6) (at 135.255 145.415 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 158.75 29.21 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C44" (id 0) (at 153.035 27.94 0))
    (property "Value" "100n" (id 1) (at 152.4 30.48 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 157.7848 25.4 0))
    (property "Datasheet" "~" (id 3) (at 158.75 29.21 0))
    (property "comment" "" (id 4) (at 158.75 29.21 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 158.75 29.21 0))
    (property "supplier" "TME" (id 6) (at 158.75 29.21 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Ferrite_Bead_Small") (at 169.545 25.4 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "FB6" (id 0) (at 169.545 22.225 0))
    (property "Value" "Ferrite_Bead_Small" (id 1) (at 170.688 22.86 0))
    (property "Footprint" "Inductor_SMD:L_1206_3216Metric_Pad1.22x1.90mm_HandSolder" (id 2) (at 169.545 27.178 90))
    (property "Datasheet" "~" (id 3) (at 169.545 25.4 0))
    (property "comment" "" (id 4) (at 169.545 25.4 0))
    (property "PN" "BLM31A260SPT" (id 5) (at 169.545 25.4 0))
    (property "supplier" "TME" (id 6) (at 169.545 25.4 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 173.99 29.21 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C45" (id 0) (at 168.275 29.845 0))
    (property "Value" "100n" (id 1) (at 168.275 31.75 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 173.0248 25.4 0))
    (property "Datasheet" "~" (id 3) (at 173.99 29.21 0))
    (property "comment" "" (id 4) (at 173.99 29.21 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 173.99 29.21 0))
    (property "supplier" "TME" (id 6) (at 173.99 29.21 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Regulator_Linear:MCP1700-1202E_SOT23") (at 226.695 34.925 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U19" (id 0) (at 226.695 28.7782 0))
    (property "Value" "DNP-MCP1700-12" (id 1) (at 226.695 31.0896 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 226.695 29.21 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf" (id 3) (at 226.695 34.925 0))
    (property "comment" "DNP" (id 4) (at 226.695 34.925 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Regulator_Linear:MCP1700-1202E_SOT23") (at 182.88 25.4 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U18" (id 0) (at 182.88 19.2532 0))
    (property "Value" "MCP1700-33" (id 1) (at 182.88 21.5646 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-23" (id 2) (at 182.88 19.685 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001826D.pdf" (id 3) (at 182.88 25.4 0))
    (property "comment" "" (id 4) (at 182.88 25.4 0))
    (property "PN" "MCP1700T-3302E" (id 5) (at 182.88 25.4 0))
    (property "supplier" "MOUSER" (id 6) (at 182.88 25.4 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "Device:C") (at 222.25 113.665 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C42" (id 0) (at 217.17 113.03 0))
    (property "Value" "100n" (id 1) (at 216.535 115.57 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 221.2848 109.855 0))
    (property "Datasheet" "~" (id 3) (at 222.25 113.665 0))
    (property "comment" "" (id 4) (at 222.25 113.665 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 222.25 113.665 0))
    (property "supplier" "TME" (id 6) (at 222.25 113.665 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 57.785 165.735 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R83" (id 0) (at 38.735 165.735 90))
    (property "Value" "24R" (id 1) (at 31.115 165.735 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.785 163.957 90))
    (property "Datasheet" "~" (id 3) (at 57.785 165.735 0))
    (property "comment" "" (id 4) (at 57.785 165.735 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 57.785 165.735 0))
    (property "supplier" "TME" (id 6) (at 57.785 165.735 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 214.63 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0166" (id 0) (at 214.63 74.93 0))
    (property "Value" "GNDD" (id 1) (at 214.63 72.7615 0))
    (property "Footprint" "" (id 2) (at 214.63 68.58 0))
    (property "Datasheet" "" (id 3) (at 214.63 68.58 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 137.16 60.325 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R54" (id 0) (at 153.67 60.325 90))
    (property "Value" "24R" (id 1) (at 161.29 60.325 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 58.547 90))
    (property "Datasheet" "~" (id 3) (at 137.16 60.325 0))
    (property "comment" "" (id 4) (at 137.16 60.325 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 60.325 0))
    (property "supplier" "TME" (id 6) (at 137.16 60.325 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 257.81 92.075 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0169" (id 0) (at 257.81 98.425 0))
    (property "Value" "GNDD" (id 1) (at 257.81 96.2565 0))
    (property "Footprint" "" (id 2) (at 257.81 92.075 0))
    (property "Datasheet" "" (id 3) (at 257.81 92.075 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 148.59 183.515 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0174" (id 0) (at 148.59 189.865 0))
    (property "Value" "GNDD" (id 1) (at 147.955 187.325 0))
    (property "Footprint" "" (id 2) (at 148.59 183.515 0))
    (property "Datasheet" "" (id 3) (at 148.59 183.515 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 226.695 42.545 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0162" (id 0) (at 226.695 48.895 0))
    (property "Value" "GNDD" (id 1) (at 231.14 45.085 0))
    (property "Footprint" "" (id 2) (at 226.695 42.545 0))
    (property "Datasheet" "" (id 3) (at 226.695 42.545 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 182.88 33.02 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0160" (id 0) (at 182.88 39.37 0))
    (property "Value" "GNDD" (id 1) (at 182.88 37.2015 0))
    (property "Footprint" "" (id 2) (at 182.88 33.02 0))
    (property "Datasheet" "" (id 3) (at 182.88 33.02 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 57.785 158.115 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R79" (id 0) (at 38.735 158.115 90))
    (property "Value" "24R" (id 1) (at 31.115 158.115 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.785 156.337 90))
    (property "Datasheet" "~" (id 3) (at 57.785 158.115 0))
    (property "comment" "" (id 4) (at 57.785 158.115 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 57.785 158.115 0))
    (property "supplier" "TME" (id 6) (at 57.785 158.115 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5VD") (at 158.75 25.4 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0155" (id 0) (at 158.75 29.21 0))
    (property "Value" "+5VD" (id 1) (at 158.75 21.7955 0))
    (property "Footprint" "" (id 2) (at 158.75 25.4 0))
    (property "Datasheet" "" (id 3) (at 158.75 25.4 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 195.58 33.02 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0161" (id 0) (at 195.58 39.37 0))
    (property "Value" "GNDD" (id 1) (at 195.58 37.2015 0))
    (property "Footprint" "" (id 2) (at 195.58 33.02 0))
    (property "Datasheet" "" (id 3) (at 195.58 33.02 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 158.75 33.02 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0158" (id 0) (at 158.75 39.37 0))
    (property "Value" "GNDD" (id 1) (at 158.75 37.2015 0))
    (property "Footprint" "" (id 2) (at 158.75 33.02 0))
    (property "Datasheet" "" (id 3) (at 158.75 33.02 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 131.445 180.975 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP10" (id 0) (at 135.89 180.975 90))
    (property "Value" "TestPoint" (id 1) (at 136.144 182.8416 90))
    (property "Footprint" "TestPoint:TestPoint_Pad_1.5x1.5mm" (id 2) (at 131.445 186.055 0))
    (property "Datasheet" "~" (id 3) (at 131.445 186.055 0))
    (property "comment" "DNP" (id 4) (at 131.445 180.975 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 135.255 155.575 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R78" (id 0) (at 151.765 155.575 90))
    (property "Value" "24R" (id 1) (at 159.385 155.575 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 135.255 153.797 90))
    (property "Datasheet" "~" (id 3) (at 135.255 155.575 0))
    (property "comment" "" (id 4) (at 135.255 155.575 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 135.255 155.575 0))
    (property "supplier" "TME" (id 6) (at 135.255 155.575 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 57.785 163.195 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R82" (id 0) (at 38.735 163.195 90))
    (property "Value" "24R" (id 1) (at 31.115 163.195 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.785 161.417 90))
    (property "Datasheet" "~" (id 3) (at 57.785 163.195 0))
    (property "comment" "" (id 4) (at 57.785 163.195 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 57.785 163.195 0))
    (property "supplier" "TME" (id 6) (at 57.785 163.195 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 90.805 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R66" (id 0) (at 153.67 90.805 90))
    (property "Value" "24R" (id 1) (at 161.29 90.805 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 92.583 90))
    (property "Datasheet" "~" (id 3) (at 137.16 90.805 0))
    (property "comment" "" (id 4) (at 137.16 90.805 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 90.805 0))
    (property "supplier" "TME" (id 6) (at 137.16 90.805 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 42.545 139.7 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0173" (id 0) (at 42.545 146.05 0))
    (property "Value" "GNDD" (id 1) (at 42.545 143.8815 0))
    (property "Footprint" "" (id 2) (at 42.545 139.7 0))
    (property "Datasheet" "" (id 3) (at 42.545 139.7 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 148.59 179.705 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R88" (id 0) (at 146.05 178.435 90))
    (property "Value" "620R" (id 1) (at 143.51 177.165 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 150.368 179.705 90))
    (property "Datasheet" "~" (id 3) (at 148.59 179.705 0))
    (property "comment" "" (id 4) (at 148.59 179.705 0))
    (property "PN" "MMA02040C6200" (id 5) (at 148.59 179.705 0))
    (property "supplier" "TME" (id 6) (at 148.59 179.705 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 95.885 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R68" (id 0) (at 153.67 95.885 90))
    (property "Value" "24R" (id 1) (at 161.29 95.885 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 97.663 90))
    (property "Datasheet" "~" (id 3) (at 137.16 95.885 0))
    (property "comment" "" (id 4) (at 137.16 95.885 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 95.885 0))
    (property "supplier" "TME" (id 6) (at 137.16 95.885 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 232.41 117.475 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0154" (id 0) (at 232.41 123.825 0))
    (property "Value" "GNDD" (id 1) (at 232.41 121.6565 0))
    (property "Footprint" "" (id 2) (at 232.41 117.475 0))
    (property "Datasheet" "" (id 3) (at 232.41 117.475 0))
    (pin "1")
  )
  (symbol (lib_id "Device:LED") (at 163.83 172.085 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D10" (id 0) (at 166.8272 171.0944 90))
    (property "Value" "LED" (id 1) (at 166.8272 173.4058 90))
    (property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (id 2) (at 163.83 172.085 0))
    (property "Datasheet" "~" (id 3) (at 163.83 172.085 0))
    (property "comment" "" (id 4) (at 163.83 172.085 0))
    (property "PN" "KP-2012YD" (id 5) (at 163.83 172.085 0))
    (property "supplier" "TME" (id 6) (at 163.83 172.085 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint") (at 131.445 173.355 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP7" (id 0) (at 135.89 173.355 90))
    (property "Value" "TestPoint" (id 1) (at 136.144 175.2216 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded" (id 2) (at 131.445 178.435 0))
    (property "Datasheet" "~" (id 3) (at 131.445 178.435 0))
    (property "comment" "" (id 4) (at 131.445 173.355 0))
    (property "PN" "optional" (id 5) (at 131.445 173.355 0))
    (property "supplier" "aliexpress" (id 6) (at 131.445 173.355 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 131.445 168.275 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP5" (id 0) (at 135.89 168.275 90))
    (property "Value" "TestPoint" (id 1) (at 136.144 170.1416 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded" (id 2) (at 131.445 173.355 0))
    (property "Datasheet" "~" (id 3) (at 131.445 173.355 0))
    (property "comment" "" (id 4) (at 131.445 168.275 0))
    (property "PN" "optional" (id 5) (at 131.445 168.275 0))
    (property "supplier" "aliexpress" (id 6) (at 131.445 168.275 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 226.695 24.765 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R52" (id 0) (at 226.06 19.685 90))
    (property "Value" "0R" (id 1) (at 226.06 22.225 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 226.695 22.987 90))
    (property "Datasheet" "~" (id 3) (at 226.695 24.765 0))
    (property "comment" "" (id 4) (at 226.695 24.765 0))
    (property "PN" "SMDMM0204-0R" (id 5) (at 226.695 24.765 0))
    (property "supplier" "TME" (id 6) (at 226.695 24.765 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint") (at 131.445 186.055 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP11" (id 0) (at 135.89 186.055 90))
    (property "Value" "TestPoint" (id 1) (at 136.144 187.9216 90))
    (property "Footprint" "TestPoint:TestPoint_Pad_1.5x1.5mm" (id 2) (at 131.445 191.135 0))
    (property "Datasheet" "~" (id 3) (at 131.445 191.135 0))
    (property "comment" "DNP" (id 4) (at 131.445 186.055 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 200.66 113.665 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C40" (id 0) (at 195.58 113.03 0))
    (property "Value" "100n" (id 1) (at 194.945 115.57 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 199.6948 109.855 0))
    (property "Datasheet" "~" (id 3) (at 200.66 113.665 0))
    (property "comment" "" (id 4) (at 200.66 113.665 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 200.66 113.665 0))
    (property "supplier" "TME" (id 6) (at 200.66 113.665 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 195.58 29.21 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C46" (id 0) (at 189.865 29.845 0))
    (property "Value" "2u2" (id 1) (at 189.865 31.75 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 194.6148 25.4 0))
    (property "Datasheet" "~" (id 3) (at 195.58 29.21 0))
    (property "comment" "" (id 4) (at 195.58 29.21 0))
    (property "PN" "CL21B225KPFNNNE" (id 5) (at 195.58 29.21 0))
    (property "supplier" "TME" (id 6) (at 195.58 29.21 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 200.66 117.475 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0151" (id 0) (at 200.66 123.825 0))
    (property "Value" "GNDD" (id 1) (at 200.66 121.6565 0))
    (property "Footprint" "" (id 2) (at 200.66 117.475 0))
    (property "Datasheet" "" (id 3) (at 200.66 117.475 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 211.455 117.475 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0152" (id 0) (at 211.455 123.825 0))
    (property "Value" "GNDD" (id 1) (at 211.455 121.6565 0))
    (property "Footprint" "" (id 2) (at 211.455 117.475 0))
    (property "Datasheet" "" (id 3) (at 211.455 117.475 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 137.16 83.185 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R63" (id 0) (at 153.67 83.185 90))
    (property "Value" "24R" (id 1) (at 161.29 83.185 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 84.963 90))
    (property "Datasheet" "~" (id 3) (at 137.16 83.185 0))
    (property "comment" "" (id 4) (at 137.16 83.185 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 83.185 0))
    (property "supplier" "TME" (id 6) (at 137.16 83.185 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 222.25 117.475 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0153" (id 0) (at 222.25 123.825 0))
    (property "Value" "GNDD" (id 1) (at 222.25 121.6565 0))
    (property "Footprint" "" (id 2) (at 222.25 117.475 0))
    (property "Datasheet" "" (id 3) (at 222.25 117.475 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 131.445 170.815 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP6" (id 0) (at 135.89 170.815 90))
    (property "Value" "TestPoint" (id 1) (at 136.144 172.6816 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded" (id 2) (at 131.445 175.895 0))
    (property "Datasheet" "~" (id 3) (at 131.445 175.895 0))
    (property "comment" "" (id 4) (at 131.445 170.815 0))
    (property "PN" "optional" (id 5) (at 131.445 170.815 0))
    (property "supplier" "aliexpress" (id 6) (at 131.445 170.815 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 163.83 179.705 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R90" (id 0) (at 161.29 178.435 90))
    (property "Value" "620R" (id 1) (at 158.75 177.165 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 165.608 179.705 90))
    (property "Datasheet" "~" (id 3) (at 163.83 179.705 0))
    (property "comment" "" (id 4) (at 163.83 179.705 0))
    (property "PN" "MMA02040C6200" (id 5) (at 163.83 179.705 0))
    (property "supplier" "TME" (id 6) (at 163.83 179.705 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 67.945 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R57" (id 0) (at 153.67 67.945 90))
    (property "Value" "24R" (id 1) (at 161.29 67.945 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 66.167 90))
    (property "Datasheet" "~" (id 3) (at 137.16 67.945 0))
    (property "comment" "" (id 4) (at 137.16 67.945 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 67.945 0))
    (property "supplier" "TME" (id 6) (at 137.16 67.945 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 257.81 136.525 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0172" (id 0) (at 257.81 142.875 0))
    (property "Value" "GNDD" (id 1) (at 257.81 140.7065 0))
    (property "Footprint" "" (id 2) (at 257.81 136.525 0))
    (property "Datasheet" "" (id 3) (at 257.81 136.525 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 61.595 142.875 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP3" (id 0) (at 57.15 142.875 90))
    (property "Value" "TestPoint" (id 1) (at 56.896 141.0084 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (id 2) (at 61.595 137.795 0))
    (property "Datasheet" "~" (id 3) (at 61.595 137.795 0))
    (property "comment" "" (id 4) (at 61.595 142.875 0))
    (property "PN" "optional" (id 5) (at 61.595 142.875 0))
    (property "supplier" "aliexpress" (id 6) (at 61.595 142.875 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 58.42 127.635 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0171" (id 0) (at 58.42 133.985 0))
    (property "Value" "GNDD" (id 1) (at 58.42 131.8165 0))
    (property "Footprint" "" (id 2) (at 58.42 127.635 0))
    (property "Datasheet" "" (id 3) (at 58.42 127.635 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 61.595 140.335 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP2" (id 0) (at 57.15 140.335 90))
    (property "Value" "TestPoint" (id 1) (at 56.896 138.4684 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (id 2) (at 61.595 135.255 0))
    (property "Datasheet" "~" (id 3) (at 61.595 135.255 0))
    (property "comment" "" (id 4) (at 61.595 140.335 0))
    (property "PN" "optional" (id 5) (at 61.595 140.335 0))
    (property "supplier" "aliexpress" (id 6) (at 61.595 140.335 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 131.445 188.595 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP12" (id 0) (at 135.89 188.595 90))
    (property "Value" "TestPoint" (id 1) (at 136.144 190.4616 90))
    (property "Footprint" "TestPoint:TestPoint_Pad_1.5x1.5mm" (id 2) (at 131.445 193.675 0))
    (property "Datasheet" "~" (id 3) (at 131.445 193.675 0))
    (property "comment" "DNP" (id 4) (at 131.445 188.595 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 232.41 113.665 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C43" (id 0) (at 227.33 113.03 0))
    (property "Value" "100n" (id 1) (at 226.695 115.57 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 231.4448 109.855 0))
    (property "Datasheet" "~" (id 3) (at 232.41 113.665 0))
    (property "comment" "" (id 4) (at 232.41 113.665 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 232.41 113.665 0))
    (property "supplier" "TME" (id 6) (at 232.41 113.665 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 211.455 113.665 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C41" (id 0) (at 206.375 113.03 0))
    (property "Value" "100n" (id 1) (at 205.74 115.57 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 210.4898 109.855 0))
    (property "Datasheet" "~" (id 3) (at 211.455 113.665 0))
    (property "comment" "" (id 4) (at 211.455 113.665 0))
    (property "PN" "CL21B104KBCNNNC" (id 5) (at 211.455 113.665 0))
    (property "supplier" "TME" (id 6) (at 211.455 113.665 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 51.435 43.815 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0164" (id 0) (at 51.435 50.165 0))
    (property "Value" "GNDD" (id 1) (at 51.435 47.9965 0))
    (property "Footprint" "" (id 2) (at 51.435 43.815 0))
    (property "Datasheet" "" (id 3) (at 51.435 43.815 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 267.335 25.4 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0157" (id 0) (at 267.335 31.75 0))
    (property "Value" "GNDD" (id 1) (at 267.335 29.5815 0))
    (property "Footprint" "" (id 2) (at 267.335 25.4 0))
    (property "Datasheet" "" (id 3) (at 267.335 25.4 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 218.44 88.265 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0168" (id 0) (at 218.44 94.615 0))
    (property "Value" "GNDD" (id 1) (at 218.44 92.4465 0))
    (property "Footprint" "" (id 2) (at 218.44 88.265 0))
    (property "Datasheet" "" (id 3) (at 218.44 88.265 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 137.16 62.865 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R55" (id 0) (at 153.67 62.865 90))
    (property "Value" "24R" (id 1) (at 161.29 62.865 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 61.087 90))
    (property "Datasheet" "~" (id 3) (at 137.16 62.865 0))
    (property "comment" "" (id 4) (at 137.16 62.865 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 62.865 0))
    (property "supplier" "TME" (id 6) (at 137.16 62.865 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 85.725 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R64" (id 0) (at 153.67 85.725 90))
    (property "Value" "24R" (id 1) (at 161.29 85.725 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 87.503 90))
    (property "Datasheet" "~" (id 3) (at 137.16 85.725 0))
    (property "comment" "" (id 4) (at 137.16 85.725 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 85.725 0))
    (property "supplier" "TME" (id 6) (at 137.16 85.725 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 266.065 121.285 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0170" (id 0) (at 266.065 127.635 0))
    (property "Value" "GNDD" (id 1) (at 266.065 125.4665 0))
    (property "Footprint" "" (id 2) (at 266.065 121.285 0))
    (property "Datasheet" "" (id 3) (at 266.065 121.285 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 131.445 175.895 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP8" (id 0) (at 135.89 175.895 90))
    (property "Value" "TestPoint" (id 1) (at 136.144 177.7616 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D1.80mm_Drill1.0mm_Beaded" (id 2) (at 131.445 180.975 0))
    (property "Datasheet" "~" (id 3) (at 131.445 180.975 0))
    (property "comment" "" (id 4) (at 131.445 175.895 0))
    (property "PN" "optional" (id 5) (at 131.445 175.895 0))
    (property "supplier" "aliexpress" (id 6) (at 131.445 175.895 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 135.255 158.115 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R80" (id 0) (at 151.765 158.115 90))
    (property "Value" "24R" (id 1) (at 159.385 158.115 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 135.255 156.337 90))
    (property "Datasheet" "~" (id 3) (at 135.255 158.115 0))
    (property "comment" "" (id 4) (at 135.255 158.115 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 135.255 158.115 0))
    (property "supplier" "TME" (id 6) (at 135.255 158.115 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 78.105 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R61" (id 0) (at 153.67 78.105 90))
    (property "Value" "24R" (id 1) (at 161.29 78.105 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 79.883 90))
    (property "Datasheet" "~" (id 3) (at 137.16 78.105 0))
    (property "comment" "" (id 4) (at 137.16 78.105 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 78.105 0))
    (property "supplier" "TME" (id 6) (at 137.16 78.105 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint") (at 61.595 145.415 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP4" (id 0) (at 57.15 145.415 90))
    (property "Value" "TestPoint" (id 1) (at 56.896 143.5484 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (id 2) (at 61.595 140.335 0))
    (property "Datasheet" "~" (id 3) (at 61.595 140.335 0))
    (property "comment" "" (id 4) (at 61.595 145.415 0))
    (property "PN" "optional" (id 5) (at 61.595 145.415 0))
    (property "supplier" "aliexpress" (id 6) (at 61.595 145.415 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 239.395 42.545 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0163" (id 0) (at 239.395 48.895 0))
    (property "Value" "GNDD" (id 1) (at 241.3 45.72 0))
    (property "Footprint" "" (id 2) (at 239.395 42.545 0))
    (property "Datasheet" "" (id 3) (at 239.395 42.545 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 137.16 80.645 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R62" (id 0) (at 153.67 80.645 90))
    (property "Value" "24R" (id 1) (at 161.29 80.645 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 82.423 90))
    (property "Datasheet" "~" (id 3) (at 137.16 80.645 0))
    (property "comment" "" (id 4) (at 137.16 80.645 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 80.645 0))
    (property "supplier" "TME" (id 6) (at 137.16 80.645 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5VD") (at 164.465 25.4 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0156" (id 0) (at 164.465 29.21 0))
    (property "Value" "+5VD" (id 1) (at 164.465 21.7955 0))
    (property "Footprint" "" (id 2) (at 164.465 25.4 0))
    (property "Datasheet" "" (id 3) (at 164.465 25.4 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 137.16 93.345 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R67" (id 0) (at 153.67 93.345 90))
    (property "Value" "24R" (id 1) (at 161.29 93.345 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 95.123 90))
    (property "Datasheet" "~" (id 3) (at 137.16 93.345 0))
    (property "comment" "" (id 4) (at 137.16 93.345 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 93.345 0))
    (property "supplier" "TME" (id 6) (at 137.16 93.345 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 75.565 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R60" (id 0) (at 153.67 75.565 90))
    (property "Value" "24R" (id 1) (at 161.29 75.565 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 73.787 90))
    (property "Datasheet" "~" (id 3) (at 137.16 75.565 0))
    (property "comment" "" (id 4) (at 137.16 75.565 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 75.565 0))
    (property "supplier" "TME" (id 6) (at 137.16 75.565 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 73.025 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R59" (id 0) (at 153.67 73.025 90))
    (property "Value" "24R" (id 1) (at 161.29 73.025 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 74.803 90))
    (property "Datasheet" "~" (id 3) (at 137.16 73.025 0))
    (property "comment" "" (id 4) (at 137.16 73.025 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 73.025 0))
    (property "supplier" "TME" (id 6) (at 137.16 73.025 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Connector:TestPoint") (at 42.545 139.7 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP1" (id 0) (at 38.1 139.7 90))
    (property "Value" "TestPoint" (id 1) (at 37.846 137.8334 90))
    (property "Footprint" "TestPoint:TestPoint_Loop_D2.60mm_Drill1.6mm_Beaded" (id 2) (at 42.545 134.62 0))
    (property "Datasheet" "~" (id 3) (at 42.545 134.62 0))
    (property "comment" "" (id 4) (at 42.545 139.7 0))
    (property "PN" "optional" (id 5) (at 42.545 139.7 0))
    (property "supplier" "aliexpress" (id 6) (at 42.545 139.7 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 163.83 183.515 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0176" (id 0) (at 163.83 189.865 0))
    (property "Value" "GNDD" (id 1) (at 163.83 187.325 0))
    (property "Footprint" "" (id 2) (at 163.83 183.515 0))
    (property "Datasheet" "" (id 3) (at 163.83 183.515 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 155.575 183.515 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0175" (id 0) (at 155.575 189.865 0))
    (property "Value" "GNDD" (id 1) (at 154.94 187.325 0))
    (property "Footprint" "" (id 2) (at 155.575 183.515 0))
    (property "Datasheet" "" (id 3) (at 155.575 183.515 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 245.11 69.215 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0167" (id 0) (at 245.11 75.565 0))
    (property "Value" "GNDD" (id 1) (at 245.11 73.3965 0))
    (property "Footprint" "" (id 2) (at 245.11 69.215 0))
    (property "Datasheet" "" (id 3) (at 245.11 69.215 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:TestPoint") (at 131.445 178.435 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "TP9" (id 0) (at 135.89 178.435 90))
    (property "Value" "TestPoint" (id 1) (at 136.144 180.3016 90))
    (property "Footprint" "TestPoint:TestPoint_Pad_1.5x1.5mm" (id 2) (at 131.445 183.515 0))
    (property "Datasheet" "~" (id 3) (at 131.445 183.515 0))
    (property "comment" "DNP" (id 4) (at 131.445 178.435 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 137.16 65.405 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R56" (id 0) (at 153.67 65.405 90))
    (property "Value" "24R" (id 1) (at 161.29 65.405 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 63.627 90))
    (property "Datasheet" "~" (id 3) (at 137.16 65.405 0))
    (property "comment" "" (id 4) (at 137.16 65.405 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 65.405 0))
    (property "supplier" "TME" (id 6) (at 137.16 65.405 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDD") (at 207.01 52.705 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0165" (id 0) (at 207.01 59.055 0))
    (property "Value" "GNDD" (id 1) (at 207.01 56.8865 0))
    (property "Footprint" "" (id 2) (at 207.01 52.705 0))
    (property "Datasheet" "" (id 3) (at 207.01 52.705 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDD") (at 173.99 33.02 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0159" (id 0) (at 173.99 39.37 0))
    (property "Value" "GNDD" (id 1) (at 173.99 37.2015 0))
    (property "Footprint" "" (id 2) (at 173.99 33.02 0))
    (property "Datasheet" "" (id 3) (at 173.99 33.02 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R") (at 137.16 98.425 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R69" (id 0) (at 153.67 98.425 90))
    (property "Value" "24R" (id 1) (at 161.29 98.425 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 100.203 90))
    (property "Datasheet" "~" (id 3) (at 137.16 98.425 0))
    (property "comment" "" (id 4) (at 137.16 98.425 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 98.425 0))
    (property "supplier" "TME" (id 6) (at 137.16 98.425 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 239.395 38.735 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C47" (id 0) (at 233.68 39.37 0))
    (property "Value" "2u2" (id 1) (at 233.68 41.275 0))
    (property "Footprint" "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder" (id 2) (at 238.4298 34.925 0))
    (property "Datasheet" "~" (id 3) (at 239.395 38.735 0))
    (property "comment" "" (id 4) (at 239.395 38.735 0))
    (property "PN" "CL21B225KPFNNNE" (id 5) (at 239.395 38.735 0))
    (property "supplier" "TME" (id 6) (at 239.395 38.735 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 57.785 160.655 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R81" (id 0) (at 38.735 160.655 90))
    (property "Value" "24R" (id 1) (at 31.115 160.655 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 57.785 158.877 90))
    (property "Datasheet" "~" (id 3) (at 57.785 160.655 0))
    (property "comment" "" (id 4) (at 57.785 160.655 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 57.785 160.655 0))
    (property "supplier" "TME" (id 6) (at 57.785 160.655 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:LED") (at 148.59 172.085 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "D8" (id 0) (at 151.5872 171.0944 90))
    (property "Value" "LED" (id 1) (at 151.5872 173.4058 90))
    (property "Footprint" "LED_SMD:LED_0805_2012Metric_Pad1.15x1.40mm_HandSolder" (id 2) (at 148.59 172.085 0))
    (property "Datasheet" "~" (id 3) (at 148.59 172.085 0))
    (property "comment" "" (id 4) (at 148.59 172.085 0))
    (property "PN" "KP-2012YD" (id 5) (at 148.59 172.085 0))
    (property "supplier" "TME" (id 6) (at 148.59 172.085 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 135.255 153.035 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R77" (id 0) (at 151.765 153.035 90))
    (property "Value" "24R" (id 1) (at 159.385 153.035 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 135.255 151.257 90))
    (property "Datasheet" "~" (id 3) (at 135.255 153.035 0))
    (property "comment" "" (id 4) (at 135.255 153.035 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 135.255 153.035 0))
    (property "supplier" "TME" (id 6) (at 135.255 153.035 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 70.485 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R58" (id 0) (at 153.67 70.485 90))
    (property "Value" "24R" (id 1) (at 161.29 70.485 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 68.707 90))
    (property "Datasheet" "~" (id 3) (at 137.16 70.485 0))
    (property "comment" "" (id 4) (at 137.16 70.485 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 70.485 0))
    (property "supplier" "TME" (id 6) (at 137.16 70.485 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 88.265 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R65" (id 0) (at 153.67 88.265 90))
    (property "Value" "24R" (id 1) (at 161.29 88.265 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 90.043 90))
    (property "Datasheet" "~" (id 3) (at 137.16 88.265 0))
    (property "comment" "" (id 4) (at 137.16 88.265 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 88.265 0))
    (property "supplier" "TME" (id 6) (at 137.16 88.265 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 137.16 57.785 90) (mirror x) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R53" (id 0) (at 153.67 57.785 90))
    (property "Value" "24R" (id 1) (at 161.29 57.785 90))
    (property "Footprint" "Resistor_SMD:R_MiniMELF_MMA-0204" (id 2) (at 137.16 56.007 90))
    (property "Datasheet" "~" (id 3) (at 137.16 57.785 0))
    (property "comment" "" (id 4) (at 137.16 57.785 0))
    (property "PN" "SMDMM0204-24R" (id 5) (at 137.16 57.785 0))
    (property "supplier" "TME" (id 6) (at 137.16 57.785 0))
    (pin "1")
    (pin "2")
  )
)
